"Non-MLRA Soil Survey Area"|"MT065"|"Musselshell County, Montana"||09/01/1996 00:00:00|"certified, all components"|05/27/2020 13:49:23|"MT065 - Musselshell County, Montana 
The ""880F nvc5-Cabbart-Delpoint loams, moist, 4 to 45 percent slopes"" mapunit was combined with the ""880F 2yk1m-Cabbart-Delpoint loams, moist, 4 to 45 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart-Delpoint loams, moist, 4 to 45 percent slopes"" EVAL project"".
The ""287F ckjk-Cabbart, moist-Delpoint, dry loams, 8 to 45 percent slopes"" mapunit was combined with the ""287F 2yk1c-Cabbart, moist-Delpoint, dry loams, 8 to 45 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart, moist-Delpoint, dry loams, 8 to 45 percent slopes"" EVAL project"".
The ""280D ckj4-Cabbart, moist-Delpoint, dry loams, 4 to 15 percent slopes"" mapunit was combined with the ""280D 2yk1b-Cabbart, moist-Delpoint, dry loams, 4 to 15 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart, moist-Delpoint, dry loams, 4 to 15 percent slopes"" EVAL project"".
The ""189C cgj8-Rentsac-Cabbart complex, 2 to 15 percent slopes"" mapunit was combined with the ""189C 2yk1j-Rentsac-Cabbart complex, 2 to 15 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Rentsac-Cabbart complex, 2 to 15 percent slopes"" EVAL project"".
The ""354C cgj0-Bonfri-Cabbart loams, 2 to 8 percent slopes"" mapunit was combined with the ""354C 2yk18-Bonfri-Cabbart loams, 2 to 8 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Bonfri-Cabbart loams, 2 to 8 percent slopes"" EVAL project"".
The ""354B 20r65-Bonfri-Cabbart loams, 0 to 4 percent slopes"" mapunit was combined with the ""354B 2yk17-Bonfri-Cabbart loams, 0 to 4 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Bonfri-Cabbart loams, 0 to 4 percent slopes"" EVAL project"".
The ""881F nvc6-Cabbart, dry-Delpoint, dry-Rock outcrop complex, 8 to 65 percent slopes"" mapunit was combined with the ""881F 2yk1d-Cabbart, dry-Delpoint, dry-Rock outcrop complex, 8 to 65 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart, dry-Delpoint, dry-Rock outcrop complex, 8 to 65 percent slopes"" EVAL project"".
The tabular database was edited and populated according to guidance in Exhibits A and B of National Instruction (NI-305), and Part 610 of the National Soil Survey Handbook. Any spatial data edits were certified correct by the Soil Survey region, State Soil Scientist (SSS), and by the National Digitizing Center. The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s) and in the Project Correlation table.
The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s) and in the Project Correlation table.
This dataset also contains the following changes:
A. All spatial data was processed and refreshed to reduce geometry size and coordinate precision of SSURGO, and to standardize the vertice density of our surveys. It is estimated that this reduced the geometry size of SSURGO to around 10 GB. This is an over 50% reduction in size, and will therefore greatly optimize our data for future usage and efficiency in publishing and interacting with it, at all levels. 
B. The five national interpretations listed below are new and revised:
FOR - Windthrow Hazard (New for FY20)
FOR - Mechanical Planting Suitability
FOR - Mechanical Site Preparation (Deep)
FOR - Mechanical Site Preparation (Surface)
FOR - Potential Erosion Hazard (Off-Road/Off-Trail)
C. Recalculated all national and local interpretations for all components."|"13028"|"70008"|"69910"
