"MT604"|8|"BLD"|"Boulder"|A spot where 0.1 to 3 percent of the surface cover is rock fragments that are greater than 26 inches in diameter where the surrounding soil has less than 0.01 percent of the surface cover of stones. Typically 1 to 5 acres.|"262162"
"MT604"|8|"ESB"|"Escarpment, bedrock"|A relatively continuous and steep slope or cliff, which generally is produced by erosion but can be produced by faulting, that breaks the general continuity of more gently sloping land surfaces. Exposed earthy material is hard or soft bedrock.|"262163"
"MT604"|8|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel. Typically less than 5 acres.|"262164"
"MT604"|8|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments. Typically less than 5 acres.|"262165"
"MT604"|8|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically less than 5 acres.|"262166"
"MT604"|8|"SAL"|"Saline spot"|An area where the surface layer has an electrical conductivity of 8 mmhos cm more than the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has an electrical conductivity of 2 mmhos cm or less. Typically less than 5 acres.|"262167"
"MT604"|8|"SLI"|"Slide or slip"|A prominent landform scar or ridge caused by fairly recent mass movement or descent of earthy material resulting from failure of earth or rock under shear stress along one or several surfaces. Typically less than 5 acres.|"262168"
"MT604"|8|"SLP"|"Short, steep slope"|A narrow area of soil having slopes that are at least two slope classes steeper than the slope class of the surrounding map unit.|"262169"
"MT604"|8|"SOD"|"Sodic spot"|An area where the surface layer has a sodium adsorption ratio that is at least 10 more than that of the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has a sodium adsorption ratio of 5 or less. Typically less than 5 acres.|"262170"
"MT604"|8|"STN"|"Stony spot"|A spot where 0.01 to 0.1 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surrounding soil has no surface stones. Typically less than 5 acres.|"262171"
"MT604"|8|"STV"|"Very stony spot"|A spot where 0.1 to 3.0 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surface of the surrounding soil is covered by less than 0.01 percent stones. Typically 1 to 5 acres.|"262172"
"MT604"|8|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically less than 5 acres.|"262173"
