"MT610"|9|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically 1 to 5 acres.|"262243"
"MT610"|9|"STV"|"Very stony spot"|A spot where 0.1 to 3.0 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surface of the surrounding soil is covered by less than 0.01 percent stones. Typically 1 to 5 acres.|"262242"
"MT610"|9|"STN"|"Stony spot"|A spot where 0.01 to 0.1 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surrounding soil has no surface stones. Typically 1 to 5 acres.|"262241"
"MT610"|9|"SLP"|"Short, steep slope"|A narrow area of soil having slopes that are at least two slope classes steeper than the slope class of the surrounding map unit.|"262240"
"MT610"|9|"SAN"|"Sandy spot"|A spot where the surface layer is loamy fine sand or coarser in areas where the surface layer of the named soils in the surrounding map unit is very fine sandy loam or finer. Typically 1 to 5 acres.|"262239"
"MT610"|9|"SAL"|"Saline spot"|An area where the surface layer has an electrical conductivity of 8 mmhos cm more than the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has an electrical conductivity of 2 mmhos cm or less. Typically 1 to 5 acres.|"262238"
"MT610"|9|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically 1 to 5 acres.|"262237"
"MT610"|9|"MIS"|"Miscellaneous water"|Small, constructed bodies of water that are used for industrial, sanitary, or mining applications and that contain water most of the year. Typically 1 to 5 acres.|"262236"
"MT610"|9|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments. Typically 1 to 5 acres.|"262235"
"MT610"|9|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel. Typically 1 to 5 acres.|"262234"
"MT610"|9|"ESB"|"Escarpment, bedrock"|A relatively continuous and steep slope or cliff, which generally is produced by erosion but can be produced by faulting, that breaks the general continuity of more gently sloping land surfaces. Exposed earthy material is hard or soft bedrock.|"262233"
"MT610"|9|"BDY"|"Bouldery"|Areas of surface rock fragments greater than 23 inches in diameter. Typically less than 5 acres.|"262232"
