"MT611"|8|"ESO"|"Escarpment, nonbedrock"|A relatively continuous and steep slope or cliff, which generally is produced by erosion but can be produced by faulting, that breaks the continuity of more gently sloping land surfaces.  Exposed earthy material is nonsoil or very shallow soil.|"297548"
"MT611"|8|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel.  Typically__to__acres.|"297549"
"MT611"|8|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments.  Typically__to__acres.|"297550"
"MT611"|8|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically__to__acres.|"297551"
"MT611"|8|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically__to__acres.|"297552"
