"MT613"|7|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel.  Typically__to__acres.|"295296"
"MT613"|7|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments.  Typically__to__acres.|"295297"
"MT613"|7|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically__to__acres.|"295298"
"MT613"|7|"SAL"|"Saline spot"|An area where the surface layer has an electrical conductivity of 8 mmhos/cm more than the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has an electrical conductivity of 2 mmhos/cm or less.Typically__to__acres.|"295299"
"MT613"|7|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically__to__acres.|"295300"
