"MT617"|7|"DEP"|"Depression, closed"|A shallow, saucer-shaped area that is slightly lower on the landscape than the surrounding area and that does not have a natural outlet for surface drainage. Typically less than 5 acres.|"287813"
"MT617"|7|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel. Typically less than 5 acres.|"287814"
"MT617"|7|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments. Typically less than 5 acres.|"287815"
"MT617"|7|"LVS"|"Levee"|An embankment that confines or controls water, especially one built along the banks of a river to prevent overflow onto lowlands.|"287816"
"MT617"|7|"MAR"|"Marsh or swamp"|A water saturated, very poorly drained area that is intermittently or permanently covered by water. Sedges, cattails, and rushes are the dominate vegetation in marshes, and trees or shrubs are the dominant vegetation in swamps. Not used in map units where the named soils are poorly drained or very poorly drained. Typically less than 5 acres.|"287817"
"MT617"|7|"MIS"|"Miscellaneous water"|Small, constructed bodies of water that are used for industrial, sanitary, or mining applications and that contain water most of the year. Typically less than 5 acres.|"287818"
"MT617"|7|"MPI"|"Mine or quarry"|An open excavation from which soil and underlying material have been removed and in which bedrock is exposed. Also denotes surface openings to underground mines. Typically less than 5 acres.|"287819"
"MT617"|7|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically less than 5 acres.|"287820"
"MT617"|7|"SAN"|"Sandy spot"|A spot where the surface layer is loamy fine sand or coarser in areas where the surface layer of the named soils in the surrounding map unit is very fine sandy loam or finer. Typically less than 5 acres.|"287821"
"MT617"|7|"SOD"|"Sodic spot"|An area where the surface layer has a sodium adsorption ratio that is at least 10 more than that of the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has a sodium adsorption ratio of 5 or less. Typically less than 5 acres.|"287822"
"MT617"|7|"STN"|"Stony spot"|A spot where 0.01 to 0.1 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surrounding soil has no surface stones. Typically less than 5 acres.|"287823"
"MT617"|7|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically less than 5 acres.|"287824"
"MT617"|7|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically less than 5 acres.|"287825"
