"MT629"|9|"CLA"|"Clay spot"|A spot where the surface texture is silty clay or clay in areas where the surface layer of the soils in the surrounding map unit is sandyloam, loam, silt loam, or coarser.  Typically__to__acres.|"297568"
"MT629"|9|"DEP"|"Depression, closed"|A shallow, saucer-shaped area that is slightly lower on the landscape than the surrounding area and that does not have a natural outlet for surface drainage. Typically__to__acres.|"297569"
"MT629"|9|"ESB"|"Escarpment, bedrock"|A relatively continuous and steep slope or cliff, produced by erosion or faulting, that breaks the general continuity of more gently sloping land surfaces. Exposed material is hard or soft bedrock.|"297570"
"MT629"|9|"ESO"|"Escarpment, nonbedrock"|A relatively continuous and steep slope or cliff, which generally is produced by erosion but can be produced by faulting, that breaks the continuity of more gently sloping land surfaces.  Exposed earthy material is nonsoil or very shallow soil.|"297571"
"MT629"|9|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel.  Typically__to__acres.|"297572"
"MT629"|9|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments.  Typically__to__acres.|"297573"
"MT629"|9|"MAR"|"Marsh or swamp"|A water saturated, very poorly drained area that is intermittently or permanently covered by water. Sedges, cattails, and rushes are the dominate vegetation in marshes, and trees or shrubs are the dominant vegetation in swamps. Not used in map units where the named soils are poorly drained or very poorly drained. Typically__to__acres.|"297574"
"MT629"|9|"MIS"|"Miscellaneous water"|Small, constructed bodies of water that are used for industrial, sanitary, or mining applications and that contain water most of the year. Typically__to__acres.|"297575"
"MT629"|9|"MPI"|"Mine or quarry"|An open excavation from which soil and underlying material have been removed and in which bedrock is exposed. Also denotes surface openings to underground mines. Typically__to__acres.|"297576"
"MT629"|9|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically__to__acres.|"297577"
"MT629"|9|"SOD"|"Sodic spot"|An area where the surface layer has a sodium adsorption ratio that is at least 10 more than that of the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has a sodium adsorption ratio of 5 or less.  Typically__to__acres.|"297578"
"MT629"|9|"STN"|"Stony spot"|A spot where 0.01 to 0.1 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surrounding soil has no surface stones.  Typically__to__acres.|"297579"
"MT629"|9|"STV"|"Very stony spot"|A spot where 0.1 to 3.0 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surface of the surrounding soil is covered by less than 0.01 percent stones. Typically__to__acres.|"297580"
"MT629"|9|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically__to__acres.|"297581"
"MT629"|9|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically__to__ acres.|"297582"
