"MT600"|6|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically 1 to 5 acres.|"262126"
"MT600"|6|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically 1 to 5 acres.|"262125"
"MT600"|6|"STV"|"Very stony spot"|A spot where 0.1 to 3.0 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surface of the surrounding soil is covered by less than 0.01 percent stones. Typically 1 to 5 acres.|"262124"
"MT600"|6|"STN"|"Stony spot"|A spot where 0.01 to 0.1 percent of the soil surface is covered by rock fragments that are more than 10 inches in diameter in areas where the surrounding soil has no surface stones. Typically 1 to 5 acres.|"262123"
"MT600"|6|"SOD"|"Sodic spot"|An area where the surface layer has a sodium adsorption ratio that is at least 10 more than that of the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has a sodium adsorption ratio of 5 or less. Typically 1 to 5 acres.|"262122"
"MT600"|6|"SAL"|"Saline spot"|An area where the surface layer has an electrical conductivity of 8 mmhos cm more than the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has an electrical conductivity of 2 mmhos cm or less. Typically 1 to 5 acres.|"262121"
"MT600"|6|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically 1 to 5 acres.|"262120"
"MT600"|6|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments. Typically 1 to 5 acres.|"262119"
"MT600"|6|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel. Typically 1 to 5 acres.|"262118"
"MT600"|6|"ESO"|"Escarpment, nonbedrock"|A relatively continuous and steep slope or cliff, which generally is produced by erosion but can be produced by faulting, that breaks the continuity of more gently sloping land surfaces. Exposed earthy material is non soil or very shallow soil.|"262117"
"MT600"|6|"BLO"|"Blowout"|A saucer-, cup-, or trough-shaped depression formed by wind erosion on a pre-existing dune or other sand deposit, especially in an area of shifting sand or loose soil or where protective vegetation is disturbed or destroyed. The adjoining accumulation of sand derived from the depression, where recognizable, is commonly included. Blowouts are commonly small. Typically 1 to 5 acres.|"262116"
