"Non-MLRA Soil Survey Area"|"MT041"|"Hill County, Montana"||06/01/1994 00:00:00|"certified, all components"|08/31/2021 23:57:54|"The ""96B ck2k-Fortbenton fine sandy loam, 0 to 4 percent slopes"" mapunit was combined with the ""96B 2sy7v-Fortbenton fine sandy loam, 0 to 4 percent slopes"" map unit as a result of the ""EVAL - MLRA 52 - Fortbenton fine sandy loam, 0 to 4 percent slopes"" EVAL project"".
The ""96C965B ck2l-Fortbenton fine sandy loam, 4 to 8 percent slopes"" ck2g-Fortbenton-Chinook fine sandy loams, 0 to 6 percent slopes"" mapunit was combined with the ""965B 2vysg-Fortbenton-Chinook fine sandy loams, 2 to 8 percent slopes"" map unit as a result of the ""EVAL - MLRA 52 - Fortbenton-Chinook fine sandy loams, 2 to 8 percent slopes"" EVAL project"".
The ""968C ck2h-Fortbenton-Hillon complex, 2 to 8 percent slopes"" mapunit was combined with the ""968C 2vysh-Fortbenton-Hillon complex, 2 to 8 percent slopes"" map unit as a result of the ""EVAL - MLRA 52 - Fortbenton-Hillon complex, 2 to 8 percent slopes"" EVAL project"".
The ""962B ck2d-Fortbenton loam, 0 to 4 percent slopes"" mapunit was combined with the ""962B 2zpd6-Kenilworth-Fortbenton complex, 0 to 4 percent slopes"" map unit as a result of the ""EVAL - MLRA 52 - Kenilworth-Fortbenton complex, 0 to 4 percent slopes"" EVAL project"".
The ""968D ck2j-Hillon-Fortbenton complex, 8 to 25 percent slopes"" mapunit was combined with the ""968D 2vysj-Hillon-Fortbenton complex, 8 to 25 percent slopes"" map unit as a result of the ""EVAL - MLRA 52 - Hillon-Fortbenton complex, 8 to 25 percent slopes"" EVAL project"".
The ""951B ck2b-Kenilworth-Fortbenton fine sandy loams, 0 to 4 percent slopes"" mapunit was combined with the ""951B 2zpd5-Kenilworth-Fortbenton fine sandy loams, 0 to 4 percent slopes"" map unit as a result of the ""EVAL - MLRA 52 - Kenilworth-Fortbenton fine sandy loams, 0 to 4 percent slopes"" EVAL project"".
The tabular database was edited and populated according to guidance in Exhibits A and B of National Instruction (NI-305), and Part 610 of the National Soil Survey Handbook. Any spatial data edits were certified correct by the Soil Survey region GIS specialist, State Soil Scientist (SSS), and by the National Digitizing Center. The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s), and in the Project Correlation tables.

The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s) and in the Project Correlation table.

This dataset also contains the following changes:

A. Recalculated all national, regional, and local interpretations for all components.

B. The dataset was populated with data elements needed to support the Water Erosion Prediction Project (WEPP).

C. The eleven national interpretations listed below are new for Fiscal Year 2021 or revised:

AGR - Industrial Hemp for Fiber and Seed Production
DHS - Emergency Land Disposal of Milk
ENG - Deep Infiltration Systems
ENG - Lined Retention Systems
ENG - Shallow Infiltration Systems
ENG - Unlined Retention Systems
ENG - Ground-based Solar Arrays, Ballast Anchor Systems
ENG - Ground-based Solar Arrays, Soil-based Anchor Systems
FOR - Drought Vulnerable Soils
SOH - Dynamic Soil Properties Response to Biochar
SOH - Limitations for Aerobic Soil Organisms"|"13025"|"74508"|"74410"
