"Non-MLRA Soil Survey Area"|"MT065"|"Musselshell County, Montana"||09/01/1996 00:00:00|"certified, all components"|09/01/2021 00:22:25|"The ""87B-21 cgll-Delpoint, calcareous-Cabbart loams, 2 to 8 percent slopes"" mapunit was combined with the ""87B 2zg60-Delpoint, calcareous-Cabbart loams, 2 to 8 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Delpoint, calcareous-Cabbart loams, 2 to 8 percent slopes"" EVAL project"".
The ""181D21 cgj5-Cabbart-Crago-Delpoint complex, 4 to 15 percent slopes"" mapunit was combined with the ""181D 2zg5v-Cabbart-Crago-Delpoint complex, 4 to 15 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart-Crago-Delpoint complex, 4 to 15 percent slopes"" EVAL project"".
The ""84C-21 cglf-Cabbart-Yawdim-Delpoint complex, 4 to 15 percent slopes"" mapunit was combined with the ""84C 2zg5w-Cabbart-Yawdim-Delpoint complex, 4 to 15 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart-Yawdim-Delpoint complex, 4 to 15 percent slopes"" EVAL project"".
The ""84D-21 cglg-Cabbart-Yawdim-Badland complex, 4 to 35 percent slopes"" mapunit was combined with the ""84D 2zg5z-Cabbart-Yawdim-Badland complex, 4 to 35 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Cabbart-Yawdim-Badland complex, 4 to 35 percent slopes"" EVAL project"".
The ""39C-21 cgk3-Delpoint, calcareous-Cabbart-Yamacall, calcareous, loams, 4 to 15 percent slopes"" mapunit was combined with the ""39C 2zg5s-Delpoint, calcareous-Cabbart-Yamacall, calcareous, loams, 4 to 15 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A - Delpoint, calcareous-Cabbart-Yamacall, calcareous, loams, 4 to 15 percent slopes"" EVAL project"".
The ""287D ckjj-Delpoint, dry-Cabbart, moist loams, 2 to 8 percent slopes"" mapunit was combined with the ""287D 2zg5r-Delpoint, dry-Cabbart, moist loams, 2 to 8 percent slopes"" map unit as a result of the ""EVAL - MLRA 58A- Delpoint, dry-Cabbart, moist loams, 2 to 8 percent slopes"" EVAL project"".
The tabular database was edited and populated according to guidance in Exhibits A and B of National Instruction (NI-305), and Part 610 of the National Soil Survey Handbook. Any spatial data edits were certified correct by the Soil Survey region GIS specialist, State Soil Scientist (SSS), and by the National Digitizing Center. The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s), and in the Project Correlation tables.

The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s) and in the Project Correlation table.

This dataset also contains the following changes:

A. Recalculated all national, regional, and local interpretations for all components.

B. The dataset was populated with data elements needed to support the Water Erosion Prediction Project (WEPP).

C. The eleven national interpretations listed below are new for Fiscal Year 2021 or revised:

AGR - Industrial Hemp for Fiber and Seed Production
DHS - Emergency Land Disposal of Milk
ENG - Deep Infiltration Systems
ENG - Lined Retention Systems
ENG - Shallow Infiltration Systems
ENG - Unlined Retention Systems
ENG - Ground-based Solar Arrays, Ballast Anchor Systems
ENG - Ground-based Solar Arrays, Soil-based Anchor Systems
FOR - Drought Vulnerable Soils
SOH - Dynamic Soil Properties Response to Biochar
SOH - Limitations for Aerobic Soil Organisms"|"13028"|"74512"|"74414"
