"MT065"|12|"CLA"|"Clay spot"|A spot where the surface texture is silty clay or clay in areas where the surface layer of the soils in the surrounding map unit is sandyloam, loam, silt loam, or coarser. Typically less than 5 acres.|"286179"
"MT065"|12|"GPI"|"Gravel pit"|An open excavation from which soil and underlying material have been removed and used, without crushing, as a source of sand or gravel. Typically less than 5 acres.|"286180"
"MT065"|12|"GRA"|"Gravelly spot"|A spot where the surface layer has more than 35 percent, by volume, rock fragments that are mostly less than 3 inches in diameter in an area that has less than 15 percent rock fragments. Typically less than 5 acres.|"286181"
"MT065"|12|"MAR"|"Marsh or swamp"|A water saturated, very poorly drained area that is intermittently or permanently covered by water. Sedges, cattails, and rushes are the dominate vegetation in marshes, and trees or shrubs are the dominant vegetation in swamps. Not used in map units where the named soils are poorly drained or very poorly drained. Typically less than 5 acres.|"286182"
"MT065"|12|"ROC"|"Rock outcrop"|An exposure of bedrock at the surface of the earth. Not used where the named soils of the surrounding map unit are shallow overbedrock or where Rock outcrop is a named component of the map unit. Typically less than 5 acres.|"286183"
"MT065"|12|"SAL"|"Saline spot"|An area where the surface layer has an electrical conductivity of 8 mmhos cm more than the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has an electrical conductivity of 2 mmhos cm or less. Typically less than 5 acres.|"286184"
"MT065"|12|"SAN"|"Sandy spot"|A spot where the surface layer is loamy fine sand or coarser in areas where the surface layer of the named soils in the surrounding map unit is very fine sandy loam or finer. Typically less than 5 acres.|"286185"
"MT065"|12|"SOD"|"Sodic spot"|An area where the surface layer has a sodium adsorption ratio that is at least 10 more than that of the surface layer of the named soils in the surrounding map unit. The surface layer of the surrounding soils has a sodium adsorption ratio of 5 or less. Typically less than 5 acres.|"286186"
"MT065"|12|"WAT"|"Perennial water"|Small, natural or constructed lakes, ponds, or pits that contain water most of the year. Typically less than 5 acres.|"286187"
"MT065"|12|"WET"|"Wet spot"|A somewhat poorly drained to very poorly drained area that is at least two drainage classes wetter than the named soils in the surrounding map unit. Typically less than 5 acres.|"286188"
