"MT025"|"Fallon County, Montana"|25|08/28/2025 16:37:17|23|08/28/2025 16:37:17|08/27/2025 20:36:12|"certified, all components"|"MT025
The 160F2tz7m-Cabbart-Rock outcrop-Yawdim complex, warm, 15 to 70 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 55E2wbz1-Twilight-Blacksheep fine sandy loams, 15 to 45 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 86C2vdkf-Yamacall loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 160F2tz7m-Cabbart-Rock outcrop-Yawdim complex, warm, 15 to 70 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 85C2tvlq-Ethridge silty clay loam, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 260E2vdkl-Cambeth-Cabbart-Yawdim complex, 15 to 25 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 70C2wbyc-Busby fine sandy loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 85A2wbyp-Ethridge silty clay loam, warm, 0 to 2 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 86D2wbxd-Yamacall loam, warm, 8 to 15 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 78C2wby4-Kobase silty clay loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 86A2wbx9-Yamacall loam, warm, 0 to 2 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 86D2wbxd-Yamacall loam, warm, 8 to 15 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 170D2wbyy-Busby-Twilight-Blacksheep fine sandy loams, 8 to 35 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 170D2wbyy-Busby-Twilight-Blacksheep fine sandy loams, 8 to 35 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 78C2wby4-Kobase silty clay loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 93C2vcqr-Lonna silt loam, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The tabular database was edited and populated according to guidance in Exhibits A and B of National Instruction (NI-305), and Part 610 of the National Soil Survey Handbook. Any spatial data edits were certified correct by the Soil Survey region GIS specialist, State Soil Scientist (SSS), and by the National Digitizing Center. The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s), and in the Project Correlation tables.

The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s) and in the Project Correlation table.

This dataset also contains the following changes:

Recalculated all national, regional, and local interpretations for all components.

Eleven national interpretations listed below are new or have been updated for Fiscal Year 2025:

ENG - Shallow Excavations
ENG - Construction Materials; Reclamation
FOR - Hand Planting Suitability
SOH - Dynamic Soil Properties Response to Biochar
PFAS - Movement Classes in Soils
FOR - Construction Limitations for Haul Roads/Log Landings
FOR - Harvest Equipment Operability
FOR - Potential Seedling Mortality
FOR - Potential Erosion Hazard (Road/Trail)
FOR - Road Suitability (Natural Surface)
FOR - Log Landing Suitability
There is seventeen new or updated regional interpretations listed below are new for Fiscal Year 2025.

VIN - Vinifera Wine Grape Site Desirability (Long)
VIN - Vinifera Wine Grape Site Desirability (Long to Medium)
VIN - Vinifera Wine Grape Site Desirability (Short to Med)
VIN - Vinifera Wine Grape Site Desirability (Short)
VIN - Hybrid Wine Grape Varieties Site Desirability (Long)
VIN - Hybrid Wine Grape Varieties Site Desirability (Medium)
VIN - Hybrid Wine Grape Varieties Site Desirability (Short)
VIN - American Wine Grape Varieties Site Desirability (VLng)
VIN - American Wine Grape Varieties Site Desirability (Med)
VIN - American Wine Grape Varieties Site Desirability (Sht)
VIN - Muscadine Wine Grape Site Desirability (Very Long)
VIN - American Wine Grape Varieties Site Desirability (Long)
CPS - Cover Crop (340)
CPS - Brush Management (314)
CPS - Heavy Use Area Protection (561)
FOR - Longleaf Pine Suitability
AGR - Suitability for Savanna Restoration
"|"<metadata><idinfo><citation><citeinfo><origin>
U.S. Department of Agriculture, Natural Resources
Conservation Service
</origin><pubdate>20250828</pubdate><title>
Soil Survey Geographic (SSURGO) database for
Fallon County, Montana
</title><pubinfo><pubplace>Fort Worth, Texas</pubplace><publish>
U.S. Department of Agriculture, Natural Resources
Conservation Service
</publish></pubinfo><othercit>mt025</othercit><onlink>URL:http://DataGateway.nrcs.usda.gov/</onlink></citeinfo></citation><descript><abstract>
This data set is a digital soil survey and generally is the most
detailed level of soil geographic data developed by the National
Cooperative Soil Survey. The information was prepared by digitizing
maps, by compiling information onto a planimetric correct base
and digitizing, or by revising digitized maps using remotely
sensed and other information.

This data set consists of georeferenced digital map data and
computerized attribute data. The map data are in a soil survey area
extent format and include a detailed, field verified inventory
of soils and miscellaneous areas that normally occur in a repeatable
pattern on the landscape and that can be cartographically shown at
the scale mapped. A special soil features layer (point and line
features) is optional. This layer displays the location of features
too small to delineate at the mapping scale, but they are large
enough and contrasting enough to significantly influence use and
management. The soil map units are linked to attributes in the
National Soil Information System relational database, which gives
the proportionate extent of the component soils and their properties.
</abstract><purpose>
SSURGO depicts information about the kinds and distribution of
soils on the landscape. The soil map and data used in the SSURGO
product were prepared by soil scientists as part of the National
Cooperative Soil Survey.
</purpose><supplinf>
Digital versions of hydrography, cultural features, and other
associated layers that are not part of the SSURGO data set may be
available from the primary organization listed in the Point of
Contact.
</supplinf></descript><timeperd><timeinfo><rngdates><begdate>19980626</begdate><enddate>20250828</enddate></rngdates></timeinfo><current>publication date</current></timeperd><status><progress>Complete</progress><update>As needed</update></status><spdom><bounding><westbc>-104.906</westbc><eastbc>-104.044</eastbc><northbc>46.685</northbc><southbc>45.882</southbc></bounding></spdom><keywords><theme><themekt>None</themekt><themekey>soil survey</themekey><themekey>soils</themekey><themekey>Soil Survey Geographic</themekey><themekey>SSURGO</themekey></theme><place><placekt>USGS Geographic Names Information System (GNIS)</placekt><placekey>Montana</placekey><placekey>Fallon County</placekey><placekey>Snider Hill Quadrangle</placekey><placekey>Flasted Hill Quadrangle</placekey><placekey>Dutchman Hills Quadrangle</placekey><placekey>Terrell Creek Quadrangle</placekey><placekey>Scole School Quadrangle</placekey><placekey>Webster Quadrangle</placekey><placekey>Willard SE Quadrangle</placekey><placekey>Medicine Rocks State Park Quadrangle</placekey><placekey>Piney Butte Quadrangle</placekey><placekey>Webster NE Quadrangle</placekey><placekey>Webster NW Quadrangle</placekey><placekey>Willard Quadrangle</placekey><placekey>Sportsman Pond Quadrangle</placekey><placekey>Seven-up Butte Quadrangle</placekey><placekey>Harmon Butte Quadrangle</placekey><placekey>Nelson Butte Quadrangle</placekey><placekey>Hooky Dam Quadrangle</placekey><placekey>Waterhole Creek Quadrangle</placekey><placekey>Buffalo Reservoir Quadrangle</placekey><placekey>Baker Quadrangle</placekey><placekey>South Sandstone Reservoir Quadrangle</placekey><placekey>Little Pine Creek Quadrangle</placekey><placekey>T G Creek Quadrangle</placekey><placekey>Bracket Butte SE Quadrangle</placekey><placekey>Foundation Spring Quadrangle</placekey><placekey>Badland Draw Quadrangle</placekey><placekey>Morris Butte Quadrangle</placekey><placekey>Baker NE Quadrangle</placekey><placekey>Baker NW Quadrangle</placekey><placekey>Plevna Quadrangle</placekey><placekey>Westmore Quadrangle</placekey><placekey>Ismay South Quadrangle</placekey><placekey>Bracket Butte Quadrangle</placekey><placekey>Ollie Quadrangle</placekey><placekey>Shell Butte Quadrangle</placekey><placekey>Rush Hall Reservoir Quadrangle</placekey><placekey>Lawrence Creek East Quadrangle</placekey><placekey>Lawrence Creek West Quadrangle</placekey><placekey>Ayer Spring Quadrangle</placekey><placekey>Carlyle Quadrangle</placekey><placekey>Carlyle NW Quadrangle</placekey><placekey>Cap Rock Quadrangle</placekey><placekey>Rocking Chair Butte Quadrangle</placekey><placekey>Ayer Spring NE Quadrangle</placekey><placekey>Dorothy Draw Quadrangle</placekey></place></keywords><accconst>None</accconst><useconst>
The U.S. Department of Agriculture, Natural Resources Conservation
Service, should be acknowledged as the data source in products
derived from these data.

This data set is not designed for use as a primary regulatory tool
in permitting or citing decisions, but may be used as a reference
source. This is public information and may be interpreted by
organizations, agencies, units of government, or others based on
needs; however, they are responsible for the appropriate
application. Federal, State, or local regulatory bodies are not to
reassign to the Natural Resources Conservation Service any
authority for the decisions that they make. The Natural Resources
Conservation Service will not perform any evaluations of these maps
for purposes related solely to State or local regulatory programs.

Photographic or digital enlargement of these maps to scales greater
than at which they were originally mapped can cause misinterpretation
of the data. If enlarged, maps do not show the small areas of
contrasting soils that could have been shown at a larger scale. The
depicted soil boundaries, interpretations, and analysis derived from
them do not eliminate the need for onsite sampling, testing, and
detailed study of specific sites for intensive uses. Thus, these data
and their interpretations are intended for planning purposes only.
Digital data files are periodically updated. Files are dated, and
users are responsible for obtaining the latest version of the data.
</useconst><ptcontac><cntinfo><cntorgp><cntorg>U.S. Department of Agriculture, Natural Resources Conservation Service</cntorg></cntorgp><cntpos>State Soil Scientist</cntpos><cntaddr><addrtype>mailing address</addrtype><address>Room 443</address><address>10 East Babcock Street</address><address/><address/><city>Bozeman</city><state>MT</state><postal>59715-4704</postal></cntaddr><cntvoice>406-587-6834</cntvoice><cnttdd/><cntfax/><cntemail>Nathan.Parry@usda.gov</cntemail></cntinfo></ptcontac></idinfo><dataqual><attracc><attraccr>
The attribute accuracy is tested by manual
comparison of the source with hard copy plots and/or symbolized
display of the map data on an interactive computer graphic system.
Selected attributes that cannot be visually verified on plots or
on screen are interactively queried and verified on screen. In
addition, the attributes are tested against a master set of valid
attributes. All attribute data conform to the attribute codes in
the signed classification and correlation document and amendment(s).
</attraccr></attracc><logic>
Certain node/geometry and topology GT- polygon/chain relationships
are collected or generated to satisfy topological requirements
(the GT-polygon corresponds to the soil delineation). Some of these
requirements include: chains must begin and end at nodes, chains
must connect to each other at nodes, chains do not extend through
nodes, left and right GT-polygons are defined for each chain
element and are consistent throughout, and the chains representing
the limits of the file are free of gaps. The tests of logical
consistency are performed using vendor software. All internal
polygons are tested for closure with vendor software and are checked
on hard copy plots. All data are checked for common soil lines (i.e.,
adjacent polygons with the same label). Edge locations generally do
not deviate from centerline to centerline by more than 0.01 inch.
The survey-wide coverage of Fallon County have been edge matched to
soil surveys of Custer County, Carter County, Wibaux County, Prairie
County, Montana soil surveys. The survey-wide coverage of Fallon
County has been edge matched to the soil survey of Golden Valley County,
North Dakota.
</logic><complete>
A map unit is a collection of areas defined and named in terms of
their soil components or miscellaneous areas or both. Each map
unit differs in some respect from all others in a survey area and
each map unit has a symbol that uniquely identifies the map unit
on a soil map. Each individual area, point, or line so identified
on the map is a delineation.

Soil Scientists identify small areas of soils or miscellaneous areas
that have properties and behavior significantly different than the
named soils in the surrounding map unit. These minor components
may be indicated as special features. If they have a minimal effect
on use and management, or could not be precisely located, they may
not be indicated on the map.

A map unit has specified kinds of soils or miscellaneous areas
(map unit components), each with a designated range in
proportionate extent. Map units include one or more kinds of soil
or miscellaneous area. Miscellaneous areas are areas that have little
or no recognizable soil.

Specific National Cooperative Soil Survey standards and procedures
were used in the classification of soils, design and name of map
units, and location of special soil features. These standards are
outlined in Agricultural Handbook 18, Soil Survey Manual, 1993,
USDA, NRCS; Agricultural Handbook 436, Soil Taxonomy, 1995,
USDA, NRCS; and all Amendments; Keys to Soil Taxonomy,
(current issue) USDA, NRCS; National Soil Survey
Handbook, title 430-VI,(current issue) USDA, NRCS.

The actual composition and interpretive purity of the map unit
delineations were based on data collected by scientists during
the course of preparing the soil maps. Adherence to National
Cooperative Soil Survey standards and procedures is based on
peer review, quality control, and quality assurance. Quality
control is outlined in the memorandum of understanding for the
soil survey area and in documents that reside with the Natural
Resources Conservation Service state soil scientist. Four kinds
of map units are used in soil surveys: consociations, complexes,
associations, and undifferentiated groups.

Consociations - Consociations are named for the dominant soil.
In a consociation, delineated areas use a single name from the
dominant component in the map unit. Dissimilar components are
minor in extent. The soil component in a consociation may be
identified at any taxonomic level. Soil series is the lowest
taxonomic level. A consociation that is named as a miscellaneous
area is dominantly that kind of area and minor components do not
significantly affect the use of the map unit. The total amount of
dissimilar inclusions of other components in a map unit generally
does not exceed about 15 percent if limiting and 25 percent if
nonlimiting. A single component of a dissimilar limiting inclusion
generally does not exceed 10 percent if very contrasting.

Complexes and associations - Complexes and associations consist
of two or more  dissimilar components that occur in a regularly
repeating pattern. The total amount of other dissimilar components
is minor extent. The following arbitrary rule determines whether
complex or association is used in the name. The major components
of an association can be separated at the scale of mapping. In
either case, because the major components are sufficiently different
in morphology or behavior, the map unit cannot be called a
consociation. In each delineation of a complex or an association,
each major component is normally present though their proportions
may vary appreciably from one delineation to another. The total
amount of inclusions in a map unit that are dissimilar to any of
the major components does not exceed 15 percent if limiting and
25 percent if nonlimiting. A single kind of dissimilar limiting
inclusion usually does not exceed 10 percent.

Undifferentiated groups - Undifferentiated groups consist of two
or more components that are not consistently associated
geographically and, therefore, do not always occur together in
the same map delineation. These components are included in the
same named map unit because their use and management are the same
or very similar for common uses. Generally they are grouped together
because some common feature, such as steepness, stoniness, or
flooding, determines their use and management. If two or more
additional map units would serve no useful purpose, they may be
included in the same unit. Each delineation has at least one of the
major components, and some may have all of them. The same principles
regarding the proportion of minor components that apply to
consociations also apply to undifferentiated groups. The same
principles regarding proportion of inclusion apply to
undifferentiated groups as to consociations.

Minimum documentation consists of three complete soil profile
descriptions that are collected for each soil added to the legend,
one additional per 3,000 acres mapped; three 10 observation
transects for each map unit, one additional 10 point transect per
3,000 acres.

A defined standard or level of confidence in the interpretive
purity of the map unit delineations is attained by adjusting the
kind and intensity of field investigations. Field investigations
and data collection are carried out in sufficient detail to name
map units and to identify accurately and consistently areas of
about 5 acres.
</complete><posacc><horizpa><horizpar>
The accuracy of these digital data is based upon their
compilation to base maps that meet National Map
Accuracy Standards at a scale of 1 inch equals 1,000
feet. The difference in positional accuracy between the
soil boundaries and special soil features locations in the
field and their digitized map locations is unknown. The
locational accuracy of soil delineations on the ground varies
with the transition between map units.

For example, on long gently sloping landscapes the transition
occurs gradually over many feet. Where landscapes change
abruptly from steep to level, the transition will be very
narrow. Soil delineation boundaries and special soil features
generally were digitized within 0.01 inch of their locations on
the digitizing source. The digital map elements are edge matched
between data sets. The data along each quadrangle edge are
matched against the data for the adjacent quadrangle. Edge
locations generally do not deviate from centerline to centerline
by more than 0.01 inch.
</horizpar></horizpa></posacc><lineage><srcinfo><srccite><citeinfo><origin>U.S. Geological Survey</origin><pubdate>1972-1991</pubdate><title>multiple 7.5 minute topographic quadrangles</title><geoform>map</geoform><pubinfo><pubplace>Reston, Virginia</pubplace><publish>U.S. Geological Survey</publish></pubinfo></citeinfo></srccite><srcscale>24000</srcscale><typesrc>paper</typesrc><srctime><timeinfo><rngdates><begdate>1975</begdate><enddate>1992</enddate></rngdates></timeinfo><srccurr>publication date</srccurr></srctime><srccitea>USGS1</srccitea><srccontr>
base maps used for compilation of soils, special
features, and as reference in compilation of cultural features
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Soil Conservation Service
</origin><pubdate>1975</pubdate><title>multiple photographs</title><geoform>remote sensing image</geoform><pubinfo><pubplace>UNKNOWN</pubplace><publish>Mark Hurd Corporation</publish></pubinfo></citeinfo></srccite><srcscale>24000</srcscale><typesrc>paper</typesrc><srctime><timeinfo><rngdates><begdate>1975</begdate><enddate>1989</enddate></rngdates></timeinfo><srccurr>publication date</srccurr></srctime><srccitea>NRCS1</srccitea><srccontr>
base materials (stereo pairs) for field
mapping and development of a special features layer
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>U.S. Geological Survey</origin><pubdate>1984</pubdate><title>quad centered photography</title><geoform>remote sensing image</geoform><pubinfo><pubplace>Denver, Colorado</pubplace><publish>U.S. Geological Survey</publish></pubinfo></citeinfo></srccite><srcscale>24000</srcscale><typesrc>stable-base material</typesrc><srctime><timeinfo><rngdates><begdate>1984</begdate><enddate>1990</enddate></rngdates></timeinfo><srccurr>publication date</srccurr></srctime><srccitea>USGS2</srccitea><srccontr>
source of soil lines, map unit labels, and
special soil features
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>unpublished material</pubdate><title>annotation overlay</title><geoform>map</geoform></citeinfo></srccite><srcscale>24000</srcscale><typesrc>stable-base material</typesrc><srctime><timeinfo><rngdates><begdate>1991</begdate><enddate>1992</enddate></rngdates></timeinfo><srccurr>1992</srccurr></srctime><srccitea>NRCS2</srccitea><srccontr>scan source</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>unpublished material</pubdate><title>
DLG DOC TAB directories of the soil survey of
Fallon County, Montana
</title><geoform>map</geoform></citeinfo></srccite><srcscale>24000</srcscale><typesrc>magnetic tape</typesrc><srctime><timeinfo><sngdate><caldate>1998</caldate></sngdate></timeinfo><srccurr>1998</srccurr></srctime><srccitea>NRCS3</srccitea><srccontr>
digital information containing area and special
soil features, attribute data and metadata for SSURGO
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>1998</pubdate><title>
Soil Survey Geographic (SSURGO) database for Fallon
County, Montana
</title><geoform>map</geoform><pubinfo><pubplace>Ft. Worth, Texas</pubplace><publish>
U.S. Department of Agriculture,
Natural Resources Conservation Service,
National Cartography and Geospatial Center
</publish></pubinfo></citeinfo></srccite><srcscale>24000</srcscale><typesrc>online</typesrc><srctime><timeinfo><sngdate><caldate>2002</caldate></sngdate></timeinfo><srccurr>publication date</srccurr></srctime><srccitea>NRCS4</srccitea><srccontr>SSURGO data used for revisions</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture, Natural Resources
Conservation Service
</origin><pubdate>2002</pubdate><title>
Soil Survey Geographic (SSURGO) database for Fallon County,
Montana
</title><geoform>map</geoform><pubinfo><pubplace>Ft. Worth, Texas</pubplace><publish>
U.S. Department of Agriculture, Natural Resources
Conservation Service, National Cartography and
Geospatial Center
</publish></pubinfo></citeinfo></srccite><srcscale>24000</srcscale><typesrc>online</typesrc><srctime><timeinfo><sngdate><caldate>2003</caldate></sngdate></timeinfo><srccurr>publication date</srccurr></srctime><srccitea>NRCS5</srccitea><srccontr>source used to for revisions</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>U.S. Department of Agriculture</origin><pubdate>2002</pubdate><title>
National Soil Information System (NASIS) database for
Fallon County, Montana
</title><geoform>tabular digital data</geoform><pubinfo><pubplace>Fort Collins, Colorado</pubplace><publish>
U.S. Department of Agriculture, Natural Resources
Conservation Service, Information Technology Center
</publish></pubinfo></citeinfo></srccite><typesrc>online</typesrc><srctime><timeinfo><sngdate><caldate>2003</caldate></sngdate></timeinfo><srccurr>export certification date</srccurr></srctime><srccitea>NRCS6</srccitea><srccontr>tabular data linked to spatial soil data</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>unpublished material</pubdate><title>MrSID compressed image for Fallon County, Montana</title><geoform>map</geoform></citeinfo></srccite><srcscale>24000</srcscale><typesrc>CD-ROM</typesrc><srctime><timeinfo><sngdate><caldate>2003</caldate></sngdate></timeinfo><srccurr>2003</srccurr></srctime><srccitea>NRCS7</srccitea><srccontr>NAD83 ortho imagery used for quality control</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>unpublished material</pubdate><title>
ARC INTERCHANGE files for the survey of Fallon County,
Montana
</title><geoform>map</geoform></citeinfo></srccite><srcscale>24000</srcscale><typesrc>CD-ROM</typesrc><srctime><timeinfo><sngdate><caldate>2003</caldate></sngdate></timeinfo><srccurr>2003</srccurr></srctime><srccitea>NRCS8</srccitea><srccontr>
digital information containing area and special
soil features for evaluation for SSURGO
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>2003</pubdate><title>National Soil Information System (NASIS) data base</title><geoform>unknown</geoform></citeinfo></srccite><srcscale>24000</srcscale><typesrc>database</typesrc><srctime><timeinfo><sngdate><caldate>2003</caldate></sngdate></timeinfo><srccurr>publication date</srccurr></srctime><srccitea>NASIS</srccitea><srccontr>attribute (tabular) information</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture,
Natural Resources Conservation Service
</origin><pubdate>unpublished material</pubdate><title>
ArcGIS geodatabase files for the soil survey of
Fallon County, Montana
</title><geoform>digitized vector data</geoform></citeinfo></srccite><srcscale>24000</srcscale><typesrc>online</typesrc><srctime><timeinfo><sngdate><caldate>20091204</caldate></sngdate></timeinfo><srccurr>2009</srccurr></srctime><srccitea>NRCS9</srccitea><srccontr>
digital information containing area and special
soil features for evaluation
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture, Natural Resources
Conservation Service
</origin><pubdate>2009</pubdate><title>
National Soil Information System (NASIS) database for
Fallon County, Montana
</title><geoform>tabular digital data</geoform><pubinfo><pubplace>Fort Collins, Colorado</pubplace><publish>
U.S. Department of Agriculture, Natural Resources
Conservation Service, Information Technology Center
</publish></pubinfo></citeinfo></srccite><typesrc>online</typesrc><srctime><timeinfo><sngdate><caldate>20091204</caldate></sngdate></timeinfo><srccurr>export certification date</srccurr></srctime><srccitea>NRCS10</srccitea><srccontr>
map unit legend used for comparison to spatial
map unit labels
</srccontr></srcinfo><srcinfo><srccite><citeinfo><origin>
U.S. Department of Agriculture, Natural Resources
Conservation Service
</origin><pubdate>unpublished material</pubdate><title>region 5 soils geodatabase</title><geoform>file geodatabase</geoform></citeinfo></srccite><typesrc>vector digital data</typesrc><srctime><timeinfo><rngdates><begdate>2006</begdate><enddate>2018</enddate></rngdates></timeinfo><srccurr>SSURGO publication date</srccurr></srctime><srccitea>NRCS11</srccitea><srccontr>Source of digital revision - recreated yearly</srccontr></srcinfo><procstep><procdesc>
Field procedures for the second order
soil survey included plotting of soil boundaries determined by field
observation and by interpretation of remotely sensed data. Boundaries
were verified at closely spaced intervals, and the soils in each
delineation were identified by traversing and transecting the
landscape. Soil scientists described and sampled the soils, analyzed
samples in the laboratory, and statistically analyzed the data. The
classification and map unit names were finalized at the final
correlation in March 1991.
</procdesc><srcused>NRCS1</srcused><procdate>1991</procdate></procstep><procstep><procdesc>
Map compilation was completed by soil scientists
on staff at the Natural Resources Conservation Service state office
in Bozeman, Montana.  Soil delineations, labels, and special
features from field sheets were compiled to quad centered
imagery.  Four control points corresponding to the four corners of
the topographic quadrangles were used during compilation of soil
lines, labels and special features from quad centered imagery.
Soil lines, labels and special features were then transferred
to stable-base material.  Sources used for digitizing were
forwarded to the Bozeman State Office State Soil Scientists staff
for digitizing and quality control routines.
</procdesc><srcused>USGS1, USGS2, NRCS1, NRCS2</srcused><procdate>1992</procdate></procstep><procstep><procdesc>
The annotated overlays were raster scanned on a
LDS4000 scanner at 300 dots per inch by the Natural Resources
Conservation Service Montana Digitizing Unit.  Four corners of
the 7.5 minute quadrangle were used during data collection in
LtPlus, Version 4.02.  The data were created and maintained in
North American Datum of 1927 by cartographic technicians.  The
processing, raster editing, map neatline development, labeling,
vector conversion and editing of the soils were accomplished in
LtPlus, Version 4.02.  County boundaries were digitized from
the 7.5 minute topographic quadrangles.  Special soil features
were manually digitized using GRASS 4.12.  The LtPlus maps were
imported to LT4X, Version 4.02, edge matched and exported to
GRASS 4.13.  The soils and special features maps were then
exported to Digital Line Graph, Optional (DLG-3) files using
the v.export command.  The data were forwarded to certification
staff at the Montana Digitizing Unit.
</procdesc><srcused>NRCS1, NRCS2, NRCS3, USGS1</srcused><procdate>1998</procdate></procstep><procstep><procdesc>
DLG DOC and TAB directories were imported
into ARC/INFO, Version 7.0.4 by certification staff at the Montana
Digitizing Unit in Bozeman, Montana.  ARCEDIT was used to correct
label and node match errors, and to remove extra vertices.  New
DLG-3's were written.  The data were forwarded to the National
Cartography and Geospatial Center in Ft. Worth, Texas for
archiving and distribution.
</procdesc><srcused>NRCS2, NRCS3</srcused><procdate>1998</procdate></procstep><procstep><procdesc>
The Map Unit Interpretations Record data base
was developed by the Natural Resources Conservation Service soil
scientists according to national standards and updated to reflect
changes in interpretations.
</procdesc><srcused>NRCS1</srcused><procdate>1998</procdate></procstep><procstep><procdesc>
The National Soil Information System data base
was developed by Natural Resources Conservation Service soil
scientists according to national standards.
</procdesc><srcused>NRCS1</srcused><procdate>2002</procdate></procstep><procstep><procdesc>
The online SSURGO data was imported to ARC/INFO,
Version 7.21 at the Natural Resources Conservation Service, Montana
Digitizing Unit.  The SSURGO data were processed through revised
evaluation program macros dated October 1998. ARCEDIT was used to
correct a label mismatch, and to correct three labels on the
quadrangle named Baker from water to miscellaneous water.  New
DLG-3's were written.  The data were forwarded to the National
Cartography and Geospatial Center in Ft. Worth, Texas for archiving
and distribution.
</procdesc><srcused>NRCS1, NRCS4, NRCS6</srcused><procdate>2002</procdate></procstep><procstep><procdesc>
The survey-wide coverages from the online SSURGO data, and MrSID
compressed imagery were imported to ARC GEODATABASE by a soil
scientist on staff at the Natural Resources Conservation Service
state office. Edit tools were used to revise temporal areas.
Small water areas were considered for special spot features.  ARC
INTERCHANGE files were written, then forwarded to certification
staff at the Montana Digitizing Unit for verification for SSURGO.
</procdesc><srcused>NRCS5, NRCS6, NRCS7, NRCS8</srcused><procdate>2003</procdate></procstep><procstep><procdesc>
The ARC INTERCHANGE files were imported to
ARC/INFO, Version 8.2 by certification staff at the Montana Digitizing
Unit.  The data were processed through evaluation macros dated June
2003. The map unit labels were linked to the National Soil Information
System data base.  ARCEDIT was used to adjust special feature linear
geometry and to correct to special point feature labels on the
Lawrence Creek East Quadrangle and the Rush Hall Reservoir Quadrangle.
Boundaries were updated to adjacent survey areas. The data were
forwarded to the National Cartography and Geospatial Center in Ft.
Worth, Texas for archiving and distribution.
</procdesc><srcused>NRCS2, NRCS6, NRCS8</srcused><procdate>2003</procdate></procstep><procstep><procdesc>
The 6/06 Update - The attribute data has been updated with soil horizon
structure and slope shape.  In addition a National Non-tech description
is included as a component text note GenSoil.  Interpretations have been updated.
</procdesc><srcused>NASIS</srcused><procdate>20050607</procdate></procstep><procstep><procdesc>
The full set of Military and Department of Homeland Security Interpretations
were added.
</procdesc><srcused>NASIS</srcused><procdate>20060602</procdate></procstep><procstep><procdesc>
The 7/27/09 update reflects adding/refreshing 11 natioanal
BLM interpretations. No edits to spatial data.
</procdesc><srcused>NASIS</srcused><procdate>20090727</procdate></procstep><procstep><procdesc>
The survey-wide ArcGIS geodatabase from the online SSURGO data were
imported to ARC/INFO 9.2 by certification staff at the Montana
Digitizing Unit. Topology errors on the boundary, that were
flagged in prepartation for the National Soils Geospatial Database,
were corrected as directed in the National Bulletin: 430-9-5. The
survey was smoothed to remove excess vertices that were flagged in
preparation for the National Soils Geospatial Database, as directed
in the National Bulletin: 430-9-5. Evaluation macros of June 2004 were
applied to the data. Map unit labels were compared to an approved
map unit legend from the National Soil Information System data base.
ARCGIS was used to join to adjacent survey boundaries and verify previous
adjacent survey joins. The data were uploaded to the soil data
warehouse staging server.
</procdesc><srcused>NRCS9, NRCS10</srcused><procdate>20091204</procdate></procstep><procstep><procdesc>
The 1/6/10 update reflects vertex reduction edits.
No substantive attribute or spatial edits.
This work is to polish the data in preparation for
the transactional National Soils Geodatabase and to
improve GIS performance without impacting data quality.
</procdesc><srcused>NASIS</srcused><procdate>20100106</procdate></procstep><procstep><procdesc>
The 9/17/10 Update includes attribute data calculations for:
Total Fragment Volume, KF-KW, Exchangeable Acidity, HSG, WEG-WEI,
concrete corrosion, Steel corrosion, Tfactor, refresh generated
brief non-tech description.
</procdesc><srcused>NASIS</srcused><procdate>20100917</procdate></procstep><procstep><procdesc>
The spatial data for Fallon County, Montana soil survey area were
downloaded from the Soil Data Mart on October 15, 2012.
The individual shapefiles were appended into a geodatabase for
region 5. The data were processed in ARCGIS 10.1 using a topology
object with a 0.1 meter cluster tolerance for the purpose of
eliminating gaps and overlaps within the region 5 soils geodatabase.
Individual soil survey area data were exported as shapefiles from the
regional geodatabase. A datum transformation from NAD83 to WGS84 using
the NAD_1983_To_WGS_1984_1 datum transformation method was applied to
the data. The data were checked with the SSURGO Evaluation scripts
provided by U.S. Department of Agriculture, Natural Resources
Conservation Service. The shapefiles were uploaded to the soil data
warehouse for archival and distribution.
</procdesc><srcused>NRCS11</srcused><procdate>2013</procdate></procstep><procstep><procdesc>
The L1639B-2qxht-Chinook-Rhame fine sandy loams, 3 to 6 percent slopes
mapunit was edited and improved. The name of the project EDIT - MLRA 58C
Chinook-Rhame fine sandy loams, 3 to 6 percent slopes indicates
what was edited.
</procdesc><srcused>NRCS11</srcused><procdate>20190808</procdate></procstep><procstep><procdesc>
The spatial data for the entire SSURGO database was recertified in October
of 2019 to reduce storage requirements and to improve map display
and geoprocessing performance.  The SSURGO data is internally managed
using 12 Regional Transactional Spatial Databases (RTSD) that are in
an ESRI File Geodatabase format.  The spatial extent of the RTSDs follow the
Soil and Plant Science Division (SPSD) regional administrative boundaries.
The XY coordinate system of this RTSD is USA Contiguous Albers Equal Area
Conic USGS Version WKID: 102039 and has an XY storage precision of 0.001
meters.  The RTSDs were recreated using a reduced storage precision of 0.1
meters to reduce the physical size of the data.  The SSURGO data was also
generalized by removing excess vertices, using a tolerance of 1 meter.
The topology was validated at the CONUS level using a tolerance of 0.2
meters.  This effort directly affects the gSSURGO and gNATSGO product since
these deliverables are in a File Geodatabase format.
</procdesc><srcused>NRCS11</srcused><procdate>2019</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate, upon completion of data quality verification, determined
that the tabular data should be released for official use. A
selected set of map units and components in the soil survey legend was
copied to a staging database, and rating values for selected
interpretations were generated. The list of selected interpretations is
stored in the database table named sainterp.
</procdesc><srcused>NASIS</srcused><procdate>20210902</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate verified that the labels on the digitized soil map units
link to map units in the tabular database, and certified the joined
data sets for release to the Soil Data Warehouse. A system assigned
version number and date stamp were added and the data were copied to
the data warehouse. The tabular data for the map units and components
were extracted from the data warehouse and reformatted into the soil
data delivery data model, then stored in the Soil Data Mart. The spatial
data were copied to the Soil Data Mart without change.
</procdesc><srcused>NASIS</srcused><procdate>20210902</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate, upon completion of data quality verification, determined
that the tabular data should be released for official use. A
selected set of map units and components in the soil survey legend was
copied to a staging database, and rating values for selected
interpretations were generated. The list of selected interpretations is
stored in the database table named sainterp.
</procdesc><srcused>NASIS</srcused><procdate>20230825</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate verified that the labels on the digitized soil map units
link to map units in the tabular database, and certified the joined
data sets for release to the Soil Data Warehouse. A system assigned
version number and date stamp were added and the data were copied to
the data warehouse. The tabular data for the map units and components
were extracted from the data warehouse and reformatted into the soil
data delivery data model, then stored in the Soil Data Mart. The spatial
data were copied to the Soil Data Mart without change.
</procdesc><srcused>NASIS</srcused><procdate>20230825</procdate></procstep><procstep><procdesc>
Minor edits to polygon geometry were made in order to comply with NRCS
cartographic standards. No changes were made to soil polygon attribute
data.
</procdesc><srcused>NASIS</srcused><procdate>20240628</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate, upon completion of data quality verification, determined
that the tabular data should be released for official use. A
selected set of map units and components in the soil survey legend was
copied to a staging database, and rating values for selected
interpretations were generated. The list of selected interpretations is
stored in the database table named sainterp.
</procdesc><srcused>NASIS</srcused><procdate>20240820</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate verified that the labels on the digitized soil map units
link to map units in the tabular database, and certified the joined
data sets for release to the Soil Data Warehouse. A system assigned
version number and date stamp were added and the data were copied to
the data warehouse. The tabular data for the map units and components
were extracted from the data warehouse and reformatted into the soil
data delivery data model, then stored in the Soil Data Mart. The spatial
data were copied to the Soil Data Mart without change.
</procdesc><srcused>NASIS</srcused><procdate>20240820</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate, upon completion of data quality verification, determined
that the tabular data should be released for official use. A
selected set of map units and components in the soil survey legend was
copied to a staging database, and rating values for selected
interpretations were generated. The list of selected interpretations is
stored in the database table named sainterp.
</procdesc><srcused>NASIS</srcused><procdate>20240827</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate verified that the labels on the digitized soil map units
link to map units in the tabular database, and certified the joined
data sets for release to the Soil Data Warehouse. A system assigned
version number and date stamp were added and the data were copied to
the data warehouse. The tabular data for the map units and components
were extracted from the data warehouse and reformatted into the soil
data delivery data model, then stored in the Soil Data Mart. The spatial
data were copied to the Soil Data Mart without change.
</procdesc><srcused>NASIS</srcused><procdate>20240827</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate, upon completion of data quality verification, determined
that the tabular data should be released for official use. A
selected set of map units and components in the soil survey legend was
copied to a staging database, and rating values for selected
interpretations were generated. The list of selected interpretations is
stored in the database table named sainterp.
</procdesc><srcused>NASIS</srcused><procdate>20250828</procdate></procstep><procstep><procdesc>
The Natural Resources Conservation Service State Soil Scientist or
delegate verified that the labels on the digitized soil map units
link to map units in the tabular database, and certified the joined
data sets for release to the Soil Data Warehouse. A system assigned
version number and date stamp were added and the data were copied to
the data warehouse. The tabular data for the map units and components
were extracted from the data warehouse and reformatted into the soil
data delivery data model, then stored in the Soil Data Mart. The spatial
data were copied to the Soil Data Mart without change.
</procdesc><srcused>NASIS</srcused><procdate>20250828</procdate></procstep></lineage></dataqual><spdoinfo><direct>Vector</direct></spdoinfo><spref><horizsys><geograph><latres>0.000001</latres><longres>0.0000001</longres><geogunit>decimal degrees</geogunit></geograph><geodetic><horizdn>World Geodetic System 1984</horizdn><ellips>World Geodetic System 1984</ellips><semiaxis>6378137.00000</semiaxis><denflat>298.257222</denflat></geodetic></horizsys></spref><eainfo><detailed><enttyp><enttypl>Special Soil Features</enttypl><enttypd>
Special Soil Features represent soil, miscellaneous area, or landform
features that are too small to be digitized as soil delineations
(area features).
</enttypd><enttypds>Agricultural Handbook 18, Soil Survey Manual, 1993, USDA, SCS.</enttypds></enttyp><attr><attrlabl>Special Soil Features Codes</attrlabl><attrdef>
Special Soil Features labels represent specific Special Soil
Features. These features are identified with a descriptive
label. The label is assigned to the point or line assigned
to represent the feature on maps.
</attrdef><attrdefs>
Agricultural Handbook 18, Soil Survey Manual, 1993, USDA, SCS;
National Soil Survey Handbook, Title 430-VI, part 647
(current issue), USDA, NRCS.
</attrdefs><attrdomv><codesetd><codesetn>
Classification and Correlation of the Soils of Fallon County,
Montana
</codesetn><codesets>
U.S. Department of Agriculture, Natural Resources
Conservation Service
</codesets></codesetd></attrdomv></attr></detailed><overview><eaover>
Map Unit Delineations are closed polygons that may be dominated
by a single soil or miscellaneous area component plus allowable
similar or dissimilar soils, or they can be geographic mixtures
of groups of soils or soils and miscellaneous areas.

The map unit symbol uniquely identifies each closed map unit
delineation. Each symbol corresponds to a map unit name. The
map unit key is used to link to information in the National
Soil Information System tables.

Map Unit Delineations are described by the National Soil
Information System database. This attribute database gives the
proportionate extent of the component soils and the properties for
each soil. The database contains both estimated and measured data
on the physical and chemical soil properties and soil
interpretations for engineering, water management, recreation,
agronomic, woodland, range, and wildlife uses of the soil.

The National Soil Information System database contains static
metadata. It documents the data structure and includes such
information as what tables, columns, indexes, and relationships
are defined as well as a variety of attributes of each of these
database objects. Attributes include table and column
descriptions and detailed domain information.

The National Soil Information System database also contains a
distribution metadata. It records the criteria used for selecting
map units and components for inclusion in the set of distributed
data.

Special features are described in the feature table.  It includes an
area symbol, feature label, feature name, and feature description for
each special and ad hoc feature in the survey area.
</eaover><eadetcit>
Soil Taxonomy: A basic system of soil classification for making and
interpreting soil surveys. Agricultural Handbook 436, 1999, USDA, SCS.

Keys to Soil Taxonomy (current issue), USDA, SCS.

National Soil Survey Handbook, Title 430-VI, part 647 (current
issue), USDA, NRCS.

Agricultural Handbook 18, Soil Survey Manual, 1993, USDA, SCS.
</eadetcit></overview></eainfo><distinfo><distrib><cntinfo><cntorgp><cntorg>
U.S. Department of Agriculture, Natural
Resources Conservation Service, National
Geospatial Center of Excellence
</cntorg></cntorgp><cntaddr><addrtype>mailing and physical address</addrtype><address>501 West Felix Street, Building 23</address><city>Fort Worth</city><state>Texas</state><postal>76115</postal></cntaddr><cntvoice>800 672 5559</cntvoice><cnttdd>202 720 2600</cnttdd><cntfax>817 509 3469</cntfax></cntinfo></distrib><resdesc>Fallon County, Montana SSURGO</resdesc><distliab>
Although these data have been processed successfully on a computer
system at the U.S. Department of Agriculture, no warranty expressed
or implied is made by the Agency regarding the utility of the data
on any other system, nor shall the act of distribution constitute
any such warranty. The U.S. Department of Agriculture will warrant
the delivery of this product in computer readable format, and will
offer appropriate adjustment of credit when the product is determined
unreadable by correctly adjusted computer input peripherals, or
when the physical medium is delivered in damaged condition. Request
for adjustment of credit must be made within 90 days from the date
of this shipment from the ordering site.

The U.S. Department of Agriculture, nor any of its agencies are
liable for misuse of the data, for damage, for transmission of
viruses, or for computer contamination through the distribution of
these data sets. The U.S. Department of Agriculture (USDA) prohibits
discrimination in all its programs and activities on the basis of race,
color, national origin, sex, religion, age, disability, political
beliefs, sexual orientation, or marital or family status. (Not all
prohibited bases apply to all programs.)
</distliab><stdorder><digform><digtinfo><formname>ESRI shapefile</formname><formcont>spatial</formcont><transize>45.0</transize></digtinfo><digtopt><onlinopt><computer><networka><networkr>URL:http://DataGateway.nrcs.usda.gov/</networkr></networka></computer><accinstr>
Select desired survey area at above Internet
Web site. An email address is required for receipt of
instructions on retrieval via anonymous FTP. Anticipate a
delay between submission of request at Web site and receipt of
email message.
</accinstr></onlinopt></digtopt></digform><fees>
There is currently no direct charge for requesting data or for
retrieval via FTP.
</fees><ordering>
Visit the above mentioned Internet Web Site, select state or
territory, then select individual soil survey area of interest.
Spatial line data and locations of special feature symbols are in
ESRI ArcGIS shapefile, format. The National Soil Information
System attribute soil data are available in variable length, pipe
delimited, ASCII file format.
</ordering><turnarnd>Typically within four hours</turnarnd></stdorder></distinfo><metainfo><metd>20250828</metd><metc><cntinfo><cntorgp><cntorg>U.S. Department of Agriculture, Natural Resources Conservation Service</cntorg></cntorgp><cntpos>State Soil Scientist</cntpos><cntaddr><addrtype>mailing address</addrtype><address>Room 443</address><address>10 East Babcock Street</address><address/><address/><city>Bozeman</city><state>MT</state><postal>59715-4704</postal></cntaddr><cntvoice>406-587-6834</cntvoice><cnttdd/><cntfax/><cntemail>Nathan.Parry@usda.gov</cntemail></cntinfo></metc><metstdn>Content Standard for Digital Geospatial Metadata</metstdn><metstdv>FGDC-STD-001-1998</metstdv></metainfo></metadata>"|"13022"
