"Non-MLRA Soil Survey Area"|"MT025"|"Fallon County, Montana"||12/01/1991 00:00:00|"certified, all components"|08/27/2025 20:36:18|"MT025
The 160F2tz7m-Cabbart-Rock outcrop-Yawdim complex, warm, 15 to 70 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 55E2wbz1-Twilight-Blacksheep fine sandy loams, 15 to 45 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 86C2vdkf-Yamacall loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 160F2tz7m-Cabbart-Rock outcrop-Yawdim complex, warm, 15 to 70 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 85C2tvlq-Ethridge silty clay loam, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 260E2vdkl-Cambeth-Cabbart-Yawdim complex, 15 to 25 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 70C2wbyc-Busby fine sandy loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 85A2wbyp-Ethridge silty clay loam, warm, 0 to 2 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 86D2wbxd-Yamacall loam, warm, 8 to 15 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 78C2wby4-Kobase silty clay loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 86A2wbx9-Yamacall loam, warm, 0 to 2 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 86D2wbxd-Yamacall loam, warm, 8 to 15 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 170D2wbyy-Busby-Twilight-Blacksheep fine sandy loams, 8 to 35 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Garfield County project
The 170D2wbyy-Busby-Twilight-Blacksheep fine sandy loams, 8 to 35 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 78C2wby4-Kobase silty clay loam, warm, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The 93C2vcqr-Lonna silt loam, 2 to 8 percent slopes"" mapunit tabular and/or spatial data was edited to improve the quality of joins between soil survey areas for soil delineations and attributes. as a result of the SI - I - MLRA 58A - ANS mapping in Rosebud County project
The tabular database was edited and populated according to guidance in Exhibits A and B of National Instruction (NI-305), and Part 610 of the National Soil Survey Handbook. Any spatial data edits were certified correct by the Soil Survey region GIS specialist, State Soil Scientist (SSS), and by the National Digitizing Center. The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s), and in the Project Correlation tables.

The SSS certified the data population for all map units, and concurred with correlation of all projects mentioned, as they were documented in Soil Survey Area Legend(s) and in the Project Correlation table.

This dataset also contains the following changes:

Recalculated all national, regional, and local interpretations for all components.

Eleven national interpretations listed below are new or have been updated for Fiscal Year 2025:

ENG - Shallow Excavations
ENG - Construction Materials; Reclamation
FOR - Hand Planting Suitability
SOH - Dynamic Soil Properties Response to Biochar
PFAS - Movement Classes in Soils
FOR - Construction Limitations for Haul Roads/Log Landings
FOR - Harvest Equipment Operability
FOR - Potential Seedling Mortality
FOR - Potential Erosion Hazard (Road/Trail)
FOR - Road Suitability (Natural Surface)
FOR - Log Landing Suitability
There is seventeen new or updated regional interpretations listed below are new for Fiscal Year 2025.

VIN - Vinifera Wine Grape Site Desirability (Long)
VIN - Vinifera Wine Grape Site Desirability (Long to Medium)
VIN - Vinifera Wine Grape Site Desirability (Short to Med)
VIN - Vinifera Wine Grape Site Desirability (Short)
VIN - Hybrid Wine Grape Varieties Site Desirability (Long)
VIN - Hybrid Wine Grape Varieties Site Desirability (Medium)
VIN - Hybrid Wine Grape Varieties Site Desirability (Short)
VIN - American Wine Grape Varieties Site Desirability (VLng)
VIN - American Wine Grape Varieties Site Desirability (Med)
VIN - American Wine Grape Varieties Site Desirability (Sht)
VIN - Muscadine Wine Grape Site Desirability (Very Long)
VIN - American Wine Grape Varieties Site Desirability (Long)
CPS - Cover Crop (340)
CPS - Brush Management (314)
CPS - Heavy Use Area Protection (561)
FOR - Longleaf Pine Suitability
AGR - Suitability for Savanna Restoration
"|"13022"|"90078"|"89979"
