"112C"|"Cambert-Cabba complex, 2 to 8 percent slopes"||5|5.4|38|||"None"|"None"|"0"|4.42|7.95|9.92|10.32|"Well drained"|"Well drained"|"C"|"3"|51|"3"|51|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.153|"Erosion hazard moderate"|"0"|0.85|"342066"
"112D"|"Cabba-Cambert complex, 4 to 15 percent slopes"||10|10.1|38|||"None"|"None"|"0"|4.34|7.24|8.27|8.51|"Well drained"|"Well drained"|"D"||100|"6"|60|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.953|"Erosion hazard severe"|"0"|0.911|"342067"
"113F"|"Badland-Benz-Parchin complex, 0 to 70 percent slopes"||39|23.5|0|||"None"|"None"|"0"|3.41|6.49|10.48|13.76|"Well drained"|"Well drained"|||100|"8"|40|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.299|"Erosion hazard moderate"|"0"|1|"342069"
"114C"|"Carfall-Assinniboine complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.15|8.24|15.68|22.15|"Well drained"|"Well drained"|"B"||55|"3"|62|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.073|"Erosion hazard moderate"|"0"|0.075|"342070"
"114D"|"Carfall-Assinniboine complex, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|4.14|8.23|15.65|22.17|"Well drained"|"Well drained"|"B"||91|"4"|97|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.071|"Erosion hazard severe"|"0"|0.641|"342071"
"119D"|"Zeona-Blacksheep-Rock outcrop complex, 4 to 15 percent slopes"||10|10|36|||"None"|"None"|"0"|3.09|5.26|8.09|10.72|"Well drained"|"Well drained"|"D"||94|"6"|75|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.612|"Erosion hazard severe"|"0"|0.95|"342072"
"11C"|"Benz clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.02|5.89|11.48|16.97|"Well drained"|"Well drained"|"C"||91|"6"|85|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.179|"Erosion hazard moderate"|"0"|0.925|"342073"
"121C"|"Parchin-Bullock complex, 2 to 8 percent slopes"||5|5.2|71|||"None"|"None"|"0"|3.81|6.97|10.28|10.57|"Well drained"|"Well drained"|"D"||98|"4"|54|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.159|"Erosion hazard moderate"|"0"|0.993|"342074"
"122C"|"Varney-Gerdrum complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.93|7.01|12.43|17.38|"Well drained"|"Well drained"|"B"|"3"|61|"3"|61|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.171|"Erosion hazard moderate"|"0"|0.416|"342075"
"128D"|"Winifred silty clay loam, 4 to 15 percent slopes"||10|9.9|79|||"None"|"None"|"0"|4.05|7.73|11.9|11.94|"Well drained"|"Well drained"|"D"||100|"4"|88|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.944|"Erosion hazard severe"|"0"|1|"342077"
"135B"|"Pachel loam, 0 to 4 percent slopes"||2|2.4||||"None"|"None"|"0"|4.45|8.86|13.63|17.63|"Well drained"|"Well drained"|"B"||88|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.118|"Erosion hazard slight"|"0"|0.072|"342082"
"L3197F"|"Badland, 9 to 150 percent slopes"||80|73.9|5|||"None"|"None"|"0"|1.33|1.65|2.07|2.49|||||100|"8"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|1|"Not rated"|"0"|0.54|"342084"
"E1333C"|"Vebar-Cohagen fine sandy loams, 6 to 9 percent slopes"||8|7.9|43|||"None"|"None"|"0"|3.87|7.09|10.05|11.13|"Well drained"|"Well drained"|"B"||100|"4"|64|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.039|"Erosion hazard moderate"|"0"|0.766|"342086"
"142D"|"Reeder-Cabba loams, 4 to 15 percent slopes"||10|10|36|||"None"|"None"|"0"|4.36|7.64|9.56|9.84|"Well drained"|"Well drained"|"C"|"4"|60|"4"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.373|"Erosion hazard severe"|"0"|0.856|"342089"
"142E"|"Reeder-Cabba loams, 15 to 45 percent slopes"||25|26|28|||"None"|"None"|"0"|4.32|6.91|8.42|8.74|"Well drained"|"Well drained"|"C"|"6"|50|"6"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.942|"Erosion hazard severe"|"0"|0.955|"342090"
"145A"|"Daglum-Adger complex, 0 to 2 percent slopes"||1|1|109|||"None"|"None"|"0"|3.5|6.46|12.16|15.18|"Well drained"|"Well drained"|"C"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.161|"Erosion hazard slight"|"1"|1|"342091"
"145C"|"Daglum-Adger complex, 2 to 8 percent slopes"||5|5|109|||"None"|"None"|"0"|3.5|6.46|12.14|15.14|"Well drained"|"Well drained"|"C"||95|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.153|"Erosion hazard moderate"|"0"|1|"342092"
"14C"|"Carfall loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.32|8.51|16.55|23.39|"Well drained"|"Well drained"|"B"||88|"3"|94|"Somewhat limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.084|"Erosion hazard moderate"|"0"|0.034|"342093"
"153D"|"Orinoco-Yawdim silty clay loams, 4 to 15 percent slopes"||10|10|38|||"None"|"None"|"0"|4.3|7.23|9.48|9.48|"Well drained"|"Well drained"|"D"||97|"6"|90|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.942|"Erosion hazard severe"|"0"|0.991|"342097"
"154C"|"Creed-Absher complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.68|6.33|10.85|15.26|"Well drained"|"Moderately well drained"|"C"|"4"|55|"4"|59|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.219|"Erosion hazard moderate"|"0"|0.96|"342098"
"155E"|"Blacksheep-Rock outcrop complex, 25 to 50 percent"||38|37.3|33|||"None"|"None"|"0"|3.78|6.49|6.65|6.65|"Well drained"|"Well drained"|"D"||100|"7"|68|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Erosion hazard severe"|"0"|1|"342099"
"156A"|"Havre loam, saline, 0 to 2 percent slopes"||1|1||122|122|"Rare"|"Rare"|"0"|2.89|5.72|11.31|16.9|"Moderately well drained"|"Moderately well drained"|"B"|"4"|90|"6"|89|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.1|"Erosion hazard slight"|"1"|0.972|"342100"
"157A"|"Harlake silty clay loam, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|3.99|7.97|15.9|23.84|"Well drained"|"Well drained"|"C"|"4"|92|"4"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.267|"Erosion hazard slight"|"1"|0.98|"342102"
"158D"|"Neldore clay, 4 to 15 percent slopes"||10|9.9|43|||"None"|"None"|"0"|3.59|6.08|6.36|6.48|"Well drained"|"Well drained"|"D"||98|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.51|"Erosion hazard moderate"|"0"|1|"342103"
"15C"|"Weingart clay loam, 2 to 8 percent slopes"||5|5|64|||"None"|"None"|"0"|4.2|6.77|8.5|8.78|"Well drained"|"Well drained"|"D"||94|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.218|"Erosion hazard moderate"|"0"|0.978|"342104"
"160D"|"Cambeth-Lonna silt loams, 8 to 15 percent slopes"||12|12.1|97|||"None"|"None"|"0"|4.57|8.71|16.08|18.81|"Well drained"|"Well drained"|"C"||94|"4"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.942|"Erosion hazard very severe"|"0"|0.661|"342105"
"160E"|"Cabbart-Rock outcrop-Delpoint complex, 15 to 50 percent slopes"||33|29.9|38|||"None"|"None"|"0"|3.79|6.37|6.95|7.16|"Well drained"|"Well drained"|"D"||100|"7"|51|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.987|"Erosion hazard severe"|"0"|1|"342106"
"160F"|"Cabbart-Rock outcrop-Yawdim complex, warm, 15 to 70 percent slopes"||43|39.7|38|||"None"|"None"|"0"|3.98|6.68|7.28|7.74|"Well drained"|"Well drained"|"D"||98|"7"|64|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Erosion hazard severe"|"0"|0.99|"342107"
"161B"|"Glendive sandy loam, saline, 0 to 4 percent slopes"||2|1.9||130|130|"Rare"|"Rare"|"0"|2.58|5.01|9.19|13.37|"Moderately well drained"|"Moderately well drained"|"A"||94|"6"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.02|"Erosion hazard slight"|"2"|0.982|"342109"
"162D"|"Yawdim silty clay loam, 4 to 15 percent slopes"||10|10|38|||"None"|"None"|"0"|4.56|6.79|6.98|6.98|"Well drained"|"Well drained"|"D"||100|"6"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.984|"Erosion hazard severe"|"0"|1|"342111"
"164C"|"Tanna-Ethridge silty clay loams, 2 to 8 percent slopes"||5|4.9|77|||"None"|"None"|"0"|4.28|8.16|13.57|16.72|"Well drained"|"Well drained"|"D"|"3"|87|"3"|87|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.235|"Erosion hazard moderate"|"0"|1|"342113"
"164D"|"Tanna-Ethridge silty clay loams, 8 to 15 percent slopes"||12|11.9|76|||"None"|"None"|"0"|4.27|8.18|13.4|16.03|"Well drained"|"Well drained"|"D"|"4"|55|"4"|85|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.974|"Erosion hazard very severe"|"0"|1|"342114"
"165A"|"Gerdrum-Absher complex, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.67|6.33|10.54|14.54|"Well drained"|"Moderately well drained"|"D"|"6"|60|"6"|63|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.225|"Erosion hazard slight"|"0"|1|"342115"
"165C"|"Gerdrum-Absher complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.4|6.05|10.78|15.39|"Well drained"|"Well drained"|"D"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.31|"Erosion hazard moderate"|"0"|1|"342116"
"166C"|"Ethridge loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.15|8.17|15.96|23.65|"Well drained"|"Well drained"|"C"|"3"|85|"3"|90|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.258|"Erosion hazard moderate"|"0"|0.953|"342117"
"167C"|"Eapa-Yamacall loams, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.53|8.76|17.19|25.29|"Well drained"|"Well drained"|"B"||48|"3"|89|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.175|"Erosion hazard moderate"|"0"|0.075|"342118"
"168B"|"Absher-Gerdrum complex, 0 to 4 percent slopes"||2|2.1||125|125|"None"|"None"|"0"|1.72|2.55|3.85|5.03|"Moderately well drained"|"Moderately well drained"|"D"|"7"|93|"7"|93|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.417|"Erosion hazard slight"|"0"|1|"342120"
"170D"|"Busby-Twilight-Blacksheep fine sandy loams, 8 to 35 percent slopes"||12|19.2|41|||"None"|"None"|"0"|3.29|6.1|9.85|12.69|"Well drained"|"Well drained"|"A"||61|"4"|39|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.44|"Erosion hazard severe"|"0"|0.833|"342124"
"170E"|"Busby-Blacksheep-Rock outcrop complex, 8 to 25 percent slopes"||12|14.8|41|||"None"|"None"|"0"|3.31|6.14|10.04|13.67|"Well drained"|"Well drained"|"D"||58|"6"|46|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.231|"Erosion hazard severe"|"0"|0.802|"342125"
"171C"|"Delpoint-Cabbart complex, 2 to 8 percent slopes"||5|5.1|30|||"None"|"None"|"0"|4.29|7.32|9.8|9.97|"Well drained"|"Well drained"|"C"|"3"|62|"3"|64|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.181|"Erosion hazard moderate"|"0"|0.738|"342126"
"171D"|"Delpoint-Cabbart complex, 8 to 15 percent slopes"||12|12.1|30|||"None"|"None"|"0"|4.32|7.18|9.43|9.68|"Well drained"|"Well drained"|"C"|"4"|53|"4"|56|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.499|"Erosion hazard severe"|"0"|0.812|"342127"
"172C"|"Kremlin-Cabbart complex, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|4.49|7.6|12.97|18.23|"Well drained"|"Well drained"|"B"|"3"|58|"3"|58|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.184|"Erosion hazard moderate"|"0"|0.431|"342128"
"173E"|"Wabek gravelly sandy loam, 8 to 35 percent slopes"||22|21.8||||"None"|"None"|"0"|2.55|4|5.65|7.19|"Excessively drained"|"Excessively drained"|"A"||100|"6"|91|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.819|"Erosion hazard moderate"|"0"|0.992|"342129"
"174C"|"Assinniboine-Ynot complex, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.76|7.38|14.11|20.72|"Well drained"|"Well drained"|"B"|"3"|56|"3"|56|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.045|"Erosion hazard moderate"|"0"|0.22|"342130"
"175A"|"Archin loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.3|8.35|15.24|21.87|"Well drained"|"Well drained"|"C"|"7"|93|"7"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.178|"Erosion hazard slight"|"0"|0.964|"342131"
"175C"|"Archin loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.38|8.56|15.67|22.48|"Well drained"|"Well drained"|"C"||88|"4"|88|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.195|"Erosion hazard moderate"|"0"|0.935|"342132"
"L3025F"|"Lonna-Kirby-Cabbart complex, 2 to 50 percent slopes"||15|21.6|46|||"None"|"None"|"0"|4.16|7.39|11.82|16.09|"Well drained"|"Well drained"|"B"||100|"7"|51|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.57|"Erosion hazard severe"|"0"|0.922|"342133"
"183C"|"Chinook-Assinniboine complex, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.84|7.5|14.42|21.23|"Well drained"|"Well drained"|"A"|"3"|46|"4"|47|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.043|"Erosion hazard moderate"|"0"|0.252|"342138"
"186A"|"Yamacall-Havre loams, 0 to 2 percent slopes"||1|1.2||||"None"|"Rare"|"0"|4.22|8.3|16.19|24.02|"Well drained"|"Well drained"|"B"|"2"|90|"3"|96|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.143|"Erosion hazard slight"|"1"|0.039|"342140"
"186C"|"Yamacall-Havre loams, 2 to 8 percent slopes"||5|4.6||||"None"|"Rare"|"0"|4.23|8.3|16.14|23.92|"Well drained"|"Well drained"|"B"|"3"|73|"3"|93|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.146|"Erosion hazard moderate"|"1"|0.05|"342141"
"191C"|"Bonfri-Cambeth complex, 2 to 8 percent slopes"||5|5.1|81|||"None"|"None"|"0"|4.22|8.23|14.01|14.45|"Well drained"|"Well drained"|"C"|"3"|88|"3"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.185|"Erosion hazard moderate"|"0"|0.954|"342144"
"193C"|"Lonna-Cambeth silt loams, 2 to 8 percent slopes"||4|3.9|89|||"None"|"None"|"0"|5.1|9.99|18.18|22.76|"Well drained"|"Well drained"|"C"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.252|"Erosion hazard moderate"|"0"|0.618|"342146"
"193D"|"Lonna-Cambeth-Cabbart silt loams, 4 to 12 percent slopes"||8|8.2|38|||"None"|"None"|"0"|4.61|8.69|15.17|19.08|"Well drained"|"Well drained"|"B"||100|"4"|81|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.295|"Erosion hazard moderate"|"0"|0.556|"342147"
"20C"|"Alona silt loam, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|4.21|7.94|14.04|19.85|"Well drained"|"Well drained"|"C"|"6"|85|"6"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.272|"Erosion hazard slight"|"0"|0.95|"342151"
"218D"|"Wayden-Barkof complex, 4 to 15 percent slopes"||10|10.7|46|||"None"|"None"|"0"|4.09|7.71|9.32|9.81|"Well drained"|"Well drained"|"D"||62|"6"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.526|"Erosion hazard severe"|"0"|0.968|"342155"
"21C"|"Parchin fine sandy loam, 2 to 8 percent slopes"||5|5.2|71|||"None"|"None"|"0"|3.95|7.36|10.3|10.46|"Well drained"|"Well drained"|"D"||100|"4"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.142|"Erosion hazard moderate"|"0"|0.978|"342156"
"22A"|"Varney loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.02|7.22|13.13|18.91|"Well drained"|"Well drained"|"B"|"3"|88|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.163|"Erosion hazard slight"|"0"|0.122|"342157"
"22C"|"Varney loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.06|7.27|13.36|19.18|"Well drained"|"Well drained"|"B"|"3"|94|"3"|98|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.158|"Erosion hazard moderate"|"0"|0.052|"342158"
"23D"|"Tricart loam, 4 to 15 percent slopes"||10|10.5||||"None"|"None"|"0"|4.26|6.39|10.32|14.13|"Well drained"|"Well drained"|"B"||97|"4"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.11|"Erosion hazard severe"|"0"|0.234|"342159"
"242D"|"Reeder-Dast complex, 4 to 15 percent slopes"||10|10.2|71|||"None"|"None"|"0"|4.1|7.73|11.08|11.4|"Well drained"|"Well drained"|"C"||49|"4"|49|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.13|"Erosion hazard severe"|"0"|0.69|"342162"
"245A"|"Daglum loam, dry, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.49|6.71|13.05|19.37|"Well drained"|"Well drained"|"C"||91|"4"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.19|"Erosion hazard slight"|"0"|1|"342163"
"245C"|"Daglum loam, dry, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|3.52|6.77|13.19|19.59|"Well drained"|"Well drained"|"C"||88|"4"|87|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.183|"Erosion hazard moderate"|"0"|1|"342164"
"251D"|"Abor-Yawdim silty clay loams, 4 to 15 percent slopes"||10|9.9|46|||"None"|"None"|"0"|4.03|7.6|10.14|10.35|"Well drained"|"Well drained"|"C"||97|"4"|63|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.523|"Erosion hazard severe"|"0"|1|"342167"
"253D"|"Orinoco-Weingart complex, 4 to 15 percent slopes"||10|10.2|69|||"None"|"None"|"0"|3.93|6.53|8.67|8.93|"Well drained"|"Well drained"|"D"||97|"6"|91|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.639|"Erosion hazard severe"|"0"|0.974|"342168"
"256A"|"Havre-Harlake complex, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.23|8.39|16.28|24.17|"Well drained"|"Well drained"|"B"|"2"|51|"3"|51|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.159|"Erosion hazard slight"|"2"|0.473|"342171"
"260C"|"Cambeth-Cabbart silt loams, 2 to 8 percent slopes"||5|5.3|30|||"None"|"None"|"0"|4.22|7.44|12.82|13.3|"Well drained"|"Well drained"|"C"|"4"|63|"4"|63|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.259|"Erosion hazard moderate"|"0"|0.656|"342174"
"260D"|"Cabbart-Cambeth silt loams, 8 to 15 percent slopes"||12|11.6|30|||"None"|"None"|"0"|3.96|6.14|9.19|9.49|"Well drained"|"Well drained"|"D"||96|"7"|55|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.947|"Erosion hazard very severe"|"0"|0.828|"342175"
"260E"|"Cambeth-Cabbart-Yawdim complex, 15 to 25 percent slopes"||20|19.7|38|||"None"|"None"|"0"|4.23|7.54|9.8|10.23|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.974|"Erosion hazard very severe"|"0"|0.998|"342176"
"262E"|"Yawdim-Blacksheep-Rock outcrop complex, 15 to 45 percent slopes"||30|29.3|30|||"None"|"None"|"0"|4.21|5.92|6.1|6.1|"Well drained"|"Well drained"|"D"||100|"7"|74|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Erosion hazard very severe"|"0"|1|"342178"
"269C"|"Twilight-Bonfri complex, 2 to 8 percent slopes"||5|5.1|76|||"None"|"None"|"0"|3.73|7.1|11.39|11.7|"Well drained"|"Well drained"|"B"|"4"|63|"4"|63|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.103|"Erosion hazard moderate"|"0"|0.973|"342179"
"269D"|"Twilight-Bonfri complex, 8 to 15 percent slopes"||12|12|76|||"None"|"None"|"0"|3.75|7.13|11.38|11.66|"Well drained"|"Well drained"|"B"||100|"4"|92|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.183|"Erosion hazard severe"|"0"|0.985|"342180"
"270E"|"Busby, gullied-Delpoint-Yawdim complex, 8 to 25 percent slopes"||12|15.8|46|||"None"|"None"|"0"|3.79|7.27|11.22|14.05|"Well drained"|"Well drained"|"A"||90|"6"|65|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.439|"Erosion hazard severe"|"0"|0.812|"342181"
"271D"|"Delpoint-Yamacall loams, 8 to 15 percent slopes"||12|12.1|71|||"None"|"None"|"0"|4.19|8.1|13.24|16.04|"Well drained"|"Well drained"|"C"|"4"|85|"4"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.243|"Erosion hazard severe"|"0"|0.657|"342182"
"275D"|"Archin, gullied-Delpoint complex, 4 to 15 percent slopes"||6|8|71|||"None"|"None"|"0"|4.19|8.16|13.47|17.42|"Well drained"|"Well drained"|"C"|"7"|48|"7"|48|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.201|"Erosion hazard moderate"|"0"|0.939|"342183"
"276F"|"Kirby-Blacksheep-Rock outcrop complex, 25 to 60 percent slopes"||43|37.1|41|||"None"|"None"|"0"|3.18|4.85|5.53|6.01|"Well drained"|"Well drained"|"D"||100|"7"|83|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Erosion hazard severe"|"0"|1|"342184"
"27C"|"Barkof clay, 2 to 8 percent slopes"||5|5.2|69|||"None"|"None"|"0"|3.88|7.51|10.31|10.34|"Well drained"|"Well drained"|"D"|"4"|85|"4"|88|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.475|"Erosion hazard moderate"|"0"|0.997|"342187"
"283C"|"Chinook-Archin complex, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.43|6.84|12.88|18.75|"Well drained"|"Well drained"|"A"|"4"|55|"4"|53|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.061|"Erosion hazard moderate"|"0"|0.686|"342189"
"286C"|"Yamacall-Delpoint loams, warm,  2 to 8 percent slopes"||5|5.3|74|||"None"|"None"|"0"|3.65|7.21|12.49|16.01|"Well drained"|"Well drained"|"B"|"3"|85|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.199|"Erosion hazard moderate"|"0"|0.314|"342190"
"291D"|"Bonfri-Cabbart loams, 8 to 15 percent slopes"||12|11.9|41|||"None"|"None"|"0"|3.96|7.4|11.49|11.93|"Well drained"|"Well drained"|"C"||100|"4"|62|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.179|"Erosion hazard severe"|"0"|0.978|"342193"
"293C"|"Lonna-Cabbart silt loams, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|4.48|7.85|13.93|19.9|"Well drained"|"Well drained"|"B"|"4"|65|"4"|65|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.239|"Erosion hazard moderate"|"0"|0.483|"342194"
"L3161F"|"Lonna-Cabbart silt loams, 6 to 35 percent slopes"||11|15.6|46|||"None"|"None"|"0"|4.94|9.25|14.79|19.5|"Well drained"|"Well drained"|"B"||100|"7"|44|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.414|"Erosion hazard severe"|"0"|0.641|"342195"
"312D"|"Cabba-Dast complex, 8 to 15 percent slopes"||12|12|30|||"None"|"None"|"0"|3.88|5.85|7.64|7.64|"Well drained"|"Well drained"|"D"||100|"6"|53|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.592|"Erosion hazard very severe"|"0"|0.907|"342198"
"E2145B"|"Shambo loam, 2 to 6 percent slopes"||4|3.7||||"None"|"None"|"0"|4.99|9.63|18.4|26.62|"Well drained"|"Well drained"|"B"||100|"2"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.117|"Erosion hazard moderate"|"0"|0.146|"342200"
"E0835A"|"Wyola-Grail silty clay loams, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.83|9|16.86|24.31|"Well drained"|"Well drained"|"C"||100|"2"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.165|"Erosion hazard slight"|"0"|0.962|"342203"
"E0837B"|"Wyola silty clay loam, 2 to 6 percent slopes"||4|3.7||||"None"|"None"|"0"|4.82|9.09|17.24|24.86|"Well drained"|"Well drained"|"C"||100|"2"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.174|"Erosion hazard moderate"|"0"|0.884|"342204"
"E1025B"|"Regent-Wyola silty clay loams, 3 to 6 percent slopes"||5|4.6|91|||"None"|"None"|"0"|4.62|8.52|14.79|16.76|"Well drained"|"Well drained"|"C"||100|"2"|91|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.185|"Erosion hazard moderate"|"0"|1|"342205"
"358D"|"Neldore-Bascovy clays, 4 to 15 percent slopes"||10|9.7|43|||"None"|"None"|"0"|3.7|6.74|9.37|9.61|"Well drained"|"Well drained"|"D"||96|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.536|"Erosion hazard moderate"|"0"|1|"342206"
"E2120A"|"Farnuf loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.69|9.19|17.63|25.27|"Well drained"|"Well drained"|"B"||100|"2"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.136|"Erosion hazard slight"|"0"|0.163|"342207"
"E2120B"|"Farnuf loam, 2 to 6 percent slopes"||4|3.8||||"None"|"None"|"0"|4.68|9.15|17.41|24.94|"Well drained"|"Well drained"|"B"||100|"2"|97|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.132|"Erosion hazard moderate"|"0"|0.154|"342208"
"360D"|"Cabbart-Bascovy complex, 4 to 15 percent slopes"||10|9.8|41|||"None"|"None"|"0"|3.65|6.45|8.62|8.9|"Well drained"|"Well drained"|"D"||100|"6"|96|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.335|"Erosion hazard severe"|"0"|1|"342209"
"369C"|"Twilight-Delpoint complex, 2 to 8 percent slopes"||5|5|71|||"None"|"None"|"0"|3.97|7.67|12.01|12.48|"Well drained"|"Well drained"|"B"|"4"|55|"4"|55|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.098|"Erosion hazard moderate"|"0"|0.426|"342210"
"369D"|"Twilight-Cabbart complex, 8 to 15 percent slopes"||12|12|41|||"None"|"None"|"0"|4.07|6.67|8.84|9.24|"Well drained"|"Well drained"|"B"||97|"4"|58|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.452|"Erosion hazard severe"|"0"|0.868|"342211"
"371E"|"Delpoint-Cooers-Kirby complex, 15 to 35 percent slopes"||25|25|76|||"None"|"None"|"0"|3.59|6.56|10.67|13.22|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.979|"Erosion hazard severe"|"0"|1|"342215"
"375C"|"Archin-Ynot complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.01|7.54|13.96|19.94|"Well drained"|"Well drained"|"C"|"7"|48|"7"|48|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.06|"Erosion hazard moderate"|"0"|0.718|"342216"
"386E"|"Yamacall-Cabbart loams, 15 to 35 percent slopes"||20|21.8|38|||"None"|"None"|"0"|4.25|7.52|12.11|16.44|"Well drained"|"Well drained"|"B"||100|"6"|56|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.728|"Erosion hazard severe"|"1"|1|"342218"
"391C"|"Bonfri-Parchin complex, 2 to 8 percent slopes"||5|5.2|71|||"None"|"None"|"0"|3.91|7.92|12.95|13.4|"Well drained"|"Well drained"|"C"|"3"|51|"3"|48|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.149|"Erosion hazard moderate"|"0"|0.97|"342220"
"393E"|"Lonna-Cambeth-Cabbart silt loams, 12 to 25 percent slopes"||14|16.5|38|||"None"|"None"|"0"|4.52|8.28|14.04|17.99|"Well drained"|"Well drained"|"C"||96|"4"|47|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.955|"Erosion hazard very severe"|"0"|0.981|"342221"
"E1625B"|"Vebar-Parshall fine sandy loams, 3 to 6 percent slopes"||5|4.4|81|||"None"|"None"|"0"|4.25|8.19|13.82|16.63|"Well drained"|"Well drained"|"B"||100|"3"|90|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.037|"Erosion hazard moderate"|"0"|0.412|"342223"
"412E"|"Cabba-Wayden complex, 8 to 45 percent slopes"||27|25.7|30|||"None"|"None"|"0"|4.1|5.26|5.54|5.54|"Well drained"|"Well drained"|"D"||97|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.984|"Erosion hazard very severe"|"0"|1|"342224"
"42C"|"Reeder loam, 2 to 8 percent slopes"||5|5.2|79|||"None"|"None"|"0"|4.52|8.42|13.08|13.46|"Well drained"|"Well drained"|"C"|"3"|89|"3"|89|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.109|"Erosion hazard moderate"|"0"|0.405|"342225"
"45A"|"Daglum loam, 0 to 2 percent slopes"||1|1.1|109|||"None"|"None"|"0"|3.56|6.84|13.29|14.93|"Well drained"|"Well drained"|"C"||95|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.15|"Erosion hazard slight"|"0"|0.98|"342230"
"E0454B"|"Daglum-Rhoades complex, 0 to 6 percent slopes"||3|3.1||130|130|"None"|"None"|"0"|4.9|8.57|14.54|19.77|"Moderately well drained"|"Moderately well drained"|"D"||100|"4"|48|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.155|"Erosion hazard slight"|"0"|1|"342231"
"486D"|"Yamacall-Busby-Blacksheep complex, 4 to 15 percent slopes"||10|10.2|38|||"None"|"None"|"0"|3.89|7.24|12.86|18.35|"Well drained"|"Well drained"|"B"|"4"|69|"4"|72|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.32|"Erosion hazard severe"|"0"|0.49|"342234"
"48D"|"Prego sandy loam, 2 to 15 percent slopes"||9|9.1||||"None"|"None"|"0"|3.13|5.51|7.71|9.8|"Well drained"|"Well drained"|"A"||94|"6"|85|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Not limited"|0.006|"Erosion hazard moderate"|"0"|0.978|"342235"
"50A"|"Chanta loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.11|8.07|11.46|14|"Well drained"|"Well drained"|"B"||94|"3"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.148|"Erosion hazard slight"|"0"|0.94|"342237"
"50C"|"Chanta loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.14|8.13|11.5|14.01|"Well drained"|"Well drained"|"B"||94|"3"|91|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.145|"Erosion hazard moderate"|"0"|0.936|"342238"
"512E"|"Cabba-Dast complex, 15 to 25 percent slopes"||20|20.8|33|||"None"|"None"|"0"|3.6|5.83|8.04|8.04|"Well drained"|"Well drained"|"D"||100|"7"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.538|"Erosion hazard moderate"|"0"|1|"342239"
"51C"|"Abor silty clay loam, 2 to 8 percent slopes"||5|5.2|74|||"None"|"None"|"0"|3.19|6.43|9.75|10.27|"Well drained"|"Well drained"|"C"|"4"|85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.268|"Erosion hazard moderate"|"0"|1|"342240"
"54A"|"Creed loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.75|6.53|11.62|16.59|"Well drained"|"Well drained"|"C"|"4"|85|"4"|88|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.222|"Erosion hazard slight"|"0"|1|"342243"
"54C"|"Creed loam, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|3.74|6.49|11.46|16.38|"Well drained"|"Well drained"|"C"|"4"|87|"4"|89|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.222|"Erosion hazard moderate"|"0"|1|"342244"
"55D"|"Blacksheep-Twilight fine sandy loams, complex,  8 to 15 percent slopes"||12|12|41|||"None"|"None"|"0"|3.32|5.85|7.69|7.99|"Well drained"|"Well drained"|"D"||100|"4"|52|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.041|"Erosion hazard severe"|"0"|0.897|"342245"
"E1423F"|"Flasher-Vebar-Parshall complex, 9 to 35 percent slopes"||25|20.5|36|||"None"|"None"|"0"|3.32|5.76|8.03|9.44|"Somewhat excessively drained"|"Well drained"|"D"||100|"7"|57|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.509|"Erosion hazard moderate"|"0"|0.944|"342246"
"E4121A"|"Havrelon loam, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"8"|4.94|9.5|17.76|25.6|"Well drained"|"Well drained"|"C"||100|"2"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.16|"Erosion hazard slight"|"8"|0.64|"342247"
"57A"|"Harlake silty clay, saline, 0 to 2 percent slopes"||1|1||130|130|"Rare"|"Rare"|"0"|3.54|6.78|12.59|18.41|"Moderately well drained"|"Moderately well drained"|"C"|"6"|85|"6"|89|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.493|"Erosion hazard slight"|"4"|1|"342248"
"586C"|"Yamacall loam, calcareous, 2 to 8 percent"||5|5||||"None"|"None"|"0"|4.23|8.35|16.12|23.55|"Well drained"|"Well drained"|"B"|"4"|91|"4"|91|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.149|"Erosion hazard moderate"|"0"|0.063|"342249"
"586D"|"Yamacall-Delpoint-Cabbart loams, 4 to 15 percent slopes"||10|10.1|38|||"None"|"None"|"0"|3.98|7.34|11.23|13.55|"Well drained"|"Well drained"|"B"|"4"|65|"4"|78|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.225|"Erosion hazard severe"|"0"|0.545|"342250"
"58D"|"Neldore-Rock outcrop complex, 4 to 15 percent slopes"||10|10|38|||"None"|"None"|"0"|3.7|5.74|6.3|6.3|"Well drained"|"Well drained"|"D"||100|"6"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.515|"Erosion hazard severe"|"0"|1|"342251"
"58E"|"Neldore-Rock outcrop complex, warm, 15 to 60 percent slopes"||22|19.3|30|||"None"|"None"|"3"|3.58|4.87|6.04|6.74|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.782|"Erosion hazard severe"|"0"|1|"342252"
"59A"|"Ynot sandy loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.17|6.47|13.05|19.54|"Well drained"|"Well drained"|"A"||91|"4"|89|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.021|"Erosion hazard slight"|"0"|0.449|"342254"
"59C"|"Ynot sandy loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.15|6.44|13.01|19.58|"Well drained"|"Well drained"|"A"||93|"4"|89|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.021|"Erosion hazard moderate"|"0"|0.435|"342255"
"59D"|"Ynot sandy loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.22|6.44|12.74|18.97|"Well drained"|"Well drained"|"A"||91|"4"|94|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.054|"Erosion hazard severe"|"0"|0.646|"342256"
"60C"|"Cambeth silt loam, 2 to 8 percent slopes"||5|5.2|97|||"None"|"None"|"0"|4.61|8.83|16.46|16.96|"Well drained"|"Well drained"|"C"|"4"|85|"4"|88|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.269|"Erosion hazard moderate"|"0"|0.094|"342257"
"60D"|"Cabbart silt loam, 4 to 15 percent slopes"||10|10|38|||"None"|"None"|"0"|3.69|5.6|5.92|5.92|"Well drained"|"Well drained"|"D"||97|"6"|87|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.906|"Erosion hazard severe"|"0"|1|"342258"
"61A"|"Glendive sandy loam, 0 to 2 percent slopes"||1|1.1||||"Rare"|"Rare"|"0"|4.02|7.39|13.43|19.46|"Well drained"|"Well drained"|"A"|"4"|91|"4"|91|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Not limited"|0.016|"Erosion hazard slight"|"3"|0.487|"342260"
"64C"|"Tanna silty clay loam, 2 to 8 percent slopes"||5|5.3|81|||"None"|"None"|"0"|4.24|8.12|12.92|13.16|"Well drained"|"Well drained"|"D"|"3"|88|"3"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.256|"Erosion hazard moderate"|"0"|0.972|"342265"
"65C"|"Gerdrum clay loam, 2 to 8 percent slopes"||4|4||||"None"|"None"|"0"|3.55|6.91|12.68|18.5|"Well drained"|"Well drained"|"D"|"7"|88|"7"|88|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.335|"Erosion hazard moderate"|"0"|0.999|"342267"
"69C"|"Twilight fine sandy loam, 2 to 8 percent slopes"||5|5.2|69|||"None"|"None"|"0"|3.74|7.25|10.1|10.59|"Well drained"|"Well drained"|"B"|"4"|92|"4"|92|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.039|"Erosion hazard moderate"|"0"|0.772|"342272"
"69D"|"Twilight fine sandy loam, 8 to 15 percent slopes"||12|12|69|||"None"|"None"|"0"|3.75|7.26|10.12|10.56|"Well drained"|"Well drained"|"B"||94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.07|"Erosion hazard severe"|"0"|0.783|"342273"
"70C"|"Busby fine sandy loam, warm,  2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.37|6.73|13.44|19.65|"Well drained"|"Well drained"|"A"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.043|"Erosion hazard moderate"|"0"|0.459|"342275"
"70D"|"Busby fine sandy loam, warm, 8 to 15 percent slopes"||12|12.3||||"None"|"None"|"0"|3.34|6.63|13.03|19.01|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.027|"Erosion hazard severe"|"0"|0.672|"342276"
"71C"|"Delpoint loam, warm, 2 to 8 percent slopes"||5|5.5|71|||"None"|"None"|"0"|4.17|8.02|11.43|11.67|"Well drained"|"Well drained"|"C"|"3"|88|"3"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.206|"Erosion hazard moderate"|"0"|0.655|"342278"
"72A"|"Kremlin loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.49|8.9|17.5|26.07|"Well drained"|"Well drained"|"B"|"3"|85|"3"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.156|"Erosion hazard slight"|"0"|0.07|"342279"
"72C"|"Kremlin loam, warm, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.33|8.3|16|23.55|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.171|"Erosion hazard moderate"|"0"|0.055|"342280"
"73E"|"Wabek sandy loam, 8 to 25 percent slopes"||17|17||||"None"|"None"|"0"|3.05|4.59|6.45|8.21|"Excessively drained"|"Excessively drained"|"A"||100|"6"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.133|"Erosion hazard severe"|"0"|0.989|"342281"
"74A"|"Assinniboine sandy clay loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.17|7.97|14.75|21.37|"Well drained"|"Well drained"|"B"|"3"|89|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.065|"Erosion hazard slight"|"0"|0.096|"342282"
"74C"|"Assinniboine sandy clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.15|7.95|14.8|21.53|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.061|"Erosion hazard moderate"|"0"|0.083|"342283"
"75A"|"Archin-Absher complex, 0 to 2 percent slopes"||1|1.2||||"None"|"Rare"|"35"|3.45|6.53|12.43|17.63|"Well drained"|"Moderately well drained"|"C"|"6"|50|"6"|51|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.134|"Erosion hazard slight"|"0"|0.914|"342284"
"75C"|"Archin-Absher complex, 2 to 8 percent slopes"||5|5||||"None"|"Rare"|"35"|3.45|6.53|12.43|17.63|"Well drained"|"Moderately well drained"|"D"|"6"|50|"6"|51|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.134|"Erosion hazard moderate"|"0"|0.934|"342285"
"78C"|"Kobase silty clay loam, warm,  2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.34|8.31|15.96|23.43|"Well drained"|"Well drained"|"C"|"3"|97|"3"|91|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.279|"Erosion hazard moderate"|"0"|0.959|"342287"
"7B"|"Hanly-Ryell fine sandy loams, 0 to 4 percent slopes"||2|1.9||||"Rare"|"Rare"|"0"|3.37|6.44|10.38|14.32|"Somewhat excessively drained"|"Well drained"|"A"|"4"|86|"4"|86|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.042|"Erosion hazard slight"|"4"|0.994|"342289"
"81C"|"Marmarth loam, 2 to 8 percent slopes"||5|5|91|||"None"|"None"|"0"|4.74|8.64|14.86|15.01|"Well drained"|"Well drained"|"C"||94|"3"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.177|"Erosion hazard moderate"|"0"|0.144|"342291"
"82A"|"Floweree silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.71|9.12|17.5|25.84|"Well drained"|"Well drained"|"C"|"2"|89|"3"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.246|"Erosion hazard slight"|"0"|0.321|"342292"
"82C"|"Floweree silt loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.69|9.09|17.48|25.82|"Well drained"|"Well drained"|"C"||88|"3"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.247|"Erosion hazard moderate"|"0"|0.331|"342293"
"L1639A"|"Chinook-Rhame fine sandy loams, 0 to 3 percent slopes"||2|1.9|89|||"None"|"None"|"0"|4.23|8.07|14.47|19.17|"Well drained"|"Well drained"|"A"||100|"3"|81|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.049|"Erosion hazard slight"|"0"|0.359|"342294"
"L1639B"|"Chinook-Rhame fine sandy loams, 3 to 6 percent slopes"||4|4.3|89|||"None"|"None"|"0"|4.21|8.04|14.25|18.32|"Well drained"|"Well drained"|"A"||100|"3"|82|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Erosion hazard moderate"|"0"|0.345|"342295"
"L1355D"|"Rhame-Chinook fine sandy loams, 9 to 15 percent slopes"||12|11.4|89|||"None"|"None"|"0"|4.05|7.72|12.75|15.21|"Well drained"|"Well drained"|"B"||100|"6"|86|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.094|"Erosion hazard moderate"|"0"|0.743|"342296"
"84A"|"Eapa loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.54|8.39|15.84|23.22|"Well drained"|"Well drained"|"B"|"2"|92|"3"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.212|"Erosion hazard slight"|"0"|0.1|"342297"
"84C"|"Eapa loam, 2 to 8 percent slopes"||4|4||||"None"|"None"|"0"|4.71|9.09|18.12|27.13|"Well drained"|"Well drained"|"B"|"2"|91|"3"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.212|"Erosion hazard moderate"|"0"|0.259|"342298"
"84D"|"Eapa loam, 8 to 15 percent slopes"||12|11.5||||"None"|"None"|"0"|4.8|9.21|18.11|26.99|"Well drained"|"Well drained"|"B"||92|"4"|93|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.173|"Erosion hazard severe"|"0"|0.632|"342299"
"85A"|"Ethridge silty clay loam, warm, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.6|9.01|17.37|25.41|"Well drained"|"Well drained"|"C"|"3"|93|"3"|97|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.3|"Erosion hazard slight"|"0"|0.94|"342300"
"85C"|"Ethridge silty clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.58|8.93|17.07|24.81|"Well drained"|"Well drained"|"C"|"3"|93|"3"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.281|"Erosion hazard moderate"|"0"|0.968|"342301"
"86A"|"Yamacall loam, warm, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.12|7.59|14.26|20.84|"Well drained"|"Well drained"|"B"|"2"|85|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.155|"Erosion hazard slight"|"0"|0.135|"342302"
"86C"|"Yamacall loam, warm, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.13|8.11|15.79|23.36|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.172|"Erosion hazard moderate"|"0"|0.122|"342303"
"86D"|"Yamacall loam, warm, 8 to 15 percent slopes"||10|10||||"None"|"None"|"0"|4.13|7.57|13.65|19.29|"Well drained"|"Well drained"|"B"|"2"|85|"3"|88|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.236|"Erosion hazard severe"|"0"|0.248|"342304"
"89A"|"Marvan silty clay, warm, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.65|7.11|13.96|20.8|"Well drained"|"Well drained"|"D"|"6"|85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.496|"Erosion hazard slight"|"0"|1|"342307"
"89C"|"Marvan silty clay, warm, 2 to 8 percent slopes"||4|4.1||||"None"|"None"|"0"|3.65|7.11|13.96|20.8|"Well drained"|"Well drained"|"D"|"6"|85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.496|"Erosion hazard moderate"|"0"|1|"342308"
"8E"|"Cooers-Kirby-Rock outcrop complex, 8 to 25 percent slopes"||17|14.8||||"None"|"None"|"0"|3.57|6.05|10.1|13.78|"Well drained"|"Well drained"|"B"||100|"7"|39|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.247|"Erosion hazard moderate"|"0"|0.85|"342309"
"90C"|"Bascovy clay, 2 to 8 percent slopes"||5|5|86|||"None"|"None"|"0"|3.65|7.15|12.17|12.67|"Well drained"|"Well drained"|"D"|"6"|88|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.488|"Erosion hazard moderate"|"0"|1|"342310"
"91C"|"Bonfri loam, 2 to 8 percent slopes"||5|5|91|||"None"|"None"|"0"|4.17|8.3|14.77|15.2|"Well drained"|"Well drained"|"C"|"3"|91|"3"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.159|"Erosion hazard moderate"|"0"|0.954|"342312"
"91D"|"Bonfri loam, 8 to 15 percent slopes"||10|10.2|91|||"None"|"None"|"0"|4.17|8.31|14.77|15.21|"Well drained"|"Well drained"|"C"||94|"4"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.182|"Erosion hazard severe"|"0"|0.954|"342313"
"93A"|"Lonna silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.5|8.27|15.93|23.78|"Well drained"|"Well drained"|"C"|"4"|88|"4"|88|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.27|"Erosion hazard slight"|"0"|0.509|"342314"
"93C"|"Lonna silt loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.26|8.44|16.39|23.82|"Well drained"|"Well drained"|"C"|"4"|91|"4"|91|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.247|"Erosion hazard moderate"|"0"|0.545|"342315"
"M-W"|"Miscellaneous water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"342321"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"342322"
"254C"|"Creed-Gerdrum complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.23|8.32|16.68|24.98|"Well drained"|"Well drained"|"C"|"4"|45|"6"|85|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.22|"Erosion hazard moderate"|"0"|0.95|"2837927"
"65A"|"Gerdrum clay loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.92|7.36|13.35|19.44|"Well drained"|"Well drained"|"D"|"7"|88|"7"|88|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.251|"Erosion hazard slight"|"0"|0.999|"2837929"
"13F"|"Badland"||39|37.9|0|||||"0"|4.24|7.52|11.55|14.75|||||100|"8"|85|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.9|"Not rated"|"0"|1|"2837972"
"L3101F"|"Badland-Cabbart complex, 6 to 70 percent slopes"||80|63.5|5|||"None"|"None"|"0"|2.34|3.35|3.9|4.4||"Well drained"|||100|"8"|62|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|1|"Not rated"|"0"|0.927|"2837973"
"L3105E"|"Badland-Patent complex, 6 to 25 percent slopes"||80|52.2|5|||"None"|"None"|"0"|2.47|4.22|7.49|10.74||"Well drained"|||100|"8"|57|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|0.947|"Not rated"|"0"|1|"2837974"
"L2601C"|"Boxwell-Cabbart loams, 6 to 9 percent slopes"||8|7.9|38|||"None"|"None"|"0"|4.49|8.29|11.48|12.33|"Well drained"|"Well drained"|"C"||100|"3"|65|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.058|"Erosion hazard moderate"|"0"|0.869|"2876671"
"55E"|"Twilight-Blacksheep fine sandy loams, 15 to 45 percent slopes"||30|26.8|41|||"None"|"None"|"0"|3.37|6.07|8.7|9.83|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.854|"Erosion hazard severe"|"0"|0.917|"2942846"
"L3109F"|"Fleak-Badland complex, 9 to 70 percent slopes"||40|47.4|5|||"None"|"None"|"0"|2.34|3.5|4.1|4.39|"Excessively drained"|"Excessively drained"|"D"||100|"7"|73|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.961|"Erosion hazard severe"|"0"|0.985|"2992076"
"L3107F"|"Cabbart-Badland complex, 6 to 70 percent slopes"||40|43.8|5|||"None"|"None"|"0"|3.54|5.55|6.97|8.29|"Well drained"|"Well drained"|"D"||100|"7"|59|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.945|"Erosion hazard very severe"|"0"|0.877|"2992144"
"E1355D"|"Vebar-Flasher-Tally complex, 9 to 15 percent slopes"||12|11.3|38|||"None"|"None"|"0"|3.58|6.43|9.51|11.14|"Well drained"|"Well drained"|"B"||100|"6"|91|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.262|"Erosion hazard moderate"|"0"|0.78|"2992171"
"176D"|"Kirby-Cabbart complex, 8 to 25 percent slopes"||17|17.3|30|||"None"|"None"|"0"|3.41|4.44|4.86|5.14|"Excessively drained"|"Well drained"|"A"||100|"7"|91|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.48|"Erosion hazard moderate"|"0"|1|"3040367"
"293D"|"Lonna-Cabbart silt loams, 8 to 25 percent slopes"||12|14|30|||"None"|"None"|"0"|4.49|7.36|12.18|16.89|"Well drained"|"Well drained"|"B"||100|"4"|50|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.926|"Erosion hazard very severe"|"0"|0.799|"3040368"
"L1425F"|"Rhame-Fleak complex, 9 to 50 percent slopes"||22|24.4|36|||"None"|"None"|"0"|3.55|6.38|9|9.94|"Well drained"|"Well drained"|"D"||100|"7"|83|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.755|"Erosion hazard moderate"|"0"|0.931|"3040490"
"83C"|"Chinook sandy loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.53|7.04|13.96|20.87|"Well drained"|"Well drained"|"A"|"4"|91|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.034|"Erosion hazard moderate"|"0"|0.468|"3079037"
"83D"|"Chinook sandy loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.55|7.09|13.95|20.69|"Well drained"|"Well drained"|"A"||90|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.033|"Erosion hazard severe"|"0"|0.636|"3079038"
"L4121A"|"Havre silt loam, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"8"|5.17|9.51|17.83|25.83|"Well drained"|"Well drained"|"C"||100|"2"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.138|"Erosion hazard slight"|"8"|0.812|"3079039"
"83A"|"Chinook sandy loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|3.56|7.06|13.98|20.76|"Well drained"|"Well drained"|"A"|"4"|94|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.034|"Erosion hazard slight"|"0"|0.496|"3079065"
"56A"|"Havre loam, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.41|8.72|16.57|24.43|"Well drained"|"Well drained"|"B"|"2"|88|"3"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.099|"Erosion hazard slight"|"3"|0.1|"3079086"
"E0813B"|"Grail-Wyola silty clay loams, 2 to 6 percent slopes"||4|3.7||||"None"|"None"|"0"|4.88|8.98|16.7|24.01|"Well drained"|"Well drained"|"C"||100|"2"|100|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.172|"Erosion hazard moderate"|"0"|1|"3155706"
"L4187A"|"Glendive fine sandy loam, 0 to 2 percent slopes, occasionally flooded"||1|1.2||130|130|"Occasional"|"Occasional"|"5"|4.28|8.32|15.98|21.94|"Moderately well drained"|"Moderately well drained"|"A"||100|"3"|87|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.07|"Erosion hazard slight"|"5"|0.686|"3155863"
"L0836A"|"Ethridge silty clay loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.78|9.03|16.82|24.16|"Well drained"|"Well drained"|"C"||100|"2"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.087|"Erosion hazard slight"|"0"|0.9|"3223491"
"L0836B"|"Ethridge silty clay loam, 2 to 6 percent slopes"||4|4.1||||"None"|"None"|"0"|4.78|9.03|16.82|24.13|"Well drained"|"Well drained"|"C"||100|"2"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.087|"Erosion hazard moderate"|"0"|0.89|"3223492"
"L3007F"|"Kirby-Badland-Patent complex, 9 to 70 percent slopes"||45|45.5|5|||"None"|"None"|"0"|2.89|4.85|7.49|10.1|"Excessively drained"|"Well drained"|"A"||100|"7"|68|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.963|"Erosion hazard severe"|"0"|1|"3223493"
"L1025B"|"Tanna-Ethridge silty clay loams, 3 to 6 percent slopes"||5|4.8|81|||"None"|"None"|"0"|4.47|8.29|13.11|14.71|"Well drained"|"Well drained"|"C"||100|"2"|86|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.124|"Erosion hazard moderate"|"0"|1|"3223495"
"E0515B"|"Rhoades-Daglum complex, 0 to 6 percent slopes"||3|3||130|130|"None"|"None"|"2"|4.65|8.07|13.84|19.02|"Moderately well drained"|"Moderately well drained"|"D"||100|"6"|55|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.168|"Erosion hazard slight"|"0"|1|"3256659"
"L0516B"|"Gerda-Maltese complex, 0 to 6 percent slopes"||3|3||130|130|"None"|"None"|"3"|4.54|8.24|14.82|21.67|"Moderately well drained"|"Moderately well drained"|"D"||100|"6"|58|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.123|"Erosion hazard slight"|"0"|1|"3256660"
"L3237D"|"Patent, gullied, frequently flooded-Sham-Patent complex, 2 to 15 percent slopes"||50|27||||"None"|"Frequent"|"0"|3.96|7.55|14.46|21.26|"Well drained"|"Well drained"|"B"||100|"6"|53|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.589|"Erosion hazard severe"|"3"|0.723|"3256718"
