"Ar"|"Arvada loam, 0 to 3 percent slopes"||2|2.1||||"None"|"None"|"0"|4.15|6.93|11.43|15.93|"Well drained"|"Well drained"|"D"|"6"|96|"6"|96|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.305|"Erosion hazard slight"|"0"|1|"345379"
"Av"|"Arvada complex"||4|3.9||||"None"|"None"|"0"|3.49|6|10.88|15.75|"Well drained"|"Well drained"|"C"|"4"|75|"4"|75|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.276|"Erosion hazard moderate"|"0"|1|"345380"
"Ax"|"Arvada-Laurel complex"||5|4.8||||"None"|"None"|"0"|3.55|6.05|10.76|15.46|"Well drained"|"Well drained"|"D"|"6"|95|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.302|"Erosion hazard moderate"|"0"|1|"345381"
"Ba"|"Badland warm"|||18.8||||||"0"|3.8|6.69|10.13|12.07|||||98||85|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.622|"Not rated"|"0"|0.951|"345382"
"Bb"|"Bainville loam, 8 to 15 percent slopes"||12|11.7|66|||"None"|"None"|"0"|4.67|9.27|12.66|13.42|"Well drained"|"Well drained"|"C"||95|"4"|92|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.889|"Erosion hazard very severe"|"0"|0.762|"345383"
"Bc"|"Bainville loam, 15 to 35 percent slopes"||25|23.6|38|||"None"|"None"|"0"|4.34|6.82|7.82|8.69|"Well drained"|"Well drained"|"D"||94|"7"|84|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.933|"Erosion hazard very severe"|"0"|0.97|"345384"
"Bf"|"Bainville-Tullock complex"||25|23.7|38|||"None"|"None"|"0"|4.24|7.03|8.65|9.5|"Well drained"|"Well drained"|"D"||96|"7"|65|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.934|"Erosion hazard very severe"|"0"|0.959|"345385"
"Bm"|"Bainville-Midway complex, 8 to 15 percent slopes"||12|11.8|66|||"None"|"None"|"0"|4.46|8.75|12.04|12.83|"Well drained"|"Well drained"|"C"||94|"4"|84|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.657|"Erosion hazard very severe"|"0"|0.872|"345386"
"Bn"|"Bainville-Midway complex, 15 to 35 percent slopes"||25|23.3|66|||"None"|"None"|"3"|4.39|8.63|11.94|12.8|"Well drained"|"Well drained"|"D"||93|"6"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.944|"Erosion hazard severe"|"0"|0.96|"345387"
"Bo"|"Bainville-Shale outcrop complex"||50|44.7|46|||"None"|"None"|"0"|4.33|7.82|8.95|9.97|"Well drained"|"Well drained"|"D"||96|"7"|63|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.965|"Erosion hazard very severe"|"0"|0.949|"345388"
"Bs"|"Banks soils"||1|1||54|54|"Occasional"|"Frequent"|"0"|2.49|4.22|7.68|11.14|"Somewhat excessively drained"|"Poorly drained"|"A"|"4"|65|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.251|"Erosion hazard slight"|"5"|1|"345389"
"Bt"|"Beaverton gravelly loam"||2|2.1||||"None"|"None"|"0"|3.85|5.69|7.91|9.86|"Well drained"|"Well drained"|"B"|"4"|90|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.128|"Erosion hazard slight"|"0"|1|"345390"
"Bu"|"Bew clay loam"||2|2||||"None"|"None"|"5"|3.81|7.07|13.54|20.62|"Well drained"|"Well drained"|"C"||100|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.506|"Erosion hazard slight"|"5"|1|"345391"
"Bw"|"Bowdoin clay"||1|1||||"Rare"|"Rare"|"0"|3.09|6.14|12.24|18.34|"Well drained"|"Well drained"|"D"|"6"|90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Erosion hazard slight"|"0"|1|"345392"
"Bx"|"Briggsdale loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.21|8.48|16.96|25.38|"Well drained"|"Well drained"|"C"|"2"|93|"3"|96|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|0.373|"Erosion hazard slight"|"0"|0.953|"345393"
"By"|"Briggsdale loam, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.21|8.54|16.97|25.3|"Well drained"|"Well drained"|"C"|"3"|95|"3"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|0.356|"Erosion hazard moderate"|"0"|0.922|"345394"
"Ca"|"Cherry clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.78|7.55|15.1|22.65|"Well drained"|"Well drained"|"C"|"4"|94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.951|"Erosion hazard slight"|"0"|0.958|"345395"
"Cb"|"Cherry clay, 1 to 3 percent slopes"||2|1.9||||"None"|"None"|"0"|3.78|7.55|15.1|22.65|"Well drained"|"Well drained"|"C"|"4"|94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.951|"Erosion hazard slight"|"0"|0.958|"345396"
"Cc"|"Cherry clay, 3 to 8 percent slopes"||6|5.7||||"None"|"None"|"0"|3.78|7.55|15.1|22.65|"Well drained"|"Well drained"|"C"|"4"|93|"4"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.943|"Erosion hazard moderate"|"0"|0.951|"345397"
"Cd"|"Cherry clay, moderately deep, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.81|7.63|14.9|22.03|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Very limited"|0.929|"Erosion hazard slight"|"0"|0.9|"345398"
"Cf"|"Cherry clay, moderately deep, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|3.79|7.59|14.84|21.94|"Well drained"|"Well drained"|"C"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Very limited"|0.962|"Erosion hazard slight"|"0"|0.95|"345399"
"Cg"|"Cherry clay, moderately deep, 3 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|3.79|7.59|14.84|21.94|"Well drained"|"Well drained"|"C"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Very limited"|0.962|"Erosion hazard moderate"|"0"|0.95|"345400"
"Ch"|"Cherry clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.27|8.68|17.48|25.42|"Well drained"|"Well drained"|"B"|"2"|93|"3"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.274|"Erosion hazard slight"|"0"|0.079|"345401"
"Ck"|"Cherry clay loam, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|4.28|8.72|17.65|25.71|"Well drained"|"Well drained"|"B"|"2"|95|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.284|"Erosion hazard slight"|"0"|0.1|"345402"
"Cm"|"Cherry clay loam, shallow, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.29|8.73|17.61|25.62|"Well drained"|"Well drained"|"B"|"2"|95|"3"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.279|"Erosion hazard slight"|"0"|0.065|"345403"
"Cn"|"Cherry-Laurel clay loams"||1|1.1||||"None"|"None"|"0"|4.13|8.29|16.55|24.06|"Well drained"|"Well drained"|"B"|"2"|82|"3"|82|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.269|"Erosion hazard slight"|"0"|0.189|"345404"
"Cp"|"Cushman loam, 2 to 4 percent slopes"||3|3.2|64|||"None"|"None"|"0"|4.23|8.7|11.23|11.94|"Well drained"|"Well drained"|"C"|"3"|90|"3"|98|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.311|"Erosion hazard slight"|"0"|0.803|"345405"
"Cr"|"Cushman loam, 4 to 8 percent slopes"||6|6|64|||"None"|"None"|"0"|4.26|8.78|11.11|11.54|"Well drained"|"Well drained"|"C"|"3"|99|"3"|100|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.318|"Erosion hazard moderate"|"0"|0.809|"345406"
"Cs"|"Cushman loam, 8 to 15 percent slopes"||12|11.7|64|||"None"|"None"|"0"|4.24|8.34|10.93|11.81|"Well drained"|"Well drained"|"C"|"4"|80|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.33|"Erosion hazard severe"|"0"|0.827|"345407"
"Ct"|"Cushman-Bainville loams, 4 to 8 percent slopes"||6|5.9|64|||"None"|"None"|"0"|4.32|8.84|11.46|12.25|"Well drained"|"Well drained"|"C"|"3"|96|"3"|99|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.337|"Erosion hazard moderate"|"0"|0.792|"345408"
"Cu"|"Cushman-Bainville loams, 8 to 15 percent slopes"||12|11.4|36|||"None"|"None"|"0"|4.32|8.03|10.28|11.33|"Well drained"|"Well drained"|"C"||94|"4"|61|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.475|"Erosion hazard severe"|"0"|0.885|"345409"
"Cv"|"Cushman-Terry fine sandy loams, 2 to 8 percent slopes"||5|5.1|66|||"None"|"None"|"0"|3.95|8.05|13.58|13.83|"Well drained"|"Well drained"|"C"||94|"4"|93|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.2|"Erosion hazard moderate"|"0"|0.466|"345410"
"Cw"|"Cushman-Tullock complex, 8 to 15 percent slopes"||12|11.5|64|||"None"|"None"|"0"|4.09|8.23|10.9|11.63|"Well drained"|"Well drained"|"C"||91|"4"|75|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.268|"Erosion hazard severe"|"0"|0.838|"345411"
"Cx"|"Bonfri-Beenom-Cabbart loams, 2 to 8 percent"||5|5|41|||"None"|"None"|"2"|4.24|7.88|10.91|11.04|"Well drained"|"Well drained"|"D"|"6"|50|"6"|55|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.232|"Erosion hazard moderate"|"2"|1|"345412"
"Cy"|"Cushman-Winnett complex"||5|5.3|64|||"None"|"None"|"0"|4.15|8|9.85|9.98|"Well drained"|"Well drained"|"C"||94|"3"|63|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.344|"Erosion hazard moderate"|"0"|0.901|"345413"
"Dw"|"Dwyer fine sand"||10|9.7||||"None"|"None"|"0"|1.88|3.72|7.25|10.78|"Excessively drained"|"Excessively drained"|"A"||96|"7"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Good"|"Good"|"Very limited"|0.961|"Erosion hazard slight"|"0"|0.98|"345414"
"Ed"|"Edgar loam, 1 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.36|8.4|16.48|24.56|"Well drained"|"Well drained"|"B"|"3"|97|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.243|"Erosion hazard moderate"|"0"|0|"345415"
"Eg"|"Edgar loam, 8 to 15 percent slopes"||12|11.5||||"None"|"None"|"0"|4.36|8.39|16.51|24.62|"Well drained"|"Well drained"|"B"|"4"|91|"4"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.262|"Erosion hazard severe"|"0"|0.577|"345416"
"Fc"|"Tanna-Beenom complex, 4 to 8 percent slopes"||5|5.3|46|||"None"|"None"|"0"|4.54|8.61|11.16|11.67|"Well drained"|"Well drained"|"D"|"3"|66|"3"|66|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.241|"Erosion hazard moderate"|"0"|0.985|"345418"
"Ff"|"Flasher fine sandy loam, 4 to 20 percent slopes"||12|11.6|66|||"None"|"None"|"0"|3.83|7.48|10.05|10.45|"Well drained"|"Well drained"|"B"||96|"6"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.112|"Erosion hazard severe"|"0"|0.875|"345419"
"Fh"|"Flasher fine sandy loam, 20 to 35 percent slopes"||28|26.7|66|||"None"|"None"|"0"|3.67|6.64|8.54|8.82|"Well drained"|"Well drained"|"C"||96|"6"|88|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.963|"Erosion hazard severe"|"0"|0.98|"345420"
"Fm"|"Flasher loamy fine sand"||13|12.8|76|||"None"|"None"|"0"|2.66|4.93|7.26|7.63|"Well drained"|"Well drained"|"A"||100|"6"|75|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Good"|"Somewhat limited"|0.812|"Erosion hazard moderate"|"0"|0.996|"345421"
"Fn"|"Fort Collins loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.3|8.71|17.69|26.67|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.25|"Erosion hazard slight"|"0"|0.06|"345422"
"Fo"|"Fort Collins loam, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.3|8.6|17.16|25.71|"Well drained"|"Well drained"|"B"|"2"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.256|"Erosion hazard slight"|"0"|0.1|"345423"
"Fr"|"Fort Collins loam, 4 to 8 percent slopes"||6|5.6||||"None"|"None"|"0"|4.31|8.62|17.29|25.95|"Well drained"|"Well drained"|"B"|"3"|89|"3"|97|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.254|"Erosion hazard moderate"|"0"|0.069|"345424"
"Fs"|"Fort Collins loam, sandy substratum, 0 to 1 percent slopes"||1|1.1||||"None"|"None"|"0"|4.49|8.97|17.33|25.4|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.244|"Erosion hazard slight"|"0"|0|"345425"
"Ft"|"Fort Collins loam, sandy substratum, 1 to 3 percent slopes"||2|2.1||||"None"|"None"|"0"|4.49|8.97|17.33|25.4|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.244|"Erosion hazard slight"|"0"|0|"345426"
"Ga"|"Gilt Edge clay loam"||2|2.1||||"None"|"None"|"2"|3.5|6.23|11.55|15.57|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.503|"Erosion hazard slight"|"2"|1|"345427"
"Gb"|"Gilt Edge-Arvada complex"||3|3||||"None"|"None"|"2"|3.38|6.05|9.83|12.96|"Well drained"|"Well drained"|"D"|"4"|55|"4"|55|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.579|"Erosion hazard slight"|"2"|1|"345428"
"Gc"|"Glendive clay"||1|1||||"Rare"|"Rare"|"0"|3.99|6.51|10.81|15.06|"Well drained"|"Well drained"|"C"|"4"|97|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.48|"Erosion hazard slight"|"0"|0.97|"345429"
"Gg"|"Glendive clay loam"||1|1||||"Rare"|"Rare"|"0"|4.47|6.67|11.05|15.36|"Well drained"|"Well drained"|"B"|"4"|96|"4"|96|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.126|"Erosion hazard slight"|"0"|0.96|"345430"
"Gh"|"Glendive fine sandy loam"||1|1||||"Occasional"|"Occasional"|"0"|3.06|6.08|12.12|18.17|"Well drained"|"Well drained"|"A"|"4"|94|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Not limited"|0.009|"Erosion hazard slight"|"0"|0.616|"345431"
"Gm"|"Glendive fine sandy loam, fans"||5|5||||"None"|"None"|"0"|3.46|6.88|13.71|20.55|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Good"|"Somewhat limited"|0.085|"Erosion hazard moderate"|"0"|0.453|"345432"
"Gn"|"Glendive fine sandy loam, shallow"||1|1||||"Rare"|"Rare"|"0"|3.72|7.2|8.88|10.55|"Well drained"|"Well drained"|"B"|"4"|97|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.104|"Erosion hazard slight"|"0"|1|"345433"
"Go"|"Glendive loam"||1|1||||"Occasional"|"Occasional"|"0"|4.91|7.99|13.87|19.74|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Erosion hazard slight"|"0"|0.62|"345434"
"Gs"|"Glendive loamy fine sand"||1|1||||"Occasional"|"Occasional"|"0"|2.56|5.09|10.15|15.21|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"|"4"|96|"6"|96|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.361|"Erosion hazard slight"|"0"|0.984|"345435"
"Gv"|"Glendive and Banks soils"||1|1||||"Occasional"|"Occasional"|"0"|3.94|6.88|12.51|18.13|"Well drained"|"Well drained"|"A"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Not limited"|0.025|"Erosion hazard slight"|"5"|0.72|"345436"
"Ha"|"Havre clay"||1|1||122|122|"Occasional"|"Occasional"|"0"|3.57|7.57|15.55|23.48|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.482|"Erosion hazard slight"|"0"|0.98|"345437"
"Hb"|"Havre clay, saline"||1|1||122|122|"Occasional"|"Occasional"|"0"|2.35|5.12|10.62|16.12|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"6"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.483|"Erosion hazard slight"|"0"|1|"345438"
"Hc"|"Havre clay loam"||1|1||122|122|"Occasional"|"Occasional"|"0"|4|8|16|24|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"2"|100|"3"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.183|"Erosion hazard slight"|"0"|0.57|"345439"
"Hd"|"Havre clay loam, high"||1|1||||"None"|"None"|"0"|4|8|16|24|"Well drained"|"Well drained"|"C"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.189|"Erosion hazard slight"|"0"|0.296|"345440"
"Hf"|"Havre clay loam, saline"||1|1||122|122|"Occasional"|"Occasional"|"0"|2.8|5.57|11.07|16.57|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"6"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.203|"Erosion hazard slight"|"0"|0.8|"345441"
"Hg"|"Havre loam"||1|1||||"Rare"|"Rare"|"0"|4.4|8.37|15.72|23.07|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.153|"Erosion hazard slight"|"2"|0.1|"345442"
"Hh"|"Havre loam, high"||1|1||||"None"|"None"|"0"|4.44|8.45|16.47|24.5|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.18|"Erosion hazard slight"|"0"|0.015|"345443"
"Hl"|"Havre loam, moderately deep"||1|1||122|122|"Rare"|"Rare"|"0"|4.46|8.91|11.57|13.42|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"|"2"|95|"3"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.147|"Erosion hazard slight"|"0"|0.95|"345444"
"Hm"|"Havre loam, saline"||1|1.2||122|122|"Occasional"|"Occasional"|"0"|2.83|5.57|11.02|16.47|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"|"4"|95|"6"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.188|"Erosion hazard slight"|"0"|0.8|"345445"
"Hn"|"Havre and Glendive soils"||1|1||||"Occasional"|"Occasional"|"0"|4.1|7.69|14.88|22.07|"Well drained"|"Well drained"|"B"|"2"|65|"3"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.146|"Erosion hazard slight"|"2"|0.64|"345446"
"Ho"|"Havre and Lohmiller soils"||1|1||||"Occasional"|"Occasional"|"0"|3.97|7.92|15.65|23.23|"Well drained"|"Well drained"|"C"|"4"|32|"3"|61|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.321|"Erosion hazard slight"|"3"|0.876|"345447"
"Hp"|"Havre and Lohmiller soils, 8 to 15 percent slopes"||12|10.9||||"None"|"None"|"0"|4.06|8|15.55|23.1|"Well drained"|"Well drained"|"B"|"4"|100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.252|"Erosion hazard severe"|"0"|0.783|"345448"
"Hr"|"Havre and Lohmiller soils, 15 to 35 percent slopes"||25|22.6||||"None"|"None"|"0"|4.06|8|15.55|23.1|"Well drained"|"Well drained"|"B"||90|"6"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.917|"Erosion hazard severe"|"0"|1|"345449"
"Hs"|"Havre and Lohmiller soils, saline"||1|1||122|122|"Occasional"|"Occasional"|"0"|2.85|5.62|11.12|16.62|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"6"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.207|"Erosion hazard slight"|"0"|0.822|"345450"
"Ht"|"Havre-Hysham loams"||1|1||||"None"|"None"|"0"|4.06|7.65|14.77|21.9|"Well drained"|"Well drained"|"B"|"2"|65|"3"|65|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.218|"Erosion hazard slight"|"0"|0.35|"345451"
"Hu"|"Hesper loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"2"|4.34|8.69|17.72|26.3|"Well drained"|"Well drained"|"C"|"2"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.501|"Erosion hazard slight"|"2"|0.366|"345452"
"Hv"|"Hesper loam, 4 to 8 percent slopes"||6|5.5||||"None"|"None"|"10"|4.4|8.82|18.02|26.85|"Well drained"|"Well drained"|"C"|"3"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.547|"Erosion hazard moderate"|"1"|0.366|"345453"
"Hw"|"Hilly gravelly land"||25|23||||||"0"|1.78|3.03|5.22|7.32|"Excessively drained"|"Somewhat excessively drained"|||94|"7"|50|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|0.93|"Erosion hazard moderate"|"0"|0.789|"345454"
"Hx"|"Hoven clay"||1|1.1||0|0|"None"|"None"|"95"|4.2|7.99|14.28|20.56|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"6"|90|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Erosion hazard slight"|"5"|1|"345455"
"Hy"|"Hoven and McKenzie soils"||2|2||||"None"|"None"|"47"|2.95|5.59|10.49|15.36|"Well drained"|"Well drained"|"D"|"7"|100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.75|"Erosion hazard slight"|"0"|1|"345456"
"Hz"|"Hysham-Havre loams"||1|1||||"Rare"|"Rare"|"0"|3.57|6.69|12.94|19.19|"Well drained"|"Well drained"|"C"|"4"|70|"6"|70|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.265|"Erosion hazard slight"|"0"|0.715|"345457"
"La"|"Laurel clay loam"||1|1.1||61|61|"None"|"None"|"95"|2.04|4.05|8.35|12.61|"Poorly drained"|"Poorly drained"|"C"|"7"|100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Erosion hazard slight"|"90"|1|"345458"
"Lb"|"Laurel loam"||2|2||61|61|"Rare"|"Rare"|"90"|2.2|4.28|8.35|12.42|"Poorly drained"|"Poorly drained"|"D"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.938|"Erosion hazard slight"|"90"|1|"345459"
"Lc"|"Lismas clay"||28|24.7|30|||"None"|"None"|"0"|3.58|4.9|5.89|6.6|"Well drained"|"Well drained"|"D"||94|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.889|"Erosion hazard severe"|"0"|0.988|"345460"
"Ld"|"Lismas-Pierre clays, saline-Alkali"||25|21.4|30|||"None"|"None"|"5"|3|4.55|5.96|6.63|"Well drained"|"Well drained"|"D"||95|"7"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.8|"Erosion hazard severe"|"0"|1|"345461"
"Lf"|"Lismas-Midway complex"||25|24.6|30|||"None"|"None"|"0"|3.89|5.63|5.94|6.15|"Well drained"|"Well drained"|"D"||100|"7"|94|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.985|"Erosion hazard severe"|"0"|1|"345462"
"Lg"|"Lismas-Shale outcrop complex"||35|33.5|30|||"None"|"None"|"1"|3.53|4.44|4.74|4.93|"Well drained"|"Well drained"|"D"||99|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.971|"Erosion hazard severe"|"0"|1|"345463"
"Lh"|"Lohmiller clay"||1|1||||"Rare"|"Rare"|"0"|3.93|7.82|14.92|21.32|"Well drained"|"Well drained"|"C"|"4"|100|"4"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.483|"Erosion hazard slight"|"0"|1|"345464"
"Lm"|"Lohmiller clay, high"||1|1||||"None"|"None"|"0"|3.93|7.82|15.57|23.32|"Well drained"|"Well drained"|"C"|"4"|100|"4"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.933|"Erosion hazard slight"|"0"|1|"345465"
"Ln"|"Lohmiller clay, wet"||1|1||38|38|"Rare"|"Rare"|"0"|2.85|5.68|11.59|17.6|"Poorly drained"|"Poorly drained"|"C/D"|"6"|90|"6"|94|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Very limited"|0.943|"Erosion hazard slight"|"90"|1|"345466"
"Lo"|"Lohmiller clay loam"||1|1||122|122|"Occasional"|"Occasional"|"0"|3.98|7.93|16.2|24.52|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"2"|95|"3"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.196|"Erosion hazard slight"|"0"|0.62|"345467"
"Lr"|"Lohmiller clay loam, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|4.03|8.06|16.11|24.11|"Well drained"|"Well drained"|"C"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.19|"Erosion hazard slight"|"0"|0.296|"345468"
"Ls"|"Lohmiller clay loam, fans, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.03|8.08|16.18|24.19|"Well drained"|"Well drained"|"C"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.196|"Erosion hazard slight"|"0"|0.266|"345469"
"Lt"|"Lohmiller clay loam, high"||1|1||||"None"|"None"|"0"|4.03|8.06|15.86|22.52|"Well drained"|"Well drained"|"C"|"3"|90|"3"|100|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.308|"Erosion hazard slight"|"0"|0.93|"345470"
"Lu"|"Lohmiller-Hysham clays"||1|1||||"Rare"|"Rare"|"0"|3.83|7.64|15.05|21.47|"Well drained"|"Well drained"|"C"|"4"|95|"4"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.482|"Erosion hazard slight"|"0"|0.98|"345471"
"Ly"|"Lohmiller-Hysham clay loams"||1|1||||"None"|"None"|"0"|3.9|7.75|15.16|21.58|"Well drained"|"Well drained"|"C"|"2"|85|"3"|85|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.314|"Erosion hazard slight"|"0"|0.98|"345472"
"Ma"|"Marias clays, saline-alkali, 0 to 1 percent slopes"||1|1||||"None"|"None"|"10"|3.93|7.47|14.42|21.37|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.55|"Erosion hazard slight"|"0"|1|"345473"
"Mb"|"Marias clay, saline-alkali, 1 to 10 percent slopes"||6|6.5||||"None"|"None"|"0"|3.81|7.21|13.72|20.02|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Erosion hazard moderate"|"0"|1|"345474"
"Mc"|"Marias clays, fans, saline-alkali"||5|4.6||||"None"|"None"|"10"|3.93|7.47|14.42|21.37|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.55|"Erosion hazard moderate"|"0"|1|"345475"
"Md"|"Marias-Hoven clays, saline"||3|3.4||||"None"|"None"|"0"|3.5|6.38|11.25|16|"Well drained"|"Well drained"|"D"|"4"|75|"4"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Erosion hazard slight"|"0"|1|"345476"
"Me"|"Marias-Pierre clays, saline-Alkali"||4|6.8|71|||"None"|"None"|"6"|3.55|6.34|10.22|13.36|"Well drained"|"Well drained"|"D"|"4"|55|"4"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.53|"Erosion hazard moderate"|"0"|1|"345477"
"Mf"|"Marias and Promise clay"||6|6.5|112|||"None"|"None"|"0"|3.71|7.16|13.83|18.09|"Well drained"|"Well drained"|"D"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.498|"Erosion hazard moderate"|"0"|1|"345478"
"Mk"|"McRae loam"||12|11.7||||"None"|"None"|"0"|4.45|8.71|16.97|25.12|"Well drained"|"Well drained"|"B"||94|"4"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.365|"Erosion hazard severe"|"0"|0.603|"345479"
"Ml"|"McRae-Bainville loams, 8 to 20 percent slopes"||14|13.2|66|||"None"|"None"|"0"|4.5|8.87|16|22.32|"Well drained"|"Well drained"|"B"||90|"4"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.495|"Erosion hazard severe"|"0"|0.888|"345480"
"Mm"|"McRae-Bainville loams, 20 to 35 percent slopes"||28|25.9|48|||"None"|"None"|"0"|4.43|8.48|13.58|18.63|"Well drained"|"Well drained"|"B"||93|"6"|53|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.945|"Erosion hazard severe"|"0"|0.93|"345481"
"Mn"|"McRae and Havre loams, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.39|8.51|16.76|25.01|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.258|"Erosion hazard slight"|"0"|0.015|"345482"
"Mo"|"McRae and Havre loams, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.39|8.51|16.76|25.01|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.258|"Erosion hazard slight"|"0"|0.015|"345483"
"Mp"|"McRae and Havre loams, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.4|8.54|16.82|25.07|"Well drained"|"Well drained"|"B"|"3"|95|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.327|"Erosion hazard moderate"|"0"|0.006|"345484"
"Mr"|"Midway clay loam, 8 to 15 percent slopes"||12|11.8|46|||"None"|"None"|"0"|4.4|8.03|8.54|8.87|"Well drained"|"Well drained"|"D"||98|"6"|93|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.325|"Erosion hazard severe"|"0"|0.963|"345485"
"Ms"|"Midway clay loam, 15 to 35 percent slopes"||25|22.1|41|||"None"|"None"|"0"|4.33|7.3|9.01|10.65|"Well drained"|"Well drained"|"D"||90|"7"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.883|"Erosion hazard severe"|"0"|0.936|"345486"
"Mt"|"Midway-Bainville complex"||48|44.1|41|||"None"|"None"|"0"|4.46|8.02|9.36|10.17|"Well drained"|"Well drained"|"D"||93|"7"|88|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.926|"Erosion hazard severe"|"0"|0.929|"345487"
"Mu"|"Midway-Nihill gravelly loam"||38|36.9|41|||"None"|"None"|"0"|4.18|6.9|8.08|9.14|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Erosion hazard severe"|"0"|1|"345488"
"Na"|"Nihill gravelly loam"||30|28.2||||"None"|"None"|"2"|3.73|6.19|10.74|14.87|"Well drained"|"Well drained"|"B"||91|"6"|87|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.954|"Erosion hazard moderate"|"0"|0.964|"345490"
"Nc"|"Nunn clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.03|8.08|16.18|24.22|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.928|"Erosion hazard slight"|"0"|0.9|"345491"
"Nd"|"Nunn clay, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|4.04|8.09|16.16|24.17|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.924|"Erosion hazard slight"|"0"|0.9|"345492"
"Nm"|"Nunn clay, 3 to 8 percent slopes"||6|5.6||||"None"|"None"|"0"|4.04|8.09|16.17|24.17|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.924|"Erosion hazard moderate"|"0"|0.9|"345493"
"Nn"|"Nunn clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.84|7.93|16.9|25.83|"Well drained"|"Well drained"|"C"|"2"|97|"3"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.306|"Erosion hazard slight"|"0"|0.93|"345494"
"No"|"Nunn clay loam, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|3.81|7.86|16.78|25.66|"Well drained"|"Well drained"|"C"|"2"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.286|"Erosion hazard slight"|"0"|0.97|"345495"
"Nu"|"Nunn clay loam, 3 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|3.8|7.8|16.54|25.26|"Well drained"|"Well drained"|"C"|"3"|90|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.327|"Erosion hazard moderate"|"0"|1|"345496"
"Nx"|"Nunn-Beckton complex, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.95|7.8|15.24|22.58|"Well drained"|"Well drained"|"C"|"4"|70|"4"|70|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.788|"Erosion hazard slight"|"0"|0.9|"345497"
"Pa"|"Pierre clay"||8|8.4|66|||"None"|"None"|"0"|3.83|7.38|10.05|10.68|"Well drained"|"Well drained"|"D"||91|"4"|94|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Erosion hazard moderate"|"0"|1|"345498"
"Pc"|"Pierre-Lismas clays"||18|17.9|30|||"None"|"None"|"0"|3.77|6.7|8.68|9.1|"Well drained"|"Well drained"|"D"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.52|"Erosion hazard severe"|"0"|1|"345499"
"Pk"|"Pierre-Lismas clays, saline-Alkali"||18|17.1|30|||"None"|"None"|"4"|3.05|5.13|7.03|7.51|"Well drained"|"Well drained"|"D"||96|"6"|69|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.521|"Erosion hazard severe"|"0"|1|"345500"
"Rn"|"Renohill clay loam"||6|6.3|76|||"None"|"None"|"0"|3.96|6.89|9.73|10|"Well drained"|"Well drained"|"D"|"3"|93|"3"|93|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Poor"|"Poor"|"Somewhat limited"|0.282|"Erosion hazard moderate"|"0"|0.992|"345501"
"Rw"|"Riverwash"|||1||||||"5"|4.35|8.85|17.85|26.85|||||100||95|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"5"|1|"345502"
"Sa"|"Sage clay"||1|1||46|46|"Rare"|"Rare"|"90"|2.06|4.2|7.59|9.5|"Poorly drained"|"Poorly drained"|"C/D"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.95|"Erosion hazard slight"|"90"|1|"345503"
"Sc"|"Sage silty clay"||2|1.9||||"None"|"None"|"90"|2.19|4.34|8.64|12.94|"Well drained"|"Well drained"|"C"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.95|"Erosion hazard slight"|"0"|1|"345504"
"Sh"|"Shale outcrop"|||35||||||"0"|3.42|4.84|4.84|4.84|||"D"||100||95|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"345505"
"Sk"|"Shonkin loam"||1|1.1||0|0|"Rare"|"Rare"|"98"|4.49|8.01|13.97|19.39|"Somewhat poorly drained"|"Somewhat poorly drained"|"C/D"||95|"6"|98|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.987|"Erosion hazard slight"|"95"|0.986|"345506"
"Tf"|"Terry-Tullock fine sandy loams"||6|6|71|||"None"|"None"|"0"|3.82|7.46|10.75|11.23|"Well drained"|"Well drained"|"C"||92|"4"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.068|"Erosion hazard moderate"|"0"|0.729|"345507"
"Tm"|"Terry-Treasure fine sandy loams"||6|5.4|71|||"None"|"None"|"0"|3.86|7.75|12.17|14.27|"Well drained"|"Well drained"|"C"||70|"4"|98|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.073|"Erosion hazard moderate"|"0"|0.471|"345508"
"Tn"|"Terry-Winnett complex"||6|6|76|||"None"|"None"|"0"|3.79|7.21|11.57|11.57|"Well drained"|"Well drained"|"C"||96|"4"|71|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.162|"Erosion hazard moderate"|"0"|0.446|"345509"
"Tp"|"Blacksheep-Twilight fine sandy loams, 15 to 40 percent slopes"||25|20.7|41|||"None"|"None"|"0"|3.31|5.82|7.23|7.44|"Well drained"|"Well drained"|"D"||95|"7"|50|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.601|"Erosion hazard very severe"|"0"|0.956|"345510"
"Tr"|"Cabbart-Blacksheep-Rock outcrop complex, 30 to 70 percent slopes"||50|49.3|41|||"None"|"None"|"0"|3.42|5.68|5.88|5.88|"Well drained"|"Well drained"|"D"||100|"7"|73|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Erosion hazard very severe"|"0"|1|"345511"
"Ts"|"Treasure fine sandy loam, 2 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|3.89|7.89|14.92|21.74|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.059|"Erosion hazard slight"|"0"|0.053|"345512"
"Tu"|"Treasure fine sandy loam, 4 to 8 percent slopes"||6|5.7||||"None"|"None"|"0"|3.89|7.89|14.75|21.33|"Well drained"|"Well drained"|"B"|"4"|91|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.056|"Erosion hazard moderate"|"0"|0.096|"345513"
"Tv"|"Tullock fine sandy loam, 4 to 20 percent slopes"||12|11.4|71|||"None"|"None"|"0"|3.82|7.64|10.75|10.79|"Well drained"|"Well drained"|"A"||97|"6"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.068|"Erosion hazard moderate"|"0"|0.976|"345514"
"Wb"|"Wanetta loam, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.65|8.83|12.77|14.32|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.309|"Erosion hazard slight"|"0"|1|"345515"
"Wc"|"Wanetta loam, 4 to 8 percent slopes"||6|5.4||||"None"|"None"|"0"|4.65|8.85|13.07|15|"Well drained"|"Well drained"|"B"|"3"|85|"3"|91|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.306|"Erosion hazard moderate"|"0"|0.94|"345516"
"Wd"|"Wanetta loam, deep, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.7|9.02|14.67|16.2|"Well drained"|"Well drained"|"B"|"2"|95|"3"|95|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.321|"Erosion hazard slight"|"0"|1|"345517"
"Wm"|"Wanetta loam, deep, 2 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.65|8.83|14.28|15.83|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.309|"Erosion hazard slight"|"0"|1|"345518"
"Wn"|"Wanetta loam, deep, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.6|8.73|14|15.48|"Well drained"|"Well drained"|"B"||90|"3"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.294|"Erosion hazard moderate"|"0"|0.993|"345519"
"Wr"|"Wibaux-Rock outcrop complex"||50|50||||"None"|"None"|"0"|2.82|3.57|4.03|4.5|"Well drained"|"Well drained"|"A"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Erosion hazard very severe"|"0"|1|"345520"
"Wt"|"Winnett complex"||5|5.1|64|||"None"|"None"|"0"|4.03|6.94|8.7|8.7|"Well drained"|"Well drained"|"D"||90|"6"|75|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.377|"Erosion hazard moderate"|"0"|0.976|"345521"
"Wx"|"Winnett-Fattig complex"||4|4.1|76|||"None"|"None"|"0"|4.07|7.28|10.51|10.51|"Well drained"|"Well drained"|"D"||100|"6"|61|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.379|"Erosion hazard moderate"|"0"|0.78|"345522"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"696020"
"Gp"|"Pits, gravel and sand"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"696021"
"83E"|"Blacksheep-Twilight complex, 4 to 25 percent slopes"||15|14.2|46|||"None"|"None"|"0"|3.71|6.89|7.65|7.79|"Well drained"|"Well drained"|"D"||98|"7"|54|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.037|"Erosion hazard severe"|"0"|0.992|"1946666"
"182D"|"Cabbart-Delpoint loams, 4 to 15 percent slopes"||10|8.1|41|||"None"|"None"|"0"|3.84|6.95|8.79|9.21|"Well drained"|"Well drained"|"D"||55|"6"|50|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.23|"Erosion hazard severe"|"0"|0.799|"1946667"
"354B"|"Bonfri-Cabbart loams, 0 to 4 percent slopes"||2|2.9|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Erosion hazard slight"|"0"|0.95|"1946668"
"453C"|"Cabbart-Bonfri loams, 2 to 8 percent slopes"||5|5.5|41|||"None"|"None"|"0"|3.87|6.98|9.88|9.88|"Well drained"|"Well drained"|"D"|"6"|50|"6"|52|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.21|"Erosion hazard moderate"|"0"|1|"1946669"
"Mv"|"Midway-Shale outcrop complex, 4 to 35 percent slopes"||15|15.9|30|||"None"|"None"|"0"|4.53|6.32|8.04|9.11|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.375|"Erosion hazard severe"|"0"|1|"3442555"
