# Lower Yellowstone River Corridor Color Infrared Digital Orthophotography, McKenzie Co., ND.

Metadata also available as

## Metadata:

- Identification_Information
- Data_Quality_Information
- Spatial_Data_Organization_Information
- Spatial_Reference_Information
- Entity_and_Attribute_Information
- Distribution_Information
- Metadata_Reference_Information

Identification_Information:
  Citation:
    Citation_Information:
      Originator: USDA-NRCS
      Publication_Date: 05-09-2002
      Publication_Time: Unknown
      Title:
        Lower Yellowstone River Corridor Color Infrared Digital Orthophotography, McKenzie Co., ND.
      Geospatial_Data_Presentation_Form: remote-sensing image
      Online_Linkage: \\199.155.252.5\/usr5\lyrc\mckenzie\mck_mo.sid
  Description:
    Abstract:
      Color infrared digital orthophotgraphy of the Lower Yellowstone River corridor,McKenzie County, ND.
    Purpose:
      Project was commissioned by the Lower Yellowstone River District Council as a basis for resources inventory and monitoring.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 08-05-2001
        Time_of_Day: between 9 a.m. and 3 p.m.
    Currentness_Reference: ground condition
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: None planned
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -104.112990
      East_Bounding_Coordinate: -103.914880
      North_Bounding_Coordinate: 48.022786
      South_Bounding_Coordinate: 47.746194
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: None
      Theme_Keyword: Color infrared imagery
      Theme_Keyword: orthorectified
    Place:
      Place_Keyword: Lower Yellowstone River
      Place_Keyword: McKenzie County
      Place_Keyword: North Dakota
  Access_Constraints:
    This is public information and may be used by organizations, agencies, units of government, or others based on needs; however they are responsible for the appropriate application.
  Use_Constraints:
    For use as a primary reference source. Not intended for site specific planning.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Doug Harrison
        Contact_Organization: USDA/NRCS
      Contact_Position: State Resource Inventory Specialist
      Contact_Voice_Telephone: 406-587-6840
      Contact_Facsimile_Telephone: 406-587-6761
      Contact_Electronic_Mail_Address: dharrison@mt.usda.gov
      Hours_of_Service: 0600-1530 MT
  Native_Data_Set_Environment:
    Microsoft Windows NT Version 4.0 (Build 1381) Service Pack 6; ESRI ArcCatalog 8.1.1.649

Data_Quality_Information:
  Lineage:
    Source_Information:
      Source_Scale_Denominator: 24000
      Type_of_Source_Media: CD-ROM
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 08-05-01
            Time_of_Day: 9 a.m. to 3 p.m.
        Source_Currentness_Reference: ground condition
      Source_Citation_Abbreviation: CIR
      Source_Contribution:
        CIR film positive aerial photography for digital orthorecitification
    Process_Step:
      Process_Description:
        Color infrared film positive aerial phography was scanned at 600 d.p.i. using a Leica Planimetric scanner. Photgraphs contained 25 percent overlap, therefore, every other frame was scanned. The scanned imagery was then processed using ERDAS Imagine 8.4. Imagery was orthorectified using ERDAS/ OrthoBase. USGS digital orthophotography was used as the horizontal reference source and 30 meter digital elevation models were used as the vertical reference source. The U.S. Geological Survey camera report was used to obtain the interior and exterior orientation and other specific camera information needed in Orthobase. Ground control points and tie points were created. Nearest neighbor resampling method was employed to produce an orthorectified image.

        Once orthorectified, the imagery was clipped to within approximately one mile on either side of the Yellowstone River centerline of flow using an area of interest (AOI). Images were then mosaiced using ERDAS mosaic tool. The overlap function was set for no cutlines and overlay. Image matching was not performed. Mosaiced images were compressed at a 20:1 ratio with MrSID Geospatial Encoder 1.4.

Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Raster
  Raster_Object_Information:
    Raster_Object_Type: Pixel
    Row_Count: 30562
    Column_Count: 14423
    Vertical_Count: 1

Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: Universal Transverse Mercator
        Universal_Transverse_Mercator:
          UTM_Zone_Number: 13
          Transverse_Mercator:
            Scale_Factor_at_Central_Meridian: 0.999600
            Longitude_of_Central_Meridian: -105.000000
            Latitude_of_Projection_Origin: 0.000000
            False_Easting: 500000.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: row and column
        Coordinate_Representation:
          Abscissa_Resolution: 1.000000
          Ordinate_Resolution: 1.000000
        Planar_Distance_Units: meters
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222

Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_1
    Attribute:
      Attribute_Label: ObjectID
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_2
    Attribute:
      Attribute_Label: ObjectID
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: Band_3
    Attribute:
      Attribute_Label: ObjectID
    Attribute:
      Attribute_Label: Value
    Attribute:
      Attribute_Label: Count

Distribution_Information:
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 30.150

Metadata_Reference_Information:
  Metadata_Date: 20020613
  Metadata_Contact:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: USDA/NRCS
        Contact_Person: Julie Tesky
      Contact_Position: Remote Sensing/Data Collection Specialist
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 10 E. Babcock, Fed, Bldg Rm. 443
        City: Bozeman
        State_or_Province: MT
        Postal_Code: 59715
        Country: USA
      Contact_Voice_Telephone: 406-587-6908
      Contact_Electronic_Mail_Address: jtesky@mt.usda.gov
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile
  Metadata_Extensions:
    Online_Linkage: <http://www.esri.com/metadata/esriprof80.html>
    Profile_Name: ESRI Metadata Profile

Generated by `mp` version 2.7.3 on Thu Jun 13 06:51:37 2002