08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769242"|"24633925"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769243"|"24633926"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"23769244"|"24633927"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, extremely stony soil is a minor component."|"23769245"|"24633928"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"23769246"|"24633929"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, extremely stony soil is a minor component."|"23769247"|"24633930"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Butchhill, stony component makes up 80 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, mountains. The parent material consists of clayey colluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769248"|"24633931"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"23769249"|"24633932"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769250"|"24633933"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769251"|"24633934"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769252"|"24633935"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, extremely stony, greater slopes soil is a minor component."|"23769253"|"24633936"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, extremely stony soil is a minor component."|"23769254"|"24633937"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23768964"|"24633647"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monad soil is a minor component."|"23768965"|"24633648"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, occasionally ponded soil is a minor component."|"23768966"|"24633649"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23768967"|"24633650"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hairpin component makes up 80 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, lake terraces, intermontane basins. The parent material consists of lacustrine deposits and/or slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768968"|"24633651"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad, stony component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769255"|"24633938"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hairpin component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of lacustrine deposits and/or slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769256"|"24633939"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, occasionally ponded soil is a minor component."|"23769257"|"24633940"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan soil is a minor component."|"23769258"|"24633941"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769259"|"24633942"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"23769095"|"24633778"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan soil is a minor component."|"23769096"|"24633779"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Butchhill component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, mountains. The parent material consists of clayey alluvium and/or colluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769097"|"24633780"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769098"|"24633781"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hairpin component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, mountains. The parent material consists of lacustrine deposits and/or clayey colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769099"|"24633782"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, stony soil is a minor component."|"23769100"|"24633783"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maurice, very stony soil is a minor component."|"23769101"|"24633784"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on escarpments, intermontane basins. The parent material consists of loamy skeletal alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769102"|"24633785"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, stony component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on escarpments, intermontane basins. The parent material consists of loamy skeletal alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769103"|"24633786"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"23769104"|"24633787"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23769105"|"24633788"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769106"|"24633789"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, stony soil is a minor component."|"23769107"|"24633790"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn, occasionally flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769108"|"24633791"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, occasionally flooded component makes up 29 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769109"|"24633792"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"23769110"|"24633793"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 31 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23769111"|"24633794"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, stony soil is a minor component."|"23769112"|"24633795"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23769113"|"24633796"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769114"|"24633797"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23769115"|"24633798"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769260"|"24633943"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, very stony component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on landslides on hillslopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769261"|"24633944"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hairpin component makes up 50 percent of the map unit. Slopes are 4 to 25 percent. This component is on hillslopes, mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769262"|"24633945"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769263"|"24633946"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, very stony soil is a minor component."|"23769264"|"24633947"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"23769265"|"24633948"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, occasionally ponded soil is a minor component."|"23769266"|"24633949"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23768969"|"24633652"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on marshes, intermontane basins. The parent material consists of mucky peat organic material over mixed alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23768970"|"24633653"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, occasionally flooded component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23768971"|"24633654"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dunkleber, frequently ponded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on marshes, intermontane basins. The parent material consists of mucky peat organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 3 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 50 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23768972"|"24633655"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slagamelt soil is a minor component."|"23768973"|"24633656"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, extremely stony, lesser slopes soil is a minor component."|"23769217"|"24633900"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"23769218"|"24633901"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely stony component makes up 55 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"23769219"|"24633902"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769220"|"24633903"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, very stony component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769221"|"24633904"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Inabnit, stony component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, intermontane basins. The parent material consists of loamy residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769403"|"24634086"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769404"|"24634087"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 50 percent of the map unit. Slopes are 8 to 25 percent. This component is on hillslopes, intermontane basins. The parent material consists of fine-loamy alluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769405"|"24634088"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, very stony soil is a minor component."|"23769406"|"24634089"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"23769407"|"24634090"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan soil is a minor component."|"23769408"|"24634091"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shewag component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768924"|"24633607"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"23768925"|"24633608"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Slagamelt component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP907MT Subirrigated Cool Woodland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23768926"|"24633609"
09/14/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redfish, occasionally flooded component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during July, August, September, October, November. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23768927"|"24633610"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, stony soil is a minor component."|"23768928"|"24633611"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23768929"|"24633612"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23769386"|"24634069"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"23769387"|"24634070"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769388"|"24634071"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23769389"|"24634072"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shewag component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769390"|"24634073"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wisdom component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769391"|"24634074"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shewag component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768902"|"24633585"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Plimpton soil is a minor component."|"23768903"|"24633586"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"23768904"|"24633587"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23768905"|"24633588"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag, stony soil is a minor component."|"23768906"|"24633589"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23768907"|"24633590"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wisdom component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768908"|"24633591"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide soil is a minor component."|"23769188"|"24633871"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769189"|"24633872"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bighole component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769190"|"24633873"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23769191"|"24633874"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lehunt, saline soil is a minor component."|"23769192"|"24633875"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"23769193"|"24633876"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23769194"|"24633877"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lehunt soil is a minor component."|"23769195"|"24633878"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"23769392"|"24634075"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foxgulch component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during May, June, July. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769393"|"24634076"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769394"|"24634077"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copperbasin component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches (depth from the mineral surface is 29 inches) during March, April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769395"|"24634078"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23769396"|"24634079"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769397"|"24634080"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wisdom component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769398"|"24634081"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769196"|"24633879"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foxgulch, rarely flooded component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769197"|"24633880"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769198"|"24633881"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"23769199"|"24633882"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, occasionally flooded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769200"|"24633883"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copperbasin, rarely flooded component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches (depth from the mineral surface is 29 inches) during March, April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769201"|"24633884"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfish, occasionally flooded soil is a minor component."|"23769202"|"24633885"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monad soil is a minor component."|"23768909"|"24633592"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, stony soil is a minor component."|"23768910"|"24633593"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, stony soil is a minor component."|"23768911"|"24633594"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Donald component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23768912"|"24633595"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monad soil is a minor component."|"23769203"|"24633886"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, stony soil is a minor component."|"23769204"|"24633887"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Donald component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769205"|"24633888"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, stony soil is a minor component."|"23769206"|"24633889"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald soil is a minor component."|"23769207"|"24633890"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan soil is a minor component."|"23769208"|"24633891"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769209"|"24633892"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussigbrod component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on mima mounds, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6c. Irrigated land capability classification is 6c. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769210"|"24633893"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769211"|"24633894"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"23769212"|"24633895"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan, greater slopes soil is a minor component."|"23768930"|"24633613"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald soil is a minor component."|"23768931"|"24633614"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lehunt soil is a minor component."|"23768932"|"24633615"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of fine-loamy alluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768933"|"24633616"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768934"|"24633617"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23768935"|"24633618"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit soil is a minor component."|"23768936"|"24633619"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monad soil is a minor component."|"23769075"|"24633758"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, stony soil is a minor component."|"23769076"|"24633759"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"23769077"|"24633760"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769078"|"24633761"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shewag component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769222"|"24633905"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23769223"|"24633906"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foxgulch soil is a minor component."|"23769224"|"24633907"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769225"|"24633908"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"23769409"|"24634092"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth, stony component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23769410"|"24634093"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23769411"|"24634094"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, very cobbly soil is a minor component."|"23769412"|"24634095"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769413"|"24634096"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"23769414"|"24634097"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, stony soil is a minor component."|"23769415"|"24634098"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide, lesser slopes soil is a minor component."|"23769416"|"24634099"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769417"|"24634100"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769418"|"24634101"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverslide component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"23769419"|"24634102"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23769420"|"24634103"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Proposal component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769421"|"24634104"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 65 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of loamy skeletal alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769422"|"24634105"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23769423"|"24634106"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23768937"|"24633620"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bighole component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768938"|"24633621"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"23768939"|"24633622"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"23768940"|"24633623"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23768941"|"24633624"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wisdom component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768942"|"24633625"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23768943"|"24633626"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Proposal component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769226"|"24633909"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23769227"|"24633910"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, very stony component makes up 85 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768944"|"24633627"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"23768945"|"24633628"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768946"|"24633629"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"23768947"|"24633630"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foxgulch, rarely flooded soil is a minor component."|"23769079"|"24633762"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769080"|"24633763"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfish, occasionally flooded soil is a minor component."|"23769081"|"24633764"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"23769082"|"24633765"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copperbasin, rarely flooded soil is a minor component."|"23769083"|"24633766"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, occasionally flooded component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769084"|"24633767"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, occasionally ponded soil is a minor component."|"23768948"|"24633631"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barbarela, greater slopes soil is a minor component."|"23768949"|"24633632"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rogert component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on ridges, mountains. The parent material consists of gravelly residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP823MT Shallow Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768950"|"24633633"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danielvil soil is a minor component."|"23768951"|"24633634"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768952"|"24633635"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rogert, greater slopes, very stony soil is a minor component."|"23768953"|"24633636"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss and/or schist. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768954"|"24633637"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23769424"|"24634107"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban, stony soil is a minor component."|"23769425"|"24634108"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 65 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of loamy skeletal alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769426"|"24634109"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, greater slopes soil is a minor component."|"23769427"|"24634110"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on mima mounds, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769428"|"24634111"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of fine-loamy alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768955"|"24633638"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23768956"|"24633639"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23768957"|"24633640"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, greater slopes soil is a minor component."|"23768958"|"24633641"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 70 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of loamy skeletal alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768959"|"24633642"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Englejard component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of coarse-loamy  over sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769228"|"24633911"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussigbrod component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on mima mounds, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769229"|"24633912"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of fine-loamy outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769230"|"24633913"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769231"|"24633914"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769232"|"24633915"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23769233"|"24633916"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768960"|"24633643"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23768961"|"24633644"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23768962"|"24633645"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23768963"|"24633646"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769234"|"24633917"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussigbrod soil is a minor component."|"23769235"|"24633918"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"23769236"|"24633919"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Donald component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769237"|"24633920"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769085"|"24633768"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23769086"|"24633769"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, very stony component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769087"|"24633770"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, bouldery, greater slopes soil is a minor component."|"23769088"|"24633771"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, stony soil is a minor component."|"23769089"|"24633772"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lehunt component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP813MT Subirrigated Saline-Sodic Grassland ecological site.  Irrigated land capability classification is 7w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 70 within 30 inches of the soil surface."|"23769090"|"24633773"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Proposal component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769091"|"24633774"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lehunt, saline soil is a minor component."|"23769092"|"24633775"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769093"|"24633776"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23769094"|"24633777"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23769238"|"24633921"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lehunt, saline component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of saline fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during December. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP813MT Subirrigated Saline-Sodic Grassland ecological site.  Irrigated land capability classification is 7w.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 70 within 30 inches of the soil surface."|"23769239"|"24633922"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lehunt component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP813MT Subirrigated Saline-Sodic Grassland ecological site.  Irrigated land capability classification is 7w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 70 within 30 inches of the soil surface."|"23769240"|"24633923"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Proposal soil is a minor component."|"23769241"|"24633924"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Proposal component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of fine-loamy outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769067"|"24633750"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wisdom component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769068"|"24633751"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769069"|"24633752"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23769070"|"24633753"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23769071"|"24633754"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foxgulch soil is a minor component."|"23769072"|"24633755"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23769073"|"24633756"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769074"|"24633757"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"23768918"|"24633601"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill soil is a minor component."|"23768919"|"24633602"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23768920"|"24633603"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 41 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768921"|"24633604"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"23768922"|"24633605"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 39 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768923"|"24633606"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"23769399"|"24634082"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769400"|"24634083"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussigbrod component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769401"|"24634084"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald soil is a minor component."|"23769402"|"24634085"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"23769456"|"24634139"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on mima mounds, intermontane basins. The parent material consists of fine-loamy outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769457"|"24634140"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of loamy skeletal outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6c. Irrigated land capability classification is 6c. This soil does not meet hydric criteria.   "|"23769458"|"24634141"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23769459"|"24634142"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23769460"|"24634143"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Plimpton component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of fine-loamy outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP820MT Upland Shrubland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769461"|"24634144"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of loamy skeletal outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769462"|"24634145"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769463"|"24634146"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23769464"|"24634147"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769465"|"24634148"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of loamy skeletal alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769466"|"24634149"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide soil is a minor component."|"23769467"|"24634150"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Plimpton component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769468"|"24634151"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769278"|"24633961"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussigbrod component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on mima mounds, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769279"|"24633962"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769280"|"24633963"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769281"|"24633964"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Briston component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769282"|"24633965"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769283"|"24633966"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769284"|"24633967"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23769285"|"24633968"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copperbasin component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches (depth from the mineral surface is 29 inches) during March, April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769126"|"24633809"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"23769127"|"24633810"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"23769128"|"24633811"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foxgulch soil is a minor component."|"23769129"|"24633812"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769130"|"24633813"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769131"|"24633814"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eachuston component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769132"|"24633815"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23768986"|"24633669"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danielvil soil is a minor component."|"23768987"|"24633670"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Englejard component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of coarse-loamy  over sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768988"|"24633671"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23768989"|"24633672"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23768990"|"24633673"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Englejard component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of coarse-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769469"|"24634152"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danielvil soil is a minor component."|"23769470"|"24634153"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769471"|"24634154"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussigbrod component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on mima mounds, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769472"|"24634155"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769473"|"24634156"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769474"|"24634157"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23769475"|"24634158"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769139"|"24633822"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussigbrod soil is a minor component."|"23769140"|"24633823"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danielvil, greater slopes soil is a minor component."|"23769141"|"24633824"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"23769142"|"24633825"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769143"|"24633826"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Englejard component makes up 29 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of coarse-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769144"|"24633827"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23769145"|"24633828"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danielvil component makes up 31 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769146"|"24633829"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769286"|"24633969"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussigbrod soil is a minor component."|"23769287"|"24633970"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, greater slopes soil is a minor component."|"23769288"|"24633971"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769289"|"24633972"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 80 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769290"|"24633973"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maybee component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of loamy skeletal  over sandy skeletal alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768991"|"24633674"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23768992"|"24633675"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23768993"|"24633676"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23768994"|"24633677"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"23768995"|"24633678"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Plimpton soil is a minor component."|"23768996"|"24633679"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, stream terraces, intermontane basins. The parent material consists of loamy skeletal alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23768997"|"24633680"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide soil is a minor component."|"23768998"|"24633681"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danielvil soil is a minor component."|"23769291"|"24633974"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769292"|"24633975"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit soil is a minor component."|"23769293"|"24633976"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769294"|"24633977"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769295"|"24633978"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of residuum weathered from metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769296"|"24633979"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Englejard soil is a minor component."|"23769297"|"24633980"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium over residuum weathered from granite and gneiss and/or schist. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769298"|"24633981"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doolittle component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, depressions, intermontane basins. The parent material consists of alluvium and/or colluvium over residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA165MT Thin Claypan (TCp) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"23769116"|"24633799"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald soil is a minor component."|"23769117"|"24633800"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak, very stony soil is a minor component."|"23769118"|"24633801"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"23769119"|"24633802"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide soil is a minor component."|"23769120"|"24633803"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of fine-loamy alluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769121"|"24633804"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"23769122"|"24633805"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, occasionally ponded soil is a minor component."|"23769123"|"24633806"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit, stony soil is a minor component."|"23769124"|"24633807"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769125"|"24633808"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"23769357"|"24634040"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"23768883"|"24633566"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Denied access is a miscellaneous area."|"23769165"|"24633848"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"23768913"|"24633596"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23768914"|"24633597"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverslide component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of calcareous clayey outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"23768915"|"24633598"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp, greater slopes soil is a minor component."|"23768916"|"24633599"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"23768917"|"24633600"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maybee soil is a minor component."|"23769476"|"24634159"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Plimpton soil is a minor component."|"23769477"|"24634160"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769478"|"24634161"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"23769479"|"24634162"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide soil is a minor component."|"23769480"|"24634163"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of loamy skeletal alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site.  Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769481"|"24634164"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maurice, greater slopes, stony soil is a minor component."|"23769429"|"24634112"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769430"|"24634113"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on ground moraines, intermontane basins. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769431"|"24634114"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, very stony soil is a minor component."|"23769432"|"24634115"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on ground moraines, intermontane basins. The parent material consists of till over residuum weathered from granite and gneiss and/or schist. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769433"|"24634116"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald soil is a minor component."|"23769434"|"24634117"
08/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maurice, bouldery component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on ground moraines, intermontane basins. The parent material consists of loamy skeletal till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769435"|"24634118"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Plimpton soil is a minor component."|"23769436"|"24634119"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maurice, very bouldery soil is a minor component."|"23769267"|"24633950"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on ground moraines, mountains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769268"|"24633951"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maurice, bouldery component makes up 55 percent of the map unit. Slopes are 8 to 25 percent. This component is on ground moraines, mountains. The parent material consists of loamy skeletal till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769269"|"24633952"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, bouldery soil is a minor component."|"23769270"|"24633953"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"23769271"|"24633954"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, bouldery soil is a minor component."|"23769272"|"24633955"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald soil is a minor component."|"23769444"|"24634127"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on fan remnants, hillslopes, intermontane basins. The parent material consists of loamy skeletal alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769445"|"24634128"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, greater slopes soil is a minor component."|"23769446"|"24634129"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, fan remnants, intermontane basins. The parent material consists of fine-loamy alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769447"|"24634130"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"23769448"|"24634131"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danielvil component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6c.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"23768974"|"24633657"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danielvil, rarely flooded, wet component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6c.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"23768975"|"24633658"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769299"|"24633982"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769300"|"24633983"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769301"|"24633984"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin, very bouldery soil is a minor component."|"23768999"|"24633682"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769000"|"24633683"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"23769001"|"24633684"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769002"|"24633685"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains, intermontane basins. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23769449"|"24634132"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foxgulch component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during May, June, July. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769450"|"24634133"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copperbasin component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches (depth from the mineral surface is 29 inches) during March, April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"23769451"|"24634134"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769452"|"24634135"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"23769453"|"24634136"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769454"|"24634137"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769455"|"24634138"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769273"|"24633956"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, stony soil is a minor component."|"23769274"|"24633957"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23769275"|"24633958"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 75 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, outwash plains, intermontane basins. The parent material consists of sandy and gravelly alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"23769276"|"24633959"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foxgulch soil is a minor component."|"23769277"|"24633960"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 90 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"23769133"|"24633816"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zelda component makes up 29 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP813MT Subirrigated Saline-Sodic Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"23769134"|"24633817"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769135"|"24633818"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23769136"|"24633819"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eine soil is a minor component."|"23769137"|"24633820"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nana component makes up 31 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP813MT Subirrigated Saline-Sodic Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"23769138"|"24633821"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"23768982"|"24633665"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kilgore component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23768983"|"24633666"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of fine-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23768984"|"24633667"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"23768985"|"24633668"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"23769029"|"24633712"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dunkleber soil is a minor component."|"23769030"|"24633713"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kilgore component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of fine-loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769031"|"24633714"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during January, February, March, April, May, December. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"23769032"|"24633715"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"23769033"|"24633716"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Upsata component makes up 35 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769158"|"24633841"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769159"|"24633842"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Petty component makes up 15 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769160"|"24633843"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Como soil is a minor component."|"23769161"|"24633844"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 25 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769162"|"24633845"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lilylake soil is a minor component."|"23769163"|"24633846"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"23769164"|"24633847"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lowder, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769307"|"24633990"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lilylake soil is a minor component."|"23769308"|"24633991"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wichup, rarely flooded component makes up 40 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 6 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 33 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.   "|"23769309"|"24633992"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, rarely flooded component makes up 30 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769310"|"24633993"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"23769335"|"24634018"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 30 percent of the map unit. Slopes are 0 to 20 percent. This component is on alluvial fans, mountains. The parent material consists of alluvium derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"23769336"|"24634019"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 25 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 6 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"23769337"|"24634020"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gambler soil is a minor component."|"23769338"|"24634021"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"23769339"|"24634022"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"23769340"|"24634023"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Petty component makes up 20 percent of the map unit. Slopes are 5 to 40 percent. This component is on fan remnants, mountains. The parent material consists of volcanic ash over alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769352"|"24634035"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea soil is a minor component."|"23769353"|"24634036"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 40 percent of the map unit. Slopes are 5 to 40 percent. This component is on alluvial fans, mountains. The parent material consists of volcanic ash over colluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769354"|"24634037"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Swifton soil is a minor component."|"23769355"|"24634038"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 20 percent of the map unit. Slopes are 5 to 40 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769356"|"24634039"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Petty component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769376"|"24634059"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Garlet soil is a minor component."|"23769377"|"24634060"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769378"|"24634061"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 30 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769379"|"24634062"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"23769380"|"24634063"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Upsata component makes up 30 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of volcanic ash over alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769381"|"24634064"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"23769382"|"24634065"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 25 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769383"|"24634066"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elvick soil is a minor component."|"23769384"|"24634067"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lowder, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769385"|"24634068"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23768860"|"24633543"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768861"|"24633544"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768862"|"24633545"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepecreek component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768863"|"24633546"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"23768864"|"24633547"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769147"|"24633830"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Howardsville component makes up 40 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769148"|"24633831"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 15 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769149"|"24633832"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 30 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"23769150"|"24633833"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepecreek soil is a minor component."|"23769151"|"24633834"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23768869"|"24633552"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dunkleber, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 10 percent. This component is on fan remnants, drainageways, mountains. The parent material consists of organic material over alluvium derived from sandstone and shale and/or conglomerate. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23768870"|"24633553"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Woodhurst soil is a minor component."|"23768871"|"24633554"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 26 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from conglomerate and/or sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768872"|"24633555"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"23768873"|"24633556"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat soil is a minor component."|"23768874"|"24633557"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wetopa component makes up 24 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from conglomerate and/or sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768875"|"24633558"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset soil is a minor component."|"23768865"|"24633548"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 55 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from conglomerate and/or sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"23768866"|"24633549"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from conglomerate and/or sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 6 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"23768867"|"24633550"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dunkleber, rarely flooded component makes up 15 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways on fan remnants, mountains. The parent material consists of organic material over alluvium derived from sandstone and shale and/or conglomerate. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"23768868"|"24633551"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 35 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768876"|"24633559"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Upsata component makes up 15 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768877"|"24633560"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elkner soil is a minor component."|"23768878"|"24633561"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768879"|"24633562"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 25 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768880"|"24633563"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"23768881"|"24633564"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Garlet soil is a minor component."|"23768882"|"24633565"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23768888"|"24633571"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on ice-margin mountain slopes, mountains. The parent material consists of alluvium and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768889"|"24633572"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23768890"|"24633573"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on ice-margin mountain slopes, mountains. The parent material consists of alluvium and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768891"|"24633574"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on ice-margin mountain slopes, mountains. The parent material consists of alluvium and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768892"|"24633575"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlesalmon soil is a minor component."|"23769341"|"24634024"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769342"|"24634025"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 30 percent of the map unit. Slopes are 0 to 10 percent. This component is on glacial-valley floors, mountains. The parent material consists of volcanic ash over glaciofluvial deposits derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP906MT Subirrigated Cold Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"23769343"|"24634026"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"23769344"|"24634027"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lilylake soil is a minor component."|"23769345"|"24634028"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lowder, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways on glacial-valley floors, mountains. The parent material consists of glaciofluvial deposits derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769346"|"24634029"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on glacial-valley floors, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769347"|"24634030"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Como soil is a minor component."|"23769361"|"24634044"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gateview component makes up 20 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769362"|"24634045"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769363"|"24634046"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769364"|"24634047"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 40 percent of the map unit. Slopes are 10 to 40 percent. This component is on ground moraines, mountains. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769365"|"24634048"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Stecum soil is a minor component."|"23769184"|"24633867"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 30 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769185"|"24633868"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lowder, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium and/or slope alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"23769186"|"24633869"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769187"|"24633870"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Como soil is a minor component."|"23769213"|"24633896"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769214"|"24633897"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769215"|"24633898"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 30 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769216"|"24633899"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 20 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769170"|"24633853"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 29 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769171"|"24633854"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"23769172"|"24633855"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"23769173"|"24633856"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 31 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769174"|"24633857"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 20 percent of the map unit. Slopes are 5 to 40 percent. This component is on landslides, mountains. The parent material consists of complex landslide deposits derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769018"|"24633701"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769019"|"24633702"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 25 percent of the map unit. Slopes are 5 to 40 percent. This component is on landslides, mountains. The parent material consists of complex landslide deposits derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769020"|"24633703"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"23769021"|"24633704"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"23769022"|"24633705"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule component makes up 30 percent of the map unit. Slopes are 5 to 40 percent. This component is on landslides, mountains. The parent material consists of complex landslide deposits derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769023"|"24633706"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 20 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768899"|"24633582"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 30 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768900"|"24633583"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 50 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768901"|"24633584"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from conglomerate. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP906MT Subirrigated Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769057"|"24633740"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elvick soil is a minor component."|"23769058"|"24633741"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP906MT Subirrigated Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769059"|"24633742"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 40 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"23769060"|"24633743"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder, frequently flooded soil is a minor component."|"23769061"|"24633744"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769042"|"24633725"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"23769043"|"24633726"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gambler soil is a minor component."|"23769044"|"24633727"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769045"|"24633728"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Howardsville component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769046"|"24633729"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769175"|"24633858"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 50 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769176"|"24633859"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769177"|"24633860"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769178"|"24633861"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769366"|"24634049"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769367"|"24634050"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769368"|"24634051"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 30 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769369"|"24634052"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 45 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769370"|"24634053"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"23769322"|"24634005"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769323"|"24634006"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth soil is a minor component."|"23769324"|"24634007"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lilylake, frequently flooded soil is a minor component."|"23769325"|"24634008"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen, rarely flooded soil is a minor component."|"23769326"|"24634009"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 35 percent of the map unit. Slopes are 0 to 20 percent. This component is on fan remnants, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769327"|"24634010"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways on fan remnants, mountains. The parent material consists of alluvium and/or slope alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"23769328"|"24634011"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 25 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769047"|"24633730"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769048"|"24633731"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769049"|"24633732"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"23769050"|"24633733"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea soil is a minor component."|"23769051"|"24633734"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769179"|"24633862"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 35 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769180"|"24633863"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769181"|"24633864"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Howardsville soil is a minor component."|"23769182"|"24633865"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769183"|"24633866"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 30 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"23768851"|"24633534"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 40 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768852"|"24633535"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"23768853"|"24633536"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 15 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768854"|"24633537"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768855"|"24633538"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"23769302"|"24633985"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wichup, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 6 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 33 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.   "|"23769303"|"24633986"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769304"|"24633987"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"23769305"|"24633988"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dunkleber, rarely flooded component makes up 30 percent of the map unit. Slopes are 0 to 10 percent. This component is on fan remnants, drainageways, mountains. The parent material consists of organic material over alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769306"|"24633989"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elvick soil is a minor component."|"23768856"|"24633539"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP906MT Subirrigated Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768857"|"24633540"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lowder, frequently flooded component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23768858"|"24633541"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake, frequently flooded component makes up 30 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 40 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"23768859"|"24633542"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 60 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768884"|"24633567"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768885"|"24633568"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 25 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768886"|"24633569"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Comad soil is a minor component."|"23768887"|"24633570"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769010"|"24633693"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elkner soil is a minor component."|"23769011"|"24633694"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 41 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769012"|"24633695"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 39 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769013"|"24633696"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 30 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769014"|"24633697"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769015"|"24633698"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769016"|"24633699"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769017"|"24633700"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore component makes up 50 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"23769358"|"24634041"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"23769359"|"24634042"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769360"|"24634043"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769371"|"24634054"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 29 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769372"|"24634055"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 31 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769373"|"24634056"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769374"|"24634057"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769375"|"24634058"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wichup, rarely flooded soil is a minor component."|"23769329"|"24634012"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wander component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways, mountains. The parent material consists of alluvium and/or slope alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769330"|"24634013"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn, frequently flooded component makes up 40 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium and/or slope alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"23769331"|"24634014"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kamack soil is a minor component."|"23769332"|"24634015"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, rarely flooded component makes up 15 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways, mountains. The parent material consists of alluvium and/or slope alluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"23769333"|"24634016"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ledgefork soil is a minor component."|"23769334"|"24634017"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on glacial-valley floors, mountains. The parent material consists of glaciofluvial deposits derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769062"|"24633745"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on glacial-valley floors, mountains. The parent material consists of glaciofluvial deposits derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769063"|"24633746"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elvick soil is a minor component."|"23769064"|"24633747"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"23769065"|"24633748"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake, occasionally flooded component makes up 20 percent of the map unit. Slopes are 0 to 10 percent. This component is on drainageways on glacial-valley floors, mountains. The parent material consists of glaciofluvial deposits derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 43 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"23769066"|"24633749"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Petty component makes up 35 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769034"|"24633717"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 55 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769035"|"24633718"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Garlet soil is a minor component."|"23769036"|"24633719"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ellena component makes up 30 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769024"|"24633707"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769025"|"24633708"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769026"|"24633709"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepecreek component makes up 35 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769027"|"24633710"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Comad soil is a minor component."|"23769028"|"24633711"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 20 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769348"|"24634031"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 45 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769349"|"24634032"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 25 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769350"|"24634033"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Como soil is a minor component."|"23769351"|"24634034"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769052"|"24633735"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gambler soil is a minor component."|"23769053"|"24633736"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 25 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769054"|"24633737"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Howardsville soil is a minor component."|"23769055"|"24633738"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769056"|"24633739"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Howardsville component makes up 20 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769311"|"24633994"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 40 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769312"|"24633995"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gateview component makes up 30 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769313"|"24633996"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769314"|"24633997"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepecreek soil is a minor component."|"23769315"|"24633998"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Targhee component makes up 25 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769316"|"24633999"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23769317"|"24634000"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 25 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769318"|"24634001"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"23769319"|"24634002"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 30 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23769320"|"24634003"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Garlet soil is a minor component."|"23769321"|"24634004"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Worock soil is a minor component."|"23769152"|"24633835"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Matcher soil is a minor component."|"23769153"|"24633836"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 45 percent of the map unit. Slopes are 0 to 25 percent. This component is on ridges, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769154"|"24633837"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"23769155"|"24633838"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moran component makes up 25 percent of the map unit. Slopes are 0 to 25 percent. This component is on ridges, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"23769156"|"24633839"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Como soil is a minor component."|"23769157"|"24633840"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wander component makes up 40 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BY021ID Mountain Loamy 22+ PZ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769166"|"24633849"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst component makes up 30 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BY021ID Mountain Loamy 22+ PZ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769167"|"24633850"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BY021ID Mountain Loamy 22+ PZ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"23769168"|"24633851"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Groomer soil is a minor component."|"23769169"|"24633852"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gateview component makes up 20 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769037"|"24633720"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"23769038"|"24633721"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 31 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769039"|"24633722"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 29 percent of the map unit. Slopes are 0 to 20 percent. This component is on gentle mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23769040"|"24633723"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"23769041"|"24633724"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"23768893"|"24633576"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gateview soil is a minor component."|"23768894"|"24633577"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redchief soil is a minor component."|"23768895"|"24633578"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 30 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BY021ID Mountain Loamy 22+ PZ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768896"|"24633579"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 25 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 7 percent. This component is in the R043BY021ID Mountain Loamy 22+ PZ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768897"|"24633580"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BY021ID Mountain Loamy 22+ PZ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"23768898"|"24633581"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, extremely stony soil is a minor component."|"23768976"|"24633659"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"23768977"|"24633660"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768978"|"24633661"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"23768979"|"24633662"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"23768980"|"24633663"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"23768981"|"24633664"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"23769003"|"24633686"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regulus, occasionally flooded soil is a minor component."|"23769004"|"24633687"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Medicinelodge, occasionally flooded component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood-plain steps, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches (depth from the mineral surface is 8 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769005"|"24633688"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769006"|"24633689"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slagamelt soil is a minor component."|"23769007"|"24633690"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, occasionally flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769008"|"24633691"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, occasionally flooded component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"23769009"|"24633692"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"23769437"|"24634120"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Plimpton component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769438"|"24634121"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Plimpton, greater slopes soil is a minor component."|"23769439"|"24634122"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"23769440"|"24634123"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp, greater slopes soil is a minor component."|"23769441"|"24634124"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat, occasionally flooded soil is a minor component."|"23769442"|"24634125"
12/06/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shewag soil is a minor component."|"23769443"|"24634126"
