08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adger component makes up 90 percent of the map unit. Slopes are 0 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE014MT Dense Clay (DC)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"24973707"|"26476472"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"24973708"|"26476473"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973709"|"26476474"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"24973710"|"26476475"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"24973872"|"26476637"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Benz soil is a minor component."|"24973873"|"26476638"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973874"|"26476639"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973875"|"26476640"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"24973876"|"26476641"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24973877"|"26476642"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"24973878"|"26476643"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fluvaquents, channeled, frequently flooded soil is a minor component."|"24973915"|"26476680"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Banks, occasionally flooded component makes up 82 percent of the map unit. Slopes are 0 to 6 percent. This component is on flood-plain steps on river valleys. The parent material consists of sandy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY042ND Sandy Terrace ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"24973916"|"26476681"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles, occasionally flooded soil is a minor component."|"24973917"|"26476682"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon, fine sandy loam, occasionally flooded soil is a minor component."|"24973918"|"26476683"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Benz component makes up 90 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE011MT Saline Upland (SU)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"24973951"|"26476716"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973952"|"26476717"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973953"|"26476718"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"24973954"|"26476719"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Benz component makes up 45 percent of the map unit. Slopes are 0 to 8 percent. This component is on dissected alluvial fans on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE011MT Saline Upland (SU)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"24974005"|"26476770"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (Sy)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974006"|"26476771"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24974007"|"26476772"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"24974008"|"26476773"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24974009"|"26476774"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"24974010"|"26476775"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"24974011"|"26476776"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowbells component makes up 90 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973711"|"26476476"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"24973712"|"26476477"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"24973713"|"26476478"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973714"|"26476479"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973715"|"26476480"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"24973716"|"26476481"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973717"|"26476482"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973718"|"26476483"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"24973911"|"26476676"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973912"|"26476677"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973913"|"26476678"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973914"|"26476679"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24973719"|"26476484"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973720"|"26476485"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973721"|"26476486"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"24973722"|"26476487"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"24973723"|"26476488"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973724"|"26476489"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973725"|"26476490"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE007MT Overflow (Ov)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24973726"|"26476491"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE007MT Overflow (Ov)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973727"|"26476492"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE007MT Overflow (Ov)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973728"|"26476493"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 60 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (Sy)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"24973955"|"26476720"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"24973956"|"26476721"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24973957"|"26476722"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas of rock outcrop soil is a minor component."|"24973958"|"26476723"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blanchard component makes up 30 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of sandy alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (Sa)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"24973959"|"26476724"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973960"|"26476725"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24973729"|"26476494"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973730"|"26476495"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"24973731"|"26476496"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 85 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE005MT Clayey-Steep (CyStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973732"|"26476497"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dooley component makes up 90 percent of the map unit. Slopes are 2 to 6 percent.  The parent material consists of sandy alluvium over loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE003MT Sandy (Sy)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973733"|"26476498"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"24973734"|"26476499"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973735"|"26476500"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"24973736"|"26476501"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"24973737"|"26476502"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farnuf component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973929"|"26476694"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973930"|"26476695"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973931"|"26476696"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973932"|"26476697"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farnuf component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973961"|"26476726"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973962"|"26476727"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973963"|"26476728"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973964"|"26476729"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie, occasionally flooded soil is a minor component."|"24973906"|"26476671"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles, occasionally flooded soil is a minor component."|"24973907"|"26476672"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fluvaquents, channeled, frequently flooded soil is a minor component."|"24973908"|"26476673"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon, occasionally flooded component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps on river valleys. The parent material consists of fine-loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY041ND Loamy Terrace ecological site. Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973909"|"26476674"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridgelawn, occasionally flooded soil is a minor component."|"24973910"|"26476675"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973738"|"26476503"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973739"|"26476504"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973740"|"26476505"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 90 percent of the map unit. Slopes are 1 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24973741"|"26476506"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridgelawn, occasionally flooded soil is a minor component."|"24973919"|"26476684"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fluvaquents, channeled, frequently flooded soil is a minor component."|"24973920"|"26476685"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles, occasionally flooded soil is a minor component."|"24973921"|"26476686"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie, occasionally flooded soil is a minor component."|"24973922"|"26476687"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon, occasionally flooded component makes up 75 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps on river valleys. The parent material consists of fine-loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY041ND Loamy Terrace ecological site. Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973923"|"26476688"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon, loam, occasionally flooded soil is a minor component."|"24973924"|"26476689"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973742"|"26476507"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973743"|"26476508"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973744"|"26476509"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridgelawn soil is a minor component."|"24973745"|"26476510"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hoffmanville component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of clayey alluvium over sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (Cy) RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973746"|"26476511"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 85 percent of the map unit. Slopes are 15 to 40 percent. This component is on hills on plains. The parent material consists of residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-Steep (SiStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973941"|"26476706"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"24973942"|"26476707"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"24973943"|"26476708"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973944"|"26476709"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973945"|"26476710"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 50 percent of the map unit. Slopes are 20 to 40 percent.  The parent material consists of residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-Steep (SiStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"24973747"|"26476512"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"24973748"|"26476513"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973749"|"26476514"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973750"|"26476515"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"24973751"|"26476516"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"24973752"|"26476517"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"24973753"|"26476518"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blanchard component makes up 40 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of sandy alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (Sa)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"24973754"|"26476519"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 50 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-Steep (SiStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"24973755"|"26476520"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973756"|"26476521"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"24973757"|"26476522"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"24973758"|"26476523"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973759"|"26476524"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kirby soil is a minor component."|"24973980"|"26476745"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"24973981"|"26476746"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"24973982"|"26476747"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"24973983"|"26476748"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 50 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 12 to 24 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-Steep (SiStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973984"|"26476749"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE005MT Clayey-Steep (CyStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973985"|"26476750"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 50 percent of the map unit. Slopes are 15 to 65 percent.  The parent material consists of residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-Steep (SiStp)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"24973760"|"26476525"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973761"|"26476526"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"24973762"|"26476527"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973763"|"26476528"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973764"|"26476529"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 30 percent of the map unit. Slopes are 15 to 65 percent.  The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE017MT Very Shallow (VSw)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24973765"|"26476530"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973766"|"26476531"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lihen component makes up 85 percent of the map unit. Slopes are 4 to 15 percent.  The parent material consists of sandy alluvium and/or sandy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE018MT Sands (Sa)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973767"|"26476532"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"24973768"|"26476533"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"24973769"|"26476534"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"24973770"|"26476535"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973771"|"26476536"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973772"|"26476537"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoffmanville soil is a minor component."|"24973773"|"26476538"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973774"|"26476539"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973775"|"26476540"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"24973776"|"26476541"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridgelawn soil is a minor component."|"24973777"|"26476542"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohler component makes up 85 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE061MT Clayey (Cy) (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24973778"|"26476543"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973779"|"26476544"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"24973780"|"26476545"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohler component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE073MT Dense Clay (DC) (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24973781"|"26476546"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lallie, occasionally flooded component makes up 92 percent of the map unit. Slopes are 0 to 1 percent. This component is on oxbows on flood plains on river valleys. The parent material consists of clayey alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is occasionally flooded. It is occasionally ponded. A seasonal zone of water saturation is at 9 inches during March, April, May, June. Organic matter content in the surface horizon is about 6 percent. This component is in the R054XY037ND Wet Meadow ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973883"|"26476648"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon, occasionally flooded soil is a minor component."|"24973884"|"26476649"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mckeen, occasionally flooded soil is a minor component."|"24973885"|"26476650"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973782"|"26476547"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"24973783"|"26476548"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marias component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (Cy) RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"24973784"|"26476549"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973785"|"26476550"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973786"|"26476551"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973787"|"26476552"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973788"|"26476553"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973789"|"26476554"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoffmanville soil is a minor component."|"24973790"|"26476555"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ridgelawn component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium over sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973791"|"26476556"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"24974021"|"26476786"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"24974022"|"26476787"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"24974023"|"26476788"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973792"|"26476557"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973793"|"26476558"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"24973794"|"26476559"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973795"|"26476560"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (Cy) RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973796"|"26476561"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"24973797"|"26476562"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973798"|"26476563"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973799"|"26476564"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973800"|"26476565"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 85 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (Cy) RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973801"|"26476566"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973802"|"26476567"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973803"|"26476568"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"24973804"|"26476569"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973805"|"26476570"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973806"|"26476571"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24973807"|"26476572"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973808"|"26476573"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"24973809"|"26476574"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973810"|"26476575"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 72 percent of the map unit. Slopes are 6 to 9 percent. This component is on hillslopes on plains. The parent material consists of slope alluvium over residuum weathered from mudstone. Depth to a root restrictive layer, bedrock, paralithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R054XY031ND Loamy ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973866"|"26476631"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arnegard soil is a minor component."|"24973867"|"26476632"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"24973868"|"26476633"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"24973869"|"26476634"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"24973870"|"26476635"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973871"|"26476636"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Strip mines is a miscellaneous area."|"24973811"|"26476576"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Haplaquents component makes up 92 percent of the map unit. Slopes are 0 to 2 percent. This component is on channels on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 12 inches during May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE012MT Saline Lowland (SL)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 19 within 30 inches of the soil surface."|"24973901"|"26476666"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24973902"|"26476667"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973903"|"26476668"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24973904"|"26476669"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973905"|"26476670"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tally component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium and/or eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (Sy)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973812"|"26476577"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"24973813"|"26476578"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973814"|"26476579"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973815"|"26476580"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tally component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium and/or eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (Sy)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973816"|"26476581"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973817"|"26476582"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lihen soil is a minor component."|"24973818"|"26476583"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973819"|"26476584"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973820"|"26476585"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tally component makes up 85 percent of the map unit. Slopes are 4 to 12 percent.  The parent material consists of loamy alluvium and/or eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (Sy)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973821"|"26476586"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973822"|"26476587"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lihen soil is a minor component."|"24973823"|"26476588"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973824"|"26476589"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"24973825"|"26476590"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24973826"|"26476591"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lihen soil is a minor component."|"24973827"|"26476592"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973828"|"26476593"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973829"|"26476594"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"24973830"|"26476595"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973831"|"26476596"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tinsley component makes up 40 percent of the map unit. Slopes are 15 to 65 percent.  The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AY716MT Sandy Gravel (SyGr) ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973832"|"26476597"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tinsley component makes up 50 percent of the map unit. Slopes are 15 to 65 percent.  The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AY716MT Sandy Gravel (SyGr) ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973833"|"26476598"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles, occasionally flooded component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps on river valleys. The parent material consists of coarse-loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY042ND Sandy Terrace ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973925"|"26476690"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fluvaquents, channeled, frequently flooded soil is a minor component."|"24973926"|"26476691"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks, occasionally flooded soil is a minor component."|"24973927"|"26476692"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon, occasionally flooded soil is a minor component."|"24973928"|"26476693"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24973834"|"26476599"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Turner component makes up 55 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"24973835"|"26476600"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973836"|"26476601"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverton component makes up 35 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE191MT Shallow to Gravel (SwGr)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973837"|"26476602"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973838"|"26476603"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 90 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE014MT Dense Clay (DC)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"24973839"|"26476604"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24973840"|"26476605"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"24973841"|"26476606"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24973842"|"26476607"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"24973886"|"26476651"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"24973887"|"26476652"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (Lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973888"|"26476653"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (Lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973889"|"26476654"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973890"|"26476655"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"24973891"|"26476656"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973892"|"26476657"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"24973972"|"26476737"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"24973973"|"26476738"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"24973974"|"26476739"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973975"|"26476740"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (Lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973976"|"26476741"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (Lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973977"|"26476742"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"24973978"|"26476743"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973979"|"26476744"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (Lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973858"|"26476623"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY704MT Limy (Ly) ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973859"|"26476624"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams, low precipitation soil is a minor component."|"24973860"|"26476625"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"24973861"|"26476626"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"24973862"|"26476627"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"24973863"|"26476628"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"24973864"|"26476629"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973865"|"26476630"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973851"|"26476616"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973852"|"26476617"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams, low precipitation soil is a minor component."|"24973853"|"26476618"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"24973854"|"26476619"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"24973855"|"26476620"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"24973856"|"26476621"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"24973857"|"26476622"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"24973843"|"26476608"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"24973844"|"26476609"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"24973845"|"26476610"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"24973846"|"26476611"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"24973847"|"26476612"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (Lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973848"|"26476613"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"24973849"|"26476614"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"24973850"|"26476615"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 75 percent of the map unit. Slopes are 15 to 60 percent. This component is on hillslopes on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY705MT Limy Steep (LyStp) ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24973986"|"26476751"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"24973987"|"26476752"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"24973988"|"26476753"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"24973989"|"26476754"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahl soil is a minor component."|"24973990"|"26476755"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arnegard soil is a minor component."|"24973991"|"26476756"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 45 percent of the map unit. Slopes are 15 to 65 percent.  The parent material consists of loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE058MT Loamy Steep (Lostp)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973992"|"26476757"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 35 percent of the map unit. Slopes are 15 to 65 percent.  The parent material consists of residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE058MT Loamy Steep (Lostp)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"24973993"|"26476758"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"24973994"|"26476759"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"24973995"|"26476760"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"24973996"|"26476761"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973997"|"26476762"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"24973669"|"26476434"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"24973670"|"26476435"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24973671"|"26476436"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Manning soil is a minor component."|"24973672"|"26476437"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on low hills on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973969"|"26476734"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"24973970"|"26476735"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on low hills on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973971"|"26476736"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"24973879"|"26476644"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"24973880"|"26476645"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin, warm component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973881"|"26476646"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"24973882"|"26476647"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24973676"|"26476441"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"24973677"|"26476442"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973678"|"26476443"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24973673"|"26476438"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"24973674"|"26476439"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973675"|"26476440"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24973965"|"26476730"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"24973966"|"26476731"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973967"|"26476732"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry, saline substratum soil is a minor component."|"24973968"|"26476733"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regent soil is a minor component."|"24973688"|"26476453"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973689"|"26476454"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24973690"|"26476455"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambert component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"24973691"|"26476456"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973692"|"26476457"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"24973693"|"26476458"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"24973694"|"26476459"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"24973933"|"26476698"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"24973934"|"26476699"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"24973935"|"26476700"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973936"|"26476701"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973946"|"26476711"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna, saline substratum soil is a minor component."|"24973947"|"26476712"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree, warm soil is a minor component."|"24973948"|"26476713"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall, warm soil is a minor component."|"24973949"|"26476714"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alona soil is a minor component."|"24973950"|"26476715"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"24973893"|"26476658"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"24973894"|"26476659"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tricart soil is a minor component."|"24973895"|"26476660"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambeth component makes up 30 percent of the map unit. Slopes are 4 to 12 percent. This component is on low hills on sedimentary plains. The parent material consists of silty residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973896"|"26476661"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 40 percent of the map unit. Slopes are 4 to 12 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"24973897"|"26476662"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 15 percent of the map unit. Slopes are 4 to 12 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (Sw)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973898"|"26476663"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"24973899"|"26476664"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"24973900"|"26476665"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"24973998"|"26476763"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"24973999"|"26476764"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambeth component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974000"|"26476765"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24974001"|"26476766"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alona soil is a minor component."|"24974002"|"26476767"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"24974003"|"26476768"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"24974004"|"26476769"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"24973937"|"26476702"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"24973938"|"26476703"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"24973939"|"26476704"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973940"|"26476705"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin component makes up 65 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973703"|"26476468"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eapa component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"24973704"|"26476469"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"24973705"|"26476470"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"24973706"|"26476471"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin component makes up 85 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973682"|"26476447"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spinekop soil is a minor component."|"24973683"|"26476448"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"24973684"|"26476449"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"24973685"|"26476450"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"24973686"|"26476451"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Degrand soil is a minor component."|"24973687"|"26476452"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Floweree component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"24973679"|"26476444"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"24973680"|"26476445"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"24973681"|"26476446"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"24974037"|"26476802"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"24974038"|"26476803"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24974039"|"26476804"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"24974040"|"26476805"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24974041"|"26476806"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"24974042"|"26476807"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24974043"|"26476808"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"24974044"|"26476809"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"24974045"|"26476810"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"24974046"|"26476811"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24974047"|"26476812"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regent soil is a minor component."|"24973695"|"26476460"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"24973696"|"26476461"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lisk soil is a minor component."|"24973697"|"26476462"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24973698"|"26476463"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambert component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"24973699"|"26476464"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"24973700"|"26476465"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY721MT Thin Breaks (TB) ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"24973701"|"26476466"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"24973702"|"26476467"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"24974048"|"26476813"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE191MT Shallow to Gravel (SwGr)   RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974049"|"26476814"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Littlemo component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974050"|"26476815"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"24974051"|"26476816"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tricart soil is a minor component."|"24974052"|"26476817"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 38 percent of the map unit. Slopes are 9 to 15 percent. This component is on ridges on sedimentary plains. The parent material consists of fine-silty residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY030ND Shallow Loamy ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"24974012"|"26476777"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chama component makes up 26 percent of the map unit. Slopes are 9 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of fine-silty residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R054XY046ND Limy Residual ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974013"|"26476778"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sen component makes up 16 percent of the map unit. Slopes are 9 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of fine-silty residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R054XY031ND Loamy ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"24974014"|"26476779"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vebar soil is a minor component."|"24974015"|"26476780"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arnegard soil is a minor component."|"24974016"|"26476781"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"24974017"|"26476782"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Janesburg soil is a minor component."|"24974018"|"26476783"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24974019"|"26476784"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maschetah soil is a minor component."|"24974020"|"26476785"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"24974053"|"26476818"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"24974054"|"26476819"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24974055"|"26476820"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AY001MT Loamy (Lo) 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"24974056"|"26476821"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24974057"|"26476822"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24974058"|"26476823"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24974059"|"26476824"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 90 percent of the map unit. Slopes are 0 to 1 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24974060"|"26476825"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24974061"|"26476826"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24974062"|"26476827"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24974063"|"26476828"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Loamy (Lo)  (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"24974064"|"26476829"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"24974065"|"26476830"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24974066"|"26476831"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"24974067"|"26476832"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohler component makes up 92 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY718MT Slough (Sl) ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974068"|"26476833"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Banks component makes up 90 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE062MT Sandy (Sy) (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"24974069"|"26476834"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24974070"|"26476835"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"24974071"|"26476836"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas of riverwash soil is a minor component."|"24974072"|"26476837"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles component makes up 85 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (Sy) (Legacy) RRU 53AE ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974073"|"26476838"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"24974074"|"26476839"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"24974075"|"26476840"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoffmanville soil is a minor component."|"24974076"|"26476841"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"24974077"|"26476842"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"24974078"|"26476843"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridgelawn soil is a minor component."|"24974079"|"26476844"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"24974034"|"26476799"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"24974035"|"26476800"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minnewaukan, frequently flooded soil is a minor component."|"24974036"|"26476801"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Janesburg soil is a minor component."|"24974024"|"26476789"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"24974025"|"26476790"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 25 percent of the map unit. Slopes are 6 to 9 percent. This component is on hillslopes on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY030ND Shallow Loamy ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"24974026"|"26476791"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sen component makes up 20 percent of the map unit. Slopes are 6 to 9 percent. This component is on hillslopes on plains. The parent material consists of residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R054XY031ND Loamy ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"24974027"|"26476792"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chama component makes up 40 percent of the map unit. Slopes are 6 to 9 percent. This component is on hillslopes on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R054XY046ND Limy Residual ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"24974028"|"26476793"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail, frequently flooded soil is a minor component."|"24974029"|"26476794"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minnewaukan, frequently flooded component makes up 82 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps on river valleys. The parent material consists of stratified sandy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during March, April, May, June. Organic matter content in the surface horizon is about 1 percent. This component is in the R054XY037ND Wet Meadow ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"24974030"|"26476795"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minnewaukan, frequently flooded soil is a minor component."|"24974031"|"26476796"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mckeen, frequently flooded soil is a minor component."|"24974032"|"26476797"
06/03/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie, frequently flooded, ponded soil is a minor component."|"24974033"|"26476798"
