05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"25049501"|"26602390"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Draft Silty (si)   Rru 46-c  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049502"|"26602391"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"25049503"|"26602392"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049426"|"26602315"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049427"|"26602316"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spring creek component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049428"|"26602317"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beckton soil is a minor component."|"25049400"|"26602289"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blythe component makes up 95 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049401"|"26602290"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, foothills. The parent material consists of slope alluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25049864"|"26602753"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castle component makes up 95 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049865"|"26602754"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049866"|"26602755"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitlash soil is a minor component."|"25049867"|"26602756"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castle component makes up 75 percent of the map unit. Slopes are 15 to 35 percent. This component is on landslides, foothills. The parent material consists of colluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049868"|"26602757"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tyzak soil is a minor component."|"25049869"|"26602758"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049870"|"26602759"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"25049871"|"26602760"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chama component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"25049872"|"26602761"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25049873"|"26602762"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chama component makes up 65 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"25049874"|"26602763"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"25049875"|"26602764"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"25049876"|"26602765"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25049877"|"26602766"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chama component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049878"|"26602767"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Big Timber component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049879"|"26602768"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twin Creek soil is a minor component."|"25049880"|"26602769"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Darret soil is a minor component."|"25049881"|"26602770"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25049882"|"26602771"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049883"|"26602772"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049884"|"26602773"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Big Timber soil is a minor component."|"25049885"|"26602774"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twin Creek soil is a minor component."|"25049886"|"26602775"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049887"|"26602776"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25049888"|"26602777"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Big Timber soil is a minor component."|"25049889"|"26602778"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twin Creek soil is a minor component."|"25049890"|"26602779"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25049891"|"26602780"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25049892"|"26602781"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25049893"|"26602782"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 90 percent of the map unit. Slopes are 4 to 35 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049894"|"26602783"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049895"|"26602784"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castle component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, foothills. The parent material consists of slope alluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049863"|"26602752"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"25049862"|"26602751"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 90 percent of the map unit. Slopes are 4 to 35 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049861"|"26602750"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049860"|"26602749"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"25049859"|"26602748"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"25049858"|"26602747"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 95 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049857"|"26602746"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimmick soil is a minor component."|"25049856"|"26602745"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowdoin component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 45 inches during May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"25049855"|"26602744"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blythe component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049854"|"26602743"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beckton soil is a minor component."|"25049853"|"26602742"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049852"|"26602741"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spring creek component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049851"|"26602740"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"25049850"|"26602739"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049849"|"26602738"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beckton component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25049848"|"26602737"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"25049847"|"26602736"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049846"|"26602735"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beckton component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25049845"|"26602734"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"25049844"|"26602733"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 25 percent of the map unit. Slopes are 0 to 8 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC602MT Dense Clay (DC) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"25049843"|"26602732"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Laurel soil is a minor component."|"25049842"|"26602731"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beckton component makes up 65 percent of the map unit. Slopes are 0 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25049841"|"26602730"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"25049840"|"26602729"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beckton component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25049839"|"26602728"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"25049838"|"26602727"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"25049837"|"26602726"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sweetgrass soil is a minor component."|"25049836"|"26602725"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverton, cold component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC507MT Shallow to Gravel (SwGr) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049835"|"26602724"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverton component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC507MT Shallow to Gravel (SwGr) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049834"|"26602723"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bainville component makes up 95 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"25049833"|"26602722"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"25049832"|"26602721"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049831"|"26602720"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashuelot component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer, undefined, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049830"|"26602719"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terrad component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC602MT Dense Clay (DC) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049829"|"26602718"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 45 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC602MT Dense Clay (DC) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"25049828"|"26602717"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Laurel soil is a minor component."|"25049827"|"26602716"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beckton soil is a minor component."|"25049826"|"26602715"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 60 percent of the map unit. Slopes are 0 to 8 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC609MT Claypan (Cp) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"25049825"|"26602714"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Laurel component makes up 30 percent of the map unit. Slopes are 0 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC609MT Claypan (Cp) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"25049824"|"26602713"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beckton soil is a minor component."|"25049823"|"26602712"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25049822"|"26602711"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beckton component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during January, February, March, April, May, June, October, November, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC597MT Saline Lowland (SL) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25049821"|"26602710"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 60 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC597MT Saline Lowland (SL) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 7w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"25049820"|"26602709"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saline land soil is a minor component."|"25049819"|"26602708"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 60 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC602MT Dense Clay (DC) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"25049818"|"26602707"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Laurel soil is a minor component."|"25049817"|"26602706"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beckton component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25049816"|"26602705"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049815"|"26602704"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alder soil is a minor component."|"25049814"|"26602703"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049813"|"26602702"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alder, clay loam surface soil is a minor component."|"25049812"|"26602701"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria.   "|"25049811"|"26602700"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049810"|"26602699"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049809"|"26602698"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"25049808"|"26602697"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"25049807"|"26602696"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"25049806"|"26602695"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 95 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria.   "|"25049805"|"26602694"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"25049804"|"26602693"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 95 percent of the map unit. Slopes are 2 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25049803"|"26602692"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blythe soil is a minor component."|"25049802"|"26602691"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 90 percent of the map unit. Slopes are 8 to 18 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25049801"|"26602690"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25049800"|"26602689"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 95 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25049799"|"26602688"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25049798"|"26602687"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"25049797"|"26602686"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 70 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049796"|"26602685"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049795"|"26602684"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049794"|"26602683"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049793"|"26602682"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049792"|"26602681"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 70 percent of the map unit. Slopes are 8 to 12 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049791"|"26602680"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049790"|"26602679"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049789"|"26602678"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049788"|"26602677"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049787"|"26602676"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"25049786"|"26602675"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049785"|"26602674"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"25049784"|"26602673"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 50 percent of the map unit. Slopes are 35 to 70 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC517MT Very Shallow (VSw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049896"|"26602785"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25049897"|"26602786"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"25049898"|"26602787"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049899"|"26602788"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25049900"|"26602789"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25049901"|"26602790"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25049902"|"26602791"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 31 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049903"|"26602792"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duncom component makes up 29 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049904"|"26602793"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049905"|"26602794"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clayey alluvial land component makes up 100 percent of the map unit. Slopes are 2 to 15 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XC602MT Dense Clay (DC) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"25049906"|"26602795"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cobbly alluvial land component makes up 100 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC507MT Shallow to Gravel (SwGr) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049907"|"26602796"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25049908"|"26602797"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Colvin component makes up 46 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during March, April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25049909"|"26602798"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lamoure component makes up 44 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049910"|"26602799"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood component makes up 90 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049911"|"26602800"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spring creek soil is a minor component."|"25049912"|"26602801"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049913"|"26602802"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood component makes up 55 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049914"|"26602803"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spring creek soil is a minor component."|"25049915"|"26602804"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049916"|"26602805"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049917"|"26602806"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049918"|"26602807"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049919"|"26602808"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049920"|"26602809"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049921"|"26602810"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049922"|"26602811"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049923"|"26602812"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049924"|"26602813"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049925"|"26602814"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"25049926"|"26602815"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049927"|"26602816"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049928"|"26602817"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049929"|"26602818"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049930"|"26602819"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049931"|"26602820"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049932"|"26602821"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25049933"|"26602822"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049934"|"26602823"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 65 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049935"|"26602824"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049936"|"26602825"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 45 percent of the map unit. Slopes are 2 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049937"|"26602826"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 50 percent of the map unit. Slopes are 2 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049938"|"26602827"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25049939"|"26602828"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049940"|"26602829"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"25049941"|"26602830"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049942"|"26602831"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049943"|"26602832"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25049944"|"26602833"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049945"|"26602834"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25049946"|"26602835"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Darret component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049947"|"26602836"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Darret soil is a minor component."|"25049948"|"26602837"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25049949"|"26602838"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Darret component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049950"|"26602839"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049951"|"26602840"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049952"|"26602841"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Darret component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049953"|"26602842"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Terrad soil is a minor component."|"25049954"|"26602843"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049417"|"26602306"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Big Timber soil is a minor component."|"25049418"|"26602307"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Darret component makes up 70 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049419"|"26602308"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049420"|"26602309"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25049955"|"26602844"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Darret component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC516MT Silty Steep (SiStp) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049956"|"26602845"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC516MT Silty Steep (SiStp) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049957"|"26602846"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimmick component makes up 100 percent of the map unit. Slopes are 0 to 1 percent. This component is on depressions. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"25049958"|"26602847"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25049959"|"26602848"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Duncom, clay loam soil is a minor component."|"25049960"|"26602849"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duncom component makes up 85 percent of the map unit. Slopes are 8 to 50 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049961"|"26602850"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049962"|"26602851"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25049963"|"26602852"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25049964"|"26602853"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duncom component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049965"|"26602854"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049966"|"26602855"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25049967"|"26602856"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duncom component makes up 29 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049968"|"26602857"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 31 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049969"|"26602858"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049970"|"26602859"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25049971"|"26602860"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fargo component makes up 65 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049972"|"26602861"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hegne component makes up 25 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049973"|"26602862"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25049974"|"26602863"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049975"|"26602864"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fargo soil is a minor component."|"25049976"|"26602865"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twin Creek soil is a minor component."|"25049977"|"26602866"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049978"|"26602867"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twin Creek soil is a minor component."|"25049979"|"26602868"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Terrad soil is a minor component."|"25049980"|"26602869"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049981"|"26602870"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Terrad soil is a minor component."|"25049982"|"26602871"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049983"|"26602872"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"25049984"|"26602873"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049985"|"26602874"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Darret soil is a minor component."|"25049986"|"26602875"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gallatin component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 36 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"25049987"|"26602876"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lamoure soil is a minor component."|"25049988"|"26602877"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gallatin component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 45 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"25049989"|"26602878"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25049990"|"26602879"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lamoure soil is a minor component."|"25049991"|"26602880"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25049992"|"26602881"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gallatin component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during January, February, March, April, May, June, November, December. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"25049993"|"26602882"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25049994"|"26602883"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gallatin component makes up 46 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC518MT Wet Meadow (WM) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"25049995"|"26602884"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gallatin, clay loam component makes up 44 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC518MT Wet Meadow (WM) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"25049996"|"26602885"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lamoure component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049998"|"26602887"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gallatin component makes up 41 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 39 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049999"|"26602888"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judell component makes up 39 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050000"|"26602889"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waltham soil is a minor component."|"25050001"|"26602890"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"25050002"|"26602891"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearpaw soil is a minor component."|"25050003"|"26602892"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerber component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050004"|"26602893"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sunburst soil is a minor component."|"25050005"|"26602894"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25050006"|"26602895"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"25050007"|"26602896"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"25050008"|"26602897"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, occasionally flooded soil is a minor component."|"25050009"|"26602898"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25050010"|"26602899"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XN162MT Bottomland Group, Clayey (Cy) 10-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"25050011"|"26602900"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hughesville component makes up 70 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25050012"|"26602901"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Little Horn soil is a minor component."|"25050013"|"26602902"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duncom component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050014"|"26602903"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050015"|"26602904"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell soil is a minor component."|"25050016"|"26602905"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashuelot component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer, undefined, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050017"|"26602906"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050018"|"26602907"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25050019"|"26602908"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell soil is a minor component."|"25050020"|"26602909"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050021"|"26602910"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050022"|"26602911"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050023"|"26602912"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050024"|"26602913"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25050025"|"26602914"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 0 to 3 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050026"|"26602915"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25050027"|"26602916"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050028"|"26602917"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25050029"|"26602918"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050030"|"26602919"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050031"|"26602920"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25050032"|"26602921"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25050033"|"26602922"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25050034"|"26602923"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050035"|"26602924"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25049411"|"26602300"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25049412"|"26602301"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049413"|"26602302"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050036"|"26602925"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Utica soil is a minor component."|"25050037"|"26602926"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050038"|"26602927"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050039"|"26602928"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25050040"|"26602929"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050041"|"26602930"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25050042"|"26602931"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050043"|"26602932"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050044"|"26602933"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25050045"|"26602934"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050046"|"26602935"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 46 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050047"|"26602936"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 44 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050048"|"26602937"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judell component makes up 46 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, foothills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050049"|"26602938"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith, gravelly loam surface soil is a minor component."|"25050050"|"26602939"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 44 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, foothills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050051"|"26602940"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"25050052"|"26602941"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 31 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050053"|"26602942"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith, gravelly component makes up 30 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050054"|"26602943"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 29 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050055"|"26602944"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050056"|"26602945"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 46 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050057"|"26602946"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 44 percent of the map unit. Slopes are 4 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050058"|"26602947"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25050059"|"26602948"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050060"|"26602949"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050061"|"26602950"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lismas component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC598MT Shallow Clay (SwC) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050062"|"26602951"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pierre component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC598MT Shallow Clay (SwC) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050063"|"26602952"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Promise soil is a minor component."|"25050064"|"26602953"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050065"|"26602954"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shale outcrop is a miscellaneous area."|"25050066"|"26602955"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lismas component makes up 40 percent of the map unit. Slopes are 15 to 70 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC599MT Thin Breaks (TB) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050067"|"26602956"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050068"|"26602957"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Little Horn component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from limestone and sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050069"|"26602958"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Little Horn soil is a minor component."|"25050070"|"26602959"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25050071"|"26602960"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loamy alluvial land is a miscellaneous area."|"25050072"|"26602961"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loamy alluvial land component makes up 41 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 15 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC597MT Saline Lowland (SL) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"25050073"|"26602962"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"25050074"|"26602963"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 85 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050075"|"26602964"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Woodhurst soil is a minor component."|"25050076"|"26602965"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25050077"|"26602966"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sapphire component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050078"|"26602967"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050079"|"26602968"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25050081"|"26602970"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Utica soil is a minor component."|"25050082"|"26602971"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050083"|"26602972"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 70 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25050084"|"26602973"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25050085"|"26602974"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alder soil is a minor component."|"25050086"|"26602975"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 70 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25050087"|"26602976"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050088"|"26602977"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050089"|"26602978"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050090"|"26602979"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25050091"|"26602980"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050092"|"26602981"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"25050093"|"26602982"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway, gravelly soil is a minor component."|"25050094"|"26602983"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 90 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050095"|"26602984"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050096"|"26602985"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shale outcrop is a miscellaneous area."|"25050097"|"26602986"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 60 percent of the map unit. Slopes are 35 to 70 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050098"|"26602987"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"25050099"|"26602988"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"25050100"|"26602989"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 60 percent of the map unit. Slopes are 25 to 70 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XN179MT Shallow Clay (SwC) 10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25050101"|"26602990"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arsite soil is a minor component."|"25050102"|"26602991"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"25050103"|"26602992"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bascovy soil is a minor component."|"25050104"|"26602993"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"25050105"|"26602994"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25050106"|"26602995"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nesda, gravelly component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050107"|"26602996"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nesda component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050108"|"26602997"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25050109"|"26602998"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Enbar soil is a minor component."|"25050110"|"26602999"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"25050111"|"26603000"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McIlwaine component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25050112"|"26603001"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050113"|"26603002"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pierre component makes up 95 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050114"|"26603003"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Promise soil is a minor component."|"25050115"|"26603004"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"25050116"|"26603005"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pierre component makes up 85 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050117"|"26603006"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Promise soil is a minor component."|"25050118"|"26603007"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050119"|"26603008"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Promise component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050120"|"26603009"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Promise component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050121"|"26603010"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050122"|"26603011"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Promise component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050123"|"26603012"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050124"|"26603013"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Promise component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050125"|"26603014"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Promise soil is a minor component."|"25050126"|"26603015"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050127"|"26603016"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"25050128"|"26603017"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 44 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25050129"|"26603018"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 46 percent of the map unit. Slopes are 2 to 4 percent. This component is on fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050130"|"26603019"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25050131"|"26603020"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"25050132"|"26603021"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 44 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25050133"|"26603022"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 46 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050134"|"26603023"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25050135"|"26603024"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 44 percent of the map unit. Slopes are 8 to 15 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25050136"|"26603025"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 46 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050137"|"26603026"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25050138"|"26603027"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25050139"|"26603028"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 44 percent of the map unit. Slopes are 4 to 15 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25050140"|"26603029"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 46 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050141"|"26603030"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 40 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC609MT Claypan (Cp) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"25050142"|"26603031"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Laurel soil is a minor component."|"25050143"|"26603032"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050144"|"26603033"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Promise soil is a minor component."|"25050145"|"26603034"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rhoades component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC609MT Claypan (Cp) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"25050146"|"26603035"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beckton soil is a minor component."|"25050147"|"26603036"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saline land component makes up 90 percent of the map unit. Slopes are 2 to 15 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 15 inches during April, May, June. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC597MT Saline Lowland (SL) RRU 46-C 15-19 PZ ecological site. Nonirrigated land capability classification is 7w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050148"|"26603037"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050149"|"26603038"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050150"|"26603039"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sapphire component makes up 50 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050151"|"26603040"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sapphire, stony component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050152"|"26603041"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050153"|"26603042"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25050154"|"26603043"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sapphire component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050155"|"26603044"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050156"|"26603045"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050157"|"26603046"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050158"|"26603047"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050159"|"26603048"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050160"|"26603049"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050161"|"26603050"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050162"|"26603051"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050163"|"26603052"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"25050164"|"26603053"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"25050165"|"26603054"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050166"|"26603055"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"25050167"|"26603056"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wyola component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050168"|"26603057"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050169"|"26603058"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050170"|"26603059"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25050171"|"26603060"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on structural benches. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 30 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050172"|"26603061"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, foothills. The parent material consists of slope alluvium over residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25050173"|"26603062"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tyzak soil is a minor component."|"25050174"|"26603063"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25050175"|"26603064"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25050176"|"26603065"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Duncom soil is a minor component."|"25050177"|"26603066"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050178"|"26603067"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050179"|"26603068"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050180"|"26603069"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25050181"|"26603070"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, lesser sloping soil is a minor component."|"25050182"|"26603071"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tyzak component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on ridges, hills, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"25050183"|"26603072"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050184"|"26603073"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25050185"|"26603074"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050186"|"26603075"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050187"|"26603076"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castle soil is a minor component."|"25050188"|"26603077"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25050189"|"26603078"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hughesville component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25050190"|"26603079"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25050191"|"26603080"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone, sandstone, and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050192"|"26603081"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duncom component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050193"|"26603082"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gallatin soil is a minor component."|"25050194"|"26603083"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Slocum component makes up 90 percent of the map unit. Slopes are 2 to 6 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP908MT Upland Aspen Woodland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050195"|"26603084"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spring creek component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050196"|"26603085"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050197"|"26603086"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Woodhurst soil is a minor component."|"25050198"|"26603087"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050199"|"26603088"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Straw component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050200"|"26603089"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"25050201"|"26603090"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Straw component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050202"|"26603091"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"25050203"|"26603092"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"25050204"|"26603093"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Straw component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050205"|"26603094"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverton component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC507MT Shallow to Gravel (SwGr) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050206"|"26603095"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sweetgrass component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050207"|"26603096"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"25050208"|"26603097"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"25050209"|"26603098"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terrad component makes up 95 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050210"|"26603099"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"25050211"|"26603100"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Darret soil is a minor component."|"25050212"|"26603101"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terrad component makes up 90 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050213"|"26603102"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderately well drained soils soil is a minor component."|"25050214"|"26603103"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Terrad soil is a minor component."|"25050215"|"26603104"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terrad component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050216"|"26603105"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sweetgrass soil is a minor component."|"25050217"|"26603106"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"25050218"|"26603107"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tamaneen component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050219"|"26603108"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"25050220"|"26603109"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sweetgrass soil is a minor component."|"25050221"|"26603110"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"25050222"|"26603111"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tamaneen component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050223"|"26603112"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairfield soil is a minor component."|"25050224"|"26603113"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sweetgrass soil is a minor component."|"25050225"|"26603114"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"25050226"|"26603115"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tamaneen component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050227"|"26603116"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"25050228"|"26603117"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairfield soil is a minor component."|"25050229"|"26603118"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050233"|"26603122"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050234"|"26603123"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"25050235"|"26603124"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050236"|"26603125"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"25050237"|"26603126"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"25050238"|"26603127"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050239"|"26603128"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 55 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050240"|"26603129"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on swales. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"25050241"|"26603130"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050242"|"26603131"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050243"|"26603132"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"25050244"|"26603133"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050245"|"26603134"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Teton soil is a minor component."|"25050246"|"26603135"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 70 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25050247"|"26603136"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050248"|"26603137"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25050249"|"26603138"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"25050250"|"26603139"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050251"|"26603140"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twin Creek component makes up 95 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050252"|"26603141"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chama soil is a minor component."|"25050253"|"26603142"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twin Creek component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050254"|"26603143"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chama soil is a minor component."|"25050255"|"26603144"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twin Creek component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050256"|"26603145"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chama soil is a minor component."|"25050257"|"26603146"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twin Creek component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050258"|"26603147"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tamaneen soil is a minor component."|"25050259"|"26603148"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050260"|"26603149"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050261"|"26603150"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050262"|"26603151"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 85 percent of the map unit. Slopes are 8 to 35 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC516MT Silty Steep (SiStp) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050263"|"26603152"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050264"|"26603153"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"25050265"|"26603154"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050266"|"26603155"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050267"|"26603156"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050268"|"26603157"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050269"|"26603158"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Benz soil is a minor component."|"25050270"|"26603159"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XN172MT Dense Clay (DC) 10-14"" p.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"25050271"|"26603160"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"25050272"|"26603161"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nonhydric soil is a minor component."|"25050274"|"26603163"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wet land component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on channels. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 12 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 6 percent. This component is in the R046XC512MT Subirrigated (Sb) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"25050275"|"26603164"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wayden component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XC598MT Shallow Clay (SwC) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25050276"|"26603165"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"25050277"|"26603166"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"25050278"|"26603167"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sagedale component makes up 35 percent of the map unit. Slopes are 25 to 45 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050279"|"26603168"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050280"|"26603169"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050281"|"26603170"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050282"|"26603171"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050283"|"26603172"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050284"|"26603173"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"25050285"|"26603174"
12/20/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"25050286"|"26603175"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050287"|"26603176"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25050288"|"26603177"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050289"|"26603178"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"25050290"|"26603179"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050291"|"26603180"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"25050292"|"26603181"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, terraces. The parent material consists of alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050293"|"26603182"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Utica soil is a minor component."|"25050294"|"26603183"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050295"|"26603184"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"25050296"|"26603185"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Laurel soil is a minor component."|"25050297"|"26603186"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25050298"|"26603187"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rhoades component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"25050299"|"26603188"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Utica component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049404"|"26602293"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winifred component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"25049405"|"26602294"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"25049406"|"26602295"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Promise soil is a minor component."|"25049407"|"26602296"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spring creek soil is a minor component."|"25050300"|"26603189"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst component makes up 90 percent of the map unit. Slopes are 8 to 50 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25050301"|"26603190"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spring creek soil is a minor component."|"25050302"|"26603191"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25050303"|"26603192"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alder component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050304"|"26603193"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050305"|"26603194"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"25050306"|"26603195"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25050307"|"26603196"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25050308"|"26603197"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"25050309"|"26603198"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castle soil is a minor component."|"25050310"|"26603199"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst component makes up 45 percent of the map unit. Slopes are 8 to 50 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25050311"|"26603200"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spring creek component makes up 40 percent of the map unit. Slopes are 8 to 50 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050312"|"26603201"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25050313"|"26603202"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049375"|"26602264"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spring creek soil is a minor component."|"25049376"|"26602265"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 25 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049377"|"26602266"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teton component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049378"|"26602267"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reeder soil is a minor component."|"25049384"|"26602273"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049385"|"26602274"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049386"|"26602275"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitlash soil is a minor component."|"25049387"|"26602276"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049388"|"26602277"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"25049393"|"26602282"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"25049394"|"26602283"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049395"|"26602284"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 50 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049396"|"26602285"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, terraces. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XN247MT Draft Clayey (cy)   Rru 46-n  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050230"|"26603119"
12/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25050231"|"26603120"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tamaneen component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XN247MT Draft Clayey (cy)   Rru 46-n  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. "|"25050232"|"26603121"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"25049997"|"26602886"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"25050273"|"26603162"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water, miscellaneous is a miscellaneous area."|"25050080"|"26602969"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"25049433"|"26602322"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klayent soil is a minor component."|"25049434"|"26602323"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 59 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC504MT Overflow (Ov) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 4 within 30 inches of the soil surface."|"25049435"|"26602324"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"25049436"|"26602325"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macar component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049441"|"26602330"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sagedale soil is a minor component."|"25049442"|"26602331"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klayent soil is a minor component."|"25049443"|"26602332"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC504MT Overflow (Ov) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 4 within 30 inches of the soil surface."|"25049444"|"26602333"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Linwell soil is a minor component."|"25049450"|"26602339"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"25049451"|"26602340"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kiev soil is a minor component."|"25049452"|"26602341"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sagedale component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on fan remnants, foothills. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049453"|"26602342"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"25049459"|"26602348"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"25049460"|"26602349"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sagedale component makes up 50 percent of the map unit. Slopes are 0 to 8 percent. This component is on eroded fan remnants, foothills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049461"|"26602350"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"25049462"|"26602351"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midnot component makes up 35 percent of the map unit. Slopes are 0 to 8 percent. This component is on eroded fan remnants, foothills. The parent material consists of slope alluvium over residuum weathered from shale and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"25049463"|"26602352"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"25049467"|"26602356"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"25049468"|"26602357"
09/15/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midnot component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on eroded fan remnants, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XN247MT Clayey (Cy) RRU 46-N 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"25049469"|"26602358"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sagedale soil is a minor component."|"25049470"|"26602359"
09/15/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wayden component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on eroded fan remnants, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XC598MT Shallow Clay (SwC) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25049471"|"26602360"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnant sideslopes, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049476"|"26602365"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnant sideslopes, foothills. The parent material consists of residuum. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XC516MT Silty Steep (SiStp) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25049477"|"26602366"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"25049478"|"26602367"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yaple soil is a minor component."|"25049479"|"26602368"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnant sideslopes, foothills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC519MT Limy Droughty (LyDr) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent.  "|"25049480"|"26602369"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 35 percent of the map unit. Slopes are 4 to 8 percent. This component is on eroded fan remnants, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC506MT Shallow (Sw) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049485"|"26602374"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"25049486"|"26602375"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on eroded fan remnants, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XC508MT Silty (Si) RRU 46-C 13-19 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"25049487"|"26602376"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"25049488"|"26602377"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"25049489"|"26602378"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Catgulch, very bouldery component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, foothills. The parent material consists of colluvium derived from igneous rock over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R043BP812MT Shallow Shrubland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049397"|"26602286"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fine-loamy, typic argiustolls, mod-deep, very bouldery component makes up 30 percent of the map unit. Slopes are 15 to 25 percent. This component is on hillslopes, foothills. The parent material consists of colluvium derived from igneous rock over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049398"|"26602287"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049399"|"26602288"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on structural benches, foothills. The parent material consists of colluvium and/or slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP822MT Limy Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049408"|"26602297"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049409"|"26602298"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on structural benches, fan remnants, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BB031MT Limy Droughty (LyDr) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049410"|"26602299"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowery component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, foothills. The parent material consists of slope alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP817MT Subirrigated Shrubland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049372"|"26602261"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolo component makes up 30 percent of the map unit. Slopes are 4 to 12 percent. This component is on stream terraces, fan remnants, foothills. The parent material consists of alluvium and/or slope alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP817MT Subirrigated Shrubland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25049373"|"26602262"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mannixlee soil is a minor component."|"25049374"|"26602263"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard component makes up 20 percent of the map unit. Slopes are 4 to 10 percent. This component is on ridges, foothills. The parent material consists of colluvium and/or slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP822MT Limy Alpine Group ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049414"|"26602303"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, stony component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges, hillslopes, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 43 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049415"|"26602304"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges, hillslopes, foothills. The parent material consists of colluvium and/or slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049416"|"26602305"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Checkerboard soil is a minor component."|"25049421"|"26602310"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, stony component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on hillslopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 43 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049422"|"26602311"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on swales, mountains. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049423"|"26602312"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on hillslopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049424"|"26602313"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049425"|"26602314"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 65 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049437"|"26602326"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25049438"|"26602327"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 30 percent of the map unit. Slopes are 30 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049439"|"26602328"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049440"|"26602329"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 25 percent of the map unit. Slopes are 15 to 30 percent. This component is on dip slopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049472"|"26602361"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on dip slopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049473"|"26602362"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25049474"|"26602363"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049475"|"26602364"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent.  "|"25049481"|"26602370"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Warneke component makes up 25 percent of the map unit. Slopes are 25 to 45 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049482"|"26602371"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"25049483"|"26602372"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049484"|"26602373"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kiev component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on dissected alluvial fans, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BB030MT Limy (Ly) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049513"|"26602402"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roundor component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on dissected alluvial fans, foothills. The parent material consists of slope alluvium over residuum weathered from mudstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049514"|"26602403"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on dissected alluvial fans, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BB031MT Limy Droughty (LyDr) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049515"|"26602404"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kiev component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on dissected alluvial fans, foothills. The parent material consists of slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB030MT Limy (Ly) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049402"|"26602291"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 75 percent of the map unit. Slopes are 8 to 15 percent. This component is on dissected alluvial fans, foothills. The parent material consists of slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BB031MT Limy Droughty (LyDr) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049403"|"26602292"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, stony component makes up 55 percent of the map unit. Slopes are 8 to 15 percent. This component is on scarp slopes, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 43 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049516"|"26602405"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"25049517"|"26602406"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 30 percent of the map unit. Slopes are 8 to 12 percent. This component is on dissected alluvial fans, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049518"|"26602407"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049519"|"26602408"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, stony component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on scarp slopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP822MT Limy Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049520"|"26602409"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, stony component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on scarp slopes, foothills. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 43 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049521"|"26602410"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on scarp slopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB031MT Limy Droughty (LyDr) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049522"|"26602411"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"25049523"|"26602412"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, extremely stony component makes up 25 percent of the map unit. Slopes are 15 to 60 percent. This component is on scarp slopes on foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049524"|"26602413"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin component makes up 35 percent of the map unit. Slopes are 20 to 50 percent. This component is on hillslopes on foothills. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 43 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049525"|"26602414"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, stony component makes up 30 percent of the map unit. Slopes are 20 to 60 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049526"|"26602415"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049527"|"26602416"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Checkerboard, very stony soil is a minor component."|"25049445"|"26602334"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049446"|"26602335"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, stony component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049447"|"26602336"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"25049448"|"26602337"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049449"|"26602338"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chivington soil is a minor component."|"25049504"|"26602393"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abac, extremely bouldery component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP822MT Limy Alpine Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049505"|"26602394"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter, very bouldery component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, foothills. The parent material consists of colluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25049506"|"26602395"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Darret, very bouldery component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from mudstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"25049507"|"26602396"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049508"|"26602397"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, very stony component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on mountains. The parent material consists of colluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP823MT Shallow Alpine Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049509"|"26602398"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg, very bouldery component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on mountains. The parent material consists of colluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049510"|"26602399"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhall, very stony component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on mountains. The parent material consists of colluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049511"|"26602400"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049512"|"26602401"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bavdark component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on swales, foothills. The parent material consists of slope alluvium derived from rhyolite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049379"|"26602268"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"25049380"|"26602269"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhall component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills, foothills. The parent material consists of slope alluvium and/or colluvium over residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049381"|"26602270"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst, very stony component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills, foothills. The parent material consists of slope alluvium and/or colluvium over residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049382"|"26602271"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049383"|"26602272"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, stony soil is a minor component."|"25049389"|"26602278"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhall, stony component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049390"|"26602279"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst, stony component makes up 25 percent of the map unit. Slopes are 15 to 25 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049391"|"26602280"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049392"|"26602281"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, stony component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049454"|"26602343"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049455"|"26602344"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Findon, stony soil is a minor component."|"25049456"|"26602345"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, very stony component makes up 17 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes on mountains. The parent material consists of colluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049457"|"26602346"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049458"|"26602347"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, bouldery component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049464"|"26602353"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, bouldery component makes up 50 percent of the map unit. Slopes are 8 to 25 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049465"|"26602354"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049466"|"26602355"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leavitt, stony component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills, foothills. The parent material consists of colluvium over residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"25049429"|"26602318"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, very stony component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049430"|"26602319"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodhurst, extremely bouldery component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049431"|"26602320"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049432"|"26602321"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden, very stony component makes up 45 percent of the map unit. Slopes are 60 to 90 percent. This component is on canyons on mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049490"|"26602379"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Warneke, extremely stony component makes up 20 percent of the map unit. Slopes are 60 to 90 percent. This component is on canyons on mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049491"|"26602380"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, stony soil is a minor component."|"25049492"|"26602381"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049493"|"26602382"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049494"|"26602383"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowery soil is a minor component."|"25049498"|"26602387"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 44 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills, foothills. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"25049499"|"26602388"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sawicki, extremely stony component makes up 46 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills, foothills. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049500"|"26602389"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcoulee, stony component makes up 45 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049623"|"26602512"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge component makes up 35 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049624"|"26602513"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Checkerboard, very stony soil is a minor component."|"25049625"|"26602514"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"25049626"|"26602515"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049627"|"26602516"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryadine, stony component makes up 45 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049671"|"26602560"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 30 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"25049672"|"26602561"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monumentpeak, very stony soil is a minor component."|"25049673"|"26602562"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"25049674"|"26602563"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049675"|"26602564"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"25049666"|"26602555"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, very stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone and sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049667"|"26602556"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanson, stony soil is a minor component."|"25049668"|"26602557"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049669"|"26602558"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049670"|"26602559"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Skaggs soil is a minor component."|"25049618"|"26602507"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, very stony component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049619"|"26602508"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049620"|"26602509"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcoulee, stony component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049621"|"26602510"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049622"|"26602511"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge, extremely stony component makes up 55 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049734"|"26602623"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, rubbly component makes up 20 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone and sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049735"|"26602624"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coalkiln, stony soil is a minor component."|"25049736"|"26602625"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Checkerboard, rubbly, dry soil is a minor component."|"25049737"|"26602626"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049738"|"26602627"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge, very stony component makes up 50 percent of the map unit. Slopes are 50 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049739"|"26602628"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reppart, rubbly soil is a minor component."|"25049740"|"26602629"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, very rubbly component makes up 25 percent of the map unit. Slopes are 50 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049741"|"26602630"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049742"|"26602631"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049743"|"26602632"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryadine, very rubbly component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049755"|"26602644"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville, very stony component makes up 15 percent of the map unit. Slopes are 45 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone and dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"25049756"|"26602645"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monumentpeak, extremely stony component makes up 30 percent of the map unit. Slopes are 45 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049757"|"26602646"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049758"|"26602647"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049759"|"26602648"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryadine, stony component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on structural benches, mountains. The parent material consists of slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049744"|"26602633"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monumentpeak, extremely stony component makes up 18 percent of the map unit. Slopes are 4 to 20 percent. This component is on structural benches, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049745"|"26602634"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville soil is a minor component."|"25049746"|"26602635"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryadine, extremely stony soil is a minor component."|"25049747"|"26602636"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Checkerboard, stony soil is a minor component."|"25049748"|"26602637"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049749"|"26602638"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049660"|"26602549"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood family, extremely stony component makes up 25 percent of the map unit. Slopes are 35 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049661"|"26602550"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Owlcan family soil is a minor component."|"25049662"|"26602551"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule family component makes up 20 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049663"|"26602552"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville family, very bouldery component makes up 35 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"25049664"|"26602553"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lingshire family soil is a minor component."|"25049665"|"26602554"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcoulee component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049612"|"26602501"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, very stony component makes up 25 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049613"|"26602502"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge, stony component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountain slopes, hillslopes, mountains. The parent material consists of slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049614"|"26602503"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kimpton soil is a minor component."|"25049615"|"26602504"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nikat soil is a minor component."|"25049616"|"26602505"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049617"|"26602506"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arrowpeak, very stony component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on ridges on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP823MT Shallow Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049676"|"26602565"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackbear, stony component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049677"|"26602566"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkpeak component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049678"|"26602567"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"25049679"|"26602568"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049680"|"26602569"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sawpit, very stony soil is a minor component."|"25049681"|"26602570"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"25049682"|"26602571"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arrowpeak, extremely stony component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on ridges on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049683"|"26602572"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkpeak, very stony component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049684"|"26602573"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049685"|"26602574"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049686"|"26602575"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge, very stony component makes up 35 percent of the map unit. Slopes are 50 to 70 percent. This component is on mountain slopes, canyons, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049655"|"26602544"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Checkerboard, extremely stony component makes up 30 percent of the map unit. Slopes are 50 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049656"|"26602545"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood, stony soil is a minor component."|"25049657"|"26602546"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049658"|"26602547"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049659"|"26602548"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25049578"|"26602467"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 20 percent of the map unit. Slopes are 1 to 8 percent. This component is on stream terraces, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"25049579"|"26602468"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 20 percent of the map unit. Slopes are 1 to 4 percent. This component is on stream terraces, mountains. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP815MT Subirrigated Grassland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent.  "|"25049580"|"26602469"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonville soil is a minor component."|"25049581"|"26602470"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, occasionally flooded component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer, abrupt textural change, is 20 to 59 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 7 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049582"|"26602471"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"25049583"|"26602472"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, stony soil is a minor component."|"25049760"|"26602649"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings, extremely stony component makes up 35 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049761"|"26602650"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sawpit, very stony component makes up 30 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049762"|"26602651"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Drywolf, very rubbly component makes up 15 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, avalanche chutes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP901MT Rubbly Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049763"|"26602652"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boatman soil is a minor component."|"25049764"|"26602653"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049765"|"26602654"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ettienridge component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049728"|"26602617"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, very stony component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049729"|"26602618"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hardhart, stony soil is a minor component."|"25049730"|"26602619"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Findon, stony soil is a minor component."|"25049731"|"26602620"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cloud Peak component makes up 20 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049732"|"26602621"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049733"|"26602622"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049782"|"26602671"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049783"|"26602672"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049636"|"26602525"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049637"|"26602526"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve, extremely stony component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049638"|"26602527"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake Creek, very stony component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049639"|"26602528"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Caseypeak, very rubbly soil is a minor component."|"25049640"|"26602529"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, extremely stony soil is a minor component."|"25049641"|"26602530"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad, rubbly component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 0 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049642"|"26602531"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve, extremely stony component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049628"|"26602517"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake Creek, very stony component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049629"|"26602518"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Caseypeak, extremely stony soil is a minor component."|"25049630"|"26602519"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, very stony soil is a minor component."|"25049631"|"26602520"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, extremely stony soil is a minor component."|"25049632"|"26602521"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad, rubbly component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 0 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049633"|"26602522"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049634"|"26602523"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049635"|"26602524"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake Creek, very stony component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049648"|"26602537"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, extremely stony component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049649"|"26602538"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, extremely stony soil is a minor component."|"25049650"|"26602539"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Surdal, stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049651"|"26602540"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin, very rubbly soil is a minor component."|"25049652"|"26602541"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049653"|"26602542"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049654"|"26602543"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Targhee, extremely stony component makes up 36 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049687"|"26602576"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049688"|"26602577"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049689"|"26602578"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, rubbly soil is a minor component."|"25049690"|"26602579"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfish, occasionally flooded, very bouldery soil is a minor component."|"25049691"|"26602580"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock, very stony component makes up 34 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049692"|"26602581"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs, stony component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of loess over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049607"|"26602496"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"25049608"|"26602497"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Herakle, very stony component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"25049609"|"26602498"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcoulee component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of loess over colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049610"|"26602499"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049611"|"26602500"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, very stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, structural benches, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049601"|"26602490"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elispring component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, structural benches, mountains. The parent material consists of loess over colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049602"|"26602491"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"25049603"|"26602492"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"25049604"|"26602493"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049605"|"26602494"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcoulee, stony component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, structural benches, mountains. The parent material consists of loess over colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049606"|"26602495"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049766"|"26602655"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049767"|"26602656"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Starman family, very rubbly component makes up 20 percent of the map unit. Slopes are 20 to 70 percent. This component is on headwalls, ridges, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049768"|"26602657"
08/01/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore family, very rubbly component makes up 15 percent of the map unit. Slopes are 20 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP901MT Rubbly Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049769"|"26602658"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very rubbly component makes up 35 percent of the map unit. Slopes are 20 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP901MT Rubbly Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049770"|"26602659"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Caseypeak, rubbly soil is a minor component."|"25049771"|"26602660"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049772"|"26602661"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049773"|"26602662"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepecreek, very rubbly component makes up 45 percent of the map unit. Slopes are 20 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from quartz-monzonite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP901MT Rubbly Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049780"|"26602669"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049781"|"26602670"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake Creek, very stony component makes up 40 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049722"|"26602611"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Findon component makes up 25 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"25049723"|"26602612"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redfern, extremely stony component makes up 15 percent of the map unit. Slopes are 35 to 50 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP904MT Shallow Warm Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049724"|"26602613"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcoulee soil is a minor component."|"25049725"|"26602614"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049726"|"26602615"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049727"|"26602616"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville, stony component makes up 20 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP902MT Shallow Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"25049750"|"26602639"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monumentpeak, rubbly component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP913MT Limy Warm Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049751"|"26602640"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049752"|"26602641"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25049753"|"26602642"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryadine, extremely stony component makes up 45 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049754"|"26602643"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skaggs component makes up 29 percent of the map unit. Slopes are 2 to 15 percent. This component is on structural benches, hillslopes, mountains. The parent material consists of loess over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049595"|"26602484"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"25049596"|"26602485"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"25049597"|"26602486"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on swales, mountains. The parent material consists of loess over colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049598"|"26602487"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal, extremely stony soil is a minor component."|"25049599"|"26602488"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elispring component makes up 31 percent of the map unit. Slopes are 2 to 15 percent. This component is on structural benches, hillslopes, mountains. The parent material consists of loess over colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"25049600"|"26602489"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Booneville, very stony component makes up 35 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049712"|"26602601"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Drywolf, very rubbly component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, avalanche chutes, mountains. The parent material consists of colluvium derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049713"|"26602602"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alta, very stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 59 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Upland Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049714"|"26602603"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049715"|"26602604"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, moist soil is a minor component."|"25049528"|"26602417"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap soil is a minor component."|"25049529"|"26602418"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden soil is a minor component."|"25049530"|"26602419"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judell component makes up 39 percent of the map unit. Slopes are 4 to 25 percent. This component is on fan remnants, structural benches, foothills. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049531"|"26602420"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 41 percent of the map unit. Slopes are 4 to 25 percent. This component is on fan remnants, structural benches, foothills. The parent material consists of slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049532"|"26602421"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on colluvial aprons, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent.  "|"25049538"|"26602427"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on colluvial aprons, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP904MT Shallow Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049539"|"26602428"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25049540"|"26602429"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049541"|"26602430"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tosca soil is a minor component."|"25049533"|"26602422"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac, very stony component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP904MT Shallow Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049534"|"26602423"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saddlehorse, stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"25049535"|"26602424"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell soil is a minor component."|"25049536"|"26602425"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049537"|"26602426"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049542"|"26602431"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25049543"|"26602432"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, dry soil is a minor component."|"25049544"|"26602433"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on structural benches, low hills, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent.  "|"25049545"|"26602434"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 45 percent of the map unit. Slopes are 4 to 25 percent. This component is on structural benches, low hills, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049546"|"26602435"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, dry soil is a minor component."|"25049547"|"26602436"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, dry soil is a minor component."|"25049548"|"26602437"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden, stony component makes up 40 percent of the map unit. Slopes are 25 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049549"|"26602438"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap, very stony component makes up 30 percent of the map unit. Slopes are 25 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent.  "|"25049550"|"26602439"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, dry soil is a minor component."|"25049551"|"26602440"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049552"|"26602441"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, dry soil is a minor component."|"25049553"|"26602442"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap, very stony component makes up 30 percent of the map unit. Slopes are 45 to 70 percent. This component is on canyons, mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent.  "|"25049554"|"26602443"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden, stony component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on canyons, mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049555"|"26602444"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, dry soil is a minor component."|"25049556"|"26602445"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049557"|"26602446"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"25049716"|"26602605"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, moist soil is a minor component."|"25049717"|"26602606"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, moist soil is a minor component."|"25049718"|"26602607"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 50 percent of the map unit. Slopes are 4 to 25 percent. This component is on structural benches, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP804MT Limy Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent.  "|"25049719"|"26602608"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on structural benches, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP804MT Limy Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"25049720"|"26602609"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25049721"|"26602610"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve, extremely stony component makes up 35 percent of the map unit. Slopes are 45 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049643"|"26602532"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake Creek, very stony component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049644"|"26602533"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, very stony soil is a minor component."|"25049645"|"26602534"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Caseypeak, very rubbly soil is a minor component."|"25049646"|"26602535"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049647"|"26602536"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, occasionally flooded component makes up 20 percent of the map unit. Slopes are 2 to 6 percent. This component is on flood plains, mountains. The parent material consists of alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 7 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049564"|"26602453"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lemroi, occasionally flooded soil is a minor component."|"25049565"|"26602454"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tetonville component makes up 20 percent of the map unit. Slopes are 2 to 6 percent. This component is on stream terraces, mountains. The parent material consists of alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 28 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049566"|"26602455"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon soil is a minor component."|"25049567"|"26602456"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on colluvial aprons, stream terraces, mountains. The parent material consists of slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"25049568"|"26602457"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"25049569"|"26602458"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25049570"|"26602459"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25049571"|"26602460"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutchhollow, occasionally flooded soil is a minor component."|"25049572"|"26602461"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 35 percent of the map unit. Slopes are 2 to 12 percent. This component is on colluvial aprons, stream terraces, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"25049573"|"26602462"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 25 percent of the map unit. Slopes are 2 to 12 percent. This component is on colluvial aprons, stream terraces, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"25049574"|"26602463"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tetonville, occasionally flooded component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains, mountains. The parent material consists of alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 28 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"25049575"|"26602464"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, stony soil is a minor component."|"25049576"|"26602465"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"25049577"|"26602466"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Slagamelt component makes up 30 percent of the map unit. Slopes are 2 to 6 percent. This component is on stream terraces, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP907MT Subirrigated Cool Woodland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"25049558"|"26602447"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"25049559"|"26602448"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25049560"|"26602449"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on colluvial aprons, stream terraces, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"25049561"|"26602450"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat, occasionally flooded soil is a minor component."|"25049562"|"26602451"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on colluvial aprons, stream terraces, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25049563"|"26602452"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely bouldery component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on landslides, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049584"|"26602473"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Guffey, extremely stony component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on landslides, mountains. The parent material consists of colluvium over residuum weathered from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049585"|"26602474"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Embargo, very stony soil is a minor component."|"25049586"|"26602475"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049587"|"26602476"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, igneous soil is a minor component."|"25049588"|"26602477"
06/25/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25049589"|"26602478"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bavdark, stony component makes up 35 percent of the map unit. Slopes are 8 to 20 percent. This component is on fan remnants, mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049590"|"26602479"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, very stony component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049591"|"26602480"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dailybasin, extremely stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on fan remnants, mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25049592"|"26602481"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"25049593"|"26602482"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slagamelt soil is a minor component."|"25049594"|"26602483"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slidemountain, stony soil is a minor component."|"25049693"|"26602582"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigcoulee soil is a minor component."|"25049694"|"26602583"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pohlod, stony component makes up 35 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049695"|"26602584"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Highwood, stony component makes up 45 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049696"|"26602585"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cavebear, stony soil is a minor component."|"25049697"|"26602586"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, igneous soil is a minor component."|"25049698"|"26602587"
06/25/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25049699"|"26602588"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slidemountain, stony soil is a minor component."|"25049700"|"26602589"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Longway component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on fan remnants, mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049701"|"26602590"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigcoulee component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 55 inches (depth from the mineral surface is 54 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP908MT Upland Aspen Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049702"|"26602591"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pohlod component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25049703"|"26602592"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cavebear, stony soil is a minor component."|"25049704"|"26602593"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, igneous soil is a minor component."|"25049705"|"26602594"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dailybasin component makes up 15 percent of the map unit. Slopes are 20 to 60 percent. This component is on swales, mountain slopes, toes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049706"|"26602595"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slidemountain, stony soil is a minor component."|"25049707"|"26602596"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigcoulee component makes up 25 percent of the map unit. Slopes are 20 to 50 percent. This component is on mountain slopes, toes, swales, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 55 inches (depth from the mineral surface is 54 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP908MT Upland Aspen Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049708"|"26602597"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pohlod component makes up 30 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049709"|"26602598"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Highwood component makes up 20 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP902MT Shallow Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25049710"|"26602599"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, igneous soil is a minor component."|"25049711"|"26602600"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings, very rubbly component makes up 35 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049774"|"26602663"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Highwood, very stony soil is a minor component."|"25049775"|"26602664"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049776"|"26602665"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25049777"|"26602666"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, rubbly component makes up 20 percent of the map unit. Slopes are 35 to 70 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP902MT Shallow Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25049778"|"26602667"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boatman, very stony soil is a minor component."|"25049779"|"26602668"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 65 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, foothills. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP822MT Limy Alpine Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 40 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049495"|"26602384"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 25 percent of the map unit. Slopes are 15 to 25 percent. This component is on hills, foothills. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BB031MT Limy Droughty (LyDr) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"25049496"|"26602385"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25049497"|"26602386"
