07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollman soil is a minor component."|"25074031"|"26626920"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Borohemists soil is a minor component."|"25074032"|"26626921"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25074033"|"26626922"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Aeric Haplaquepts component makes up 85 percent of the map unit. Slopes are 1 to 3 percent. This component is on flood plains.  Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during January, February, March, April, May, June, July, August, September, October, November, December.  This component is in the R043AP802MT Bottomland Group ecological site.   This soil meets hydric criteria.   "|"25074034"|"26626923"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074066"|"26626955"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074067"|"26626956"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074068"|"26626957"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074069"|"26626958"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slickspots is a miscellaneous area."|"25074422"|"26627311"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marklepass component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 83 within 30 inches of the soil surface."|"25074423"|"26627312"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bolack soil is a minor component."|"25074424"|"26627313"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selon soil is a minor component."|"25074425"|"26627314"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCollum component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074426"|"26627315"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"25074427"|"26627316"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074428"|"26627317"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCollum component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074429"|"26627318"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074430"|"26627319"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCollum component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074431"|"26627320"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"25074432"|"26627321"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074433"|"26627322"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCollum component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074434"|"26627323"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Potholes in kicking horse area soil is a minor component."|"25074435"|"26627324"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald, stony loam soil is a minor component."|"25074436"|"26627325"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074437"|"26627326"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Connah soil is a minor component."|"25074438"|"26627327"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McDonald component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"25074439"|"26627328"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074440"|"26627329"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Potholes in kicking horse area soil is a minor component."|"25074441"|"26627330"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald, stony loam soil is a minor component."|"25074442"|"26627331"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074443"|"26627332"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Connah soil is a minor component."|"25074444"|"26627333"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McDonald component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"25074445"|"26627334"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074446"|"26627335"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald, stony loam soil is a minor component."|"25074447"|"26627336"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074448"|"26627337"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Connah soil is a minor component."|"25074449"|"26627338"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McDonald component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25074450"|"26627339"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slopes more than 15 percent soil is a minor component."|"25074451"|"26627340"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074452"|"26627341"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Connah soil is a minor component."|"25074453"|"26627342"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald, stony loam soil is a minor component."|"25074454"|"26627343"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074455"|"26627344"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl, 3 soil is a minor component."|"25074456"|"26627345"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McDonald component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, alluvial fans. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria.   "|"25074457"|"26627346"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowlake soil is a minor component."|"25074458"|"26627347"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074459"|"26627348"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"25074460"|"26627349"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger soil is a minor component."|"25074461"|"26627350"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074070"|"26626959"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074071"|"26626960"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowlake soil is a minor component."|"25074462"|"26627351"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074463"|"26627352"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074464"|"26627353"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walstead component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"25074465"|"26627354"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 65 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"25074466"|"26627355"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074467"|"26627356"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074468"|"26627357"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074469"|"26627358"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten, shallow to bedrock soil is a minor component."|"25074470"|"26627359"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite and/or colluvium derived from argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074471"|"26627360"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074472"|"26627361"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074473"|"26627362"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten, shallow to bedrock soil is a minor component."|"25074474"|"26627363"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25074475"|"26627364"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite and/or colluvium derived from argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074476"|"26627365"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074477"|"26627366"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite and/or colluvium derived from argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074478"|"26627367"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074479"|"26627368"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25074480"|"26627369"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074481"|"26627370"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074482"|"26627371"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite and/or colluvium derived from argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074483"|"26627372"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25074484"|"26627373"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten, shallow to bedrock soil is a minor component."|"25074485"|"26627374"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074486"|"26627375"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074487"|"26627376"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074488"|"26627377"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074489"|"26627378"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moiese component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on outwash plains, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074490"|"26627379"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moiese soil is a minor component."|"25074491"|"26627380"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slopes of 2 to 8 percent soil is a minor component."|"25074492"|"26627381"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollman component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074493"|"26627382"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074494"|"26627383"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074495"|"26627384"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollman component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074496"|"26627385"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25074497"|"26627386"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25074498"|"26627387"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay soil is a minor component."|"25074499"|"26627388"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"25074500"|"26627389"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollman component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074501"|"26627390"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25074502"|"26627391"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollman component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074503"|"26627392"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25074504"|"26627393"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074505"|"26627394"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074072"|"26626961"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25074073"|"26626962"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowlake soil is a minor component."|"25074074"|"26626963"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074075"|"26626964"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, stony loam soil is a minor component."|"25074506"|"26627395"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074507"|"26627396"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074508"|"26627397"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 85 percent of the map unit. Slopes are 0 to 5 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074509"|"26627398"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, stony loam soil is a minor component."|"25074510"|"26627399"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074511"|"26627400"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074512"|"26627401"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on moraines. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074513"|"26627402"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, stony loam soil is a minor component."|"25074514"|"26627403"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074515"|"26627404"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074516"|"26627405"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074517"|"26627406"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, stony loam soil is a minor component."|"25074518"|"26627407"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074519"|"26627408"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074520"|"26627409"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074521"|"26627410"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074522"|"26627411"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25074523"|"26627412"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074524"|"26627413"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074525"|"26627414"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074526"|"26627415"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074527"|"26627416"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, stony loam soil is a minor component."|"25074528"|"26627417"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074529"|"26627418"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074530"|"26627419"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074531"|"26627420"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerl component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074532"|"26627421"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074533"|"26627422"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ninepipe component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, alluvial fans, drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during June, July, August, September. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3c. Irrigated land capability classification is 2c. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074534"|"26627423"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"25074535"|"26627424"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Phillcher component makes up 85 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074536"|"26627425"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway, shallow soil is a minor component."|"25074537"|"26627426"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074538"|"26627427"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074539"|"26627428"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Phillcher component makes up 70 percent of the map unit. Slopes are 45 to 75 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074540"|"26627429"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Phillcher, shallow to rock soil is a minor component."|"25074541"|"26627430"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway, cool soil is a minor component."|"25074542"|"26627431"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074543"|"26627432"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074544"|"26627433"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"25074545"|"26627434"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas supporting vegetation soil is a minor component."|"25074546"|"26627435"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP805MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"25074076"|"26626965"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 55 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074077"|"26626966"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, 2 soil is a minor component."|"25074078"|"26626967"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074079"|"26626968"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074547"|"26627436"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Polson component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"25074548"|"26627437"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074549"|"26627438"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074550"|"26627439"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slick spots soil is a minor component."|"25074551"|"26627440"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074552"|"26627441"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074553"|"26627442"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Polson component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"25074554"|"26627443"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074555"|"26627444"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074556"|"26627445"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074557"|"26627446"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 15 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074558"|"26627447"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Polson component makes up 70 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"25074559"|"26627448"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25074560"|"26627449"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post, cobbly loam soil is a minor component."|"25074561"|"26627450"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Post component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"25074562"|"26627451"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074563"|"26627452"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ronan soil is a minor component."|"25074564"|"26627453"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25074565"|"26627454"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post, cobbly loam soil is a minor component."|"25074566"|"26627455"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Post component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"25074567"|"26627456"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074568"|"26627457"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ronan soil is a minor component."|"25074569"|"26627458"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25074570"|"26627459"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post, cobbly loam soil is a minor component."|"25074571"|"26627460"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Post component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"25074572"|"26627461"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074573"|"26627462"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ronan soil is a minor component."|"25074574"|"26627463"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"25074575"|"26627464"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074576"|"26627465"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074577"|"26627466"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ronan component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25074578"|"26627467"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Post component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"25074579"|"26627468"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bolack soil is a minor component."|"25074580"|"26627469"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"25074581"|"26627470"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post, cobbly loam soil is a minor component."|"25074582"|"26627471"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074583"|"26627472"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074584"|"26627473"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ronan component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25074585"|"26627474"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Post component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 35 within 30 inches of the soil surface."|"25074586"|"26627475"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bolack soil is a minor component."|"25074587"|"26627476"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The shallow to bedrock soil is a minor component."|"25074588"|"26627477"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repp component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074589"|"26627478"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074590"|"26627479"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074591"|"26627480"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The shallow to bedrock soil is a minor component."|"25074592"|"26627481"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repp component makes up 75 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074593"|"26627482"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074594"|"26627483"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074595"|"26627484"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074080"|"26626969"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074081"|"26626970"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 55 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074082"|"26626971"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074083"|"26626972"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25074084"|"26626973"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074596"|"26627485"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25074597"|"26627486"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Esteslake soil is a minor component."|"25074598"|"26627487"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post soil is a minor component."|"25074599"|"26627488"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ronan component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25074600"|"26627489"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Esteslake soil is a minor component."|"25074601"|"26627490"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074602"|"26627491"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post soil is a minor component."|"25074603"|"26627492"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ronan component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25074604"|"26627493"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post soil is a minor component."|"25074605"|"26627494"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074606"|"26627495"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ronan component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 18 within 30 inches of the soil surface."|"25074607"|"26627496"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bolack soil is a minor component."|"25074608"|"26627497"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marklepass soil is a minor component."|"25074609"|"26627498"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Round Butte component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 37 within 30 inches of the soil surface."|"25074610"|"26627499"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonepine soil is a minor component."|"25074611"|"26627500"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ronan soil is a minor component."|"25074612"|"26627501"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marklepass soil is a minor component."|"25074613"|"26627502"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074614"|"26627503"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Round Butte component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 37 within 30 inches of the soil surface."|"25074615"|"26627504"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonepine soil is a minor component."|"25074616"|"26627505"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ronan soil is a minor component."|"25074617"|"26627506"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marklepass soil is a minor component."|"25074618"|"26627507"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074619"|"26627508"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074620"|"26627509"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Round Butte component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 37 within 30 inches of the soil surface."|"25074621"|"26627510"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074622"|"26627511"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marklepass soil is a minor component."|"25074623"|"26627512"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Round Butte component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 37 within 30 inches of the soil surface."|"25074624"|"26627513"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074625"|"26627514"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slick spots soil is a minor component."|"25074626"|"26627515"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderatly well drained soils soil is a minor component."|"25074627"|"26627516"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Esteslake soil is a minor component."|"25074628"|"26627517"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Irvine component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of varved clayey lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP809MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"25074629"|"26627518"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Round Butte component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP804MT Saline-Sodic Shrubland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 37 within 30 inches of the soil surface."|"25074630"|"26627519"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marklepass soil is a minor component."|"25074631"|"26627520"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Irvine component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on lake plains. The parent material consists of varved clayey lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP809MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"25074632"|"26627521"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Round Butte component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP804MT Saline-Sodic Shrubland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 37 within 30 inches of the soil surface."|"25074633"|"26627522"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills, intermontane basins. The parent material consists of colluvium over residuum weathered from argillite and/or quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (Swdr) LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25079315"|"26632204"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm, greater slopes soil is a minor component."|"25079316"|"26632205"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills, intermontane basins. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA038MT Droughty Steep (Drstp)   LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25079317"|"26632206"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25079318"|"26632207"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079319"|"26632208"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25079320"|"26632209"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollman soil is a minor component."|"25074634"|"26627523"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Connah soil is a minor component."|"25074635"|"26627524"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074636"|"26627525"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074637"|"26627526"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074638"|"26627527"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollman soil is a minor component."|"25074639"|"26627528"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074640"|"26627529"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074641"|"26627530"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074642"|"26627531"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074643"|"26627532"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074644"|"26627533"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074645"|"26627534"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074646"|"26627535"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dune, sand soil is a minor component."|"25074647"|"26627536"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"25074648"|"26627537"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sacheen component makes up 85 percent of the map unit. Slopes are 3 to 10 percent. This component is on dunes. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074649"|"26627538"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074650"|"26627539"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sacheen component makes up 90 percent of the map unit. Slopes are 0 to 8 percent. This component is on dunes. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria.   "|"25074651"|"26627540"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"25074652"|"26627541"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074653"|"26627542"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selon component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria.   "|"25074654"|"26627543"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"25074655"|"26627544"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074656"|"26627545"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selon component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25074657"|"26627546"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"25074658"|"26627547"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074659"|"26627548"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selon component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria.   "|"25074660"|"26627549"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay soil is a minor component."|"25074661"|"26627550"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074662"|"26627551"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074663"|"26627552"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"25074664"|"26627553"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074665"|"26627554"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selon component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25074666"|"26627555"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074085"|"26626974"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074086"|"26626975"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074087"|"26626976"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074088"|"26626977"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25074089"|"26626978"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow, gravelly substratum soil is a minor component."|"25074667"|"26627556"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074668"|"26627557"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074669"|"26627558"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selow component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074670"|"26627559"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow, gravelly substratum soil is a minor component."|"25074671"|"26627560"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074672"|"26627561"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074673"|"26627562"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selow component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074674"|"26627563"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074675"|"26627564"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074676"|"26627565"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25074677"|"26627566"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074678"|"26627567"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25074679"|"26627568"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074680"|"26627569"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25074681"|"26627570"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25074682"|"26627571"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074683"|"26627572"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25074684"|"26627573"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074685"|"26627574"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074686"|"26627575"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074687"|"26627576"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074688"|"26627577"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truscreek component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, alluvial fans. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074689"|"26627578"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074690"|"26627579"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074691"|"26627580"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Polson component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"25074692"|"26627581"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truscreek component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, alluvial fans. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074693"|"26627582"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074694"|"26627583"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074695"|"26627584"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Polson component makes up 25 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"25074696"|"26627585"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truscreek component makes up 60 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074697"|"26627586"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074698"|"26627587"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074699"|"26627588"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074700"|"26627589"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Polson component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"25074701"|"26627590"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truscreek component makes up 60 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074702"|"26627591"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"25074703"|"26627592"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bolack soil is a minor component."|"25074704"|"26627593"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitearth soil is a minor component."|"25074705"|"26627594"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Haplaquepts component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains.  Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, November, December.  This component is in the R044AP806MT Subirrigated Grassland Group ecological site.   This soil meets hydric criteria.   "|"25074706"|"26627595"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Colake soil is a minor component."|"25074090"|"26626979"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bohnly component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 15 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 6 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"25074091"|"26626980"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Borohemists and similar soils soil is a minor component."|"25074092"|"26626981"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland, lake sediment outcrop soil is a minor component."|"25074707"|"26627596"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074708"|"26627597"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074709"|"26627598"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 85 percent of the map unit. Slopes are 15 to 60 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AA162MT Thin Loamy (Tlo) LRU 44A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074710"|"26627599"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonepine soil is a minor component."|"25074711"|"26627600"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vincom, gravelly loam soil is a minor component."|"25074712"|"26627601"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074713"|"26627602"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074714"|"26627603"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074715"|"26627604"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074716"|"26627605"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074717"|"26627606"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonepine component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074718"|"26627607"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074719"|"26627608"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vincom, gravelly loam soil is a minor component."|"25074720"|"26627609"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074721"|"26627610"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074722"|"26627611"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074723"|"26627612"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074724"|"26627613"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074725"|"26627614"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074726"|"26627615"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074727"|"26627616"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074728"|"26627617"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074729"|"26627618"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25074730"|"26627619"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walstead component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"25074731"|"26627620"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074732"|"26627621"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074733"|"26627622"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25074734"|"26627623"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074735"|"26627624"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walstead component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"25074736"|"26627625"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074737"|"26627626"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25074738"|"26627627"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074739"|"26627628"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walstead component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"25074740"|"26627629"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074741"|"26627630"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074742"|"26627631"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25074743"|"26627632"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walstead component makes up 75 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074744"|"26627633"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074745"|"26627634"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074746"|"26627635"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Esteslake component makes up 25 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP804MT Saline-Sodic Shrubland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 160 within 30 inches of the soil surface."|"25074747"|"26627636"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitearth component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP804MT Saline-Sodic Shrubland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 50 within 30 inches of the soil surface."|"25074748"|"26627637"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonepine soil is a minor component."|"25074749"|"26627638"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vincom soil is a minor component."|"25074750"|"26627639"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"25074751"|"26627640"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074752"|"26627641"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25074753"|"26627642"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"25074754"|"26627643"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very gravelly subsoil layers soil is a minor component."|"25074093"|"26626982"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very stony surface layers soil is a minor component."|"25074094"|"26626983"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sandy, wet soils soil is a minor component."|"25074095"|"26626984"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"25074096"|"26626985"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Borohemists and similar soils soil is a minor component."|"25074097"|"26626986"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bolack component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"25074098"|"26626987"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074755"|"26627644"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"25074756"|"26627645"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25074757"|"26627646"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074758"|"26627647"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25074759"|"26627648"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"25074760"|"26627649"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 50 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074761"|"26627650"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 40 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074762"|"26627651"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074763"|"26627652"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074764"|"26627653"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074765"|"26627654"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074766"|"26627655"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074767"|"26627656"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074768"|"26627657"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074769"|"26627658"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074770"|"26627659"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074771"|"26627660"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074772"|"26627661"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074773"|"26627662"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074774"|"26627663"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074775"|"26627664"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074776"|"26627665"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 65 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074777"|"26627666"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25074778"|"26627667"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074779"|"26627668"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074780"|"26627669"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074781"|"26627670"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074782"|"26627671"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074783"|"26627672"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25074784"|"26627673"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074785"|"26627674"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074786"|"26627675"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074787"|"26627676"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler, cool soil is a minor component."|"25074788"|"26627677"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074789"|"26627678"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP906MT Shallow Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074790"|"26627679"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074791"|"26627680"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074792"|"26627681"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074793"|"26627682"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Xerofluvents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R044AP801MT Bottomland Group ecological site.   This soil does not meet hydric criteria.   "|"25074794"|"26627683"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074795"|"26627684"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bolack soil is a minor component."|"25074796"|"26627685"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Xerofluvents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R044AP801MT Bottomland Group ecological site.   This soil does not meet hydric criteria.   "|"25074797"|"26627686"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074099"|"26626988"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Borohemists component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains.  Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, July, August, September, October, November, December.  This component is in the R044AP801MT Bottomland Group ecological site.   This soil meets hydric criteria.   "|"25074100"|"26626989"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay, dark surface soil is a minor component."|"25074798"|"26627687"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowbay component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria.   "|"25074799"|"26627688"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gravelly loamy sand subsoil soil is a minor component."|"25074800"|"26627689"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay, dark surface soil is a minor component."|"25074801"|"26627690"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowbay component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25074802"|"26627691"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074803"|"26627692"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074804"|"26627693"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowbay component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074805"|"26627694"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"25074035"|"26626924"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas supporting vegetation soil is a minor component."|"25074036"|"26626925"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Garceau gulch-indurated lime soil is a minor component."|"25074101"|"26626990"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowlake component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on relict stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074102"|"26626991"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger soil is a minor component."|"25074103"|"26626992"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074104"|"26626993"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowlake, stony loam soil is a minor component."|"25074105"|"26626994"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl, 2 soil is a minor component."|"25074106"|"26626995"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowlake component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on relict stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB033MT Loamy Argillic (Loa)   LRU 44A-B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074107"|"26626996"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on relict stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA032MT Loamy (Lo) LRU 44A-A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"25074108"|"26626997"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074109"|"26626998"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074110"|"26626999"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074111"|"26627000"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Colake component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on till plains. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R043AP807MT Subirrigated Grassland Group ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"25074112"|"26627001"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"25074113"|"26627002"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074114"|"26627003"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Colake component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on till plains. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R044AP806MT Subirrigated Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"25074115"|"26627004"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074116"|"26627005"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074117"|"26627006"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Colake, undrained soil is a minor component."|"25074118"|"26627007"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Indurated lime at 12 inches soil is a minor component."|"25074119"|"26627008"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Colake component makes up 60 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R044AP806MT Subirrigated Grassland Group ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"25074120"|"26627009"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074121"|"26627010"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Borohemists soil is a minor component."|"25074122"|"26627011"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sacheen component makes up 25 percent of the map unit. Slopes are 1 to 2 percent. This component is on stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria.   "|"25074123"|"26627012"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas of short, steep slopes soil is a minor component."|"25074124"|"26627013"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Connah component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on till plains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074125"|"26627014"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074126"|"26627015"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25074127"|"26627016"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074128"|"26627017"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25074129"|"26627018"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25074130"|"26627019"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Connah component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on till plains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074131"|"26627020"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074132"|"26627021"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25074133"|"26627022"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074134"|"26627023"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"25074135"|"26627024"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Connah component makes up 65 percent of the map unit. Slopes are 2 to 4 percent. This component is on till plains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074136"|"26627025"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074137"|"26627026"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074138"|"26627027"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25074139"|"26627028"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074140"|"26627029"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074141"|"26627030"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25074142"|"26627031"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"25074143"|"26627032"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074144"|"26627033"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen, south aspects soil is a minor component."|"25074145"|"26627034"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"25074146"|"26627035"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 90 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountain slopes. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074037"|"26626926"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074038"|"26626927"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen, south aspects soil is a minor component."|"25074147"|"26627036"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074148"|"26627037"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"25074149"|"26627038"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074150"|"26627039"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074151"|"26627040"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074152"|"26627041"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074153"|"26627042"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074154"|"26627043"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen, south aspects soil is a minor component."|"25074155"|"26627044"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074156"|"26627045"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 35 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074157"|"26627046"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25074158"|"26627047"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"25074159"|"26627048"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Aeric haplaquept soils soil is a minor component."|"25074160"|"26627049"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Craddock component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074161"|"26627050"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074162"|"26627051"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074163"|"26627052"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Craddock component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074164"|"26627053"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074165"|"26627054"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074166"|"26627055"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Craddock component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074167"|"26627056"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074168"|"26627057"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"25074169"|"26627058"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Borohemists soil is a minor component."|"25074170"|"26627059"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doker component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of volcanic ash over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 6 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"25074171"|"26627060"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074172"|"26627061"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerrdam soil is a minor component."|"25074173"|"26627062"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryfork component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074174"|"26627063"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074175"|"26627064"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074039"|"26626928"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074040"|"26626929"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074041"|"26626930"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils shallow to bedrock soil is a minor component."|"25074042"|"26626931"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selow component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074176"|"26627065"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerrdam soil is a minor component."|"25074177"|"26627066"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074178"|"26627067"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryfork component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on lake plains. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074179"|"26627068"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Selow component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074180"|"26627069"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerrdam soil is a minor component."|"25074181"|"26627070"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Irvine soil is a minor component."|"25074182"|"26627071"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryfork component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on lake plains. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074183"|"26627072"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dubay component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"25074184"|"26627073"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074185"|"26627074"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dubay soil is a minor component."|"25074186"|"26627075"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dubay component makes up 90 percent of the map unit. Slopes are 2 to 6 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"25074187"|"26627076"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074188"|"26627077"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selon soil is a minor component."|"25074189"|"26627078"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eaglewing component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074190"|"26627079"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074191"|"26627080"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing, stony loam soil is a minor component."|"25074192"|"26627081"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074193"|"26627082"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074194"|"26627083"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eaglewing component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074195"|"26627084"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing, stony loam soil is a minor component."|"25074196"|"26627085"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074197"|"26627086"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eaglewing component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074198"|"26627087"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074199"|"26627088"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074200"|"26627089"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dayton area-sodic soils soil is a minor component."|"25074201"|"26627090"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074202"|"26627091"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slick spots is a miscellaneous area."|"25074203"|"26627092"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland, lake sediment outcrop soil is a minor component."|"25074204"|"26627093"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Esteslake component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 160 within 30 inches of the soil surface."|"25074205"|"26627094"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074206"|"26627095"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Felan component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074207"|"26627096"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074208"|"26627097"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074209"|"26627098"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Felan component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074210"|"26627099"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollman, on warmer aspects soil is a minor component."|"25074211"|"26627100"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074212"|"26627101"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074213"|"26627102"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074043"|"26626932"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Belton component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on till plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074044"|"26626933"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074045"|"26626934"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074046"|"26626935"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074214"|"26627103"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074215"|"26627104"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074216"|"26627105"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"25074217"|"26627106"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074218"|"26627107"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074219"|"26627108"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25074220"|"26627109"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, very stony loam soil is a minor component."|"25074221"|"26627110"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074222"|"26627111"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074223"|"26627112"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074224"|"26627113"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074225"|"26627114"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074226"|"26627115"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074227"|"26627116"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074228"|"26627117"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074229"|"26627118"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074230"|"26627119"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074231"|"26627120"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25074232"|"26627121"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074233"|"26627122"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074234"|"26627123"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074235"|"26627124"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074236"|"26627125"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074237"|"26627126"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25074238"|"26627127"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074239"|"26627128"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074240"|"26627129"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074241"|"26627130"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25074242"|"26627131"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25074243"|"26627132"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074244"|"26627133"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Flott component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074245"|"26627134"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074246"|"26627135"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074247"|"26627136"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074248"|"26627137"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Flott component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074249"|"26627138"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074250"|"26627139"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074251"|"26627140"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074252"|"26627141"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Flott component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074253"|"26627142"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074254"|"26627143"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074255"|"26627144"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074256"|"26627145"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post soil is a minor component."|"25074047"|"26626936"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074048"|"26626937"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Belton component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074049"|"26626938"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074050"|"26626939"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Flott component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25074257"|"26627146"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074258"|"26627147"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074259"|"26627148"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Flott component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074260"|"26627149"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074261"|"26627150"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074262"|"26627151"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gardencreek component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during March, April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"25074263"|"26627152"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marklepass soil is a minor component."|"25074264"|"26627153"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"25074265"|"26627154"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gird component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074266"|"26627155"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074267"|"26627156"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074268"|"26627157"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074269"|"26627158"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dubay soil is a minor component."|"25074270"|"26627159"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074271"|"26627160"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dubay soil is a minor component."|"25074272"|"26627161"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gird component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074273"|"26627162"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074274"|"26627163"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074275"|"26627164"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slickspots soil is a minor component."|"25074276"|"26627165"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Indurated lime below 30 inches soil is a minor component."|"25074277"|"26627166"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gird component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 42 inches during June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074278"|"26627167"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Colake soil is a minor component."|"25074279"|"26627168"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dryfork component makes up 40 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 42 inches during June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074280"|"26627169"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gird component makes up 55 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074281"|"26627170"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 35 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074282"|"26627171"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074283"|"26627172"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074284"|"26627173"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074285"|"26627174"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerrdam soil is a minor component."|"25074286"|"26627175"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truscreek soil is a minor component."|"25074287"|"26627176"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gird component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074288"|"26627177"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074289"|"26627178"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074290"|"26627179"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074291"|"26627180"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Half Moon soil is a minor component."|"25074292"|"26627181"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074293"|"26627182"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on outwash plains, stream terraces. The parent material consists of volcanic ash over outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"25074294"|"26627183"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25074295"|"26627184"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on outwash plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074296"|"26627185"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074297"|"26627186"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25074298"|"26627187"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074299"|"26627188"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Belton component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074051"|"26626940"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074052"|"26626941"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post soil is a minor component."|"25074053"|"26626942"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074054"|"26626943"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash plains. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074300"|"26627189"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074301"|"26627190"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25074302"|"26627191"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074303"|"26627192"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25074304"|"26627193"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043AP906MT Shallow Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074305"|"26627194"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25074306"|"26627195"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074307"|"26627196"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25074308"|"26627197"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074309"|"26627198"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25074310"|"26627199"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25074311"|"26627200"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 60 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP805MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074312"|"26627201"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074313"|"26627202"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25074314"|"26627203"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074315"|"26627204"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074316"|"26627205"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074317"|"26627206"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils 10 to 40 inches to rock soil is a minor component."|"25074318"|"26627207"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25074319"|"26627208"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25074320"|"26627209"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25074321"|"26627210"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074322"|"26627211"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils 10 to 40 inches to rock soil is a minor component."|"25074323"|"26627212"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25074324"|"26627213"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074325"|"26627214"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils 10 to 40 inches to rock soil is a minor component."|"25074326"|"26627215"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Felan soil is a minor component."|"25074327"|"26627216"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074328"|"26627217"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074329"|"26627218"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074330"|"26627219"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074331"|"26627220"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25074332"|"26627221"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Felan soil is a minor component."|"25074333"|"26627222"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils 10 to 40 inches to rock soil is a minor component."|"25074334"|"26627223"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074335"|"26627224"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils 10 to 40 inches to rock soil is a minor component."|"25074336"|"26627225"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 70 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25074337"|"26627226"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25074338"|"26627227"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis, south aspects soil is a minor component."|"25074339"|"26627228"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 55 percent of the map unit. Slopes are 45 to 75 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25074340"|"26627229"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils 10 to 40 inches to rock soil is a minor component."|"25074341"|"26627230"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074342"|"26627231"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"25074343"|"26627232"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland, lake sediment outcrop soil is a minor component."|"25074344"|"26627233"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Irvine component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on lake plains. The parent material consists of varved clayey lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"25074345"|"26627234"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas of steeper slopes soil is a minor component."|"25074346"|"26627235"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074347"|"26627236"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ronan soil is a minor component."|"25074348"|"26627237"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Belton component makes up 50 percent of the map unit. Slopes are 2 to 4 percent. This component is on till plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074055"|"26626944"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerl component makes up 35 percent of the map unit. Slopes are 2 to 4 percent. This component is on till plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074056"|"26626945"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074057"|"26626946"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074058"|"26626947"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte, moist soil is a minor component."|"25074059"|"26626948"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland, lake sediment outcrop soil is a minor component."|"25074349"|"26627238"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074350"|"26627239"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vincom soil is a minor component."|"25074351"|"26627240"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonepine soil is a minor component."|"25074352"|"26627241"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Irvine component makes up 85 percent of the map unit. Slopes are 15 to 60 percent. This component is on lake plains. The parent material consists of varved clayey lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AA161MT Thin Clayey (Tcy) LRU 44A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"25074353"|"26627242"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko, very gravelly loam soil is a minor component."|"25074354"|"26627243"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lamoose soil is a minor component."|"25074355"|"26627244"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25074356"|"26627245"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jocko component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"25074357"|"26627246"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko, stony loam soil is a minor component."|"25074358"|"26627247"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25074359"|"26627248"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074360"|"26627249"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jocko component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"25074361"|"26627250"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Steep slopes along escarpments soil is a minor component."|"25074362"|"26627251"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074363"|"26627252"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"25074364"|"26627253"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jocko component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"25074365"|"26627254"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl, 2 soil is a minor component."|"25074366"|"26627255"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074367"|"26627256"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074368"|"26627257"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074369"|"26627258"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074370"|"26627259"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerl component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074371"|"26627260"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074372"|"26627261"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gird soil is a minor component."|"25074373"|"26627262"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Belton soil is a minor component."|"25074374"|"26627263"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074375"|"26627264"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerl component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of glaciofluvial deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074376"|"26627265"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerrdam component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake plains. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074377"|"26627266"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074378"|"26627267"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerrdam component makes up 90 percent of the map unit. Slopes are 2 to 6 percent. This component is on lake plains. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074379"|"26627268"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074380"|"26627269"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 25 percent of the map unit. Slopes are 6 to 15 percent. This component is on relict stream terraces. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP809MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074381"|"26627270"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerrdam component makes up 65 percent of the map unit. Slopes are 6 to 15 percent. This component is on relict stream terraces. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP809MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074382"|"26627271"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074383"|"26627272"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074384"|"26627273"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 35 percent of the map unit. Slopes are 15 to 30 percent. This component is on relict stream terraces. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AA162MT Thin Loamy (Tlo) LRU 44A-A ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074385"|"26627274"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerrdam component makes up 55 percent of the map unit. Slopes are 15 to 30 percent. This component is on relict stream terraces. The parent material consists of eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074386"|"26627275"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dryfork soil is a minor component."|"25074387"|"26627276"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074388"|"26627277"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ninepipe soil is a minor component."|"25074060"|"26626949"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polson soil is a minor component."|"25074061"|"26626950"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25074062"|"26626951"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Belton component makes up 45 percent of the map unit. Slopes are 4 to 8 percent. This component is on till plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25074063"|"26626952"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kerl component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on till plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074064"|"26626953"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte, moist soil is a minor component."|"25074065"|"26626954"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"25074389"|"26627278"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint, stony loam soil is a minor component."|"25074390"|"26627279"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074391"|"26627280"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25074392"|"26627281"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25074393"|"26627282"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25074394"|"26627283"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint, stony loam soil is a minor component."|"25074395"|"26627284"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25074396"|"26627285"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25074397"|"26627286"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25074398"|"26627287"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074399"|"26627288"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25074400"|"26627289"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074401"|"26627290"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25074402"|"26627291"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas that frequently flood soil is a minor component."|"25074403"|"26627292"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Areas that rarely flood soil is a minor component."|"25074404"|"26627293"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25074405"|"26627294"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lamoose component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074406"|"26627295"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonepine component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074407"|"26627296"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074408"|"26627297"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonepine component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074409"|"26627298"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074410"|"26627299"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vincom soil is a minor component."|"25074411"|"26627300"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl, 3 soil is a minor component."|"25074412"|"26627301"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonepine component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP809MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074413"|"26627302"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Selow soil is a minor component."|"25074414"|"26627303"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Esteslake soil is a minor component."|"25074415"|"26627304"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vincom component makes up 35 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"25074416"|"26627305"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonepine component makes up 55 percent of the map unit. Slopes are 4 to 8 percent. This component is on lake plains. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25074417"|"26627306"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl, 2 soil is a minor component."|"25074418"|"26627307"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marklepass component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP803MT Saline-Sodic Grassland Group ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 83 within 30 inches of the soil surface."|"25074419"|"26627308"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25074420"|"26627309"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitearth soil is a minor component."|"25074421"|"26627310"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Miscellaneous water is a miscellaneous area."|"25074806"|"26627695"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"25074807"|"26627696"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Post soil is a minor component."|"25079916"|"26632805"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"25079917"|"26632806"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Belton component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"25079918"|"26632807"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Round Butte soil is a minor component."|"25079919"|"26632808"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25079920"|"26632809"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079921"|"26632810"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25079922"|"26632811"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25079923"|"26632812"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen, south aspects soil is a minor component."|"25079924"|"26632813"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079925"|"26632814"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"25079926"|"26632815"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eaglewing component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079927"|"26632816"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing, stony silt loam soil is a minor component."|"25079928"|"26632817"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25079929"|"26632818"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25079930"|"26632819"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25079931"|"26632820"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing, stony loam soil is a minor component."|"25079932"|"26632821"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eaglewing component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079933"|"26632822"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25079934"|"26632823"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25079935"|"26632824"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25079936"|"26632825"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"25079937"|"26632826"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"25079938"|"26632827"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25079939"|"26632828"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25079940"|"26632829"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"25079941"|"26632830"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, very stony loam soil is a minor component."|"25079942"|"26632831"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25079998"|"26632887"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25079999"|"26632888"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"25080000"|"26632889"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25080001"|"26632890"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"25079943"|"26632832"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25079944"|"26632833"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25079945"|"26632834"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25079946"|"26632835"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25079947"|"26632836"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Flott component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AP808MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25079948"|"26632837"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25079949"|"26632838"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash plains. The parent material consists of volcanic ash over glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079950"|"26632839"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash plains. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079951"|"26632840"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"25079952"|"26632841"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"25079953"|"26632842"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint, stony loam soil is a minor component."|"25079954"|"26632843"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McDonald soil is a minor component."|"25079955"|"26632844"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"25079956"|"26632845"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing soil is a minor component."|"25079957"|"26632846"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079958"|"26632847"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25079959"|"26632848"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25079960"|"26632849"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten, shallow to bedrock soil is a minor component."|"25079961"|"26632850"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite and/or colluvium derived from argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079962"|"26632851"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay soil is a minor component."|"25079963"|"26632852"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"25079964"|"26632853"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollman component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25079965"|"26632854"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25079966"|"26632855"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada, stony loam soil is a minor component."|"25079967"|"26632856"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25079968"|"26632857"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jocko soil is a minor component."|"25079969"|"26632858"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Niarada component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079970"|"26632859"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25079971"|"26632860"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25079972"|"26632861"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079973"|"26632862"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25079974"|"26632863"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25079975"|"26632864"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walstead soil is a minor component."|"25079976"|"26632865"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"25079977"|"26632866"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flott soil is a minor component."|"25079978"|"26632867"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walstead component makes up 75 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079979"|"26632868"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"25079980"|"26632869"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079981"|"26632870"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"25079982"|"26632871"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25079983"|"26632872"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25079984"|"26632873"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"25079985"|"26632874"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"25079986"|"26632875"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 50 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079987"|"26632876"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 40 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP911MT Upland Warm Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25079988"|"26632877"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25079989"|"26632878"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25079990"|"26632879"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25079991"|"26632880"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines. The parent material consists of glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25079992"|"26632881"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay, dark surface soil is a minor component."|"25079993"|"26632882"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowbay component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria.   "|"25079994"|"26632883"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"25079995"|"26632884"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"25079996"|"26632885"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowbay component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on outwash plains. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"25079997"|"26632886"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25079295"|"26632184"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 90 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25079296"|"26632185"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25079297"|"26632186"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25079298"|"26632187"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"25079299"|"26632188"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079300"|"26632189"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"25079301"|"26632190"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25079302"|"26632191"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25079732"|"26632621"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak soil is a minor component."|"25079733"|"26632622"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pleasantvalley soil is a minor component."|"25079734"|"26632623"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"25079735"|"26632624"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"25079736"|"26632625"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"25079737"|"26632626"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tallcreek soil is a minor component."|"25079738"|"26632627"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25079456"|"26632345"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"25079457"|"26632346"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"25079458"|"26632347"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lynchlake soil is a minor component."|"25079459"|"26632348"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079460"|"26632349"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 55 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079461"|"26632350"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25079462"|"26632351"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"25079694"|"26632583"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079695"|"26632584"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"25079449"|"26632338"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig, greater slope soil is a minor component."|"25079450"|"26632339"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079451"|"26632340"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25079452"|"26632341"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"25079453"|"26632342"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Stevie soil is a minor component."|"25079454"|"26632343"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25079455"|"26632344"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from argillite or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25079696"|"26632585"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway, cool soil is a minor component."|"25079697"|"26632586"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"25079698"|"26632587"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25079699"|"26632588"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowlake component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB033MT Loamy Argillic (Loa)   LRU 44A-B ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079303"|"26632192"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB036MT Droughty (Dr) LRU 44A-B ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"25079304"|"26632193"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Camascreek soil is a minor component."|"25079305"|"26632194"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger, stony soil is a minor component."|"25079306"|"26632195"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, stream terraces, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA036MT Droughty (Dr) LRU 44A-A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"25079307"|"26632196"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger, greater slope soil is a minor component."|"25079308"|"26632197"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowlake soil is a minor component."|"25079309"|"26632198"
07/12/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper soil is a minor component."|"25079746"|"26632635"
07/12/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"25079747"|"26632636"
07/12/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25079748"|"26632637"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079749"|"26632638"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"25079750"|"26632639"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashleylake, greater slope soil is a minor component."|"25079799"|"26632688"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashleylake component makes up 65 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from argillite and/or calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25079800"|"26632689"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"25079801"|"26632690"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"25079802"|"26632691"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bendahl soil is a minor component."|"25079803"|"26632692"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079804"|"26632693"
07/12/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"25079754"|"26632643"
07/12/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25079755"|"26632644"
07/12/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"25079756"|"26632645"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 70 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079757"|"26632646"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079758"|"26632647"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 25 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"25080010"|"26632899"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AA138MT Shallow Droughty (Swdr) LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"25080011"|"26632900"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"25080012"|"26632901"
07/11/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"25080013"|"26632902"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25080014"|"26632903"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashleylake component makes up 50 percent of the map unit. Slopes are 40 to 60 percent. This component is on glacially scoured ridges, mountains. The parent material consists of volcanic ash over till derived from argillite and/or calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25079811"|"26632700"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25079812"|"26632701"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"25079813"|"26632702"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 15 percent of the map unit. Slopes are 40 to 70 percent. This component is on glacially scoured ridges, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP905MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25079814"|"26632703"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079815"|"26632704"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repp component makes up 50 percent of the map unit. Slopes are 40 to 80 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of colluvium derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079751"|"26632640"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 25 percent of the map unit. Slopes are 40 to 60 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"25079752"|"26632641"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079753"|"26632642"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on hills. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA038MT Droughty Steep (Drstp)   LRU 43A-A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25079310"|"26632199"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 20 percent of the map unit. Slopes are 8 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from argillite and/or quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (Swdr) LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"25079311"|"26632200"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm, greater slope soil is a minor component."|"25079312"|"26632201"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"25079313"|"26632202"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25079314"|"26632203"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"25081523"|"26634412"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kawuneeche component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. This component is in the R043AP802MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"25081524"|"26634413"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elvick soil is a minor component."|"25081525"|"26634414"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"25081526"|"26634415"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCay component makes up 90 percent of the map unit. Slopes are 10 to 35 percent. This component is on broadly convex ridges on mountains, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 35 to 59 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25081527"|"26634416"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"25081528"|"26634417"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25081529"|"26634418"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCay component makes up 35 percent of the map unit. Slopes are 10 to 40 percent. This component is on broadly convex ridges on mountains, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25081530"|"26634419"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCay component makes up 60 percent of the map unit. Slopes are 10 to 40 percent. This component is on broadly convex ridges on mountains, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP910MT Upland Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"25081531"|"26634420"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"25081532"|"26634421"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCay component makes up 60 percent of the map unit. Slopes are 10 to 35 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"25081533"|"26634422"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crabtree component makes up 30 percent of the map unit. Slopes are 2 to 10 percent. This component is on drainageways, swales, mountains. The parent material consists of alluvium over high bulk density till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 28 inches (depth from the mineral surface is 26 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 6 percent. This component is in the F043AP907MT Subirrigated Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"25081534"|"26634423"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jurvannah soil is a minor component."|"25081535"|"26634424"
