"1"|"Aeric Haplaquepts, 1 to 3 percent slopes"||2|2.2||31|31|"Frequent"|"Frequent"|"0"|6.17|10.7|17.69|25.33|"Poorly drained"|"Poorly drained"|||87||85|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.032|"Not rated"|"87"|0.367|"144979"
"10"|"Bigarm cobbly loam, 15 to 30 percent slopes"||23|23.4||||"None"|"None"|"0"|3.23|5.12|8.42|11.73|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.924|"Severe"|"0"|1|"144980"
"100"|"Marklepass-Slickspots complex, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|2.75|5.26|9.9|14.44|"Well drained"|"Well drained"|"D"|"7"|60|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.305|"Slight"|"10"|1|"144982"
"101"|"McCollum fine sandy loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.76|7.26|14.02|20.57|"Well drained"|"Well drained"|"A"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.001|"Slight"|"0"|0.45|"144983"
"102"|"McCollum fine sandy loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|3.77|7.31|14.14|20.76|"Well drained"|"Well drained"|"A"|"4"|90|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.031|"Slight"|"0"|0.433|"144984"
"103"|"McCollum fine sandy loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.76|7.36|14.27|20.97|"Well drained"|"Well drained"|"A"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.014|"Moderate"|"0"|0.405|"144985"
"104"|"McCollum fine sandy loam, gravelly substratum, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|3.69|7.06|13.19|16.14|"Well drained"|"Well drained"|"A"|"4"|100|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.023|"Slight"|"0"|0.533|"144986"
"105"|"McDonald cobbly silty clay loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.58|7.51|14.98|22.3|"Well drained"|"Well drained"|"C"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.076|"Slight"|"2"|0.965|"144987"
"106"|"McDonald cobbly silty clay loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.57|7.51|14.97|22.29|"Well drained"|"Well drained"|"C"|"3"|89|"3"|89|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.077|"Moderate"|"2"|0.967|"144988"
"107"|"McDonald cobbly silty clay loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.61|7.53|14.95|22.29|"Well drained"|"Well drained"|"C"|"4"|89|"4"|89|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.103|"Moderate"|"0"|0.967|"144989"
"108"|"McDonald silty clay loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.49|8.37|15.95|23.43|"Well drained"|"Well drained"|"C"|"2"|88|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.09|"Slight"|"2"|0.964|"144990"
"109"|"Minesinger stony loam, 4 to 15 percent slopes"||10|11.2||||"None"|"None"|"0"|3.44|6.42|10.95|15.01|"Well drained"|"Well drained"|"C"||90|"6"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.135|"Moderate"|"0"|0.982|"144991"
"11"|"Bigarm cobbly loam, cool, 15 to 30 percent slopes"||23|23.7||||"None"|"None"|"0"|3.56|5.73|9.78|13.83|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.928|"Severe"|"0"|1|"144992"
"110"|"Minesinger-Walstead very stony loams, 15 to 45 percent slopes"||30|28.9||||"None"|"None"|"0"|2.98|5.56|9.83|13.72|"Well drained"|"Well drained"|"C"||96|"7"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.959|"Severe"|"0"|0.993|"144993"
"111"|"Mitten gravelly silt loam, 8 to 30 percent slopes"||19|20.8||||"None"|"None"|"0"|5.9|8.34|10.38|11.98|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.417|"Severe"|"0"|1|"144994"
"112"|"Mitten very gravelly silt loam, 30 to 60 percent slopes"||45|44.9||||"None"|"None"|"0"|5.52|7.62|9.65|11.23|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"144995"
"113"|"Mitten very gravelly silt loam, dry, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.62|7.76|9.84|11.46|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"144996"
"114"|"Mitten, dry-Rock outcrop complex, 30 to 60 percent slopes"||45|44.9||||"None"|"None"|"0"|5.43|7.52|9.62|11.27|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"144997"
"115"|"Moiese loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.91|5.94|8.23|10.5|"Excessively drained"|"Excessively drained"|"B"|"4"|100|"6"|94|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.117|"Slight"|"0"|0.967|"144998"
"116"|"Mollman gravelly loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|6.02|9.81|15.78|21.19|"Well drained"|"Well drained"|"B"|"6"|85|"6"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0.006|"Slight"|"5"|0.102|"144999"
"117"|"Mollman gravelly loam, 4 to 15 percent slopes"||10|12||||"None"|"None"|"0"|6.06|9.68|15.23|20.78|"Well drained"|"Well drained"|"B"|"6"|85|"6"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0.056|"Moderate"|"0"|0.252|"145000"
"118"|"Mollman gravelly loam, 15 to 30 percent slopes"||23|24.1||||"None"|"None"|"0"|5.98|9.42|14.56|19.71|"Well drained"|"Well drained"|"B"|"6"|95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.924|"Severe"|"0"|1|"145001"
"119"|"Mollman very gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.37|8.02|13.2|18.37|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"145003"
"12"|"Bigarm gravelly loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.74|6.3|10.94|15.58|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.114|"Moderate"|"0"|0.67|"145004"
"120"|"Niarada gravelly loam, 0 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.15|5.21|9.34|13.44|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.083|"Slight"|"0"|0.195|"145005"
"121"|"Niarada gravelly loam, 4 to 8 percent slopes"||6|6.2||||"None"|"None"|"0"|3.15|5.21|9.34|13.44|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.083|"Moderate"|"0"|0.195|"145007"
"122"|"Niarada gravelly loam, 8 to 15 percent slopes"||12|11.6||||"None"|"None"|"0"|3.09|5.1|9.11|13.09|"Well drained"|"Well drained"|"B"|"4"|95|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.078|"Moderate"|"0"|0.642|"145008"
"123"|"Niarada gravelly loam, cool, 15 to 30 percent slopes"||23|22.7||||"None"|"None"|"0"|3.29|5.49|9.16|12.81|"Well drained"|"Well drained"|"B"||95|"6"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.88|"Severe"|"0"|1|"145009"
"124"|"Niarada gravelly loam, cool, 30 to 60 percent slopes"||45|43.9||||"None"|"None"|"0"|3.37|5.6|9.45|13.25|"Well drained"|"Well drained"|"B"||97|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.971|"Severe"|"0"|0.974|"145010"
"125"|"Niarada-Kerl complex, 8 to 15 percent slopes"||12|11.4||||"None"|"None"|"0"|3.92|7.01|13.3|19.57|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.098|"Moderate"|"0"|0.619|"145011"
"126"|"Ninepipe silt loam, 0 to 2 percent slopes"||1|1||153|153|"None"|"None"|"0"|4.51|8.88|17.67|26.02|"Moderately well drained"|"Moderately well drained"|"B"|"2"|85|"3"|95|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.184|"Slight"|"5"|0.15|"145012"
"127"|"Phillcher gravelly silt loam, 15 to 45 percent slopes"||30|28.9||||"None"|"None"|"0"|6.19|8.88|12.13|14.08|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.947|"Severe"|"0"|1|"145013"
"128"|"Phillcher-Rock outcrop complex, 45 to 75 percent slopes"||60|59.4||||"None"|"None"|"0"|6.22|8.91|12.13|14.06|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145014"
"129"|"Pits, gravel"|||1||||||"0"|3.95|5.9|7.9|9.9|||||90||90|"Not rated"|"Not rated"|"Not limited"|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.015|"Not rated"|"0"|1|"145015"
"13"|"Bigarm, cool-Hogsby-Rock outcrop complex, 30 to 60 percent slopes"||45|45|46|||"None"|"None"|"0"|3.5|5.56|8.93|11.34|"Somewhat excessively drained"|"Well drained"|"B"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145016"
"130"|"Polson silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.29|7.87|15.03|22.21|"Well drained"|"Well drained"|"C"|"3"|90|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.158|"Slight"|"0"|0.9|"145017"
"131"|"Polson silt loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.28|7.88|15.06|22.25|"Well drained"|"Well drained"|"C"|"3"|85|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.154|"Moderate"|"0"|0.895|"145019"
"132"|"Polson-Vincom silt loams, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.31|7.99|15.34|22.67|"Well drained"|"Well drained"|"C"|"3"|80|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.172|"Moderate"|"0"|0.85|"145020"
"133"|"Post silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.43|7.41|13.37|19.33|"Well drained"|"Well drained"|"D"|"4"|97|"4"|97|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.133|"Slight"|"2"|1|"145021"
"134"|"Post silty clay loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.44|7.43|13.4|19.36|"Well drained"|"Well drained"|"D"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.133|"Moderate"|"2"|1|"145022"
"135"|"Post silty clay loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.59|8|13.96|19.93|"Well drained"|"Well drained"|"D"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.133|"Moderate"|"2"|1|"145023"
"136"|"Post-Ronan-Water complex, 2 to 8 percent slopes"||5|4.8||||"None"|"None"|"0"|4.28|7.55|13.41|19.23|"Well drained"|"Well drained"|"D"|"4"|70|"4"|70|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.148|"Moderate"|"2"|0.907|"145026"
"137"|"Post-Ronan-Water complex, 8 to 15 percent slopes"||12|11||||"None"|"None"|"0"|4.1|7.25|13.01|18.73|"Well drained"|"Well drained"|"D"|"6"|65|"6"|65|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.836|"Severe"|"3"|0.932|"145027"
"138"|"Repp gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.59|6.52|9.15|11.79|"Well drained"|"Well drained"|"B"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145028"
"139"|"Repp, cool-Rock outcrop complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.6|6.53|9.18|11.84|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145030"
"14"|"Bigarm, cool-Rubble land complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|3.3|5|7.04|9.08|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145031"
"140"|"Rock outcrop-Rubble land complex"|||||||||"0"|||||||"D"||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"145032"
"141"|"Ronan silty clay loam, 0 to 2 percent slopes"||1|1.3||||"None"|"None"|"0"|3.49|6.14|11.16|16.19|"Well drained"|"Well drained"|"D"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.22|"Slight"|"0"|1|"145034"
"142"|"Ronan silty clay loam, 2 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|3.45|6.05|10.98|15.9|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.225|"Moderate"|"0"|1|"145036"
"143"|"Ronan silty clay loam, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|3.57|6.32|11.49|16.63|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.217|"Moderate"|"5"|1|"145037"
"144"|"Round Butte silty clay loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.88|6.24|10.54|14.84|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.324|"Slight"|"0"|0.975|"145038"
"145"|"Round Butte silty clay loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|3.92|6.27|10.57|14.87|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.321|"Moderate"|"0"|0.975|"145039"
"146"|"Round Butte silty clay loam, 4 to 8 percent slopes"||6|5.7||||"None"|"None"|"0"|3.88|6.17|10.37|14.58|"Well drained"|"Well drained"|"D"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.321|"Moderate"|"3"|1|"145040"
"147"|"Round Butte silty clay loam, dry, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.82|6.15|10.37|14.6|"Well drained"|"Well drained"|"D"|"4"|90|"6"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Slight"|"0"|1|"145043"
"148"|"Round Butte-Irvine silty clay loams, dry, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.79|5.93|9.9|13.87|"Well drained"|"Well drained"|"D"|"4"|60|"4"|60|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.3|"Moderate"|"0"|1|"145045"
"149"|"Round Butte-Irvine silty clay loams, dry, 4 to 15 percent slopes"||10|9.1||||"None"|"None"|"0"|3.75|5.91|9.9|13.9|"Well drained"|"Well drained"|"D"|"4"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.933|"Severe"|"0"|1|"145046"
"15"|"Bigarm-Hogsby-Rock outcrop complex, 30 to 60 percent slopes"||45|46.7|43|||"None"|"None"|"0"|3|4.76|7.02|8.42|"Somewhat excessively drained"|"Well drained"|"B"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145048"
"150"|"Rumblecreek gravelly loam, 2 to 8 percent slopes"||5|4.7||||"None"|"None"|"0"|5.86|9.23|14.03|18.31|"Well drained"|"Well drained"|"C"|"6"|89|"6"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.007|"Moderate"|"3"|0.485|"145049"
"151"|"Rumblecreek gravelly loam, 8 to 15 percent slopes"||12|11.8||||"None"|"None"|"0"|6.01|9.34|13.89|18.04|"Well drained"|"Well drained"|"C"|"6"|100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.002|"Moderate"|"0"|0.586|"145051"
"152"|"Rumblecreek gravelly loam, 15 to 30 percent slopes"||23|24.2||||"None"|"None"|"0"|5.79|8.97|13.31|17.24|"Well drained"|"Well drained"|"C"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.924|"Severe"|"0"|1|"145052"
"153"|"Rumblecreek gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.85|9.12|13.61|17.66|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"145053"
"154"|"Sacheen fine sand, hummocky, 3 to 10 percent slopes"||7|7||||"None"|"None"|"0"|3.75|6.25|11.25|16.25|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|85|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Not rated"|"Somewhat limited"|0.336|"Moderate"|"0"|1|"145055"
"155"|"Sacheen loamy fine sand, 0 to 8 percent slopes"||4|4.2||||"None"|"None"|"0"|3.74|6.34|11.52|16.67|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"|"4"|100|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.302|"Moderate"|"0"|0.945|"145056"
"156"|"Selon fine sandy loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.32|7.77|14.65|21.5|"Well drained"|"Well drained"|"A"|"2"|85|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.024|"Slight"|"0"|0.478|"145057"
"157"|"Selon fine sandy loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|4.32|7.77|14.65|21.5|"Well drained"|"Well drained"|"A"|"4"|100|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.024|"Slight"|"0"|0.478|"145058"
"158"|"Selon fine sandy loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.32|7.77|14.65|21.5|"Well drained"|"Well drained"|"A"|"2"|85|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.024|"Moderate"|"0"|0.478|"145059"
"159"|"Selon sandy loam, 8 to 15 percent slopes"||12|11.4||||"None"|"None"|"0"|4.4|7.79|14.47|21.14|"Well drained"|"Well drained"|"A"|"4"|100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.017|"Moderate"|"0"|0.641|"145060"
"16"|"Bigarm-Rock outcrop-Rubble land complex, 30 to 60 percent slopes"||45|45|||||"None"|"0"|3.68|5.98|8.72|11.45||"Somewhat excessively drained"|"B"||100|"8"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145061"
"160"|"Selow silty clay loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.16|7.66|15.49|23.2|"Well drained"|"Well drained"|"D"|"4"|94|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.295|"Slight"|"0"|0.962|"145062"
"161"|"Selow silty clay loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.17|7.67|15.54|23.1|"Well drained"|"Well drained"|"D"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.304|"Moderate"|"0"|0.973|"145064"
"162"|"Tevis very gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|3.94|5.49|7.64|9.75|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145065"
"163"|"Trapps gravelly loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|4.74|7.7|12.61|17.67|"Well drained"|"Well drained"|"C"|"6"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.018|"Moderate"|"0"|0.633|"145066"
"164"|"Trapps gravelly loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.68|7.66|12.72|17.97|"Well drained"|"Well drained"|"C"|"6"|90|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145067"
"165"|"Truscreek silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.49|8.87|17.63|26.41|"Well drained"|"Well drained"|"B"|"2"|90|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.197|"Slight"|"0"|0.1|"145068"
"166"|"Truscreek-Polson silt loams, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.43|8.56|16.82|25.1|"Well drained"|"Well drained"|"B"|"2"|65|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.185|"Slight"|"0"|0.35|"145069"
"167"|"Truscreek-Polson silt loams, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.44|8.56|16.81|25.09|"Well drained"|"Well drained"|"B"|"2"|65|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.189|"Moderate"|"0"|0.35|"145070"
"168"|"Truscreek-Polson silt loams, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.43|8.62|16.98|25.33|"Well drained"|"Well drained"|"B"|"3"|95|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.184|"Moderate"|"0"|0.3|"145071"
"169"|"Typic Haplaquepts, 0 to 2 percent slopes"||1|1.1||0|0|||"0"|4.21|7.99|15.56|22.26|"Very poorly drained"|"Very poorly drained"|||95||85|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.45|"Not rated"|"95"|1|"145072"
"17"|"Bohnly silt loam, 0 to 2 percent slopes"||1|1||38|38|"Occasional"|"Occasional"|"0"|4.74|9.29|18.34|26.38|"Poorly drained"|"Poorly drained"|"B/D"|"5"|90|"5"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.824|"Slight"|"92"|1|"145073"
"170"|"Vincom silt loam, 15 to 60 percent slopes"||38|35.2||||"None"|"None"|"0"|4.38|8.15|15.65|23.16|"Well drained"|"Well drained"|"C"||89|"7"|87|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.95|"Severe"|"0"|0.958|"145074"
"171"|"Vincom-Lonepine silt loams, 8 to 15 percent slopes"||12|11.7||||"None"|"None"|"0"|4.44|8.46|16.42|24.37|"Well drained"|"Well drained"|"C"|"4"|94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.935|"Severe"|"0"|0.843|"145076"
"172"|"Waldbillig gravelly silt loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.56|7.07|11.45|15.82|"Well drained"|"Well drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145077"
"173"|"Waldbillig gravelly silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.56|7.07|11.45|15.82|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145078"
"174"|"Walstead gravelly loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.61|6.31|10.43|13.71|"Well drained"|"Well drained"|"B"|"3"|96|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Slight"|"0"|0.144|"145079"
"175"|"Walstead gravelly loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|3.57|6.39|10.84|14.22|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Slight"|"0"|0.111|"145080"
"176"|"Walstead gravelly loam, 4 to 15 percent slopes"||10|9.9||||"None"|"None"|"0"|3.57|6.39|10.84|14.22|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.228|"145082"
"177"|"Walstead-Rock outcrop complex, 15 to 30 percent slopes"||23|23.6||||"None"|"None"|"0"|3.45|6.15|9.52|12.52|"Well drained"|"Well drained"|"B"|"6"|79|"6"|82|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.927|"Severe"|"0"|1|"145084"
"178"|"Whitearth-Esteslake complex, 2 to 8 percent slopes"||5|4.6||||"None"|"None"|"0"|3.19|5.91|11.1|15.92|"Well drained"|"Well drained"|"C"||85|"7"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.316|"Moderate"|"0"|0.96|"145085"
"179"|"Wildgen gravelly loam, 8 to 30 percent slopes"||19|19.7||||"None"|"None"|"0"|4.48|7.13|11.86|16.58|"Well drained"|"Well drained"|"B"|"6"|90|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.413|"Severe"|"0"|1|"145086"
"18"|"Bolack silt loam, 0 to 2 percent slopes"||1|1||61|61|"Occasional"|"Occasional"|"0"|4.36|8.69|17.23|25.13|"Poorly drained"|"Poorly drained"|"D"||98|"5"|89|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.178|"Slight"|"90"|1|"145087"
"180"|"Wildgen very gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|3.63|6.23|10.94|15.63|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"145088"
"181"|"Wildgen-Finleypoint gravelly loams, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.44|7.1|11.93|16.73|"Well drained"|"Well drained"|"B"|"6"|50|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145093"
"182"|"Winfall very gravelly loam, 4 to 15 percent slopes"||10|9.8||||"None"|"None"|"0"|5.35|8.17|12.91|17.46|"Well drained"|"Well drained"|"B"|"6"|92|"6"|92|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.006|"Moderate"|"2"|0.935|"145094"
"183"|"Winfall very gravelly loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|5.38|8.15|12.8|17.33|"Well drained"|"Well drained"|"B"|"6"|90|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145095"
"184"|"Winfall very gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.25|7.95|12.47|16.87|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"145097"
"185"|"Winkler, cool-Rock outcrop complex, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|2.98|4.52|7.12|9.58|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|73|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145099"
"186"|"Winkler very gravelly loam, cool, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|2.99|4.58|7.29|9.87|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145100"
"187"|"Winkler-Sharrott-Rock outcrop complex, 30 to 60 percent slopes"||45|45|51|||"None"|"None"|"0"|3.15|4.78|6.97|9.06|"Somewhat excessively drained"|"Well drained"|"A"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145101"
"188"|"Xerofluvents, 0 to 2 percent slopes"||1|1||||"Frequent"|"Frequent"|"0"|4.25|8.5|17|24.74|||||100||90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"10"|1|"145102"
"189"|"Xerofluvents, dry, 0 to 2 percent slopes"||1|1.1||||"Rare"|"Rare"|"0"|4.64|9.02|17.77|26.14|||||95||90|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.137|"Not rated"|"5"|0.75|"145103"
"19"|"Borohemists, 0 to 1 percent slopes"||1|1.1||15|15|"Frequent"|"Frequent"|"0"|4.25|8.5|17|21.7|"Very poorly drained"|"Very poorly drained"|||90||90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.042|"Not rated"|"90"|0.677|"145105"
"190"|"Yellowbay very gravelly loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|2.94|4.09|6.1|8.1|"Excessively drained"|"Excessively drained"|"A"|"4"|100|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.003|"Slight"|"0"|1|"145106"
"191"|"Yellowbay very gravelly loam, 4 to 15 percent slopes, lake effect"||10|10||||"None"|"None"|"0"|2.94|4.09|6.1|8.1|"Excessively drained"|"Excessively drained"|"A"|"4"|95|"6"|95|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.003|"Moderate"|"0"|1|"145108"
"192"|"Yellowbay very gravelly loam, 15 to 30 percent slopes"||23|22.4||||"None"|"None"|"0"|3.1|4.4|6.68|8.96|"Excessively drained"|"Excessively drained"|"A"|"6"|95|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.876|"Severe"|"0"|1|"145109"
"2"|"Badland"||40|37||||||"0"|3.79|5.79|9.79|13.79|||||90||90|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"145113"
"20"|"Bowlake gravelly loam, 4 to 8 percent slopes"||6|6.1||||"None"|"None"|"0"|3.53|6.4|11.87|17.1|"Well drained"|"Well drained"|"C"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.064|"Moderate"|"0"|0.966|"145114"
"21"|"Bowlake-Minesinger gravelly loams, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.57|6.51|11.72|16.75|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.152|"Moderate"|"0"|0.945|"145115"
"22"|"Colake silt loam, 0 to 1 percent slopes"||1|1||46|46|"None"|"None"|"0"|4.24|8.47|16.98|25.4|"Poorly drained"|"Poorly drained"|"B/D"||85|"5"|93|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.458|"Slight"|"93"|1|"145117"
"23"|"Colake silt loam, drained, 0 to 1 percent slopes"||1|1.1||76|76|"None"|"None"|"0"|4.2|8.33|16.4|24.42|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|95|"4"|90|"Not limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.211|"Slight"|"5"|0.85|"145118"
"24"|"Colake-Sacheen complex, 0 to 3 percent slopes"||2|1.9||46|46|"None"|"None"|"0"|4.33|8.25|15.8|23.59|"Poorly drained"|"Poorly drained"|"B/D"||70|"5"|65|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.384|"Slight"|"65"|0.971|"145122"
"25"|"Connah cobbly silt loam, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.84|9.1|17.34|25.06|"Well drained"|"Well drained"|"C"|"3"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.113|"Moderate"|"3"|0.968|"145124"
"26"|"Connah silt loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|5.13|9.38|17.63|25.34|"Well drained"|"Well drained"|"C"|"3"|85|"3"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.112|"Slight"|"2"|0.968|"145125"
"27"|"Connah-Water complex, 2 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|5.04|9.23|17.49|25|"Well drained"|"Well drained"|"C"|"3"|65|"3"|69|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.098|"Moderate"|"3"|0.947|"145126"
"28"|"Courville gravelly silt loam, 4 to 15 percent slopes"||10|10.5||||"None"|"None"|"0"|4.77|7.92|12.61|16.96|"Well drained"|"Well drained"|"B"|"6"|95|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Not limited"|0.016|"Severe"|"0"|0.247|"145127"
"29"|"Courville gravelly silt loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.7|7.83|12.66|17.2|"Well drained"|"Well drained"|"B"||93|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145130"
"3"|"Bata gravelly silt loam, 8 to 30 percent slopes"||19|19.4||||"None"|"None"|"0"|4.16|6.15|9.97|13.77|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.38|"Severe"|"0"|1|"145132"
"30"|"Courville gravelly silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.62|7.75|12.59|17.13|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"145133"
"31"|"Courville gravelly silt loam, warm, 4 to 15 percent slopes"||10|10||||"None"|"None"|"0"|4.66|7.82|12.68|17.23|"Well drained"|"Well drained"|"B"|"6"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0.004|"Severe"|"0"|0.247|"145134"
"32"|"Courville gravelly silt loam, warm, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.64|7.79|12.64|17.19|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145135"
"33"|"Courville gravelly silt loam, warm, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.54|7.69|12.55|17.1|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"145136"
"34"|"Courville-Rumblecreek complex, 8 to 30 percent slopes"||19|18.9||||"None"|"None"|"0"|5.28|8.46|13.03|17.16|"Well drained"|"Well drained"|"B"|"6"|56|"6"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.35|"Severe"|"2"|0.994|"145142"
"35"|"Craddock channery silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.35|7.31|12.52|17.67|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"145145"
"36"|"Craddock silt loam, 4 to 15 percent slopes"||10|10.5||||"None"|"None"|"0"|4.89|8.1|13.42|18.69|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.916|"Severe"|"0"|0.466|"145146"
"37"|"Craddock silt loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.89|8.1|13.42|18.69|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.992|"Severe"|"0"|1|"145147"
"38"|"Doker silt loam, 0 to 2 percent slopes"||1|1||31|31|"Occasional"|"Occasional"|"0"|5.31|9.78|17.12|24.58|"Poorly drained"|"Poorly drained"|"B/D"||90|"5"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.983|"Slight"|"100"|1|"145155"
"39"|"Dryfork silt loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.48|8.66|17.02|25.37|"Well drained"|"Well drained"|"B"|"4"|93|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not rated"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.329|"Slight"|"0"|0.959|"145162"
"4"|"Bata gravelly silt loam, 30 to 60 percent slopes"||45|46||||"None"|"None"|"0"|4.07|6.13|9.87|13.59|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"145174"
"40"|"Dryfork-Selow complex, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|4.39|8.3|16.43|24.53|"Well drained"|"Well drained"|"B"|"4"|85|"4"|50|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.323|"Slight"|"0"|0.9|"145175"
"41"|"Dryfork-Selow complex, 4 to 15 percent slopes"||10|10.1||||"None"|"None"|"0"|4.39|8.3|16.43|24.53|"Well drained"|"Well drained"|"B"|"4"|100|"4"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|0.937|"145179"
"42"|"Dubay silt loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.83|9.54|18.96|28.38|"Well drained"|"Well drained"|"C"|"3"|95|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.145|"Slight"|"0"|0.5|"145183"
"43"|"Dubay silt loam, 2 to 6 percent slopes"||4|3.9||||"None"|"None"|"0"|4.84|9.51|18.83|28.16|"Well drained"|"Well drained"|"C"|"3"|90|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.137|"Moderate"|"0"|0.473|"145195"
"44"|"Eaglewing gravelly silt loam, 8 to 15 percent slopes"||12|11.2||||"None"|"None"|"0"|4.74|8.5|15.88|23.03|"Well drained"|"Well drained"|"C"|"4"|96|"4"|96|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.055|"Severe"|"3"|0.601|"145196"
"45"|"Eaglewing gravelly silt loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.73|8.33|15.53|22.73|"Well drained"|"Well drained"|"C"||88|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145200"
"46"|"Eaglewing silt loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|5.29|9.59|16.96|24.11|"Well drained"|"Well drained"|"C"|"3"|86|"3"|86|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.057|"Moderate"|"3"|0.489|"145208"
"47"|"Esteslake-Slickspots complex, 0 to 4 percent slopes"||2|1.8||||"None"|"None"|"0"|2.4|4.24|7.83|11.42|"Well drained"|"Well drained"|"D"||88|"7"|55|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.329|"Slight"|"0"|1|"145215"
"48"|"Felan gravelly silt loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|5.47|7.89|12.55|17.18|"Well drained"|"Well drained"|"B"||100|"6"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145218"
"49"|"Felan gravelly silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.46|7.94|12.8|17.64|"Well drained"|"Well drained"|"B"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145222"
"5"|"Belton silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.48|7.84|14.76|21.87|"Well drained"|"Well drained"|"C"|"3"|92|"3"|99|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.233|"Slight"|"1"|0.93|"145223"
"50"|"Finleypoint cobbly loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.24|6.88|11.88|16.44|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.038|"Moderate"|"3"|0.245|"145224"
"51"|"Finleypoint cobbly loam, 8 to 15 percent slopes"||12|11.9||||"None"|"None"|"0"|4.22|6.76|11.56|16.09|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.055|"Moderate"|"0"|0.67|"145227"
"52"|"Finleypoint gravelly loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.2|6.78|11.38|15.91|"Well drained"|"Well drained"|"B"|"6"|90|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145243"
"53"|"Finleypoint gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.15|6.7|11.2|15.54|"Well drained"|"Well drained"|"B"||100|"7"|99|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145244"
"54"|"Finleypoint gravelly loam, dry, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.17|6.73|11.33|15.86|"Well drained"|"Well drained"|"B"|"6"|85|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145245"
"55"|"Finleypoint very gravelly loam, dry, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.09|6.61|11.12|15.47|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"145246"
"56"|"Finleypoint-Wildgen gravelly loams, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.27|6.84|11.41|15.87|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145248"
"57"|"Flott gravelly loam, 2 to 8 percent slopes"||5|5.3||||"None"|"None"|"0"|5.04|7.77|12.77|17.47|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.039|"Moderate"|"0"|0.067|"145249"
"58"|"Flott gravelly loam, 8 to 15 percent slopes"||12|11.8||||"None"|"None"|"0"|5.04|7.77|12.77|17.47|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.039|"Moderate"|"0"|0.628|"145250"
"59"|"Flott gravelly loam, 15 to 30 percent slopes"||23|23||||"None"|"None"|"0"|4.99|7.68|12.66|17.35|"Well drained"|"Well drained"|"B"|"6"|95|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"145251"
"6"|"Belton silt loam, 8 to 15 percent slopes"||12|11.9||||"None"|"None"|"0"|4.51|7.78|14.48|21.38|"Well drained"|"Well drained"|"C"|"4"|95|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.956|"Severe"|"0"|0.982|"145252"
"60"|"Flott gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.07|7.75|12.75|17.45|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145253"
"61"|"Flott very gravelly loam, dry, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.52|7.07|11.73|16.27|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145254"
"62"|"Gardencreek silty clay loam, 0 to 2 percent slopes"||1|1||153|153|"Rare"|"Rare"|"0"|4.41|8.8|17.11|25.35|"Moderately well drained"|"Moderately well drained"|"C"|"3"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.355|"Slight"|"5"|1|"145260"
"63"|"Gird silt loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.45|8.8|17.17|25.52|"Well drained"|"Well drained"|"B"|"2"|88|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.132|"Slight"|"0"|0.083|"145264"
"64"|"Gird silt loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.45|8.8|17.17|25.52|"Well drained"|"Well drained"|"B"|"2"|88|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.132|"Moderate"|"0"|0.083|"145269"
"65"|"Gird-Dryfork silt loams, moderately wet, 0 to 1 percent slopes"||1|1||107|107|"Rare"|"Rare"|"0"|4.49|8.86|17.36|25.86|"Moderately well drained"|"Moderately well drained"|"B"||100|"3"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.193|"Slight"|"5"|0.546|"145274"
"66"|"Gird-Vincom silt loams, 4 to 8 percent slopes"||6|6.2||||"None"|"None"|"0"|4.46|8.62|16.77|24.93|"Well drained"|"Well drained"|"B"|"3"|59|"3"|59|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.241|"Moderate"|"0"|0.41|"145275"
"67"|"Gird-Vincom silt loams, 8 to 15 percent slopes"||12|11.7||||"None"|"None"|"0"|4.46|8.59|16.7|24.8|"Well drained"|"Well drained"|"B"|"4"|97|"4"|54|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.545|"Severe"|"0"|0.774|"145278"
"68"|"Glaciercreek gravelly silt loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|6.08|8.21|9.77|11.3|"Excessively drained"|"Excessively drained"|"B"||95|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.007|"Moderate"|"0"|0.925|"145281"
"69"|"Half Moon silt loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|6.06|10.56|18.61|26.09|"Well drained"|"Well drained"|"C"|"6"|90|"6"|95|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Moderate"|"2"|0.484|"145284"
"7"|"Belton silt loam, 15 to 35 percent slopes"||25|23||||"None"|"None"|"0"|4.51|7.78|14.48|21.38|"Well drained"|"Well drained"|"C"||85|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.956|"Severe"|"0"|0.982|"145288"
"70"|"Half Moon-Courville complex, 4 to 15 percent slopes"||10|10.1||||"None"|"None"|"0"|5.61|9.58|16.23|22.42|"Well drained"|"Well drained"|"C"||85|"6"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.501|"Severe"|"2"|0.403|"145289"
"71"|"Hogsby-Finleypoint gravelly loams, 30 to 60 percent slopes"||45|45|33|||"None"|"None"|"0"|3.45|5.34|7.01|8.69|"Well drained"|"Well drained"|"D"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145295"
"72"|"Hogsby-Rock outcrop complex, 15 to 45 percent slopes"||30|29|46|||"None"|"None"|"0"|3.06|4.67|5.32|5.96|"Well drained"|"Well drained"|"D"||95|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.989|"Severe"|"0"|1|"145305"
"73"|"Holloway gravelly silt loam, 15 to 30 percent slopes"||23|23.6||||"None"|"None"|"0"|5.51|7.41|9.65|11.68|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|94|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.876|"Severe"|"0"|1|"145308"
"74"|"Holloway gravelly silt loam, 30 to 60 percent slopes"||45|45.4||||"None"|"None"|"0"|5.51|7.42|9.66|11.7|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145310"
"75"|"Holloway gravelly silt loam, cool, 15 to 30 percent slopes"||23|22.9||||"None"|"None"|"0"|5.58|7.26|9.44|11.31|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.903|"Severe"|"0"|1|"145316"
"76"|"Holloway gravelly silt loam, cool, 30 to 60 percent slopes"||45|45.4||||"None"|"None"|"0"|5.58|7.47|9.78|11.89|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145317"
"77"|"Holloway, dry-Rock outcrop complex, 15 to 30 percent slopes"||23|22.4||||"None"|"None"|"0"|5.29|6.99|8.3|9.62|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.815|"Severe"|"0"|1|"145322"
"78"|"Holloway-Rubble land complex, 45 to 75 percent slopes"||60|59.2||||"None"|"None"|"0"|5.28|7.13|9.15|11|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145323"
"79"|"Irvine silty clay, 8 to 15 percent slopes"||12|13.2||||"None"|"None"|"0"|3.8|5.84|9.86|13.88|"Well drained"|"Well drained"|"D"||93|"6"|92|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145325"
"8"|"Belton-Kerl silt loams, 2 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.65|8.36|15.89|23.52|"Well drained"|"Well drained"|"C"|"3"|55|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.189|"Moderate"|"0"|0.775|"145326"
"80"|"Irvine silty clay, 15 to 60 percent slopes"||38|36||||"None"|"None"|"0"|3.99|6.43|10.71|15|"Well drained"|"Well drained"|"D"||93|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|0.992|"145327"
"81"|"Jocko gravelly loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.72|6.43|8.1|9.23|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"|"4"|90|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.107|"Slight"|"0"|0.954|"145328"
"82"|"Jocko gravelly loam, 4 to 15 percent slopes"||10|9.9||||"None"|"None"|"0"|3.79|6.6|8.91|10.72|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"|"4"|100|"6"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.061|"Moderate"|"0"|0.945|"145329"
"83"|"Jocko very stony sandy loam, 0 to 8 percent slopes"||4|4||||"None"|"None"|"0"|2.5|4.69|6.52|8.34|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||87|"7"|85|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Not rated"|"Somewhat limited"|0.047|"Slight"|"0"|0.941|"145330"
"84"|"Kerl loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.9|9.23|17.89|26.56|"Well drained"|"Well drained"|"C"|"2"|92|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.118|"Moderate"|"0"|0.509|"145340"
"85"|"Kerl loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.9|9.23|17.89|26.56|"Well drained"|"Well drained"|"C"|"3"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.118|"Moderate"|"0"|0.509|"145343"
"86"|"Kerrdam silt loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.84|9.36|18.19|26.69|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.322|"Slight"|"0"|0.1|"145345"
"87"|"Kerrdam silt loam, 2 to 6 percent slopes"||4|3.8||||"None"|"None"|"0"|4.84|9.36|18.19|26.69|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.322|"Moderate"|"0"|0.1|"145349"
"88"|"Kerrdam-Vincom silt loams, 6 to 15 percent slopes"||11|10.9||||"None"|"None"|"0"|4.71|8.99|17.45|25.67|"Well drained"|"Well drained"|"B"|"4"|100|"4"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|0.589|"145350"
"89"|"Kerrdam-Vincom silt loams, 15 to 30 percent slopes"||23|21.7||||"None"|"None"|"0"|4.66|8.86|17.18|25.31|"Well drained"|"Well drained"|"B"|"6"|90|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"145358"
"9"|"Belton-Kerl silt loams, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.61|8.38|16.02|23.75|"Well drained"|"Well drained"|"C"|"3"|92|"3"|97|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.178|"Moderate"|"0"|0.733|"145364"
"90"|"Kingspoint gravelly loam, 4 to 15 percent slopes"||10|9.6||||"None"|"None"|"0"|5.75|9.3|14.68|19.88|"Well drained"|"Well drained"|"B"|"4"|91|"4"|91|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.036|"Moderate"|"2"|0.261|"145365"
"91"|"Kingspoint very gravelly loam, 15 to 30 percent slopes"||23|22.6||||"None"|"None"|"0"|5.16|7.74|12.85|17.94|"Well drained"|"Well drained"|"B"|"6"|88|"6"|96|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.889|"Severe"|"0"|1|"145368"
"92"|"Kingspoint very gravelly loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.24|7.7|12.51|17.32|"Well drained"|"Well drained"|"B"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"145371"
"93"|"Lamoose loam, 0 to 2 percent slopes"||1|1.1||15|15|"Occasional"|"Occasional"|"0"|4.39|8.29|9.79|11.27|"Poorly drained"|"Poorly drained"|"B/D"||95|"5"|85|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.948|"Slight"|"85"|1|"145372"
"94"|"Lonepine silt loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.56|9.06|17.96|26.86|"Well drained"|"Well drained"|"C"|"2"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Slight"|"0"|0.55|"145374"
"95"|"Lonepine silt loam, 2 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|4.55|8.93|17.49|26.07|"Well drained"|"Well drained"|"C"|"2"|85|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.315|"Moderate"|"0"|0.575|"145378"
"96"|"Lonepine silt loam, dry, 2 to 8 percent slopes"||5|4.7||||"None"|"None"|"0"|4.56|9.06|17.96|26.86|"Well drained"|"Well drained"|"C"|"3"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Moderate"|"0"|0.55|"145379"
"97"|"Lonepine-Vincom silt loams, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.39|8.49|16.58|24.68|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.306|"Moderate"|"0"|0.725|"145380"
"99"|"Marklepass silty clay loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|2.69|4.95|9.06|13.11|"Well drained"|"Well drained"|"D"|"7"|85|"7"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Slight"|"0"|1|"145382"
"M-W"|"Miscellaneous water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"145384"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"145385"
"193"|"Belton silt loam, 15 to 35 percent slopes, lake effect"||25|23||||"None"|"None"|"0"|4.51|7.78|14.48|21.38|"Well drained"|"Well drained"|"C"||85|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.955|"Severe"|"0"|0.982|"1715932"
"194"|"Bigarm cobbly loam, 15 to 30 percent slopes, lake effect"||23|23.4||||"None"|"None"|"0"|3.23|5.12|8.42|11.73|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.924|"Severe"|"0"|1|"1715933"
"195"|"Courville gravelly silt loam, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|4.7|7.83|12.66|17.2|"Well drained"|"Well drained"|"B"||93|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1715934"
"1044D"|"Eaglewing gravelly silt loam, 8 to 15 percent slopes, lake effect"||12|11.2||||"None"|"None"|"0"|4.74|8.5|15.88|23.03|"Well drained"|"Well drained"|"C"|"4"|96|"4"|96|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.034|"Severe"|"3"|0.61|"1715935"
"196"|"Eaglewing gravelly silt loam, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|4.73|8.33|15.53|22.73|"Well drained"|"Well drained"|"C"||88|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1715937"
"197"|"Finleypoint cobbly loam, 2 to 8 percent slopes, lake effect"||5|5.1||||"None"|"None"|"0"|4.24|6.88|11.88|16.44|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.044|"Moderate"|"3"|0.245|"1715938"
"198"|"Finleypoint cobbly loam, 8 to 15 percent slopes, lake effect"||12|11.9||||"None"|"None"|"0"|4.22|6.76|11.56|16.09|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.059|"Moderate"|"0"|0.67|"1715939"
"199"|"Finleypoint gravelly loam, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|4.2|6.78|11.38|15.91|"Well drained"|"Well drained"|"B"|"6"|90|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1715943"
"200"|"Finleypoint gravelly loam, dry, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|4.17|6.73|11.33|15.86|"Well drained"|"Well drained"|"B"|"6"|85|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1715944"
"201"|"Flott gravelly loam, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|4.99|7.68|12.66|17.35|"Well drained"|"Well drained"|"B"|"6"|95|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1715984"
"202"|"Half Moon-Courville complex, 4 to 15 percent slopes, lake effect"||10|10.1||||"None"|"None"|"0"|5.61|9.58|16.23|22.42|"Well drained"|"Well drained"|"C"||85|"6"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.505|"Severe"|"2"|0.403|"1715985"
"203"|"Kingspoint very gravelly loam, 15 to 30 percent slopes, lake effect"||23|22.6||||"None"|"None"|"0"|5.16|7.74|12.85|17.94|"Well drained"|"Well drained"|"B"|"6"|88|"6"|96|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.89|"Severe"|"0"|1|"1715989"
"204"|"Mitten gravelly silt loam, 8 to 30 percent slopes, lake effect"||19|20.8||||"None"|"None"|"0"|5.9|8.34|10.38|11.98|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.417|"Severe"|"0"|1|"1715990"
"205"|"Mollman gravelly loam, 15 to 30 percent slopes, lake effect"||23|24.1||||"None"|"None"|"0"|5.98|9.42|14.56|19.71|"Well drained"|"Well drained"|"B"|"6"|95|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.924|"Severe"|"0"|1|"1716000"
"206"|"Niarada gravelly loam, cool, 15 to 30 percent slopes, lake effect"||23|22.7||||"None"|"None"|"0"|3.29|5.49|9.16|12.81|"Well drained"|"Well drained"|"B"||95|"6"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.88|"Severe"|"0"|1|"1716001"
"207"|"Rumblecreek gravelly loam, 15 to 30 percent slopes, lake effect"||23|24.2||||"None"|"None"|"0"|5.79|8.97|13.31|17.24|"Well drained"|"Well drained"|"C"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.924|"Severe"|"0"|1|"1716002"
"208"|"Walstead-Rock outcrop complex, 15 to 30 percent slopes, lake effect"||23|23.6||||"None"|"None"|"0"|3.45|6.15|9.52|12.52|"Well drained"|"Well drained"|"B"|"6"|79|"6"|82|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.927|"Severe"|"0"|1|"1716003"
"209"|"Wildgen gravelly loam, 8 to 30 percent slopes, lake effect"||19|19.7||||"None"|"None"|"0"|4.48|7.13|11.86|16.58|"Well drained"|"Well drained"|"B"|"6"|90|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.413|"Severe"|"0"|1|"1716004"
"210"|"Wildgen-Finleypoint gravelly loams, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|4.44|7.1|11.93|16.73|"Well drained"|"Well drained"|"B"|"6"|50|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1716005"
"211"|"Winfall very gravelly loam, 15 to 30 percent slopes, lake effect"||23|23||||"None"|"None"|"0"|5.38|8.15|12.8|17.33|"Well drained"|"Well drained"|"B"|"6"|90|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.92|"Severe"|"0"|1|"1716006"
"212"|"Yellowbay very gravelly loam, 0 to 4 percent slopes, lake effect"||2|2||||"None"|"None"|"0"|2.94|4.09|6.1|8.1|"Excessively drained"|"Excessively drained"|"A"|"4"|100|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.003|"Slight"|"0"|1|"1716007"
"213"|"Yellowbay very gravelly loam, 15 to 30 percent slopes, lake effect"||23|22.4||||"None"|"None"|"0"|3.1|4.4|6.68|8.96|"Excessively drained"|"Excessively drained"|"A"|"6"|95|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.876|"Severe"|"0"|1|"1716008"
"22F"|"Winkler gravelly sandy loam, cool, 35 to 60 percent slopes"||48|47.8||||"None"|"None"|"0"|3.53|4.84|7.21|9.16|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409899"
"32E"|"Mitten gravelly ashy silt loam, 15 to 35 percent slopes"||25|26.2||||"None"|"None"|"0"|4.86|7.26|10.69|13.64|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"2409900"
"35D"|"Courville-Winfall complex, 4 to 15 percent slopes"||10|9.2||||"None"|"None"|"0"|4.19|6.92|11.88|16.78|"Well drained"|"Well drained"|"B"||100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.025|"Severe"|"5"|0.648|"2409901"
"35E"|"Courville-Pleasantvalley complex, 8 to 30 percent slopes"||19|19.4||||"None"|"None"|"0"|4.32|7.09|12.12|17.07|"Well drained"|"Well drained"|"B"||100|"6"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.402|"Severe"|"0"|1|"2409902"
"45D"|"Waldbillig gravelly ashy silt loam, 4 to 15 percent slopes"||10|10||||"None"|"None"|"0"|4.45|6.95|11.4|15.85|"Well drained"|"Well drained"|"B"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0|"Moderate"|"0"|0.247|"2409903"
"45E"|"Waldbillig gravelly ashy silt loam, 15 to 30 percent slopes"||22|22.9||||"None"|"None"|"0"|4.45|6.95|11.4|15.85|"Well drained"|"Well drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.829|"Severe"|"0"|1|"2409904"
"45F"|"Waldbillig gravelly ashy silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|4.46|7.04|11.46|15.86|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409905"
"47F"|"Holloway gravelly ashy silt loam, 30 to 60 percent slopes"||45|45||||"None"|"None"|"0"|5.07|6.76|9.36|11.97|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409906"
"56B"|"Bowlake-Minesinger gravelly loams, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.45|6.3|11.51|16.56|"Well drained"|"Well drained"|"C"|"3"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.173|"Moderate"|"0"|1|"2409908"
"57D"|"Minesinger gravelly loam, 4 to 15 percent slopes"||10|10.4||||"None"|"None"|"0"|3.5|6.56|11.14|15.21|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.185|"Moderate"|"0"|1|"2409909"
"71E"|"Kingspoint gravelly silt loam, 15 to 30 percent slopes"||23|22.5||||"None"|"None"|"0"|4.12|6.95|12.54|18.11|"Well drained"|"Well drained"|"B"||100|"6"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.856|"Severe"|"0"|1|"2409910"
"83F"|"Ashleylake-Rock outcrop complex, 30 to 50 percent slopes"||40|41.2||||"None"|"None"|"0"|4.81|8.09|13.71|19.27|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409911"
"712E"|"Kingspoint-Rock outcrop complex, 8 to 30 percent slopes"||20|19.8||||"None"|"None"|"0"|4.07|6.79|11.93|16.99|"Well drained"|"Well drained"|"B"||100|"6"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.502|"Severe"|"0"|1|"2409913"
"761F"|"Castner-Wimper-Rock outcrop complex, 15 to 50 percent slopes"||30|30|48|||"None"|"None"|"0"|3.81|6.91|10.1|13.13|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409914"
"835G"|"Ashleylake-Rock outcrop-Rockhill complex, 40 to 70 percent slopes"||50|52.9|48|||"None"|"None"|"0"|4.53|7.55|12.02|16.38|"Well drained"|"Well drained"|"B"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409915"
"931G"|"Repp-Kingspoint-Rock outcrop complex, 40 to 80 percent slopes"||55|53.3||||"None"|"None"|"0"|4.3|7.52|11.85|15.35|"Well drained"|"Well drained"|"B"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2409916"
"150E"|"Bigarm-Hogsby-Rock outcrop complex, 8 to 30 percent slopes"||19|20.7|43|||"None"|"None"|"0"|3.58|5.68|8.22|10.36|"Somewhat excessively drained"|"Well drained"|"B"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.365|"Severe"|"0"|1|"2409919"
"10UB"|"Kawuneeche family, stream bottoms"||2|2.2||15|15|"Frequent"|"Frequent"|"0"|4.58|8.52|13.5|14.5|"Very poorly drained"|"Very poorly drained"|"B/D"|"5"|80|"5"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.889|"Slight"|"80"|1|"2995303"
"32QA"|"McCay family, broadly convex ridges, weakly weathered metamorphic bedrock"||22|23.2|96|||"None"|"None"|"0"|5.86|7.74|9.88|9.98|"Well drained"|"Well drained"|"C"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2995304"
"33UA"|"McCay, cold-McCay families, complex, broadly convex ridges"||25|25|180|||"None"|"None"|"0"|3.18|4.62|6.12|7.62|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Moderate"|"0"|1|"2995305"
"38QA"|"McCay-Crabtree families, complex, undulating uplands"||22|14.8||70|70|"None"|"None"|"0"|5.51|7.57|11.37|14.26|"Well drained"|"Somewhat poorly drained"|"B"||60|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.592|"Severe"|"10"|0.983|"2995306"
