Metadata for Index of Aerial Photography Acquisition Dates, Montana 2011 NAIP Images

- Identification Information
- Spatial Reference Information
- Entity and Attribute Information
- Distribution Information
- Metadata Reference Information
- Download full XML Metadata

Identification Information:

Citation:
  Originator: Surdex Corporation
  Publication date: 02/08/2012
  Title:
    Index of Aerial Photography Acquisition Dates, Montana 2011 NAIP Images
  Publication place: Helena, MT
  Publisher: Montana State Library
  Online linkage: ftp://ftp.geoinfo.msl.mt.gov/Data/Spatial/MSDI/Imagery/2011_NAIP/24_km_tiles/00_NAIP_2011_Dates.zip
  Browse graphic file name: ftp://ftp.geoinfo.msl.mt.gov/Documents/Maps/Individual/20110301_688_NAIP_2011_dates.gif
  Browse graphic file description: Map showing aerial photography dates
Abstract:
  This data set contains polygons delineating the seam boundaries between images used in the creation of the 2011 National Agriculture Imagery Program (NAIP) images of Montana. These seam polygons can be used as a tool in determining the image source and date and time of each portion of the NAIP imagery. See http://apps.msl.mt.gov/Geographic_Information/Data/Aerial_Photos/naip_2011_default.aspx for access to the images.
Purpose:
  This index will aid NAIP image users in identifying and delineating source acquistion date boundaries for the NAIP images.
Time period of content:
  Calendar date: 2011
  Currentness reference: ground condition
Status:
  Progress: Complete
  Maintenance and update frequency:
    This is a static data set describing the 2011 NAIP imagery. For information on future updates of the NAIP, see the Aerial Photography Field Office web site.
Access constraints: None
Use constraints:
  The Montana State Library provides this product/service for informational purposes only. The Library did not produce it for, nor is it suitable for legal, engineering, or surveying purposes. Consumers of this information should review or consult the primary data and information sources to ascertain the viability of the information for their purposes. The Library provides these data in good faith but does not represent or warrant its accuracy, adequacy, or completeness. In no event shall the Library be liable for any incorrect results or analysis; any direct, indirect, special, or consequential damages to any party; or any lost profits arising out of or in connection with the use or the inability to use the data or the services provided. The Library makes these data and services available as a convenience to the public, and for no other purpose. The Library reserves the right to change or revise published data and/or services at any time.
Point of contact:
  Tim Bohn
  Surdex Corporation
  520 Spirit of Saint Louis Boulevard
  Chesterfield, MO 63005
  Telephone: 636-368-4400
  E-Mail: TimB@surdex.com

Back to Top

Spatial Reference Information:

Horizontal coordinate system definition:
  Grid coordinate system name: State Plane Coordinate System 1983
  SPCS zone identifier: 2500
  Lambert conformal conic:
  Standard parallel: 45.000000
  Standard parallel: 49.000000
  Longitude of central meridian: -109.500000
  Latitude of projection origin: 44.250000
  False easting: 600000.000000
  False northing: 0.000000
  Planar distance units: Meters
  Geodetic model:
    Horizontal datum name: North American Datum of 1983
    Ellipsoid name: Geodetic Reference System 80
    Semi-major axis: 6378137.000000
    Denominator of flattening ratio: 298.257222

Back to Top

Entity and Attribute Information:

Entity type label: naip_2011_dates
  Attribute label: FID
    Attribute definition: Internal feature number.
  Attribute label: Shape
    Attribute definition: Feature geometry.
  Attribute label: IDATE
    Attribute definition: Image Acquisition Date
  Attribute label: SDATE
    Attribute definition: Date and time of imagery aquisition
  Attribute label: BCON
    Attribute definition: Acquisition collection medium

    Attribute Value | Definition of Attribute Value
    NC | Natural Color
    CIR | Color Infra Red
    M4 | Multi Band Imagery
    MB4 | Multi Band Imagery, 4 Bands

  Attribute label: CAM_TYPE
    Attribute definition: Camera Type, Digital or Film
  Attribute label: CAM_MAN
    Attribute definition: Camera Manufacturer
  Attribute label: CAM_MOD
    Attribute definition: Camera Model
  Attribute label: SENSNUM
    Attribute definition: Sensor head or lens serial number
  Attribute label: AC_TYPE
    Attribute definition: Aircraft Type

    Attribute Value | Definition of Attribute Value
    C441 | Cessna 441 twin turboprop

  Attribute label: ACTAILNUM
    Attribute definition: Aircraft Tail Number

Back to Top

Distribution Information:

Distributor:
  Montana State Library
  PO Box 201800
  Helena, MT 59620-1800
  Telephone: 406-444-5354
  TDD/TTY telephone: 406-444-4799
  Fax: 406-444-0266
  E-Mail: geoinfo@mt.gov
Resource description: Downloadable Data
Distribution liability:
  The Montana State Library provides this product/service for informational purposes only. The Library did not produce it for, nor is it suitable for legal, engineering, or surveying purposes. Consumers of this information should review or consult the primary data and information sources to ascertain the viability of the information for their purposes. The Library provides these data in good faith but does not represent or warrant its accuracy, adequacy, or completeness. In no event shall the Library be liable for any incorrect results or analysis; any direct, indirect, special, or consequential damages to any party; or any lost profits arising out of or in connection with the use or the inability to use the data or the services provided. The Library makes these data and services available as a convenience to the public, and for no other purpose. The Library reserves the right to change or revise published data and/or services at any time.
Standard order process:
  Digital form:
    Format name: ESRI shapefile
    Online option:
    ftp://ftp.geoinfo.msl.mt.gov/Data/Spatial/MSDI/Imagery/2011_NAIP/24_km_tiles/00_NAIP_2011_Dates.zip

Back to Top

Metadata Reference Information:

Metadata date: 01/17/2014
Metadata review date: 02/07/2012
Metadata contact:
  Montana State Library
  PO Box 201800
  Helena, MT 59620-1800
  Telephone: 406-444-5354
  TDD/TTY telephone: 406-444-4799
  Fax: 406-444-0266
  E-Mail: geoinfo@mt.gov

Back to Top