"10B"|"Ryell, rarely flooded-Rivra, frequently flooded complex, 0 to 4 percent slopes"||2|2||84|84|"Rare"|"Frequent"|"0"|3.58|6.2|8.44|10.15|"Well drained"|"Well drained"|"C"|"3"|58|"3"|58|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.221|"Slight"|"2"|0.969|"148090"
"117B"|"Ashbough silt loam, 0 to 4 percent slopes"||2|2||130|130|"Very rare"|"Very rare"|"0"|4|8.33|17.15|24.54|"Moderately well drained"|"Moderately well drained"|"B"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.222|"Slight"|"0"|0.08|"148091"
"11B"|"Riverrun, frequently flooded-Beavrock, occasionally flooded complex, 0 to 4 percent slopes"||2|2||45|45|"Frequent"|"Frequent"|"0"|4.09|6.5|9.58|11.32|"Moderately well drained"|"Poorly drained"|"A"|"4"|47|"6"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.442|"Slight"|"44"|1|"148092"
"135D"|"Kalsted gravelly sandy loam, 4 to 15 percent slopes"||12|12||||"None"|"None"|"0"|2.97|5.88|11.64|16.9|"Well drained"|"Well drained"|"A"|"4"|86|"4"|86|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.095|"Moderate"|"0"|0.652|"148094"
"15B"|"Glendive sandy loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|3.53|7.2|14.16|22.1|"Well drained"|"Well drained"|"A"|"4"|98|"4"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.018|"Slight"|"1"|0.485|"148098"
"225B"|"Scravo cobbly loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.15|4.33|5.58|6.64|"Well drained"|"Well drained"|"B"|"6"|89|"6"|94|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.041|"Slight"|"0"|1|"148106"
"227B"|"Bronec cobbly loam, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|3.36|5.93|10.41|14.11|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.068|"Slight"|"0"|0.1|"148108"
"227C"|"Bronec-Kalsted gravelly sandy loams, 2 to 8 percent slopes, stony"||5|5||||"None"|"None"|"0"|2.93|5.78|10.98|15.37|"Well drained"|"Well drained"|"B"|"4"|89|"4"|89|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.033|"Moderate"|"0"|0.17|"148109"
"30B"|"Thess loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.34|8.52|13.62|15.35|"Well drained"|"Well drained"|"B"|"4"|96|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.114|"Slight"|"0"|0.96|"148123"
"32B"|"Yamacall loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|4.26|8.4|16.21|23.49|"Well drained"|"Well drained"|"B"|"4"|98|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.203|"Slight"|"0"|0.05|"148125"
"35B"|"Kalsted sandy loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|3.14|6.2|12.21|17.58|"Well drained"|"Well drained"|"A"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.034|"Slight"|"0"|0.414|"148128"
"35C"|"Kalsted sandy loam, 4 to 8 percent slopes"||6|6.2||||"None"|"None"|"0"|3.13|6.19|12.19|17.62|"Well drained"|"Well drained"|"A"|"4"|95|"4"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.036|"Moderate"|"0"|0.419|"148129"
"36B"|"Amesha loam, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|3.97|7.84|15.46|22.56|"Well drained"|"Well drained"|"B"|"4"|97|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.104|"Slight"|"0"|0.063|"148133"
"36C"|"Amesha loam, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|3.99|7.85|15.54|22.81|"Well drained"|"Well drained"|"B"|"4"|95|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.158|"Moderate"|"0"|0.057|"148134"
"37B"|"Brockway silt loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.71|9.06|17.16|25.17|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.317|"Slight"|"0"|0.451|"148136"
"586B"|"Rominell loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.84|7.47|15.14|21.25|"Well drained"|"Well drained"|"C"|"6"|90|"6"|98|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.245|"Slight"|"0"|0.94|"148144"
"142B"|"Beavrock, occasionally flooded-Threeriv, frequently flooded complex, 0 to 4 percent slopes"||2|1.7||15|15|"Occasional"|"Frequent"|"0"|5.84|9.71|14.11|16.39|"Poorly drained"|"Very poorly drained"|"B/D"|"4"|59|"4"|59|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.619|"Slight"|"83"|0.969|"148156"
"27E"|"Bronec very cobbly loam, 8 to 35 percent slopes"||22|21.3||||"None"|"None"|"0"|3.34|6.07|10.97|15.07|"Well drained"|"Well drained"|"B"||96|"6"|96|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.791|"Moderate"|"0"|0.969|"148160"
"627C"|"Bronec-Kalsted gravelly sandy loams, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3|5.93|11.4|16.13|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.036|"Moderate"|"0"|0.156|"148161"
"127C"|"Bronec gravelly sandy loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|2.88|5.61|10.46|14.47|"Well drained"|"Well drained"|"B"|"4"|98|"4"|98|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.034|"Moderate"|"0"|0.074|"148162"
"127A"|"Bronec gravelly sandy loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|2.93|5.69|10.55|14.51|"Well drained"|"Well drained"|"B"|"4"|98|"4"|98|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.036|"Slight"|"0"|0.072|"148163"
"136C"|"Amesha-Kalsted complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.61|7.15|14.01|20.28|"Well drained"|"Well drained"|"B"|"4"|91|"4"|91|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.102|"Moderate"|"0"|0.22|"148164"
"77C"|"Sappington loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.99|7.43|13.89|20.53|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.181|"Moderate"|"1"|0.039|"148166"
"85C"|"Trudau loam, 2 to 8 percent slopes"||5|5.3||||"None"|"None"|"0"|3.21|5.87|10.87|15.64|"Well drained"|"Well drained"|"C"|"4"|100|"6"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.124|"Moderate"|"0"|0.448|"148167"
"49E"|"Geohrock very cobbly loam, very stony, 15 to 35 percent slopes"||25|25.1||||"None"|"None"|"0"|1.54|2.94|6.43|10.07|"Well drained"|"Well drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.984|"Moderate"|"0"|0.983|"148168"
"83A"|"Dillon silt loam, 0 to 2 percent slopes, rarely flooded"||1|1||84|84|"Rare"|"Rare"|"0"|4.43|8.27|14.03|16.32|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|98|"4"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.283|"Slight"|"4"|0.98|"148169"
"84A"|"Madbeaver silt loam, 0 to 2 percent slopes"||1|1||107|107|"None"|"None"|"0"|4.4|8.41|16.13|20.3|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"|"4"|98|"4"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.296|"Slight"|"2"|0.95|"148170"
"130B"|"Thess-Scravo complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.82|6.78|10.41|12.02|"Well drained"|"Well drained"|"B"|"4"|60|"4"|53|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.124|"Slight"|"0"|0.92|"148172"
"133C"|"Varney-Sappington complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.68|6.96|13.28|19.96|"Well drained"|"Well drained"|"B"|"3"|91|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.17|"Moderate"|"0"|0.025|"148173"
"177C"|"Sappington-Kalsted complex, 2 to 8 percent slopes"||5|5.3||||"None"|"None"|"0"|3.43|6.71|13.01|19.15|"Well drained"|"Well drained"|"B"|"3"|50|"3"|50|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.112|"Moderate"|"0"|0.223|"148174"
"291E"|"Haxby-Blackleaf-Zbart complex, 4 to 25 percent slopes"||15|17.4|16|||"None"|"None"|"0"|2.69|4.25|4.64|4.64|"Well drained"|"Well drained"|"D"||100|"7"|61|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.17|"Moderate"|"0"|1|"148177"
"327E"|"Bronec-Spudbar-Rencot complex, 8 to 35 percent slopes"||22|22.7|38|||"None"|"None"|"0"|2.94|5.27|8.09|10.37|"Well drained"|"Well drained"|"B"||100|"6"|76|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.814|"Severe"|"0"|0.98|"148178"
"372E"|"Rencot-Spudbar-Rock outcrop complex, 8 to 25 percent slopes"||17|17.8|38|||"None"|"None"|"0"|2.47|4.16|4.93|5.51|"Well drained"|"Well drained"|"D"||100|"7"|43|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.213|"Moderate"|"0"|0.943|"148179"
"533D"|"Varney-Kalsted, stony-Cabbart, stony complex, 4 to 15 percent slopes"||10|10.2|41|||"None"|"None"|"0"|3.65|6.85|11.89|16.73|"Well drained"|"Well drained"|"B"|"4"|62|"4"|62|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.201|"Moderate"|"0"|0.436|"148180"
"627D"|"Bronec-Kalsted complex, 4 to 15 percent slopes"||10|10.3||||"None"|"None"|"0"|2.79|5.71|11.15|15.86|"Well drained"|"Well drained"|"B"||100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.136|"Moderate"|"0"|0.279|"148181"
"182B"|"Dillon-Ashbough-Beavrock silt loams, 0 to 4 percent slopes, rarely flooded"||2|2||61|61|"Rare"|"Rare"|"0"|3.89|7.84|13.97|17.81|"Somewhat poorly drained"|"Poorly drained"|"C"|"4"|75|"4"|73|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.246|"Slight"|"24"|0.682|"148182"
"336D"|"Amesha-Bronec-Sappington complex, 4 to 15 percent slopes"||10|10.7||||"None"|"None"|"0"|3.55|6.73|12.91|18.68|"Well drained"|"Well drained"|"B"||85|"4"|45|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.415|"Moderate"|"0"|0.406|"148185"
"433D"|"Varney-Udecide-Geohrock complex, 4 to 15 percent slopes"||10|10.5|74|||"None"|"None"|"0"|3.63|6.58|10.97|14.66|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.181|"Moderate"|"0"|0.442|"148186"
"335E"|"Kalsted-Scravo, stony-Cabbart complex, 15 to 45 percent slopes"||30|28.5|41|||"None"|"None"|"0"|2.92|5.13|8.29|11.2|"Well drained"|"Well drained"|"A"||97|"7"|82|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.946|"Severe"|"0"|0.971|"148189"
"289E"|"Geohrock-Bronec-Geohrock, stony complex, 8 to 45 percent slopes"||27|25.7||||"None"|"None"|"0"|2.05|3.89|7.79|11.49|"Well drained"|"Well drained"|"B"||100|"6"|91|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.935|"Severe"|"0"|0.939|"148190"
"111B"|"Rivra complex, 0 to 4 percent slopes, occassionally flooded"||2|2||137|137|"Occasional"|"Occasional"|"0"|2.03|3.26|5.36|7.2|"Well drained"|"Well drained"|"B"|"7"|85|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.127|"Slight"|"1"|0.95|"148201"
"242B"|"Beavrock-Dillon silt loams, 0 to 4 percent slopes, rarely flooded"||2|2||61|61|"Rare"|"Rare"|"0"|5.53|9.39|14.3|16.43|"Poorly drained"|"Poorly drained"|"C"||63|"5"|61|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.267|"Slight"|"61"|0.98|"148202"
"183B"|"Dillon-Riverrun-Beavrock complex, 0 to 4 percent slopes, rarely flooded"||2|2||45|45|"Rare"|"Rare"|"0"|4.01|7.04|11.32|13.2|"Somewhat poorly drained"|"Poorly drained"|"C"|"4"|69|"4"|69|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.239|"Slight"|"18"|1|"148203"
"181B"|"Nippt-Scravo-Nippt complex, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|3.09|4.73|6.13|7.43|"Well drained"|"Well drained"|"B"|"6"|49|"6"|87|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.049|"Slight"|"0"|0.92|"148204"
"180B"|"Thessvo-Scravo complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.56|5.42|7.01|8.32|"Well drained"|"Well drained"|"B"|"4"|63|"6"|93|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.088|"Slight"|"0"|1|"148205"
"927E"|"Bronec-Trimad-Kalsted complex, 15 to 45 percent slopes"||30|28.7||||"None"|"None"|"0"|2.82|5.34|9.81|13.73|"Well drained"|"Well drained"|"B"||100|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.943|"Severe"|"0"|0.989|"148207"
"436D"|"Amesha-Haxby-Rencot complex, 4 to 15 percent slopes"||10|10.2|38|||"None"|"None"|"0"|3.82|7.25|12.01|16.28|"Well drained"|"Well drained"|"B"||100|"4"|55|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Very limited"|0.583|"Severe"|"0"|0.542|"148208"
"278D"|"Sappington-Geohrock-Delpoint, stony complex, 4 to 25 percent slopes"||6|11.7|69|||"None"|"None"|"0"|3.47|6.33|10.6|14.24|"Well drained"|"Well drained"|"B"|"3"|35|"3"|35|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.27|"Moderate"|"0"|0.532|"148219"
"189E"|"Geohrock, bouldery-Sappington, stony-Bronec, bouldery complex, 8 to 35 percent slopes"||22|20.1||||"None"|"None"|"0"|2.61|4.73|9.08|13.39|"Well drained"|"Well drained"|"B"||100|"6"|92|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.612|"Moderate"|"0"|0.98|"148225"
"233C"|"Varney-Sappington-Kalsted complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.58|6.83|13.11|19.61|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.149|"Moderate"|"0"|0.09|"148227"
"194D"|"Musselshell-Roto-Pensore complex, 4 to 15 percent slopes"||10|10|36|||"None"|"None"|"0"|3.3|6.12|10.81|12.84|"Well drained"|"Well drained"|"B"|"4"|82|"4"|52|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.145|"Severe"|"0"|0.611|"148230"
"190E"|"Blackleaf, stony-Twinadams-Rock outcrop complex, 8 to 35 percent slopes"||22|23.7|33|||"None"|"None"|"0"|2.36|3.28|3.68|3.68|"Well drained"|"Well drained"|"D"||100|"7"|76|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.845|"Severe"|"0"|1|"148231"
"191D"|"Haxby-Kalsted-Zbart complex, 4 to 15 percent slopes"||10|10.2|16|||"None"|"None"|"0"|3.33|6.13|8.67|10.64|"Well drained"|"Well drained"|"C"||100|"6"|47|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.149|"Severe"|"0"|0.796|"148232"
"277C"|"Sappington-Kalsted-Kalsted, stony complex, 2 to 8 percent slopes"||5|4.8||||"None"|"None"|"0"|3.42|6.66|12.94|19.05|"Well drained"|"Well drained"|"B"|"4"|51|"4"|51|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.094|"Moderate"|"0"|0.232|"148233"
"130A"|"Thess-Ashbough complex, 0 to 2 percent slopes"||1|1.1||130|130|"None"|"None"|"0"|4.21|8.49|15.27|19.49|"Well drained"|"Moderately well drained"|"B"|"4"|99|"4"|98|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.156|"Slight"|"0"|0.55|"148237"
"272F"|"Rencot, stony-Spudbar-Rock outcrop complex, 25 to 50 percent slopes"||38|35.2|38|||"None"|"None"|"0"|2.31|3.75|3.87|3.87|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.889|"Severe"|"0"|1|"148242"
"9100F"|"Blackleaf, stony-Twinadams, very stony-Rock outcrop complex, 20 to 60 percent slopes"||40|39.4|33|||"None"|"None"|"0"|2.24|3.23|3.71|3.71|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"148249"
"9101E"|"Twinadams-Thunderhead-Blackleaf, stony complex, 8 to 25 percent slopes"||17|15|33|||"None"|"None"|"0"|2.84|4.97|6.45|6.84|"Well drained"|"Well drained"|"C"||100|"6"|41|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.156|"Severe"|"0"|0.897|"148250"
"9103D"|"Faith, rarely flooded-Geohrock, stony-Beavrock, occasionally flooded complex, 2 to 15 percent slopes"||5|7||61|61|"Rare"|"Occasional"|"0"|3.44|6.77|12.67|17.27|"Well drained"|"Poorly drained"|"B"|"3"|35|"3"|35|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.267|"Moderate"|"22"|0.622|"148251"
"198E"|"Cabbart, very stony-Rentsac, bouldery-Rock outcrop complex, 15 to 45 percent slopes"||30|28|41|||"None"|"None"|"0"|3.36|5.77|5.84|5.84|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.944|"Severe"|"0"|1|"148252"
"DA"|"Denied access"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"148257"
"GP"|"Gravel pits"|||||||||"0"|||||||||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"148258"
"M-W"|"Miscellaneous water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"148259"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"148260"
"535D"|"Kalsted-Blacksheep-Rock outcrop complex, 4 to 15 percent slopes"||10|10.1|41|||"None"|"None"|"0"|3.31|6.01|8.96|11.53|"Well drained"|"Well drained"|"D"||55|"4"|45|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.465|"Severe"|"0"|0.73|"148263"
"112B"|"Neen-Ashbough, saline-Beavrock complex, 0 to 4 percent slopes, rarely flooded"||3|2.1||61|61|"Rare"|"Rare"|"0"|3.44|7.21|13.84|19.22|"Somewhat poorly drained"|"Poorly drained"|"C"|"6"|65|"6"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.268|"Slight"|"25"|0.747|"148264"
"9105F"|"Ratiopeak, bouldery-Poin complex, 15 to 45 percent slopes"||30|28.3|46|||"None"|"None"|"0"|2.88|4.96|8.21|11.13|"Well drained"|"Well drained"|"C"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.895|"Severe"|"0"|0.954|"148265"
"333E"|"Varney-Delpoint, stony-Geohrock complex, 4 to 35 percent slopes"||10|19.2|69|||"None"|"None"|"0"|3.41|6.31|10.57|14.18|"Well drained"|"Well drained"|"B"||97|"6"|56|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.677|"Severe"|"0"|0.687|"148266"
"9102F"|"Nathale, very bouldery-Poin, very stony-Rock outcrop complex, 20 to 60 percent slopes"||40|38.9|46|||"None"|"None"|"0"|2.69|4.53|6.85|7.07|"Well drained"|"Well drained"|"C"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.963|"Severe"|"0"|0.991|"148268"
"187C"|"Chinook-Glendive sandy loams, 0 to 8 percent slopes"||5|4.2||||"None"|"None"|"0"|3.43|6.66|12.87|17.82|"Well drained"|"Well drained"|"A"|"4"|93|"4"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.035|"Moderate"|"0"|0.791|"148274"
"193A"|"Attewan-Nippt complex, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.04|7.15|9.61|11.44|"Well drained"|"Well drained"|"B"|"3"|65|"3"|65|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.172|"Slight"|"0"|0.94|"148275"
"195B"|"Dillon, saline-Dillon-Riverrun, saline complex, 0 to 4 percent slopes, rarely flooded"||2|2||84|84|"Rare"|"Rare"|"0"|3.79|7|11.87|14.2|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"6"|66|"6"|68|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.2|"Slight"|"4"|0.96|"148276"
"270E"|"Pensore-Crago-Rock outcrop complex, 8 to 45 percent slopes"||27|20.2|36|||"None"|"None"|"0"|2.5|3.77|4.97|5.94|"Well drained"|"Well drained"|"D"||90|"7"|50|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.695|"Severe"|"0"|0.938|"148278"
"148E"|"Rentsac, extremely bouldery-Rock outcrop complex, 15 to 45 percent slopes"||30|30|46|||"None"|"None"|"0"|2.57|4.41|4.41|4.41|"Well drained"|"Well drained"|"D"||100|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"148280"
"217B"|"Havre-Glendive complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.66|7.47|14.69|22.01|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.088|"Slight"|"7"|0.301|"148281"
"241F"|"Whitlash, very stony-Rock outcrop-Perma, very stony complex, 25 to 60 percent slopes"||43|41.6|28|||"None"|"None"|"0"|2.46|3.32|4.38|4.9|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.988|"Severe"|"0"|1|"148314"
"541D"|"Whitlash, very stony-Brickner, stony-Rock outcrop complex, 4 to 25 percent slopes"||15|16.1|28|||"None"|"None"|"0"|2.33|2.88|3.31|3.48|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.335|"Moderate"|"0"|1|"148328"
"998E"|"Libeg-Nieman, stony complex, 8 to 25 percent slopes"||17|16.8|38|||"None"|"None"|"0"|3.51|5.51|7.36|8.67|"Well drained"|"Well drained"|"B"||100|"6"|62|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.086|"Severe"|"0"|1|"148335"
"1003E"|"Tiban, bouldery-Cheadle, very bouldery complex, 15 to 35 percent slopes"||25|23.8|48|||"None"|"None"|"0"|2.72|4.86|7.75|10.42|"Well drained"|"Well drained"|"B"||100|"6"|63|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.882|"Severe"|"0"|0.97|"148339"
"1690F"|"Cheadle, very stony-Rock outcrop-Tiban, bouldery complex, 15 to 45 percent slopes"||30|27.9|48|||"None"|"None"|"0"|2.74|4.81|6.98|8.86|"Well drained"|"Well drained"|"D"||95|"7"|46|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.88|"Severe"|"0"|0.94|"148344"
"2125F"|"Rubble land-Elve, very stony-Rock outcrop complex, 25 to 60 percent slopes"|||43|||||"None"|"0"|1.5|2.31|3.81|5.31||"Somewhat excessively drained"|||100|"8"|75|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"148349"
"2213E"|"Sebud, stony-Surdal, stony-Poin, very stony complex, 8 to 35 percent slopes"||22|21.7|46|||"None"|"None"|"0"|2.74|5.04|8.42|10.69|"Well drained"|"Well drained"|"B"||100|"6"|81|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.774|"Severe"|"0"|0.972|"148354"
"2712D"|"Libeg-Mooseflat, frequently flooded complex, 4 to 25 percent slopes"||15|14.5||15|15|"None"|"Frequent"|"0"|3.82|7|9.76|11.89|"Well drained"|"Very poorly drained"|"B"||100|"6"|74|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.356|"Severe"|"25"|0.987|"148366"
"331C"|"Geohrock-Bronec gravelly loams, 2 to 8 percent slopes"||5|5.5||||"None"|"None"|"0"|2.84|4.92|9.17|13.11|"Well drained"|"Well drained"|"B"|"4"|93|"4"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.121|"Moderate"|"0"|0.351|"148379"
"537P"|"Elve-Gambler-Libeg families, complex, moderately steep mountain slopes"||33|33||||"None"|"None"|"0"|4.12|6.84|10.84|14.52|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"148384"
"999E"|"Ermont-Ratiopeak-Rock outcrop complex, 4 to 35 percent slopes"||20|20.9|48|||"None"|"None"|"0"|2.89|4.94|5.67|6.37|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.588|"Severe"|"0"|1|"599780"
"1E"|"Kounter-Rock outcrop complex, 15 to 45 percent slopes"||30|29|41|||"None"|"None"|"0"|1.78|2.2|2.39|2.47|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||99|"7"|57|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.931|"Severe"|"0"|0.995|"608777"
"2D"|"Kounter-Rock outcrop complex, 4 to 15 percent slopes"||10|11.8|41|||"None"|"None"|"0"|1.84|2.2|2.26|2.26|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.128|"Moderate"|"0"|1|"608778"
"4E"|"Libeg, very stony-Oro Fino-Poin, stony complex, 15 to 60 percent slopes"||43|38.1|46|||"None"|"None"|"0"|3.32|5.88|9.1|10.98|"Well drained"|"Well drained"|"B"||100|"7"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.989|"Severe"|"0"|0.997|"608779"
"5E"|"Barbarela-Poin, stony complex, 15 to 35 percent slopes"||25|24.2|46|||"None"|"None"|"0"|3.18|5.88|9.39|9.43|"Well drained"|"Well drained"|"C"||99|"6"|66|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.9|"Severe"|"1"|1|"608780"
"6E"|"Cheadle family, very stony-Rock outcrop complex, 25 to 60 percent slopes"||43|39.4|48|||"None"|"None"|"0"|2.68|4.39|4.99|5.27|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.992|"Severe"|"0"|1|"608781"
"7B"|"Trudau loam, cool, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.25|5.92|10.78|15.3|"Well drained"|"Well drained"|"C"|"4"|100|"6"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.127|"Moderate"|"0"|0.498|"608782"
"8A"|"Beavrock, occasionally flooded-Ashbough, rarely flooded complex, 0 to 2 percent slopes"||1|1.3||61|61|"Occasional"|"Occasional"|"0"|5.08|9.09|15.09|18.75|"Poorly drained"|"Poorly drained"|"C"|"4"|76|"4"|76|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.26|"Slight"|"50"|0.747|"609109"
"9B"|"Threeriv, frequently flooded-Beavrock, occasionally flooded complex, 0 to 2 percent slopes"||1|1||15|15|"Frequent"|"Frequent"|"0"|5.47|9.13|12.66|14.16|"Very poorly drained"|"Very poorly drained"|"B/D"|"5"|52|"5"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.632|"Slight"|"77"|0.967|"609111"
"10D"|"Crago, stony-Crago complex, 4 to 10 percent slopes"||7|8||||"None"|"None"|"0"|2.37|3.58|5.95|8.27|"Well drained"|"Well drained"|"B"|"4"|91|"6"|86|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.28|"Moderate"|"1"|0.95|"609112"
"11D"|"Barbarela-Foolhen, occasionally flooded complex, 2 to 15 percent slopes"||9|8.1|86|15|15|"None"|"Occasional"|"0"|4.03|7.7|13.39|16.15|"Well drained"|"Very poorly drained"|"C"||69|"6"|97|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.287|"Severe"|"31"|0.951|"609113"
"12C"|"Attewan cobbly loam, cool, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|3.37|6.52|8.43|10.23|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.152|"Moderate"|"0"|0.91|"609114"
"14E"|"Farlin, very bouldery-Farlin, stony complex, 8 to 25 percent slopes"||17|15.1||||"None"|"None"|"0"|3.97|6.47|10.2|13.23|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.28|"Moderate"|"0"|0.835|"609115"
"17A"|"Beavwan-Sieberell complex, 1 to 4 percent slopes"||3|3.4||||"None"|"None"|"0"|3.31|6.01|7.47|8.64|"Well drained"|"Well drained"|"B"|"4"|88|"4"|63|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.129|"Slight"|"0"|1|"609117"
"18E"|"Libeg, stony-Poin, very stony-Rock outcrop complex, 25 to 60 percent slopes"||43|40.1|46|||"None"|"None"|"0"|3.49|5.92|9.1|11.28|"Well drained"|"Well drained"|"B"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.948|"Severe"|"0"|0.996|"609118"
"21B"|"Thess loam, cool, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.43|8.78|14.18|16.05|"Well drained"|"Well drained"|"B"|"4"|98|"4"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.095|"Slight"|"0"|0.955|"609120"
"22E"|"Tiban, very stony-Maciver complex, 15 to 60 percent slopes"||38|37.1||||"None"|"None"|"0"|3.19|5.73|10.33|14.88|"Well drained"|"Well drained"|"B"||100|"7"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"2"|1|"609121"
"23B"|"Newtman-Dougcliff complex, 0 to 4 percent slopes"||1|1.3||8|8|"None"|"None"|"0"|9.24|15.58|27.4|37.3|"Very poorly drained"|"Very poorly drained"|"C/D"||90|"5"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.863|"Slight"|"90"|1|"609122"
"24C"|"Kalsted-Sappington complex, 2 to 8 percent slopes"||5|5.9||||"None"|"None"|"0"|3.37|6.54|12.4|17.81|"Well drained"|"Well drained"|"A"|"4"|86|"4"|86|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.072|"Moderate"|"0"|0.41|"609123"
"25E"|"Scravo, stony-Kalsted-Cabbart complex, 15 to 45 percent slopes"||30|30|41|||"None"|"None"|"0"|2.65|4.47|7.02|9.27|"Well drained"|"Well drained"|"A"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"609124"
"27D"|"Barbarela-Nieman-Oro Fino complex, 2 to 15 percent slopes"||9|10.1|38|||"None"|"None"|"0"|3.28|5.81|9.22|9.88|"Well drained"|"Well drained"|"C"||100|"6"|64|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.1|"Severe"|"0"|0.636|"609125"
"19D"|"Blaine stony loam, 2 to 15 percent slopes"||9|9.5|64|||"None"|"None"|"0"|3.44|5.53|7.52|8.34|"Well drained"|"Well drained"|"C"||95|"6"|98|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.024|"Moderate"|"0"|0.954|"609126"
"23C"|"Bridger clay loam, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|4.75|8.75|14.56|20.14|"Well drained"|"Well drained"|"C"|"6"|100|"6"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.052|"Moderate"|"0"|0.9|"609127"
"29F"|"Brocko-Crago complex, cool, 8 to 45 percent slopes"||27|26.6||||"None"|"None"|"0"|3.99|7.39|13.72|20.03|"Well drained"|"Well drained"|"B"||98|"7"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.989|"Severe"|"2"|1|"609128"
"28C"|"Beavwan gravelly sandy loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.57|7.3|9.41|11.03|"Well drained"|"Well drained"|"C"|"4"|87|"4"|87|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.093|"Moderate"|"0"|0.893|"609129"
"29E"|"Poin, stony-Barbarela-Rock outcrop complex, 8 to 25 percent slopes"||17|16.6|46|||"None"|"None"|"0"|3.13|5.18|7.27|7.45|"Well drained"|"Well drained"|"D"||100|"7"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.106|"Severe"|"0"|0.989|"609130"
"30E"|"Nieman, very stony-Rock outcrop complex, 8 to 60 percent slopes"||34|28.2|38|||"None"|"None"|"0"|2.7|4.14|5.68|6.21|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.728|"Severe"|"0"|0.949|"609131"
"31A"|"Ashbough silt loam, 0 to 2 percent slopes, rarely flooded"||1|1.2||130|130|"Rare"|"Rare"|"0"|4.01|8.34|17.17|24.69|"Moderately well drained"|"Moderately well drained"|"B"|"4"|99|"4"|98|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.19|"Slight"|"1"|0.045|"609132"
"32E"|"Fourmile-Fourmile, extremely bouldery complex, 8 to 25 percent slopes"||12|14.5||||"None"|"None"|"0"|3.88|7.08|10.6|11.91|"Well drained"|"Well drained"|"B"||100|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.272|"Moderate"|"2"|0.933|"609133"
"33E"|"Shadow complex, 15 to 70 percent slopes"||40|38.6||||"None"|"None"|"0"|3.53|5.73|8.65|10.82|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||100|"7"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.978|"Severe"|"0"|0.993|"609134"
"34C"|"Nippt-Scravo gravelly loams, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.25|4.9|6.43|7.57|"Well drained"|"Well drained"|"B"|"6"|86|"6"|89|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.044|"Slight"|"0"|0.99|"609135"
"36E"|"Kounter-Amesha-Rock outcrop complex, 8 to 35 percent slopes"||22|16.7|41|||"None"|"None"|"0"|2.75|4.59|7.94|11.17|"Somewhat excessively drained"|"Well drained"|"D"||90|"7"|44|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.742|"Severe"|"0"|0.76|"609136"
"37C"|"Tiban-Maciver gravelly loams, 2 to 8 percent slopes"||5|5.8||||"None"|"None"|"0"|3.29|6.07|10.17|14.22|"Well drained"|"Well drained"|"B"|"6"|90|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.003|"Moderate"|"0"|0.359|"609137"
"37E"|"Crago-Scravo complex, 15 to 45 percent slopes"||30|30||||"None"|"None"|"0"|2.06|3.71|6.01|7.86|"Well drained"|"Well drained"|"B"||100|"7"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.972|"Severe"|"0"|1|"609138"
"39C"|"Trimad gravelly loam, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.4|5.86|9.25|12|"Well drained"|"Well drained"|"B"|"4"|94|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.158|"Moderate"|"0"|0.458|"609140"
"40E"|"Philipsburg-Tiban-Houlihan complex, 15 to 45 percent slopes"||30|30.6||||"None"|"None"|"0"|4.05|7.81|13.85|19.56|"Well drained"|"Well drained"|"B"||99|"7"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.97|"Severe"|"1"|1|"609141"
"41E"|"Bronec, Amesha, and Riverrun, occasionally flooded soils, 0 to 35 percent slopes"||18|15.4||130|130|"None"|"Occasional"|"0"|2.95|5.68|10.84|15.55|"Well drained"|"Moderately well drained"|"B"||78|"6"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.206|"Severe"|"2"|0.979|"609142"
"42E"|"Spudbar, extremely bouldery-Rubble land-Rock outcrop complex, 15 to 45 percent slopes"||30|27.9|56|||"None"|"None"|"0"|2.35|4.34|4.73|4.85|"Well drained"|"Well drained"|"C"||95|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.923|"Severe"|"0"|1|"609143"
"44E"|"Tiban-Philipsburg-Shineberger complex, 15 to 45 percent slopes"||30|29.4||||"None"|"None"|"0"|3.43|6.41|10.37|14.15|"Well drained"|"Well drained"|"B"||100|"7"|71|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.968|"Severe"|"0"|0.988|"609144"
"45E"|"Maciver gravelly loam, 1 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|3.19|5.58|9.84|14.11|"Well drained"|"Well drained"|"B"||100|"6"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.026|"Slight"|"2"|0.175|"609145"
"47D"|"Spudbar complex, 2 to 15 percent slopes"||9|9.2|56|||"None"|"None"|"0"|2.88|4.95|5.46|5.63|"Well drained"|"Well drained"|"C"|"6"|53|"6"|73|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.459|"Moderate"|"0"|0.96|"609146"
"53E"|"Hanson-Rock outcrop complex, 25 to 45 percent slopes"||35|31.6||||"None"|"None"|"0"|3.63|5.88|9.99|13.95|"Well drained"|"Well drained"|"B"||93|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.902|"Severe"|"0"|0.916|"609148"
"58A"|"Havre loam, cool, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.37|7.92|14.72|21.52|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.089|"Slight"|"0"|0.073|"609149"
"60C"|"Kalsted loamy sand, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|2.17|4.96|10.2|14.55|"Well drained"|"Well drained"|"A"|"6"|90|"6"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.722|"Moderate"|"0"|0.455|"609150"
"61A"|"Kalsted sandy loam, 0 to 2 percent slopes"||1|1.3||||"None"|"None"|"0"|2.93|5.77|10.71|14.91|"Well drained"|"Well drained"|"A"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.038|"Slight"|"0"|0.505|"609151"
"62C"|"Kalsted sandy loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3|5.88|10.62|14.81|"Well drained"|"Well drained"|"A"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.028|"Moderate"|"0"|1|"609152"
"63D"|"Kalsted sandy loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|2.97|5.8|10.72|14.92|"Well drained"|"Well drained"|"A"|"4"|95|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.029|"Moderate"|"0"|0.67|"609153"
"64E"|"Kalsted gravelly sandy loam, 15 to 35 percent slopes"||25|24.4||||"None"|"None"|"0"|2.57|5.08|10.08|15.03|"Well drained"|"Well drained"|"A"||97|"6"|97|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.982|"Severe"|"0"|1|"609154"
"89D"|"Nuley sandy loam, 2 to 12 percent slopes"||7|6.8|107|||"None"|"None"|"0"|3.54|6.68|9.22|9.4|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Not limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.034|"Moderate"|"0"|0.963|"609155"
"90C"|"Nuley clay loam, 2 to 8 percent slopes"||5|5|127|||"None"|"None"|"0"|3.84|7.12|9.67|10.46|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.111|"Moderate"|"0"|0.989|"609156"
"91E"|"Nuley-Rock outcrop complex, 8 to 35 percent slopes"||22|20.8|107|||"None"|"None"|"0"|3.39|6.24|8.42|8.6|"Well drained"|"Well drained"|"B"||100|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.688|"Severe"|"0"|1|"609157"
"110A"|"Ryell, rarely flooded-Rivra complex, cool, 0 to 2 percent slopes"||1|1||54|54|"Rare"|"Rare"|"0"|3.76|6.88|9.49|11.43|"Well drained"|"Well drained"|"B"|"4"|60|"4"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.095|"Slight"|"0"|0.92|"609158"
"147C"|"Varney clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.12|7.53|14.03|19.83|"Well drained"|"Well drained"|"C"|"3"|97|"3"|97|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.187|"Moderate"|"0"|1|"609159"
"161A"|"Rivra, stony-Riverrun complex, 0 to 2 percent slopes"||1|1.1||76|76|"None"|"None"|"0"|3.03|5.18|7.76|9.4|"Excessively drained"|"Somewhat poorly drained"|"A"||100|"4"|93|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.036|"Slight"|"43"|0.98|"1697481"
"60A"|"Riverrun, occasionally flooded-Rivra complex, 0 to 2 percent slopes"||1|1||76|76|"Occasional"|"Occasional"|"0"|3.16|5.61|8.21|9.94|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"||100|"4"|93|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.065|"Slight"|"61"|0.98|"1697484"
"394E"|"Minestope, very stony-Beeftrail, very stony-Rock outcrop complex, 8 to 30 percent slopes"||20|20|43|||"None"|"None"|"0"|2.67|3.77|4|4|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.556|"Severe"|"0"|1|"1697489"
"547P"|"Elve-Gambler-Sebud families, complex, steep mountain slopes"||58|58||||"None"|"None"|"0"|3.72|6.23|10.04|13.61|"Well drained"|"Well drained"|"B"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1703804"
"229F"|"Pensore, very stony-Ferball, stony-Rock outcrop complex, 4 to 45 percent slopes"||15|17.9|46|||"None"|"None"|"0"|3.24|5.78|8.81|11.41|"Well drained"|"Well drained"|"D"||100|"7"|74|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.763|"Severe"|"0"|1|"2450828"
"240F"|"Blaine-Madigan complex, 15 to 45 percent slopes"||25|26.8|61|||"None"|"None"|"0"|3.58|6.82|8.78|8.78|"Well drained"|"Well drained"|"C"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Moderate"|"0"|1|"2450829"
"268F"|"Spudbar, very stony-Rencot, very stony-Rock outcrop complex, 25 to 50 percent slopes"||38|38|38|||"None"|"None"|"0"|2.34|3.95|4.12|4.12|"Well drained"|"Well drained"|"C"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2450830"
"269F"|"Pensore, extremely stony-Crago, very stony-Rock outcrop complex, 8 to 50 percent slopes"||25|24.9|46|||"None"|"None"|"0"|2.81|4.74|5.78|6.62|"Well drained"|"Well drained"|"D"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.948|"Severe"|"0"|0.977|"2450831"
"300F"|"Pensore-Kelmbeck-Rock outcrop complex, 15 to 60 percent slopes"||37|34.2|15|||"None"|"None"|"0"|2.22|3.61|4.46|5.22|"Well drained"|"Well drained"|"D"||100|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.943|"Severe"|"0"|1|"2450832"
"328E"|"Bronec, very stony-Spudbar, very stony-Rencot complex, 8 to 35 percent slopes"||22|22|38|||"None"|"None"|"0"|2.67|4.52|6.61|8.24|"Well drained"|"Well drained"|"B"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.829|"Severe"|"0"|1|"2450833"
"373E"|"Rencot, extremely stony-Spudbar-Rock outcrop complex, 4 to 35 percent slopes"||20|17.1|38|||"None"|"None"|"0"|2.61|4.45|5.59|6.53|"Well drained"|"Well drained"|"D"||92|"7"|65|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.586|"Severe"|"0"|0.917|"2450834"
"565G"|"Sebud, extremely stony-Rubble land-Shadow, very stony complex, 35 to 75 percent slopes"||50|48.7||||"None"|"None"|"0"|2.76|5.06|7.85|10.03|"Well drained"|"Well drained"|"B"||98|"8"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"2"|1|"2450835"
"808G"|"Rock outcrop-Rubble land-Tropal, extremely stony complex, 45 to 80 percent slopes"|||45.7|48||||"None"|"0"|3.57|5.54|6.55|7.27||"Well drained"|||100|"8"|90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"2450836"
"902G"|"Tropal, extremely stony-Rock outcrop-Whitore, stony complex, 25 to 80 percent slopes"||50|43.1|48|||"None"|"None"|"0"|3.71|5.81|7.34|8.3|"Well drained"|"Well drained"|"D"||100|"8"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2450837"
"192E"|"Bronec, bouldery-Geohrock, extremely bouldery-Kalsted, stony complex, 4 to 35 percent slopes"||20|19.6||||"None"|"None"|"0"|2.62|4.47|7.66|10.38|"Well drained"|"Well drained"|"B"||100|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.656|"Severe"|"0"|1|"2450838"
"193B"|"Attawan-Varney complex, 1 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.05|7.45|10.83|13.5|"Well drained"|"Well drained"|"B"|"4"|100|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.197|"Slight"|"0"|0.723|"2450839"
"288E"|"Geohrock, stony-Bronec-Geohrock, extremely stony complex, 8 to 45 percent slopes"||27|24.2||||"None"|"None"|"0"|2.38|4.13|7.4|10.27|"Well drained"|"Well drained"|"B"||87|"7"|87|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.898|"Severe"|"0"|0.979|"2450840"
"628D"|"Bronec-Kalsted-Geohrock, very stony complex, 4 to 15 percent slopes"||8|8||||"None"|"None"|"0"|2.9|5.19|9.49|13.22|"Well drained"|"Well drained"|"B"|"4"|98|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.157|"Moderate"|"0"|0.59|"2450841"
"928C"|"Dutchhollow-Medicinelodge-Foolhen complex, 1 to 6 percent slopes, frequently flooded"||2|2.4||15|15|"Frequent"|"Frequent"|"0"|6.18|11.23|18.33|22.02|"Very poorly drained"|"Very poorly drained"|"B/D"|"5"|55|"5"|55|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.675|"Slight"|"80"|0.978|"2537032"
"750D"|"Rooset-Maciver, stony complex, 4 to 15 percent slopes"||8|7.6||||"None"|"None"|"0"|3.35|6.42|11.78|17.91|"Well drained"|"Well drained"|"C"|"6"|100|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Poor"|"Poor"|"Somewhat limited"|0.005|"Moderate"|"0"|0.327|"2537033"
"38D"|"Philipsburg gravelly loam, 2 to 15 percent slopes"||9|9.6||||"None"|"None"|"0"|4.32|8.65|15.83|22.29|"Well drained"|"Well drained"|"C"||99|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.014|"Moderate"|"1"|0.409|"2597989"
"931D"|"Tibson, stony-Farlin, extremely bouldery-Rooset complex, 4 to 15 percent slopes, landslides"||10|10||||"None"|"None"|"0"|3.87|6.76|11.24|15.95|"Well drained"|"Well drained"|"B"||88|"6"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.332|"Moderate"|"3"|0.607|"2633470"
"52C"|"Redsage loam, 1 to 8 percent slopes"||4|4||||"None"|"None"|"0"|4.25|8.34|15.91|23.31|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.283|"Moderate"|"0"|0.085|"2820837"
"85F"|"Bronec, stony-Rockisland association, 15 to 50 percent slopes"||30|27.8||||"None"|"None"|"0"|3.21|5.48|8.96|12.02|"Well drained"|"Well drained"|"B"||100|"7"|83|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.908|"Severe"|"0"|1|"2820838"
"133D"|"Nieman-Madigan complex, 2 to 15 percent slopes"||9|9|46|||"None"|"None"|"0"|3.75|6.5|7.93|8.62|"Well drained"|"Well drained"|"D"||100|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.076|"Slight"|"0"|0.947|"2820839"
"138E"|"Philipsburg-Rockisland complex, 8 to 35 percent slopes"||20|19.2||||"None"|"None"|"0"|4.28|7.72|13.37|18.59|"Well drained"|"Well drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.45|"Severe"|"0"|0.952|"2820840"
"170F"|"Sebud, very stony-Poin, extremely stony-Rock outcrop complex, 20 to 60 percent slopes"||35|32|46|||"None"|"None"|"0"|3.3|5.82|9.21|12.07|"Well drained"|"Well drained"|"B"||99|"7"|74|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.938|"Severe"|"1"|1|"2820841"
