09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19708966"|"19687139"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19708967"|"19687140"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19708968"|"19687141"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ryell, rarely flooded component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708969"|"19687142"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708970"|"19687143"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"19708971"|"19687144"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra, frequently flooded component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS331MT Gravel (gr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708972"|"19687145"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709927"|"19688100"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709928"|"19688101"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is very rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709929"|"19688102"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709930"|"19688103"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun, frequently flooded component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 42 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP801MT Bottomland, Gravelly (gr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709693"|"19687866"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand, occasionally flooded soil is a minor component."|"19709694"|"19687867"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv, occasionally flooded soil is a minor component."|"19709695"|"19687868"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon, rarely flooded soil is a minor component."|"19709696"|"19687869"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell, rarely flooded soil is a minor component."|"19709697"|"19687870"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"19709698"|"19687871"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709699"|"19687872"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 16 to 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY080MT Bottomland, Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709700"|"19687873"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709714"|"19687887"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709715"|"19687888"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BA030MT Limy (ly)   Lru 43b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709716"|"19687889"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709717"|"19687890"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709718"|"19687891"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19710088"|"19688261"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19710089"|"19688262"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"19710090"|"19688263"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"19710091"|"19688264"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"19710092"|"19688265"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710093"|"19688266"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19710094"|"19688267"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo, stony soil is a minor component."|"19710318"|"19688491"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo, very stony soil is a minor component."|"19710319"|"19688492"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces, valleys. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS331MT Gravel (gr) 9-14"" P.z., Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710320"|"19688493"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"19710321"|"19688494"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19710322"|"19688495"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19710323"|"19688496"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt, stony soil is a minor component."|"19710324"|"19688497"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, stream terraces, alluvial fans. The parent material consists of sandy and gravelly colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710111"|"19688284"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19710112"|"19688285"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19710113"|"19688286"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19710114"|"19688287"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"19710115"|"19688288"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19710116"|"19688289"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19710117"|"19688290"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted, stony component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19710118"|"19688291"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, stony component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710119"|"19688292"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19710120"|"19688293"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, bouldery soil is a minor component."|"19710121"|"19688294"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709912"|"19688085"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19709913"|"19688086"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19709914"|"19688087"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709915"|"19688088"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709916"|"19688089"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, terraces, valleys. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19709917"|"19688090"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19709918"|"19688091"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19709919"|"19688092"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709920"|"19688093"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709921"|"19688094"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709922"|"19688095"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brockway soil is a minor component."|"19709923"|"19688096"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709924"|"19688097"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709925"|"19688098"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709926"|"19688099"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709701"|"19687874"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709702"|"19687875"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709703"|"19687876"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709704"|"19687877"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709705"|"19687878"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709706"|"19687879"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709707"|"19687880"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"19709708"|"19687881"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19710310"|"19688483"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19710311"|"19688484"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19710312"|"19688485"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19710313"|"19688486"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19710314"|"19688487"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19710315"|"19688488"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 80 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710316"|"19688489"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19710317"|"19688490"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19710095"|"19688268"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19710096"|"19688269"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19710097"|"19688270"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19710098"|"19688271"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19710099"|"19688272"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"19710100"|"19688273"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19710101"|"19688274"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19710102"|"19688275"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19710103"|"19688276"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"19710104"|"19688277"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19710105"|"19688278"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19710106"|"19688279"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19710107"|"19688280"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19710108"|"19688281"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 80 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19710109"|"19688282"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19710110"|"19688283"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brockway component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Limy (ly)   Lru 44b-a, Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19709709"|"19687882"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709710"|"19687883"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"19709711"|"19687884"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709712"|"19687885"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709713"|"19687886"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rominell component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on valleys, terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS604MT Saline Upland (su) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 17 within 30 inches of the soil surface."|"19709719"|"19687892"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19709720"|"19687893"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19709721"|"19687894"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709097"|"19687270"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough, rarely flooded soil is a minor component."|"19709098"|"19687271"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon, rarely flooded soil is a minor component."|"19709099"|"19687272"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg, rarely flooded soil is a minor component."|"19709100"|"19687273"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Threeriv, frequently flooded component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R044BY181MT Bottomland, Wet Meadow (wm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709101"|"19687274"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 16 to 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY150MT Bottomland, Subirrigated (sb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709102"|"19687275"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709103"|"19687276"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverrun, occasionally flooded soil is a minor component."|"19709104"|"19687277"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Newtman soil is a minor component."|"19709105"|"19687278"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 85 percent of the map unit. Slopes are 8 to 35 percent. This component is on intermontane basins, hills. The parent material consists of slope alluvium over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709404"|"19687577"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"19709405"|"19687578"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709406"|"19687579"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"19709407"|"19687580"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted, lesser slopes soil is a minor component."|"19709408"|"19687581"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709409"|"19687582"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709410"|"19687583"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, stony soil is a minor component."|"19708860"|"19687033"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708861"|"19687034"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708862"|"19687035"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19708863"|"19687036"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, greater slopes soil is a minor component."|"19708864"|"19687037"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted, stony soil is a minor component."|"19708865"|"19687038"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709411"|"19687584"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709412"|"19687585"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709413"|"19687586"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709414"|"19687587"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709415"|"19687588"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709416"|"19687589"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708545"|"19686718"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708546"|"19686719"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708547"|"19686720"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19708548"|"19686721"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708549"|"19686722"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708550"|"19686723"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708551"|"19686724"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708552"|"19686725"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19708553"|"19686726"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708554"|"19686727"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19708555"|"19686728"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"19708556"|"19686729"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19708557"|"19686730"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708558"|"19686731"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19708559"|"19686732"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708560"|"19686733"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708561"|"19686734"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock, occasionally flooded soil is a minor component."|"19708562"|"19686735"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708563"|"19686736"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708564"|"19686737"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708565"|"19686738"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19708566"|"19686739"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708567"|"19686740"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708568"|"19686741"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708569"|"19686742"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trudau component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces, alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS604MT Saline Upland (su) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"19708570"|"19686743"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19708571"|"19686744"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708866"|"19687039"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708867"|"19687040"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708868"|"19687041"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19708869"|"19687042"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19708870"|"19687043"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, very stony component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on north facing slopes on hills, escarpments, uplands. The parent material consists of alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19708871"|"19687044"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709417"|"19687590"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709418"|"19687591"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dillon, rarely flooded component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BY081MT Bottomland, Riparian Subirrigated (rsb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709419"|"19687592"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv, occasionally flooded soil is a minor component."|"19709420"|"19687593"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock, rarely flooded soil is a minor component."|"19709421"|"19687594"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough, rarely flooded soil is a minor component."|"19709422"|"19687595"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19708872"|"19687045"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19708873"|"19687046"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Madbeaver component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on valleys, alluvial fans. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 42 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS343MT Subirrigated (sb) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708874"|"19687047"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"19708875"|"19687048"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19708876"|"19687049"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709124"|"19687297"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709125"|"19687298"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, alluvial fans, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP804MT Limy (ly)   Lru 44b-a, Limy Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19709126"|"19687299"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19709127"|"19687300"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo, cobbly sandy loam soil is a minor component."|"19709128"|"19687301"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19709129"|"19687302"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709130"|"19687303"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP804MT Limy Grassland, Shallow To Gravel Limy (swgrly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709131"|"19687304"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709132"|"19687305"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on valleys, alluvial fans. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709133"|"19687306"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709134"|"19687307"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709135"|"19687308"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709136"|"19687309"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709137"|"19687310"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709138"|"19687311"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709139"|"19687312"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709140"|"19687313"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted, greater slopes soil is a minor component."|"19709141"|"19687314"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, lesser slopes soil is a minor component."|"19709142"|"19687315"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709143"|"19687316"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zbart component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on strike ridges, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 5 to 10 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS348MT Very Shallow (vsw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708979"|"19687152"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haxby component makes up 30 percent of the map unit. Slopes are 4 to 25 percent. This component is on foothills, strike ridges. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708980"|"19687153"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"19708981"|"19687154"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19708982"|"19687155"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708983"|"19687156"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackleaf component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on foothills, strike ridges. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"19708984"|"19687157"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twinadams soil is a minor component."|"19708985"|"19687158"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby soil is a minor component."|"19708986"|"19687159"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709596"|"19687769"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackleaf soil is a minor component."|"19709597"|"19687770"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, ridges, foothills. The parent material consists of colluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA031MT Limy Droughty (lydr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709598"|"19687771"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, foothills, ridges. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA135MT Shallow Limy Droughty (swlydr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709599"|"19687772"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spudbar soil is a minor component."|"19709600"|"19687773"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709601"|"19687774"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, ridges, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709602"|"19687775"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709603"|"19687776"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709604"|"19687777"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709605"|"19687778"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709284"|"19687457"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spudbar soil is a minor component."|"19709285"|"19687458"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on foothills, hills. The parent material consists of residuum weathered from tuff. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709286"|"19687459"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709287"|"19687460"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zbart soil is a minor component."|"19709288"|"19687461"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709289"|"19687462"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19709290"|"19687463"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot, lower slopes component makes up 35 percent of the map unit. Slopes are 8 to 25 percent. This component is on foothills, hills. The parent material consists of residuum weathered from tuff. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709291"|"19687464"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on uplands, hillsides. The parent material consists of loamy residuum over calcareous shale and/or sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709606"|"19687779"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709607"|"19687780"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709608"|"19687781"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709609"|"19687782"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709610"|"19687783"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"19709611"|"19687784"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709612"|"19687785"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, uplands. The parent material consists of mixed alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709613"|"19687786"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, stony soil is a minor component."|"19708987"|"19687160"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"19708988"|"19687161"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708989"|"19687162"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708990"|"19687163"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, greater slopes soil is a minor component."|"19708991"|"19687164"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"19708992"|"19687165"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19708993"|"19687166"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19709614"|"19687787"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"19709615"|"19687788"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709616"|"19687789"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19709617"|"19687790"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19709618"|"19687791"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709619"|"19687792"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"19709620"|"19687793"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709621"|"19687794"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough, rarely flooded component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709622"|"19687795"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dillon, rarely flooded component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS343MT Subirrigated (sb) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709623"|"19687796"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, rarely flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, flood plains. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044XS349MT Wet Meadow (wm) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709624"|"19687797"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19708830"|"19687003"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708831"|"19687004"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 15 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708832"|"19687005"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19708833"|"19687006"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708834"|"19687007"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on uplands, alluvial fans. The parent material consists of gravelly tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19708514"|"19686687"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"19708515"|"19686688"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19708516"|"19686689"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, uplands. The parent material consists of fine-loamy slope alluvium from semiconsolidated sandstone, siltstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708517"|"19686690"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"19708518"|"19686691"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Udecide component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on uplands, alluvial fans. The parent material consists of calcareous fine-loamy slope alluvium over residuum weathered from semiconsolidated sandstone-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"19708519"|"19686692"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, intermontane basins, hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19708822"|"19686995"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo, stony component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Sagebrush Shrubland, Shallow To Gravel Limy (swgrly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708823"|"19686996"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19708824"|"19686997"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19708825"|"19686998"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted, lesser slopes soil is a minor component."|"19708826"|"19686999"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708827"|"19687000"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Loamy (swlo)   Lru 44b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708828"|"19687001"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708829"|"19687002"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709115"|"19687288"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709116"|"19687289"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 30 percent of the map unit. Slopes are 8 to 45 percent. This component is on hillsides, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709117"|"19687290"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709118"|"19687291"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock component makes up 40 percent of the map unit. Slopes are 8 to 45 percent. This component is on hillsides, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709119"|"19687292"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709120"|"19687293"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709121"|"19687294"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, stony component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on hillsides, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709122"|"19687295"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19709123"|"19687296"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"19709042"|"19687215"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra, occassionally flooded, very cobbly component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of mixed alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA060MT Overflow (ov)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709043"|"19687216"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"19709044"|"19687217"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra, occasionally flooded component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of mixed alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA060MT Overflow (ov)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709045"|"19687218"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19709046"|"19687219"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19709047"|"19687220"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709089"|"19687262"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"19709090"|"19687263"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dillon, rarely flooded component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BY081MT Riparian Subirrigated (rsb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709091"|"19687264"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, rarely flooded component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY080MT Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709092"|"19687265"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19709093"|"19687266"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19709094"|"19687267"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709095"|"19687268"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"19709096"|"19687269"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19708807"|"19686980"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19708808"|"19686981"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dillon, rarely flooded component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 39 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BY081MT Bottomland, Riparian Subirrigated (rsb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708809"|"19686982"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, rarely flooded component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 16 to 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY080MT Bottomland, Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708810"|"19686983"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv, occasionally flooded soil is a minor component."|"19708811"|"19686984"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 42 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP801MT Bottomland, Gravelly (gr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708812"|"19686985"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708813"|"19686986"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19708814"|"19686987"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg, rarely flooded soil is a minor component."|"19708815"|"19686988"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 29 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Sagebrush Shrubland, Shallow To Gravel Limy (swgrly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709392"|"19687565"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nippt, very cobbly loam component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Shallow To Gravel (swgr)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709393"|"19687566"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nippt component makes up 31 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP819MT Shallow To Gravel (swgr)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709394"|"19687567"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709395"|"19687568"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo, greater slopes soil is a minor component."|"19709396"|"19687569"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19709397"|"19687570"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"19709398"|"19687571"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, stream terraces, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP804MT Limy Grassland, Shallow To Gravel Limy (swgrly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708816"|"19686989"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo, very gravelly soil is a minor component."|"19708817"|"19686990"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thessvo component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 11 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Shallow To Gravel Limy (swgrly)   Lru 44b-a, Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent.  "|"19708818"|"19686991"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708819"|"19686992"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19708820"|"19686993"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo, stony soil is a minor component."|"19708821"|"19686994"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on uplands, hillsides. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709106"|"19687279"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"19709107"|"19687280"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709108"|"19687281"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709109"|"19687282"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on uplands, north facing hillsides. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709110"|"19687283"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709111"|"19687284"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709112"|"19687285"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillsides, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709113"|"19687286"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709114"|"19687287"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708843"|"19687016"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"19708844"|"19687017"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haxby component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP806MT Limy Shrubland, Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708845"|"19687018"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, intermontane basins. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP812MT Shallow Limy Droughty (swlydr)   Lru 44b-a, Shallow Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19708846"|"19687019"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spudbar soil is a minor component."|"19708847"|"19687020"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708848"|"19687021"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP806MT Limy (ly)   Lru 44b-a, Limy Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19708849"|"19687022"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708850"|"19687023"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708529"|"19686702"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19708530"|"19686703"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackleaf soil is a minor component."|"19708531"|"19686704"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708532"|"19686705"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708533"|"19686706"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 30 percent of the map unit. Slopes are 4 to 8 percent. This component is on uplands, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708534"|"19686707"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"19708535"|"19686708"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"19708536"|"19686709"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708537"|"19686710"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"19708538"|"19686711"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, stony component makes up 20 percent of the map unit. Slopes are 15 to 25 percent. This component is on hillsides, uplands. The parent material consists of alluvium over residuum. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708539"|"19686712"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington, stony component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills, uplands. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS347MT Silty-steep (sistp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709273"|"19687446"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709274"|"19687447"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackleaf soil is a minor component."|"19709275"|"19687448"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twinadams soil is a minor component."|"19709276"|"19687449"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, bouldery component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, uplands. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709277"|"19687450"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, bouldery component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, uplands. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709278"|"19687451"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709279"|"19687452"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709280"|"19687453"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709281"|"19687454"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709282"|"19687455"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709283"|"19687456"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby soil is a minor component."|"19708973"|"19687146"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708974"|"19687147"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, uplands. The parent material consists of alluvium derived from limestone over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"19708975"|"19687148"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on uplands, alluvial fans. The parent material consists of alluvium derived from limestone over colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708976"|"19687149"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19708977"|"19687150"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roto component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on structural benches, uplands. The parent material consists of alluvium derived from limestone over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"19708978"|"19687151"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709588"|"19687761"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackleaf, stony component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 44b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"19709589"|"19687762"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"19709590"|"19687763"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twinadams component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, strike ridges. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 35 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent.  "|"19709591"|"19687764"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twinadams, stony soil is a minor component."|"19709592"|"19687765"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby, stony soil is a minor component."|"19709593"|"19687766"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot, very stony soil is a minor component."|"19709594"|"19687767"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zbart soil is a minor component."|"19709595"|"19687768"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"19708681"|"19686854"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haxby component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on structural benches, mountains. The parent material consists of alluvium and/or slope alluvium over residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Sagebrush Shrubland, Loamy (lo)    Lru 43b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708682"|"19686855"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 43b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19708683"|"19686856"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby, greater slopes soil is a minor component."|"19708684"|"19686857"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708685"|"19686858"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zbart component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, structural benches. The parent material consists of colluvium and/or residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 5 to 10 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland, Very Shallow (vsw)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708686"|"19686859"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19708687"|"19686860"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708688"|"19686861"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708689"|"19686862"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19708690"|"19686863"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708691"|"19686864"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708692"|"19686865"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19708693"|"19686866"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708694"|"19686867"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708695"|"19686868"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted, cobbly component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708696"|"19686869"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19708994"|"19687167"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708995"|"19687168"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans on valleys, stream terraces on valleys. The parent material consists of mixed alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19708996"|"19687169"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19708997"|"19687170"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708998"|"19687171"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19708999"|"19687172"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709000"|"19687173"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709001"|"19687174"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"19709002"|"19687175"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709003"|"19687176"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709292"|"19687465"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"19709293"|"19687466"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar component makes up 20 percent of the map unit. Slopes are 25 to 50 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and shale and/or residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BA031MT Limy Droughty (lydr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709294"|"19687467"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spudbar soil is a minor component."|"19709295"|"19687468"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zbart soil is a minor component."|"19709296"|"19687469"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot, stony component makes up 30 percent of the map unit. Slopes are 25 to 50 percent. This component is on hills. The parent material consists of residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BA135MT Shallow Limy Droughty (swlydr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709297"|"19687470"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19709298"|"19687471"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackleaf, stony component makes up 35 percent of the map unit. Slopes are 20 to 60 percent. This component is on foothills, strike ridges. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 44b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"19709004"|"19687177"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"19709005"|"19687178"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709006"|"19687179"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"19709007"|"19687180"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twinadams, very stony component makes up 30 percent of the map unit. Slopes are 20 to 60 percent. This component is on strike ridges, foothills. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 35 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent.  "|"19709008"|"19687181"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19709009"|"19687182"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spudbar soil is a minor component."|"19709010"|"19687183"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twinadams, bouldery soil is a minor component."|"19709011"|"19687184"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thunderhead component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on strike ridges, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 22 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.   The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709625"|"19687798"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby soil is a minor component."|"19709626"|"19687799"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709627"|"19687800"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twinadams component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on strike ridges, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 36 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent.  "|"19709628"|"19687801"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709629"|"19687802"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709630"|"19687803"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackleaf component makes up 20 percent of the map unit. Slopes are 8 to 25 percent. This component is on foothills, strike ridges. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"19709631"|"19687804"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spudbar soil is a minor component."|"19709632"|"19687805"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, stony component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709299"|"19687472"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 20 percent of the map unit. Slopes are 2 to 4 percent. This component is on flood plains, valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY080MT Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709300"|"19687473"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19709301"|"19687474"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19709302"|"19687475"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709303"|"19687476"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709304"|"19687477"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Faith, rarely flooded component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BA060MT Overflow (ov)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709305"|"19687478"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709306"|"19687479"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"19709307"|"19687480"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709308"|"19687481"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19709309"|"19687482"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"19709030"|"19687203"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby soil is a minor component."|"19709031"|"19687204"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709032"|"19687205"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on foothills, strike ridges. The parent material consists of residuum. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709033"|"19687206"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on foothills, strike ridges. The parent material consists of residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709034"|"19687207"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Denied access is a miscellaneous area."|"19709072"|"19687245"
07/27/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Gravel pits is a miscellaneous area."|"19709671"|"19687844"
07/27/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Miscellaneous water is a miscellaneous area."|"19709330"|"19687503"
07/08/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"19709073"|"19687246"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708716"|"19686889"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby soil is a minor component."|"19708717"|"19686890"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"19708718"|"19686891"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on cuestas, foothills. The parent material consists of residuum. Depth to a root restrictive layer, bedrock, lithic, is 6 to 22 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708719"|"19686892"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"19708720"|"19686893"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"19708721"|"19686894"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708722"|"19686895"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19708723"|"19686896"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, rarely flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways on valleys, flood plains on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044XS349MT Wet Meadow (wm) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708724"|"19686897"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19708725"|"19686898"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19708726"|"19686899"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough, saline component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS327MT Saline Overflow (sov) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708727"|"19686900"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19708728"|"19686901"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neen, rarely flooded component makes up 40 percent of the map unit. Slopes are 2 to 4 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044XS333MT Saline Subirrigated (ssb) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"19708729"|"19686902"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"19709012"|"19687185"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin soil is a minor component."|"19709013"|"19687186"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, bouldery component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills, foothills. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709014"|"19687187"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, igneous soil is a minor component."|"19709015"|"19687188"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak, lesser slopes soil is a minor component."|"19709016"|"19687189"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19709017"|"19687190"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nathale, bouldery soil is a minor component."|"19709018"|"19687191"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban, bouldery soil is a minor component."|"19709019"|"19687192"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillsides, foothills. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709020"|"19687193"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"19709021"|"19687194"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709022"|"19687195"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709023"|"19687196"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709024"|"19687197"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709025"|"19687198"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709026"|"19687199"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, hillsides. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709027"|"19687200"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillsides. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709028"|"19687201"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillsides. The parent material consists of alluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy (ly)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709029"|"19687202"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nathale component makes up 40 percent of the map unit. Slopes are 20 to 60 percent. This component is on strike ridges, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709639"|"19687812"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 30 percent of the map unit. Slopes are 20 to 60 percent. This component is on strike ridges, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709640"|"19687813"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanson soil is a minor component."|"19709641"|"19687814"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"19709642"|"19687815"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"19709643"|"19687816"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709644"|"19687817"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"19709645"|"19687818"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19708730"|"19686903"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19708731"|"19686904"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19708732"|"19686905"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708733"|"19686906"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS335MT Sandy (sy) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708734"|"19686907"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708735"|"19686908"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708736"|"19686909"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708737"|"19686910"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708738"|"19686911"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19708739"|"19686912"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708740"|"19686913"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon, rarely flooded soil is a minor component."|"19708741"|"19686914"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brockway soil is a minor component."|"19708742"|"19686915"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19708743"|"19686916"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt, greater slopes soil is a minor component."|"19708744"|"19686917"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nippt component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Shallow To Gravel (swgr)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708745"|"19686918"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708746"|"19686919"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708747"|"19686920"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19708748"|"19686921"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dillon, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS343MT Subirrigated (sb) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708749"|"19686922"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19708750"|"19686923"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun, rarely flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS333MT Saline Subirrigated (ssb) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"19708751"|"19686924"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19708752"|"19686925"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neen soil is a minor component."|"19708753"|"19686926"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"19708754"|"19686927"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dillon, rarely flooded, saline component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS333MT Saline Subirrigated (ssb) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708755"|"19686928"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19708756"|"19686929"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709633"|"19687806"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709634"|"19687807"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roto soil is a minor component."|"19709635"|"19687808"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, foothills. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"19709636"|"19687809"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"19709637"|"19687810"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on foothills, hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"19709638"|"19687811"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708705"|"19686878"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"19708706"|"19686879"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"19708707"|"19686880"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on foothills, strike ridges. The parent material consists of residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708708"|"19686881"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708709"|"19686882"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19708710"|"19686883"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708711"|"19686884"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19708712"|"19686885"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19708713"|"19686886"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19708714"|"19686887"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19708715"|"19686888"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wickes soil is a minor component."|"19709339"|"19687512"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, very stony component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillsides, escarpments on foothills, ridges on foothills. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709340"|"19687513"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709341"|"19687514"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brickner soil is a minor component."|"19709342"|"19687515"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, very stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillsides on foothills, escarpments on foothills, ridges on foothills. The parent material consists of gravelly slope alluvium derived from metavolcanics. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709343"|"19687516"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708769"|"19686942"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"19708770"|"19686943"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wickes soil is a minor component."|"19708771"|"19686944"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brickner, stony component makes up 30 percent of the map unit. Slopes are 4 to 25 percent. This component is on ridges, hillsides, foothills, escarpments. The parent material consists of gravelly residuum weathered from sandstone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708772"|"19686945"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, very stony component makes up 40 percent of the map unit. Slopes are 4 to 25 percent. This component is on escarpments on foothills, hillsides on foothills, ridges on foothills. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708773"|"19686946"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708774"|"19686947"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 55 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountain slopes on mountains. The parent material consists of gravelly till, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19708775"|"19686948"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin soil is a minor component."|"19708776"|"19686949"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountain slopes on mountains, ridges on mountains. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708777"|"19686950"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"19708778"|"19686951"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"19708779"|"19686952"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans on mountains, mountain slopes on mountains. The parent material consists of gravelly slope alluvium derived from metavolcanics. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BE038MT Droughty Steep (drstp)   Lru 44b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708780"|"19686953"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"19708781"|"19686954"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes on mountains, ridges on mountains. The parent material consists of gravelly residuum weathered from sandstone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708782"|"19686955"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"19708783"|"19686956"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kimpton soil is a minor component."|"19708784"|"19686957"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19708785"|"19686958"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19708786"|"19686959"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"19708787"|"19686960"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708788"|"19686961"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes on foothills, ridges on foothills. The parent material consists of gravelly residuum weathered from sandstone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708789"|"19686962"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"19708790"|"19686963"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillsides on foothills. The parent material consists of gravelly slope alluvium derived from metavolcanics. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708791"|"19686964"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kimpton soil is a minor component."|"19708792"|"19686965"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19708793"|"19686966"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"19709678"|"19687851"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709679"|"19687852"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes on mountains. The parent material consists of gravelly slope alluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709680"|"19687853"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19709074"|"19687247"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes on mountains, ridges on mountains. The parent material consists of gravelly residuum weathered from tuffaceous volcanic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709075"|"19687248"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709076"|"19687249"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"19709077"|"19687250"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Surdal component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on ridges on mountains, mountain slopes on mountains. The parent material consists of gravelly slope alluvium derived from basalt over residuum weathered from basalt. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19709078"|"19687251"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 55 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, alluvial fans, mountain slopes. The parent material consists of gravelly slope alluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19709079"|"19687252"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"19709080"|"19687253"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 60 percent of the map unit. Slopes are 4 to 25 percent. This component is on hillsides on foothills. The parent material consists of gravelly till, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19710277"|"19688450"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"19710278"|"19688451"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, frequently flooded component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on flood plains on foothills. The parent material consists of organic material over fine-loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"19710279"|"19688452"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19710280"|"19688453"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19710281"|"19688454"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709672"|"19687845"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709673"|"19687846"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on valleys. The parent material consists of gravelly tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709674"|"19687847"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19709675"|"19687848"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709676"|"19687849"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, valleys. The parent material consists of sandy and gravelly colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709677"|"19687850"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"19709666"|"19687839"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"19709667"|"19687840"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 20 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709668"|"19687841"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 29 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Douglas-fir/elk Sedge, Douglas-fir/heartleaf Arnica, Douglas-fir/mountain Snowberry, Douglas-fir/pinegrass, Douglas-fir/white Spirea ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709669"|"19687842"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 31 percent of the map unit. Slopes are 20 to 45 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Douglas-fir/elk Sedge, Douglas-fir/heartleaf Arnica, Douglas-fir/mountain Snowberry, Douglas-fir/pinegrass, Douglas-fir/white Spirea ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709670"|"19687843"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709813"|"19687986"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709814"|"19687987"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ermont component makes up 70 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709815"|"19687988"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709827"|"19688000"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Branham soil is a minor component."|"19709828"|"19688001"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zbart soil is a minor component."|"19709829"|"19688002"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19709830"|"19688003"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kounter component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills, foothills. The parent material consists of residuum weathered from schist residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 12 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BS291MT Shallow (sw) 9-14"" P.z. Not Known ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"19709831"|"19688004"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19710432"|"19688605"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Branham soil is a minor component."|"19710433"|"19688606"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kounter soil is a minor component."|"19710434"|"19688607"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19710435"|"19688608"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kounter component makes up 70 percent of the map unit. Slopes are 4 to 15 percent. This component is on strike ridges, foothills. The parent material consists of residuum weathered from schist residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 12 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BS291MT Shallow (sw) 9-14"" P.z. Not Known ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"19710436"|"19688609"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"19710039"|"19688212"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oro Fino component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillsides, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BS318MT Thin Silty (tsi) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710040"|"19688213"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barbarela soil is a minor component."|"19710041"|"19688214"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710042"|"19688215"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nathale soil is a minor component."|"19710043"|"19688216"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 15 percent of the map unit. Slopes are 20 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from gneiss and/or residuum weathered from schist. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BS308MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19710044"|"19688217"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19710045"|"19688218"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 40 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BS720MT Silty-droughty-steep (sidrstp) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19710046"|"19688219"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710047"|"19688220"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19710048"|"19688221"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Branham soil is a minor component."|"19710049"|"19688222"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillsides, foothills. The parent material consists of colluvium over residuum weathered from gneiss and/or residuum weathered from schist. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BS317MT Thin Sandy (tsy) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19710050"|"19688223"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillsides, foothills. The parent material consists of colluvium over residuum weathered from gneiss and/or residuum weathered from schist. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R043BS308MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19710051"|"19688224"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"19710052"|"19688225"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kounter soil is a minor component."|"19710053"|"19688226"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin soil is a minor component."|"19710426"|"19688599"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19710427"|"19688600"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 45 percent of the map unit. Slopes are 25 to 60 percent. This component is on foothills, hillsides. The parent material consists of colluvium over residuum weathered from gneiss and/or residuum weathered from schist. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BS311MT Shallow Limy (swly) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19710428"|"19688601"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19710429"|"19688602"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"19710430"|"19688603"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"19710431"|"19688604"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709816"|"19687989"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709817"|"19687990"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709818"|"19687991"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trudau component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces, alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS604MT Saline Upland (su) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"19709819"|"19687992"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19710216"|"19688389"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710217"|"19688390"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neen soil is a minor component."|"19710218"|"19688391"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairway soil is a minor component."|"19710219"|"19688392"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"19710220"|"19688393"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY080MT Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19710221"|"19688394"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19710222"|"19688395"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19710223"|"19688396"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Newtman soil is a minor component."|"19710224"|"19688397"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Newtman soil is a minor component."|"19710225"|"19688398"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BY080MT Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19710226"|"19688399"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"19710227"|"19688400"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairway soil is a minor component."|"19710228"|"19688401"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Threeriv, frequently flooded component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BY080MT Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710229"|"19688402"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19710230"|"19688403"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, stony component makes up 50 percent of the map unit. Slopes are 4 to 10 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"19709820"|"19687993"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, very cobbly loam soil is a minor component."|"19709821"|"19687994"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock, rarely flooded soil is a minor component."|"19709822"|"19687995"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neen, rarely flooded soil is a minor component."|"19709823"|"19687996"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709824"|"19687997"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, very stony component makes up 15 percent of the map unit. Slopes are 4 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"19709825"|"19687998"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 20 percent of the map unit. Slopes are 4 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"19709826"|"19687999"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"19709832"|"19688005"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 55 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillsides, mountains. The parent material consists of colluvium. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BD032MT Loamy (lo)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19709833"|"19688006"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss, schist soil is a minor component."|"19709834"|"19688007"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19709835"|"19688008"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19709836"|"19688009"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin, stony soil is a minor component."|"19709837"|"19688010"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oro Fino soil is a minor component."|"19709838"|"19688011"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, occasionally flooded component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains, drainageways, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 7 percent. This component is in the R044BP801MT Bottomland, Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"19709839"|"19688012"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, rarely flooded soil is a minor component."|"19709840"|"19688013"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"19709931"|"19688104"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709932"|"19688105"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19709933"|"19688106"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"19709934"|"19688107"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, very stony soil is a minor component."|"19710231"|"19688404"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, stony component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710232"|"19688405"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710233"|"19688406"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban, very stony soil is a minor component."|"19710234"|"19688407"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, very bouldery component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on fan remnants, mountains. The parent material consists of alluvium and/or slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710235"|"19688408"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sieberell component makes up 25 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"19710236"|"19688409"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19710237"|"19688410"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19710238"|"19688411"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavwan component makes up 55 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19710239"|"19688412"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavwan soil is a minor component."|"19710240"|"19688413"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19710241"|"19688414"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19710242"|"19688415"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"19710243"|"19688416"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, very stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19710244"|"19688417"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, very stony soil is a minor component."|"19710245"|"19688418"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bavdark soil is a minor component."|"19710246"|"19688419"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19710247"|"19688420"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19710248"|"19688421"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, very stony soil is a minor component."|"19710249"|"19688422"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, valleys. The parent material consists of Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19710437"|"19688610"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19710438"|"19688611"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neen soil is a minor component."|"19710439"|"19688612"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19710440"|"19688613"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19710441"|"19688614"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"19709841"|"19688014"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on uplands, moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BD038MT Droughty Steep (drstp)   Lru 44b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709842"|"19688015"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bavdark soil is a minor component."|"19709843"|"19688016"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19709844"|"19688017"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanson soil is a minor component."|"19709845"|"19688018"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 45 percent of the map unit. Slopes are 15 to 60 percent. This component is on moraines, uplands. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BD038MT Droughty Steep (drstp)   Lru 44b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709846"|"19688019"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"19710442"|"19688615"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19710443"|"19688616"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Newtman component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on marshes on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BY181MT Wet Meadow (wm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710444"|"19688617"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairway soil is a minor component."|"19710445"|"19688618"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dougcliff component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on valleys, marshes. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BY181MT Wet Meadow (wm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"19710446"|"19688619"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709847"|"19688020"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709848"|"19688021"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709849"|"19688022"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"19709850"|"19688023"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709851"|"19688024"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709852"|"19688025"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19709853"|"19688026"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on uplands, swales on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709854"|"19688027"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"19709855"|"19688028"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo, stony component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments. The parent material consists of colluvium over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA137MT Shallow To Gravel Limy (swgrly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710054"|"19688227"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710055"|"19688228"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710056"|"19688229"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710057"|"19688230"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"19710058"|"19688231"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19710059"|"19688232"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Branham soil is a minor component."|"19709263"|"19687436"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"19709264"|"19687437"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"19709265"|"19687438"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"19709266"|"19687439"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oro Fino component makes up 15 percent of the map unit. Slopes are 2 to 15 percent. This component is on foothills, structural benches. The parent material consists of colluvium derived from gneiss or schist. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BS318MT Thin Silty (tsi) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709267"|"19687440"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills, foothills. The parent material consists of colluvium or residuum derived from gneiss or schist. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BS307MT Sandy (sy) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19709268"|"19687441"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709269"|"19687442"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19709270"|"19687443"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on structural benches, foothills. The parent material consists of alluvium over schist and/or gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BS308MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709271"|"19687444"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin soil is a minor component."|"19709272"|"19687445"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710325"|"19688498"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"19710326"|"19688499"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leavitt soil is a minor component."|"19710327"|"19688500"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 85 percent of the map unit. Slopes are 2 to 15 percent. This component is on ridges, hillsides. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710328"|"19688501"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leavitt soil is a minor component."|"19710122"|"19688295"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19710123"|"19688296"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BD033MT Loamy Argillic (loa)   Lru 44b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710124"|"19688297"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"19709935"|"19688108"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 60 percent of the map unit. Slopes are 8 to 45 percent. This component is on escarpments on stream terraces. The parent material consists of coarse-silty alluvium and/or eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709936"|"19688109"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709937"|"19688110"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19709938"|"19688111"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 30 percent of the map unit. Slopes are 8 to 45 percent. This component is on dissected terraces. The parent material consists of gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709939"|"19688112"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"19708674"|"19686847"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavwan component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on uplands, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19708675"|"19686848"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19708676"|"19686849"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19708677"|"19686850"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavwan soil is a minor component."|"19708678"|"19686851"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19708679"|"19686852"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19708680"|"19686853"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19708669"|"19686842"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708670"|"19686843"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19708671"|"19686844"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on foothills, hillsides. The parent material consists of colluvium over residuum weathered from gneiss and/or residuum weathered from schist. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BS317MT Thin Sandy (tsy) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19708672"|"19686845"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on foothills, hillsides. The parent material consists of colluvium over residuum weathered from gneiss and/or residuum weathered from schist. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R043BS308MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708673"|"19686846"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman component makes up 40 percent of the map unit. Slopes are 8 to 60 percent. This component is on hills, ridges, foothills. The parent material consists of residuum over gneiss and/or schist. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BS308MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709582"|"19687755"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barbarela soil is a minor component."|"19709583"|"19687756"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin soil is a minor component."|"19709584"|"19687757"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709585"|"19687758"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oro Fino soil is a minor component."|"19709586"|"19687759"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19709587"|"19687760"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"19709646"|"19687819"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"19709647"|"19687820"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19709648"|"19687821"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough, rarely flooded component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709649"|"19687822"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavrock soil is a minor component."|"19709650"|"19687823"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Faith soil is a minor component."|"19709651"|"19687824"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19709258"|"19687431"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fourmile component makes up 65 percent of the map unit. Slopes are 8 to 15 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty (dr)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"19709259"|"19687432"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fourmile, extremely bouldery component makes up 15 percent of the map unit. Slopes are 8 to 25 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"19709260"|"19687433"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban, very stony soil is a minor component."|"19709261"|"19687434"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, rarely flooded soil is a minor component."|"19709262"|"19687435"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very stony component makes up 35 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709251"|"19687424"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, stony component makes up 20 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709252"|"19687425"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow component makes up 15 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709253"|"19687426"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, very stony soil is a minor component."|"19709254"|"19687427"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin soil is a minor component."|"19709255"|"19687428"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709256"|"19687429"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19709257"|"19687430"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709574"|"19687747"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19709575"|"19687748"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709576"|"19687749"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19709577"|"19687750"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nippt soil is a minor component."|"19709578"|"19687751"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19709579"|"19687752"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 39 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS331MT Gravel (gr) 9-14"" P.z., Limy Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709580"|"19687753"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nippt component makes up 41 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS338MT Shallow To Gravel (swgr) 9-14"" P.z., Upland Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709581"|"19687754"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708697"|"19686870"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19708698"|"19686871"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, uplands. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19708699"|"19686872"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"19708700"|"19686873"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708701"|"19686874"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"19708702"|"19686875"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kounter soil is a minor component."|"19708703"|"19686876"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kounter component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on foothills, strike ridges. The parent material consists of gravelly residuum over schist and/or gneiss. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 18 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BS291MT Shallow (sw) 9-14"" P.z. Not Known ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"19708704"|"19686877"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BD036MT Droughty (dr)   Lru 44b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708540"|"19686713"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"19708541"|"19686714"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19708542"|"19686715"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19708543"|"19686716"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BD036MT Droughty (dr)   Lru 44b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"19708544"|"19686717"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on dissected terraces. The parent material consists of gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710125"|"19688298"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710126"|"19688299"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19710127"|"19688300"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710128"|"19688301"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"19710129"|"19688302"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments on stream terraces. The parent material consists of calcareous sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS338MT Shallow To Gravel (swgr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710130"|"19688303"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708851"|"19687024"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708852"|"19687025"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19708853"|"19687026"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"19708854"|"19687027"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"19708855"|"19687028"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19708856"|"19687029"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, swales on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BD060MT Overflow (ov)   Lru 44b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708835"|"19687008"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"19708836"|"19687009"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"19708837"|"19687010"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708838"|"19687011"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BD040MT Loamy Steep (lostp)   Lru 44b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708839"|"19687012"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"19708840"|"19687013"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BD038MT Droughty Steep (drstp)   Lru 44b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708841"|"19687014"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"19708842"|"19687015"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"19709331"|"19687504"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 35 percent of the map unit. Slopes are 1 to 35 percent. This component is on intermontane basins, alluvial fans, hillsides. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru A (9-14 Pz), Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709332"|"19687505"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun, occasionally flooded component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, flood plains, flood-plain steps, drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BY081MT Bottomland, Riparian Subirrigated (rsb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"19709333"|"19687506"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand, occasionally flooded soil is a minor component."|"19709334"|"19687507"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 30 percent of the map unit. Slopes are 1 to 35 percent. This component is on hillsides, intermontane basins, alluvial fans. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19709335"|"19687508"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"19709336"|"19687509"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, greater slopes soil is a minor component."|"19709337"|"19687510"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19709338"|"19687511"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"19709310"|"19687483"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar component makes up 60 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, foothills. The parent material consists of gravelly colluvium over residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BA031MT Limy Droughty (lydr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709311"|"19687484"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709312"|"19687485"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19709313"|"19687486"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shineberger component makes up 10 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BC135MT Shallow Limy Droughty (swlydr)   Lru 43b-c ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19708520"|"19686693"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19708521"|"19686694"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708522"|"19686695"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"19708523"|"19686696"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19708524"|"19686697"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on intermontane basins, hillslopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19708525"|"19686698"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"19708526"|"19686699"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"19708527"|"19686700"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins, escarpments. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BD038MT Droughty Steep (drstp)   Lru 44b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19708528"|"19686701"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 80 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS690MT Silty-droughty (sidr) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709399"|"19687572"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19709400"|"19687573"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"19709401"|"19687574"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"19709402"|"19687575"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"19709403"|"19687576"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar, very stony component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on foothills, hillslopes. The parent material consists of colluvium over residuum weathered from basalt. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709035"|"19687208"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar, extremely bouldery component makes up 15 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillslopes, foothills. The parent material consists of colluvium over residuum weathered from basalt. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709036"|"19687209"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709037"|"19687210"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twinadams soil is a minor component."|"19709038"|"19687211"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on foothills, hillslopes. The parent material consists of colluvium over residuum weathered from basalt. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709039"|"19687212"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709040"|"19687213"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"19709041"|"19687214"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"19710131"|"19688304"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"19710132"|"19688305"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19710133"|"19688306"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanson soil is a minor component."|"19710134"|"19688307"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hanson component makes up 50 percent of the map unit. Slopes are 25 to 45 percent. This component is on hills, moraines. The parent material consists of gravelly colluvium derived from limestone and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710135"|"19688308"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre, rarely flooded component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710329"|"19688502"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"19710330"|"19688503"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"19710331"|"19688504"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710332"|"19688505"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"19710333"|"19688506"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19710334"|"19688507"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709722"|"19687895"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19709723"|"19687896"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19710304"|"19688477"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills, stream terraces. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710305"|"19688478"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19710306"|"19688479"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709940"|"19688113"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"19709941"|"19688114"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"19709942"|"19688115"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709513"|"19687686"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709514"|"19687687"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"19709515"|"19687688"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"19709516"|"19687689"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"19709517"|"19687690"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709518"|"19687691"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710136"|"19688309"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nuley component makes up 85 percent of the map unit. Slopes are 2 to 12 percent. This component is on hills, structural benches. The parent material consists of loamy residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS335MT Sandy (sy) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710137"|"19688310"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"19710138"|"19688311"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nuley component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on structural benches, hills. The parent material consists of loamy residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710139"|"19688312"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"19710140"|"19688313"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710141"|"19688314"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nuley soil is a minor component."|"19710142"|"19688315"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nuley soil is a minor component."|"19710143"|"19688316"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nuley component makes up 65 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, structural benches. The parent material consists of loamy residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BA040MT Loamy Steep (lostp)   Lru 43b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709724"|"19687897"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709725"|"19687898"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"19709726"|"19687899"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nuley soil is a minor component."|"19709727"|"19687900"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ryell, rarely flooded component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS342MT Limy-droughty (lydr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710335"|"19688508"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra, rarely flooded component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 21 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS331MT Gravel (gr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710336"|"19688509"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"19710337"|"19688510"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"19710338"|"19688511"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"19710339"|"19688512"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, stream terraces, intermontane basins. The parent material consists of alluvium and/or slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709908"|"19688081"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709909"|"19688082"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, cobbly loam soil is a minor component."|"19709910"|"19688083"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 35 percent of the map unit. Slopes are 0 to 1 percent. This component is on stream terraces. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BY150MT Subirrigated (sb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"19708589"|"19686762"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"19708590"|"19686763"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anamac soil is a minor component."|"19708591"|"19686764"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra, stony component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA110MT Sandy (sy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"19708592"|"19686765"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vendome soil is a minor component."|"19708593"|"19686766"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"19708584"|"19686757"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonebasin soil is a minor component."|"19708585"|"19686758"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"19708586"|"19686759"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun, occasionally flooded component makes up 50 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BY081MT Riparian Subirrigated (rsb)   Lru 44b-y ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"19708587"|"19686760"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA110MT Sandy (sy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"19708588"|"19686761"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beeftrail, very stony component makes up 30 percent of the map unit. Slopes are 8 to 30 percent. This component is on south tending hills. The parent material consists of residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BA110MT Sandy (sy)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7e.    There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 6 within 30 inches of the soil surface."|"19710250"|"19688423"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minestope, very stony component makes up 40 percent of the map unit. Slopes are 8 to 30 percent. This component is on south tending hills. The parent material consists of residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BA138MT Shallow Droughty (swdr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7e.    There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"19710251"|"19688424"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minestope soil is a minor component."|"19710252"|"19688425"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19710253"|"19688426"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zonite soil is a minor component."|"19710254"|"19688427"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708764"|"19686937"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19708765"|"19686938"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"19708766"|"19686939"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 31 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708767"|"19686940"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 29 percent of the map unit. Slopes are 45 to 70 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19708768"|"19686941"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, very stony soil is a minor component."|"19710060"|"19688233"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dyce, stony soil is a minor component."|"19710061"|"19688234"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore, very stony component makes up 19 percent of the map unit. Slopes are 4 to 45 percent. This component is on ridges on anticlines, mountains. The parent material consists of colluvium and/or residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Unspecified ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"19710062"|"19688235"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ferball, stony component makes up 20 percent of the map unit. Slopes are 4 to 45 percent. This component is on mountains, anticlines on mountain slopes, strike valleys on mountain slopes. The parent material consists of colluvium and/or slope alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Thin Loamy (tlo)   Lru 43b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19710063"|"19688236"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"19710064"|"19688237"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackleaf, extremely stony soil is a minor component."|"19710065"|"19688238"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twinadams, stony component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, scarp slopes on anticlines. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 24 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710066"|"19688239"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19710067"|"19688240"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Madigan component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, hills. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, paralithic, is 25 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d, Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent.  "|"19710073"|"19688246"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Woodhurst soil is a minor component."|"19710074"|"19688247"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710075"|"19688248"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman soil is a minor component."|"19710076"|"19688249"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, hillslopes. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Droughty Steep (drstp)   Lru 43b-d, Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710077"|"19688250"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot, very stony component makes up 25 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountains, hills. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19709376"|"19687549"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709377"|"19687550"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar, very stony component makes up 40 percent of the map unit. Slopes are 25 to 50 percent. This component is on hills, mountains. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock over residuum. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709378"|"19687551"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"19709379"|"19687552"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hangmans soil is a minor component."|"19709380"|"19687553"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, very stony component makes up 20 percent of the map unit. Slopes are 8 to 50 percent. This component is on ridges, hillslopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Droughty (lydr)   Lru 43b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709364"|"19687537"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polaris soil is a minor component."|"19709365"|"19687538"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore, extremely stony component makes up 45 percent of the map unit. Slopes are 8 to 50 percent. This component is on ridges, hillslopes, mountains. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland, Shallow Limy Droughty (swlydr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"19709366"|"19687539"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709367"|"19687540"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kelmbeck soil is a minor component."|"19709368"|"19687541"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709369"|"19687542"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"19709358"|"19687531"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709359"|"19687532"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, very stony soil is a minor component."|"19709360"|"19687533"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709361"|"19687534"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 35 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from limestone over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"19709362"|"19687535"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kelmbeck component makes up 25 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountains, mountain slopes, ridges. The parent material consists of colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Fractured Rock Limy (frly)   Lru 43b-y, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"19709363"|"19687536"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709370"|"19687543"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, very stony component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru A (9-14 Pz), Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709371"|"19687544"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium and/or colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19709372"|"19687545"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19709373"|"19687546"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar, very stony component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, intermontane basins. The parent material consists of colluvium over residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709374"|"19687547"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackleaf, extremely stony soil is a minor component."|"19709375"|"19687548"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709681"|"19687854"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Spudbar component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on ridges, hillslopes, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709682"|"19687855"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19709683"|"19687856"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polaris soil is a minor component."|"19709684"|"19687857"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot, extremely stony component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on hillslopes, intermontane basins, ridges. The parent material consists of slope alluvium and/or colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-a, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"19709685"|"19687858"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19709686"|"19687859"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"19709687"|"19687860"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, extremely stony component makes up 40 percent of the map unit. Slopes are 35 to 75 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"19709347"|"19687520"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin, extremely stony soil is a minor component."|"19709348"|"19687521"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat, occasionally flooded soil is a minor component."|"19709349"|"19687522"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss soil is a minor component."|"19709350"|"19687523"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"19709351"|"19687524"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very stony component makes up 15 percent of the map unit. Slopes are 35 to 75 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"19709352"|"19687525"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scudder, stony soil is a minor component."|"19708760"|"19686933"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19708761"|"19686934"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"19708762"|"19686935"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, extremely stony component makes up 25 percent of the map unit. Slopes are 45 to 80 percent. This component is on mountains, mountain slopes, canyon walls. The parent material consists of colluvium derived from limestone and dolomite over calcareous residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE135MT Shallow Cool Woodland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"19708763"|"19686936"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709856"|"19688029"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"19709857"|"19688030"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scudder, stony component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"19709858"|"19688031"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, extremely stony component makes up 35 percent of the map unit. Slopes are 25 to 80 percent. This component is on mountains, mountain slopes, canyon walls. The parent material consists of colluvium derived from limestone and dolomite over calcareous residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE135MT Shallow Cool Woodland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"19709859"|"19688032"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hardhart, very stony soil is a minor component."|"19709860"|"19688033"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, bouldery component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru A (9-14 Pz), Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709894"|"19688067"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19709895"|"19688068"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twinadams soil is a minor component."|"19709896"|"19688069"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted, stony component makes up 15 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19709897"|"19688070"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackleaf, stony soil is a minor component."|"19709898"|"19688071"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dyce soil is a minor component."|"19709899"|"19688072"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"19709900"|"19688073"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, extremely bouldery component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on escarpments, hills, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19709901"|"19688074"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"19710472"|"19688645"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thessvo soil is a minor component."|"19710473"|"19688646"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19710474"|"19688647"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 60 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Loamy (lo)   Lru 44b-a, Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710475"|"19688648"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 25 percent of the map unit. Slopes are 1 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Loamy (lo)   Lru 44b-a, Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"19710476"|"19688649"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"19710287"|"19688460"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"19710288"|"19688461"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dyce, stony soil is a minor component."|"19710289"|"19688462"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, stony component makes up 40 percent of the map unit. Slopes are 8 to 45 percent. This component is on escarpments, hills, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19710290"|"19688463"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 30 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru A (9-14 Pz), Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19710291"|"19688464"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot, very stony soil is a minor component."|"19710292"|"19688465"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, extremely stony component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on escarpments, hills, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19710293"|"19688466"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 44b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"19710447"|"19688620"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haxby soil is a minor component."|"19710448"|"19688621"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polaris soil is a minor component."|"19710449"|"19688622"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Geohrock, very stony component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Droughty (dr)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"19710450"|"19688623"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"19710451"|"19688624"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru A (9-14 Pz), Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19710452"|"19688625"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"19710453"|"19688626"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 20 percent of the map unit. Slopes are 1 to 4 percent. This component is on mountains, flood plains on drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland, Meadow (m)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"19708594"|"19686767"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently flooded component makes up 35 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains on drainageways, mountains. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BY181MT Bottomland, Wet Meadow (wm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"19708595"|"19686768"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crookedrun soil is a minor component."|"19708596"|"19686769"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truaxcreek soil is a minor component."|"19708597"|"19686770"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Medicinelodge, frequently flooded component makes up 25 percent of the map unit. Slopes are 1 to 6 percent. This component is on flood plains on drainageways, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 14 inches) during May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland, Meadow (m)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"19708598"|"19686771"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 65 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, ridges. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709455"|"19687628"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"19709456"|"19687629"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges, mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"19709457"|"19687630"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19709458"|"19687631"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"19709902"|"19688075"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 80 percent of the map unit. Slopes are 2 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of slope alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy (lo)   Lru 44b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709903"|"19688076"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"19709904"|"19688077"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"19709905"|"19688078"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19709906"|"19688079"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"19709907"|"19688080"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"19709465"|"19687638"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"19709466"|"19687639"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"19709467"|"19687640"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, stony component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"19709468"|"19687641"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709469"|"19687642"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"19709470"|"19687643"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, extremely bouldery component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"19709471"|"19687644"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"19708857"|"19687030"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redsage component makes up 90 percent of the map unit. Slopes are 1 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy (ly)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"19708858"|"19687031"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"19708859"|"19687032"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP819MT Limy Droughty (lydr)   Lru 43b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"19709448"|"19687621"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gullied land soil is a minor component."|"19709449"|"19687622"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polaris, stony soil is a minor component."|"19709450"|"19687623"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"19709451"|"19687624"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson, stony soil is a minor component."|"19709452"|"19687625"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"19709453"|"19687626"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, extremely stony soil is a minor component."|"19709454"|"19687627"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, low hills. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19710068"|"19688241"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Madigan component makes up 25 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, low hills. The parent material consists of slope alluvium over residuum weathered from andesite. Depth to a root restrictive layer, bedrock, paralithic, is 25 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD032MT Loamy (lo)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent.  "|"19710069"|"19688242"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"19710070"|"19688243"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, very stony soil is a minor component."|"19710071"|"19688244"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"19710072"|"19688245"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, mountains. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"19709660"|"19687833"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, hills. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"19709661"|"19687834"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shineberger, stony soil is a minor component."|"19709662"|"19687835"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"19709663"|"19687836"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"19709664"|"19687837"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19709665"|"19687838"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"19709323"|"19687496"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"19709324"|"19687497"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"19709325"|"19687498"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve, very stony soil is a minor component."|"19709326"|"19687499"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"19709327"|"19687500"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, extremely stony component makes up 15 percent of the map unit. Slopes are 20 to 60 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"19709328"|"19687501"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, very stony component makes up 50 percent of the map unit. Slopes are 20 to 60 percent. This component is on hills, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"19709329"|"19687502"
