08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120253"|"21328254"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120254"|"21328255"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absher component makes up 90 percent of the map unit. Slopes are 0 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE634MT Panspots (ps)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"21120255"|"21328256"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Benz soil is a minor component."|"21120256"|"21328257"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"21120257"|"21328258"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21120258"|"21328259"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21120259"|"21328260"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21120260"|"21328261"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21120261"|"21328262"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"21120262"|"21328263"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21120263"|"21328264"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hanly component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120264"|"21328265"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hanly component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120265"|"21328266"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21120266"|"21328267"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hanly component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120267"|"21328268"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120268"|"21328269"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120269"|"21328270"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120270"|"21328271"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120271"|"21328272"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120272"|"21328273"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120273"|"21328274"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120274"|"21328275"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Benz component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE011MT Saline Upland (su)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 20 within 30 inches of the soil surface."|"21120275"|"21328276"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21120276"|"21328277"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21120277"|"21328278"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21120278"|"21328279"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 35 percent of the map unit. Slopes are 2 to 4 percent. This component is on drainageways on dissected alluvial fans on plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120279"|"21328280"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21120280"|"21328281"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Benz component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on dissected alluvial fans on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE011MT Saline Upland (su)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21120281"|"21328282"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120282"|"21328283"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanly soil is a minor component."|"21120283"|"21328284"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21120284"|"21328285"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21120285"|"21328286"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 35 percent of the map unit. Slopes are 8 to 80 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE005MT Clayey-steep (cystp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120286"|"21328287"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120287"|"21328288"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yetull component makes up 45 percent of the map unit. Slopes are 8 to 70 percent. This component is on hills on plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120288"|"21328289"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120289"|"21328290"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120290"|"21328291"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120291"|"21328292"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120292"|"21328293"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on plains. The parent material consists of silty slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120293"|"21328294"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120294"|"21328295"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 35 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120295"|"21328296"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120296"|"21328297"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on draws on plains, flood plains on plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE007MT Overflow (ov)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120297"|"21328298"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120298"|"21328299"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on plains, draws on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE007MT Overflow (ov)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120299"|"21328300"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanly soil is a minor component."|"21120300"|"21328301"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21120301"|"21328302"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces on plains, draws on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120302"|"21328303"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120303"|"21328304"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120304"|"21328305"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120305"|"21328306"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120306"|"21328307"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"21120307"|"21328308"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120308"|"21328309"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120309"|"21328310"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yetull component makes up 35 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120310"|"21328311"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120311"|"21328312"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 60 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120312"|"21328313"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120313"|"21328314"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120314"|"21328315"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120315"|"21328316"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 60 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120316"|"21328317"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yetull component makes up 35 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120317"|"21328318"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"21120318"|"21328319"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120319"|"21328320"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 85 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE005MT Clayey-steep (cystp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120320"|"21328321"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120321"|"21328322"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21120322"|"21328323"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120323"|"21328324"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wolf Point soil is a minor component."|"21120324"|"21328325"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120325"|"21328326"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21120326"|"21328327"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120327"|"21328328"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120328"|"21328329"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wolf Point soil is a minor component."|"21120329"|"21328330"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21120330"|"21328331"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 90 percent of the map unit. Slopes are 20 to 40 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120331"|"21328332"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120332"|"21328333"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120333"|"21328334"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120334"|"21328335"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120335"|"21328336"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120336"|"21328337"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21120337"|"21328338"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120338"|"21328339"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120339"|"21328340"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"21120340"|"21328341"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 55 percent of the map unit. Slopes are 15 to 40 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120341"|"21328342"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kirby soil is a minor component."|"21120342"|"21328343"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120343"|"21328344"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120344"|"21328345"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120345"|"21328346"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120346"|"21328347"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120347"|"21328348"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yetull component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120348"|"21328349"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120349"|"21328350"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kirby soil is a minor component."|"21120752"|"21328754"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"21120753"|"21328755"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120754"|"21328756"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120755"|"21328757"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE005MT Clayey-steep (cystp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120756"|"21328758"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 50 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 12 to 24 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120757"|"21328759"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120350"|"21328351"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kirby component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE017MT Very Shallow (vsw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120351"|"21328352"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120352"|"21328353"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120353"|"21328354"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120354"|"21328355"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lihill component makes up 85 percent of the map unit. Slopes are 4 to 20 percent. This component is on paleoterraces on plains. The parent material consists of sandy alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120355"|"21328356"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120356"|"21328357"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120357"|"21328358"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120358"|"21328359"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120359"|"21328360"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wolf Point component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of stratified clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120360"|"21328361"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21120361"|"21328362"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120362"|"21328363"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"21120363"|"21328364"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21120364"|"21328365"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21120365"|"21328366"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marias component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120366"|"21328367"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120367"|"21328368"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wolf Point soil is a minor component."|"21120368"|"21328369"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21120369"|"21328370"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21120370"|"21328371"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marias component makes up 85 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120371"|"21328372"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21120372"|"21328373"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120373"|"21328374"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marias component makes up 85 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120374"|"21328375"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120375"|"21328376"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21120376"|"21328377"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 85 percent of the map unit. Slopes are 8 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120377"|"21328378"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"21120378"|"21328379"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120379"|"21328380"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21120380"|"21328381"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120381"|"21328382"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120382"|"21328383"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120383"|"21328384"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutton component makes up 90 percent of the map unit. Slopes are 1 to 4 percent. This component is on low hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120384"|"21328385"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutton soil is a minor component."|"21120385"|"21328386"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120386"|"21328387"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120387"|"21328388"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120388"|"21328389"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutton component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120389"|"21328390"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutton component makes up 50 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120390"|"21328391"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 30 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120391"|"21328392"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120392"|"21328393"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120393"|"21328394"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120394"|"21328395"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21120395"|"21328396"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutton component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120396"|"21328397"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120397"|"21328398"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120398"|"21328399"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120399"|"21328400"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21120400"|"21328401"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanly soil is a minor component."|"21120401"|"21328402"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21120402"|"21328403"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saline land component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains, stream terraces on valleys. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 5 percent. This component is in the R058AE012MT Saline Lowland (sl)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120403"|"21328404"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21120404"|"21328405"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sonnett soil is a minor component."|"21120767"|"21328769"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120768"|"21328770"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120769"|"21328771"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120770"|"21328772"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge, warm component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of clayey alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120771"|"21328773"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of clayey alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120731"|"21328732"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Creed soil is a minor component."|"21120732"|"21328733"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21120733"|"21328734"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120734"|"21328735"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120735"|"21328736"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120405"|"21328406"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120406"|"21328407"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120407"|"21328408"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120408"|"21328409"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120409"|"21328410"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120410"|"21328411"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills, plains. The parent material consists of coarse-loamy alluvium and/or coarse-loamy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120411"|"21328412"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120412"|"21328413"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120413"|"21328414"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120414"|"21328415"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21120415"|"21328416"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120416"|"21328417"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"21120417"|"21328418"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terrace escarpments component makes up 100 percent of the map unit. Slopes are 15 to 70 percent. This component is on stream terraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21120418"|"21328419"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tinsley component makes up 55 percent of the map unit. Slopes are 15 to 65 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE016MT Gravel (gr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120419"|"21328420"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120420"|"21328421"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120421"|"21328422"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lihill soil is a minor component."|"21120422"|"21328423"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 30 percent of the map unit. Slopes are 15 to 65 percent. This component is on paleoterraces on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120423"|"21328424"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21120424"|"21328425"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tinsley component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE016MT Gravel (gr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120425"|"21328426"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tinsley component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE016MT Gravel (gr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120426"|"21328427"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120427"|"21328428"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120428"|"21328429"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120429"|"21328430"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lihill soil is a minor component."|"21120430"|"21328431"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120431"|"21328432"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanly soil is a minor component."|"21120432"|"21328433"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120433"|"21328434"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21120434"|"21328435"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wolf Point soil is a minor component."|"21120435"|"21328436"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120436"|"21328437"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21120437"|"21328438"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wolf Point soil is a minor component."|"21120438"|"21328439"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120439"|"21328440"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120440"|"21328441"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120441"|"21328442"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120442"|"21328443"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120443"|"21328444"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120444"|"21328445"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120445"|"21328446"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120446"|"21328447"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120447"|"21328448"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120448"|"21328449"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120449"|"21328450"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120450"|"21328451"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120451"|"21328452"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120452"|"21328453"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120453"|"21328454"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120454"|"21328455"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120455"|"21328456"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120456"|"21328457"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120457"|"21328458"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120458"|"21328459"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120459"|"21328460"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120460"|"21328461"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 55 percent of the map unit. Slopes are 2 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120461"|"21328462"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 35 percent of the map unit. Slopes are 2 to 4 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120462"|"21328463"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120463"|"21328464"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120464"|"21328465"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120465"|"21328466"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21120466"|"21328467"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 45 percent of the map unit. Slopes are 4 to 8 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120467"|"21328468"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lihill soil is a minor component."|"21120468"|"21328469"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120469"|"21328470"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 45 percent of the map unit. Slopes are 4 to 8 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120470"|"21328471"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21120471"|"21328472"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"21120472"|"21328473"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21120473"|"21328474"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 90 percent of the map unit. Slopes are 0 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE014MT Dense Clay (dc)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21120474"|"21328475"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21120724"|"21328725"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120725"|"21328726"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21120726"|"21328727"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120727"|"21328728"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"21120728"|"21328729"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"21120729"|"21328730"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21120730"|"21328731"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21120682"|"21328683"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21120683"|"21328684"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"21120684"|"21328685"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21120685"|"21328686"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21120686"|"21328687"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"21120687"|"21328688"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120688"|"21328689"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21120711"|"21328712"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120712"|"21328713"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21120713"|"21328714"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY706MT Loamy (lo) ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120714"|"21328715"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"21120715"|"21328716"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21120716"|"21328717"
06/25/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21120717"|"21328718"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21120689"|"21328690"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"21120690"|"21328691"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120691"|"21328692"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21120692"|"21328693"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120693"|"21328694"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21120694"|"21328695"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"21120695"|"21328696"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21120696"|"21328697"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"21120697"|"21328698"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahl soil is a minor component."|"21120698"|"21328699"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 75 percent of the map unit. Slopes are 15 to 60 percent. This component is on hillslopes on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY040MT Loamy Steep (lostp)   Lru 53a-y ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120699"|"21328700"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arnegard soil is a minor component."|"21120700"|"21328701"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21120701"|"21328702"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"21120702"|"21328703"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"21120475"|"21328476"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"21120476"|"21328477"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 40 percent of the map unit. Slopes are 15 to 65 percent. This component is on coulees on till plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120477"|"21328478"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120478"|"21328479"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on coulees on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120479"|"21328480"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (Si) RRU 58A-E 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120511"|"21328512"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21120512"|"21328513"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"21120513"|"21328514"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120514"|"21328515"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21120503"|"21328504"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120504"|"21328505"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"21120505"|"21328506"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE001MT Silty (Si) RRU 58A-E 10-14 P.Z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120506"|"21328507"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"21120778"|"21328780"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120779"|"21328781"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambeth component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120780"|"21328782"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120781"|"21328783"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21120782"|"21328784"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alona soil is a minor component."|"21120783"|"21328785"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21120784"|"21328786"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21120736"|"21328737"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 40 percent of the map unit. Slopes are 4 to 12 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21120737"|"21328738"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tricart soil is a minor component."|"21120738"|"21328739"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 15 percent of the map unit. Slopes are 4 to 12 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120739"|"21328740"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21120740"|"21328741"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120741"|"21328742"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambeth component makes up 30 percent of the map unit. Slopes are 4 to 12 percent. This component is on low hills on sedimentary plains. The parent material consists of silty residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120742"|"21328743"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21120743"|"21328744"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambeth component makes up 25 percent of the map unit. Slopes are 15 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120744"|"21328745"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120745"|"21328746"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21120746"|"21328747"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21120746"|"21328748"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 45 percent of the map unit. Slopes are 12 to 15 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21120747"|"21328749"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 20 percent of the map unit. Slopes are 12 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120748"|"21328750"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21120749"|"21328751"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120750"|"21328752"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21120751"|"21328753"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eapa component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (Si) RRU 58A-E 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120500"|"21328501"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120501"|"21328502"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120502"|"21328503"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120481"|"21328482"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120482"|"21328483"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Floweree component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (Si) RRU 58A-E 10-14 P.Z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120483"|"21328484"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120484"|"21328485"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120485"|"21328486"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Degrand soil is a minor component."|"21120486"|"21328487"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21120487"|"21328488"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spinekop soil is a minor component."|"21120488"|"21328489"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin component makes up 85 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120489"|"21328490"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120507"|"21328508"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin component makes up 65 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120508"|"21328509"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eapa component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120509"|"21328510"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"21120510"|"21328511"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon component makes up 50 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120718"|"21328719"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21120719"|"21328720"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tricart component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of gravelly slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE016MT Gravel (gr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120720"|"21328721"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120721"|"21328722"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littlemo soil is a minor component."|"21120722"|"21328723"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120723"|"21328724"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsheep soil is a minor component."|"21120494"|"21328495"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120495"|"21328496"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Peerless component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120496"|"21328497"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120497"|"21328498"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Subwell component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE191MT Shallow To Gravel (swgr)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120498"|"21328499"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna, saline substratum soil is a minor component."|"21120758"|"21328760"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree, warm soil is a minor component."|"21120759"|"21328761"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall, warm soil is a minor component."|"21120760"|"21328762"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120761"|"21328763"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alona soil is a minor component."|"21120762"|"21328764"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21120772"|"21328774"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21120773"|"21328775"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120774"|"21328776"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21120775"|"21328777"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120776"|"21328778"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of and/or silty alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120777"|"21328779"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21120490"|"21328491"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21120491"|"21328492"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21120492"|"21328493"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21120493"|"21328494"
07/16/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21120499"|"21328500"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21120480"|"21328481"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"21120665"|"21328666"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsheep soil is a minor component."|"21120666"|"21328667"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21120667"|"21328668"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tinsley soil is a minor component."|"21120668"|"21328669"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"21120703"|"21328704"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21120704"|"21328705"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21120705"|"21328706"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21120706"|"21328707"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120707"|"21328708"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120708"|"21328709"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120709"|"21328710"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21120710"|"21328711"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"21120585"|"21328586"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on low hills on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120586"|"21328587"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on low hills on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120587"|"21328588"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"21120522"|"21328523"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120523"|"21328524"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120524"|"21328525"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120515"|"21328516"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120516"|"21328517"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"21120517"|"21328518"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120518"|"21328519"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry, saline substratum soil is a minor component."|"21120519"|"21328520"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"21120520"|"21328521"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120521"|"21328522"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Golva component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120525"|"21328526"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120526"|"21328527"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120527"|"21328528"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"21120537"|"21328538"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120538"|"21328539"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"21120539"|"21328540"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"21120540"|"21328541"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"21120541"|"21328542"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120542"|"21328543"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120532"|"21328533"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"21120533"|"21328534"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21120534"|"21328535"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"21120535"|"21328536"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120536"|"21328537"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21120528"|"21328529"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"21120529"|"21328530"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"21120530"|"21328531"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120531"|"21328532"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120550"|"21328551"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120551"|"21328552"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lisk soil is a minor component."|"21120552"|"21328553"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"21120553"|"21328554"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regent soil is a minor component."|"21120554"|"21328555"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambert component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21120555"|"21328556"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120556"|"21328557"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120557"|"21328558"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120543"|"21328544"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21120544"|"21328545"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regent soil is a minor component."|"21120545"|"21328546"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambert component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21120546"|"21328547"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120547"|"21328548"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Golva soil is a minor component."|"21120548"|"21328549"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120549"|"21328550"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"21120558"|"21328559"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Banks, loamy fine sand component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120559"|"21328560"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"21120560"|"21328561"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"21120561"|"21328562"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Banks, fine sand component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120562"|"21328563"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Banks, fine sandy loam component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on valleys. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21120563"|"21328564"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on plains. The parent material consists of silty slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120564"|"21328565"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 35 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120565"|"21328566"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120566"|"21328567"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120567"|"21328568"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120568"|"21328569"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120569"|"21328570"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains on plains, draws on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120588"|"21328589"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cherry component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces on plains, draws on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21120589"|"21328590"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on draws on plains, flood plains on plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120590"|"21328591"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"21120591"|"21328592"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21120592"|"21328593"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21120593"|"21328594"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120594"|"21328595"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120595"|"21328596"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"21120596"|"21328597"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120597"|"21328598"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 60 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120598"|"21328599"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blanchard component makes up 35 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120599"|"21328600"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"21120600"|"21328601"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 60 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120601"|"21328602"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120602"|"21328603"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120603"|"21328604"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blanchard component makes up 35 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120604"|"21328605"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"21120605"|"21328606"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"21120669"|"21328670"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"21120670"|"21328671"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120671"|"21328672"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21120672"|"21328673"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regent soil is a minor component."|"21120673"|"21328674"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120674"|"21328675"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 55 percent of the map unit. Slopes are 20 to 40 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120675"|"21328676"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120614"|"21328615"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120615"|"21328616"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"21120616"|"21328617"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blanchard component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21120617"|"21328618"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120618"|"21328619"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120619"|"21328620"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21120620"|"21328621"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimyaw component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE005MT Clayey-steep (cystp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120676"|"21328677"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regent soil is a minor component."|"21120677"|"21328678"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120678"|"21328679"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 50 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120679"|"21328680"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"21120680"|"21328681"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"21120681"|"21328682"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 35 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE080MT Very Shallow (vsw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120652"|"21328653"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120653"|"21328654"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120654"|"21328655"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimyaw soil is a minor component."|"21120655"|"21328656"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120656"|"21328657"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohler component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of stratified clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE061MT Clayey (cy) (legacy) Rru 53ae ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120621"|"21328622"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"21120622"|"21328623"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"21120623"|"21328624"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120624"|"21328625"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120606"|"21328607"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"21120607"|"21328608"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120608"|"21328609"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"21120609"|"21328610"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces on plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21120610"|"21328611"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120611"|"21328612"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"21120612"|"21328613"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles soil is a minor component."|"21120613"|"21328614"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120632"|"21328633"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21120633"|"21328634"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21120634"|"21328635"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanchard soil is a minor component."|"21120635"|"21328636"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tally component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on till plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120636"|"21328637"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120637"|"21328638"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21120628"|"21328629"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21120629"|"21328630"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120630"|"21328631"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tally component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120631"|"21328632"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120625"|"21328626"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tally component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on swales on till plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120626"|"21328627"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"21120627"|"21328628"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120643"|"21328644"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"21120644"|"21328645"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120645"|"21328646"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"21120646"|"21328647"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trembles component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on valleys. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120638"|"21328639"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"21120639"|"21328640"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"21120640"|"21328641"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cherry soil is a minor component."|"21120641"|"21328642"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"21120642"|"21328643"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21120647"|"21328648"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Turner component makes up 55 percent of the map unit. Slopes are 2 to 4 percent. This component is on paleoterraces on plains. The parent material consists of loamy alluvium over gravelly alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21120648"|"21328649"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21120649"|"21328650"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverton component makes up 35 percent of the map unit. Slopes are 2 to 4 percent. This component is on paleoterraces on plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE079MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120650"|"21328651"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"21120651"|"21328652"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21120659"|"21328660"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saline land component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 5 percent. This component is in the R053AE072MT Saline Overflow (sov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21120660"|"21328661"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21120657"|"21328658"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Banks soil is a minor component."|"21120658"|"21328659"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"21120580"|"21328581"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Telstad soil is a minor component."|"21120581"|"21328582"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 40 percent of the map unit. Slopes are 15 to 65 percent. This component is on coulees on till plains. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21120582"|"21328583"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Joplin soil is a minor component."|"21120583"|"21328584"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hillon component makes up 45 percent of the map unit. Slopes are 15 to 65 percent. This component is on coulees on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120584"|"21328585"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"21120577"|"21328578"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Telstad component makes up 46 percent of the map unit. Slopes are 4 to 8 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE081MT Silty (Si) 10-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120578"|"21328579"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Joplin component makes up 44 percent of the map unit. Slopes are 4 to 8 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE081MT Silty (Si) 10-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120579"|"21328580"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Joplin soil is a minor component."|"21120574"|"21328575"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Telstad component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21120575"|"21328576"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"21120576"|"21328577"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120570"|"21328571"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alona soil is a minor component."|"21120571"|"21328572"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21120572"|"21328573"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ismay component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during May, June, July, August. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE012MT Saline Lowland (sl)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"21120573"|"21328574"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"21120661"|"21328662"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alona component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE193MT Silty-saline (sis)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"21120662"|"21328663"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ismay soil is a minor component."|"21120663"|"21328664"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Alona, saline soil is a minor component."|"21120664"|"21328665"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21120763"|"21328765"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21120764"|"21328766"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21120765"|"21328767"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin, warm component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21120766"|"21328768"
