"10A"|"Havre loam, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.06|7.98|15.74|23.49|"Well drained"|"Well drained"|"B"|"2"|75|"3"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.227|"Slight"|"5"|0.661|"344469"
"11A"|"Havre-Glendive complex, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.03|7.84|15.07|22.3|"Well drained"|"Well drained"|"B"|"2"|50|"3"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.173|"Slight"|"4"|0.308|"344470"
"12A"|"Havre-Harlake complex, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.01|7.94|15.69|23.43|"Well drained"|"Well drained"|"B"|"2"|50|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.286|"Slight"|"3"|0.743|"344473"
"131C"|"Delpoint-Yamacall loams, 2 to 8 percent slopes"||5|5.3|56|||"None"|"None"|"0"|4.12|8.01|11.56|14.31|"Well drained"|"Well drained"|"C"|"3"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Moderate"|"0"|0.632|"344474"
"132B"|"Twilight-Blacksheep sandy loams, 2 to 8 percent slopes"||8|7.5|46|||"None"|"None"|"0"|3.42|6.38|9.16|9.61|"Well drained"|"Well drained"|"B"|"4"|54|"4"|52|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.962|"344475"
"138B"|"Zatoville-Orinoco silty clay loams, 2 to 8 percent slopes"||5|5|61|||"None"|"None"|"0"|4|7.44|11.48|14.88|"Well drained"|"Well drained"|"C"||95|"6"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Moderate"|"0"|1|"344476"
"13A"|"Havre loam, calcareous, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.15|8.09|15.9|23.71|"Well drained"|"Well drained"|"B"|"4"|93|"4"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.224|"Slight"|"3"|0.116|"344477"
"140B"|"Kobase-Megonot silty clay loams, 1 to 8 percent slopes"||5|4.9|89|||"None"|"None"|"0"|4.24|7.8|13.51|17.45|"Well drained"|"Well drained"|"D"||53|"3"|45|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.332|"Moderate"|"0"|1|"344478"
"140C"|"Kobase-Megonot silty clay loams, calcareous, 1 to 8 percent slopes"||5|4.9|89|||"None"|"None"|"0"|4.24|7.8|13.51|17.45|"Well drained"|"Well drained"|"D"||53|"4"|87|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.332|"Moderate"|"0"|1|"344479"
"142A"|"Rothiemay loam, calcareous, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.2|8.1|15.08|21.93|"Well drained"|"Well drained"|"C"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.176|"Slight"|"0"|0.258|"344480"
"142B"|"Rothiemay loam, calcareous, 2 to 8 percent slopes"||5|4.7||||"None"|"None"|"0"|4.2|8.1|15.08|21.93|"Well drained"|"Well drained"|"C"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.176|"Moderate"|"0"|0.258|"344481"
"142C"|"Rothiemay-Crago complex, 4 to 15 percent slopes"||10|9.6||||"None"|"None"|"0"|3.61|6.93|12.25|17.26|"Well drained"|"Well drained"|"C"|"4"|98|"4"|68|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.191|"Severe"|"0"|0.494|"344482"
"14A"|"Havre, calcareous-Glendive complex, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.03|7.84|15.12|22.4|"Well drained"|"Well drained"|"B"|"4"|83|"4"|83|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Slight"|"7"|0.335|"344483"
"14B"|"Havre, calcareous-Glendive complex, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|3.81|7.61|14.74|21.84|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.143|"Slight"|"5"|0.62|"344484"
"152A"|"Eapa-Attewan loams, 0 to 2 percent slopes"||1|1.7||||"None"|"None"|"0"|4.25|8.28|15.04|21.39|"Well drained"|"Well drained"|"B"||50|"3"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.228|"Slight"|"0"|0.47|"344485"
"153C"|"Tanna-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4.18|7.15|8.32|8.48|"Well drained"|"Well drained"|"D"|"3"|58|"3"|58|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.247|"Moderate"|"0"|0.998|"344487"
"153D"|"Cabbart-Tanna loams, 4 to 15 percent slopes"||10|10|41|||"None"|"None"|"0"|4.25|7.16|8.2|8.2|"Well drained"|"Well drained"|"D"||55|"6"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.237|"Severe"|"0"|0.975|"344488"
"158A"|"Ethridge-Verson clay loams, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.34|8.3|14.34|20.09|"Well drained"|"Well drained"|"C"|"3"|90|"3"|95|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.286|"Slight"|"0"|0.95|"344492"
"15A"|"Havre-Harlake complex, calcareous, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.07|8|15.77|23.54|"Well drained"|"Well drained"|"B"|"4"|88|"4"|88|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.31|"Slight"|"5"|0.456|"344493"
"167D"|"Yawdim-Orinoco silty clay loams, 4 to 15 percent slopes"||10|9.6|41|||"None"|"None"|"0"|4.13|7.09|8.14|8.48|"Well drained"|"Well drained"|"D"||98|"6"|93|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.658|"Severe"|"0"|1|"344494"
"167E"|"Yawdim-Orinoco silty clay loams, 15 to 35 percent slopes"||25|24.5|28|||"None"|"None"|"0"|4.06|5.79|6.3|6.3|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.974|"Severe"|"0"|1|"344495"
"16A"|"Havre, occasionally flooded-Yamacall loams, calcareous, 0 to 4 percent slopes"||1|1.4||||"Occasional"|"Occasional"|"0"|4.16|8.28|16.22|24.06|"Well drained"|"Well drained"|"B"|"4"|92|"4"|89|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.219|"Slight"|"3"|0.4|"344496"
"17A"|"Harlake-Havre complex, calcareous, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.08|8.05|15.92|23.78|"Well drained"|"Well drained"|"C"|"4"|93|"4"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.352|"Slight"|"3"|0.538|"344497"
"181D"|"Cabbart-Crago-Delpoint complex, 4 to 15 percent slopes"||10|9.6|41|||"None"|"None"|"0"|2.79|5.09|7.85|9.88|"Well drained"|"Well drained"|"D"||93|"6"|93|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.317|"Severe"|"0"|0.95|"344498"
"181E"|"Cabbart, calcareous-Crago-Delpoint, calcareous complex, 8 to 35 percent slopes"||25|24.1|41|||"None"|"None"|"0"|3.41|5.99|7.17|7.88|"Well drained"|"Well drained"|"D"||98|"6"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.979|"Severe"|"0"|1|"344499"
"189C"|"Rentsac-Cabbart complex, 2 to 15 percent slopes"||9|9.4|41|||"None"|"None"|"0"|2.84|4.58|4.73|4.73|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.109|"Slight"|"0"|1|"344501"
"189E"|"Rentsac-Rock outcrop complex, 15 to 45 percent slopes"||30|28.3|30|||"None"|"None"|"0"|2.55|3.38|3.51|3.51|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.937|"Severe"|"0"|0.992|"344502"
"1E"|"Badland"|||15.5||||||"0"|4.11|6.41|8.88|11.21|||||98|"8"|85|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.696|"Not rated"|"0"|0.927|"344504"
"20B"|"Harlake-Marvan-Vanda silty clays, 0 to 4 percent slopes"||1|1.8||||"None"|"Occasional"|"0"|3.53|6.85|12.88|18.87|"Well drained"|"Well drained"|"D"|"4"|70|"4"|70|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.483|"Slight"|"0"|1|"344505"
"21A"|"McKenzie silty clay, 0 to 2 percent slopes"||1|1.1||30|30|"None"|"None"|"85"|3.6|7.13|14.11|21.08|"Poorly drained"|"Poorly drained"|"D"||90|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.925|"Slight"|"85"|1|"344506"
"22B"|"Nobe-Absher complex, 0 to 4 percent slopes"||2|2||84|84|"None"|"None"|"0"|2.24|4.01|7.41|10.82|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.423|"Slight"|"0"|1|"344507"
"230C"|"Macar loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.29|8.31|15.84|23.04|"Well drained"|"Well drained"|"B"||95|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.085|"Moderate"|"0"|0.05|"344508"
"234F"|"Tibs-Whitecow cobbly clay loams, 25 to 60 percent slopes"||43|39.5||||"None"|"None"|"0"|4.04|6.56|10.34|13.73|"Well drained"|"Well drained"|"C"||100|"7"|84|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.889|"Severe"|"0"|1|"344511"
"23A"|"Gerdrum-Vanda complex, 0 to 8 percent slopes"||4|3.7||||"None"|"None"|"0"|3.3|6.16|11.18|16.08|"Well drained"|"Well drained"|"D"|"6"|50|"6"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.399|"Moderate"|"0"|1|"344512"
"23B"|"Gerdrum-Vanda-Creed complex, 0 to 8 percent slopes"||5|4.1||||"None"|"None"|"0"|3.8|7.44|14.73|21.96|"Well drained"|"Well drained"|"D"|"6"|42|"6"|62|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.349|"Moderate"|"0"|1|"344513"
"23C"|"Gerdrum-Creed loams, 1 to 8 percent slopes"||5|4.7||||"None"|"None"|"0"|3.58|6.48|11.55|16.52|"Well drained"|"Well drained"|"D"|"6"|47|"6"|47|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.357|"Moderate"|"0"|1|"344514"
"240E"|"Ridge-Dast-Rock outcrop complex, 4 to 35 percent slopes"||10|15.9|41|||"None"|"None"|"0"|3.59|6.26|8.03|8.03|"Well drained"|"Well drained"|"D"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.366|"Severe"|"0"|1|"344515"
"241E"|"Twilight-Blacksheep-Rock outcrop complex, 4 to 35 percent slopes"||15|18.6|46|||"None"|"None"|"0"|3.84|7.03|8.42|8.42|"Well drained"|"Well drained"|"D"||100|"4"|35|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.514|"Severe"|"0"|1|"344516"
"242D"|"Dast-Ridge sandy loams, 2 to 8 percent slopes"||5|6.5|46|||"None"|"None"|"0"|3.56|6.58|9.27|9.27|"Well drained"|"Well drained"|"D"||55|"4"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.114|"Moderate"|"0"|1|"344517"
"242F"|"Ridge-Dast sandy loams, 8 to 45 percent slopes"||30|23.4|41|||"None"|"None"|"0"|3.52|6.2|8.2|8.2|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.565|"Severe"|"0"|1|"344518"
"243F"|"Blacksheep-Twilight sandy loams, 8 to 45 percent slopes"||30|23.8|46|||"None"|"None"|"0"|3.81|7.04|8.33|8.33|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.603|"Severe"|"0"|1|"344519"
"245C"|"Lamedeer-Ringling channery loams, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|2.99|5.48|8.89|11.11|"Well drained"|"Well drained"|"B"||95|"4"|65|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.054|"Moderate"|"0"|0.365|"344520"
"245F"|"Lamedeer-Ringling channery loams, 4 to 45 percent slopes"||30|26.8||||"None"|"None"|"0"|2.94|5.15|7.92|9.77|"Well drained"|"Well drained"|"B"||100|"6"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"344521"
"246F"|"Lamedeer-Ringling channery loams, moist, 4 to 45 percent slopes"||30|26.8||||"None"|"None"|"0"|2.94|5.15|7.92|9.77|"Well drained"|"Well drained"|"B"||100|"6"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"344522"
"250E"|"Macmeal-Rock outcrop complex, 4 to 35 percent slopes"||20|19.2||||"None"|"None"|"0"|3.84|6.02|9.38|12.74|"Well drained"|"Well drained"|"C"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.48|"Slight"|"0"|1|"344523"
"251C"|"Savage loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.25|8.16|15.37|22.24|"Well drained"|"Well drained"|"C"|"3"|90|"3"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.125|"Moderate"|"0"|0.965|"344524"
"252D"|"Hilger-Rock outcrop complex, 4 to 35 percent slopes"||20|19.5||||"None"|"None"|"0"|2.35|4.12|7|9.83|"Well drained"|"Well drained"|"B"||95|"6"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.917|"Moderate"|"0"|0.978|"344525"
"252E"|"Hilger stony loam, 4 to 25 percent slopes"||15|15.1||||"None"|"None"|"0"|2.34|4.1|7|9.84|"Well drained"|"Well drained"|"B"||95|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.926|"Moderate"|"0"|0.981|"344526"
"254C"|"Fergus clay loam, 2 to 8 percent slopes"||5|5.6||||"None"|"None"|"0"|4.04|7.82|14.46|20.41|"Well drained"|"Well drained"|"C"|"3"|85|"3"|92|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.1|"Moderate"|"0"|0.402|"344527"
"255C"|"Shambo-Korchea-Barvon loams, 2 to 8 percent slopes"||3|4|74|||"None"|"Rare"|"0"|4.47|8.71|15.94|22.02|"Well drained"|"Well drained"|"B"|"3"|35|"3"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.076|"Moderate"|"0"|0.212|"344528"
"255D"|"Barvon-Cabba-Shambo loams, 4 to 15 percent slopes"||6|7.7|43|||"None"|"None"|"0"|4.3|8.13|12.6|15.72|"Well drained"|"Well drained"|"C"||65|"4"|35|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.354|"Moderate"|"0"|0.489|"344529"
"256C"|"Yamacall-Havre-Delpoint loams, 2 to 8 percent slopes"||4|4.4|76|||"None"|"Rare"|"0"|4.15|8.13|14.85|20.05|"Well drained"|"Well drained"|"B"|"3"|65|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.178|"Moderate"|"0"|0.175|"344530"
"25A"|"Vanda silty clay, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|2.64|5.15|10.01|14.86|"Well drained"|"Well drained"|"D"||78|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.486|"Slight"|"0"|1|"344531"
"260F"|"Kuro-Wayden-Rock outcrop complex, 4 to 35 percent slopes"||22|19.7|38|||"None"|"None"|"0"|3.84|5.97|5.97|5.97|"Well drained"|"Well drained"|"D"||100|"7"|40|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.852|"Severe"|"0"|1|"344532"
"261F"|"Wayden-Castner complex, 8 to 45 percent slopes"||30|23.3|43|||"None"|"None"|"0"|3.71|5.91|5.91|5.91|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.609|"Severe"|"0"|1|"344533"
"262E"|"Wayden-Windham complex, 4 to 25 percent slopes"||17|12.4|43|||"None"|"None"|"0"|3.71|5.8|6.94|8.02|"Well drained"|"Well drained"|"D"||100|"6"|47|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.562|"Severe"|"0"|0.91|"344534"
"26A"|"Weingart loam, 1 to 8 percent slopes"||5|5|81|||"None"|"None"|"0"|3.83|6.67|8.98|8.98|"Well drained"|"Well drained"|"D"||100|"6"|97|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.328|"Moderate"|"0"|1|"344536"
"26B"|"Weingart-Warhorse loams, 1 to 8 percent slopes"||5|5.4|41|||"None"|"None"|"0"|4|6.61|8.18|8.18|"Well drained"|"Well drained"|"D"||100|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.324|"Moderate"|"0"|1|"344537"
"280D"|"Cabbart, moist-Delpoint, dry loams, 4 to 15 percent slopes"||10|8.5|41|||"None"|"None"|"0"|3.74|6.69|7.66|8.03|"Well drained"|"Well drained"|"D"||55|"6"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.24|"Severe"|"0"|0.95|"344538"
"280E"|"Castner-Kuro complex, 4 to 25 percent slopes"||15|14.7|38|||"None"|"None"|"0"|3.3|4.95|4.95|4.95|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.189|"Severe"|"0"|1|"344539"
"281D"|"Doney-Cabba-Macar loams, 4 to 15 percent slopes"||12|9.9|43|||"None"|"None"|"0"|4.18|7.84|11.25|13.5|"Well drained"|"Well drained"|"C"||100|"4"|40|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.36|"Severe"|"0"|0.677|"344540"
"281E"|"Castner-Rock outcrop complex, 8 to 45 percent slopes"||27|25.2|46|||"None"|"None"|"0"|3.06|4.61|4.61|4.61|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.942|"Slight"|"0"|1|"344541"
"282D"|"Castner channery loam, 4 to 25 percent slopes"||15|14.8|46|||"None"|"None"|"0"|3.08|4.63|4.63|4.63|"Well drained"|"Well drained"|"D"||100|"7"|88|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.208|"Slight"|"0"|1|"344542"
"283D"|"Barvon-Cabba loams, 2 to 8 percent slopes"||5|6.2|43|||"None"|"None"|"0"|4.01|7.53|9.98|10.35|"Well drained"|"Well drained"|"C"||95|"4"|50|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.104|"Moderate"|"0"|0.743|"344543"
"283F"|"Cabba-Rock outcrop complex, 8 to 45 percent slopes"||27|24.2|30|||"None"|"None"|"0"|4.08|5.33|5.48|5.48|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.873|"Severe"|"0"|1|"344544"
"284D"|"Cabba-Barvon loams, 4 to 15 percent slopes"||12|9.4|43|||"None"|"None"|"0"|4.02|7.43|9.38|9.38|"Well drained"|"Well drained"|"D"||95|"6"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.537|"Severe"|"0"|0.816|"344545"
"284F"|"Doney-Wayden complex, 15 to 60 percent slopes"||38|36.1|43|||"None"|"None"|"0"|4.14|7.47|8.3|8.3|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344546"
"285D"|"Cabba-Doney loams, 4 to 15 percent slopes"||12|9.2|43|||"None"|"None"|"0"|4.15|7.59|9.19|9.57|"Well drained"|"Well drained"|"D"||100|"6"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.543|"Severe"|"0"|0.927|"344547"
"286F"|"Cabbart, calcareous-Rock outcrop complex, 8 to 45 percent slopes"||27|24.4|0|||"None"|"None"|"0"|3.57|4.64|4.78|4.78|"Well drained"|"Well drained"|"D"|"7"|75|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.938|"Severe"|"0"|1|"344549"
"287D"|"Delpoint, dry-Cabbart, moist loams, 2 to 8 percent slopes"||4|5|41|||"None"|"None"|"0"|3.76|6.78|7.79|8.17|"Well drained"|"Well drained"|"D"|"4"|50|"6"|90|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.191|"Moderate"|"0"|0.95|"344550"
"287F"|"Cabbart, moist-Delpoint, dry loams, 8 to 45 percent slopes"||35|28.6|41|||"None"|"None"|"0"|3.77|6.7|7.08|7.08|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.924|"Severe"|"0"|1|"344551"
"288D"|"Delpoint-Cabbart-Havre loams, 4 to 25 percent slopes"||10|10.6|30|||"None"|"Rare"|"0"|4.19|7.34|11.46|13.86|"Well drained"|"Well drained"|"C"||70|"4"|40|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.177|"Severe"|"0"|0.507|"344552"
"288F"|"Cabbart-Delpoint loams, 15 to 65 percent slopes"||25|24.8|41|||"None"|"None"|"0"|3.67|6.48|7.05|7.25|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.978|"Severe"|"0"|0.989|"344553"
"289D"|"Barvon-Cabba-Korchea loams, 3 to 25 percent slopes"||14|11.5|30|||"None"|"None"|"0"|4.2|7.48|11.87|14.77|"Well drained"|"Well drained"|"C"||75|"4"|40|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.307|"Severe"|"0"|0.636|"344554"
"289F"|"Cabba-Barvon loams, 15 to 65 percent slopes"||45|33.9|30|||"None"|"None"|"0"|4.03|6.49|8.35|8.35|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.942|"Severe"|"0"|1|"344555"
"291C"|"Windham very stony loam, 2 to 15 percent slopes"||9|8.2||||"None"|"None"|"0"|3.61|5.94|8.73|11.25|"Well drained"|"Well drained"|"C"||85|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.405|"Moderate"|"0"|0.564|"344557"
"292A"|"Straw-Korchea loams, 0 to 2 percent slopes"||1|1.5||||"Rare"|"Rare"|"0"|4.74|9.31|17.58|25.13|"Well drained"|"Well drained"|"B"|"2"|50|"3"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.07|"Slight"|"0"|0.05|"344558"
"294C"|"Shambo loam, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|4.85|9.35|18.28|27.26|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.076|"Moderate"|"0"|0|"344559"
"295F"|"Bitton-Winifred-Castner complex, 15 to 60 percent slopes"||38|32.6|46|||"None"|"None"|"0"|3.68|6.6|10.29|11.98|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.954|"Severe"|"0"|1|"344560"
"296D"|"Borky-Sinnigam very stony clay loams, 2 to 15 percent slopes"||9|8.8|43|||"None"|"None"|"0"|2.36|4.12|5.48|5.48|"Well drained"|"Well drained"|"D"||95|"7"|95|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.122|"Slight"|"0"|1|"344561"
"2E"|"Rock outcrop"|||||||||"0"|||||||||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344562"
"030C"|"Busby fine sandy loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.36|6.76|13.62|19.94|"Well drained"|"Well drained"|"A"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.034|"Moderate"|"0"|0.432|"344563"
"030D"|"Busby fine sandy loam, 8 to 15 percent slopes"||12|11.7||||"None"|"None"|"0"|3.35|6.74|13.5|19.81|"Well drained"|"Well drained"|"A"|"3"|85|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.046|"Severe"|"0"|0.654|"344564"
"31B"|"Delpoint loam, 2 to 8 percent slopes"||5|5.5|56|||"None"|"None"|"0"|4.18|8.03|9.45|9.69|"Well drained"|"Well drained"|"C"|"3"|83|"3"|85|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.201|"Moderate"|"0"|0.912|"344565"
"31C"|"Delpoint-Cabbart-Yamacall loams, 4 to 15 percent slopes"||10|9.2|41|||"None"|"None"|"0"|4.23|7.74|10.42|12.23|"Well drained"|"Well drained"|"D"||77|"4"|50|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.21|"Severe"|"0"|0.763|"344566"
"32B"|"Twilight sandy loam, 2 to 8 percent slopes"||5|5|89|||"None"|"None"|"0"|3.77|7.3|12.52|12.96|"Well drained"|"Well drained"|"B"|"4"|89|"4"|89|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Moderate"|"0"|0.519|"344567"
"32D"|"Twilight-Blacksheep-Rock outcrop, complex, 4 to 25 percent slopes"||12|12.2|46|||"None"|"None"|"0"|3.71|7.09|8.78|9.36|"Well drained"|"Well drained"|"B"||93|"4"|50|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.041|"Severe"|"0"|0.88|"344568"
"33A"|"Yamacall loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.09|7.54|14.19|20.71|"Well drained"|"Well drained"|"B"|"2"|85|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.197|"Slight"|"0"|0.15|"344569"
"33B"|"Yamacall loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.06|8.02|15.7|23.13|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.198|"Moderate"|"0"|0.132|"344570"
"35B"|"Yamacall-Busby complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.91|7.7|14.84|21.66|"Well drained"|"Well drained"|"B"|"3"|55|"3"|57|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.125|"Moderate"|"0"|0.261|"344573"
"36B"|"Yamacall-Delpoint loams, 2 to 8 percent slopes"||5|5.2|71|||"None"|"None"|"0"|3.76|7.34|12.36|16|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Moderate"|"0"|0.359|"344574"
"38A"|"Kobase-Zatoville silty clay loams, 1 to 8 percent slopes"||4|3.8||||"None"|"None"|"0"|4.09|7.81|14.62|21.41|"Well drained"|"Well drained"|"C"|"3"|45|"3"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.353|"Moderate"|"0"|1|"344577"
"38B"|"Zatoville silty clay loam, 1 to 8 percent slopes"||4|3.8||||"None"|"None"|"0"|4.01|7.59|13.66|19.72|"Well drained"|"Well drained"|"C"||78|"6"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.353|"Moderate"|"0"|1|"344578"
"39B"|"Delpoint loam, calcareous, 2 to 8 percent slopes"||5|5.6|56|||"None"|"None"|"0"|4.16|7.97|9.32|9.48|"Well drained"|"Well drained"|"C"|"4"|83|"4"|83|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.196|"Moderate"|"0"|0.917|"344579"
"39C"|"Delpoint, calcareous-Cabbart-Yamacall, calcareous, loams, 4 to 15 percent slopes"||9|8.6|41|||"None"|"None"|"0"|3.55|6.53|8.67|10.29|"Well drained"|"Well drained"|"C"||80|"6"|70|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.19|"Severe"|"0"|0.77|"344580"
"3A"|"Riverwash"||1|1||||||"0"|3.73|7.42|14.21|20.87|||||88||85|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.158|"Not rated"|"3"|0.68|"344581"
"40B"|"Kobase silty clay loam, 2 to 8 percent slopes"||5|4.8||||"None"|"None"|"0"|4.3|8.25|16.06|23.88|"Well drained"|"Well drained"|"C"|"3"|82|"3"|82|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.321|"Moderate"|"0"|0.93|"344583"
"40C"|"Kobase silty clay loam, calcareous surface, 1 to 8 percent slopes"||4|3.9||||"None"|"None"|"0"|4.26|8.22|16.09|23.96|"Well drained"|"Well drained"|"C"|"4"|77|"4"|77|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Moderate"|"0"|0.93|"344584"
"41A"|"Yamacall loam, calcareous, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.26|8.6|16.7|24.57|"Well drained"|"Well drained"|"B"|"4"|92|"4"|92|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.199|"Slight"|"0"|0.112|"344585"
"41B"|"Yamacall loam, calcareous, 2 to 8 percent slopes"||5|4.8||||"None"|"None"|"0"|4.29|8.67|16.63|24.33|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.21|"Moderate"|"0"|0.108|"344586"
"41C"|"Yamacall-Delpoint loams, calcareous, 2 to 8 percent slopes"||5|5|56|||"None"|"None"|"0"|4.21|8.36|13.34|17.81|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.198|"Moderate"|"0"|0.461|"344587"
"50B"|"Hinterland loam, 2 to 8 percent slopes"||5|5.3|30|||"None"|"None"|"0"|3.57|4.45|4.53|4.53|"Well drained"|"Well drained"|"D"|"6"|80|"6"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.245|"Slight"|"0"|1|"344590"
"50C"|"Hinterland loam, 6 to 15 percent slopes"||11|10.6|30|||"None"|"None"|"0"|3.63|4.48|4.64|4.64|"Well drained"|"Well drained"|"D"||100|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.255|"Severe"|"0"|1|"344591"
"50D"|"Hinterland-Delplain complex, 8 to 25 percent slopes"||12|14.4|30|||"None"|"None"|"0"|3.04|3.58|3.58|3.58|"Well drained"|"Well drained"|"D"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.276|"Slight"|"0"|1|"344592"
"51A"|"Ethridge clay loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.38|8.47|16.25|24.01|"Well drained"|"Well drained"|"C"|"3"|92|"3"|97|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.304|"Slight"|"0"|0.95|"344593"
"51B"|"Ethridge clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.37|8.41|15.86|23.23|"Well drained"|"Well drained"|"C"|"3"|92|"3"|97|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.301|"Moderate"|"0"|0.95|"344594"
"52A"|"Eapa loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.45|8.84|17.61|26.57|"Well drained"|"Well drained"|"B"||82|"3"|98|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.226|"Slight"|"0"|0.13|"344595"
"52B"|"Eapa loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.46|8.88|17.83|26.82|"Well drained"|"Well drained"|"B"||90|"3"|98|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.219|"Moderate"|"0"|0.029|"344596"
"53A"|"Tanna loam, 1 to 6 percent slopes"||4|4.3|64|||"None"|"None"|"0"|4.05|7.06|8.93|9.17|"Well drained"|"Well drained"|"D"|"3"|83|"3"|83|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.271|"Moderate"|"0"|1|"344597"
"54A"|"Marmarth fine sandy loam, 1 to 8 percent slopes"||5|5.3|79|||"None"|"None"|"0"|3.96|7.92|12.55|13.03|"Well drained"|"Well drained"|"C"||100|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.054|"Moderate"|"0"|0.5|"344598"
"56A"|"Crago-Musselshell-Attewan complex, 1 to 4 percent slopes"||1|1.3||||"None"|"None"|"0"|3.38|6.44|9.53|11.93|"Well drained"|"Well drained"|"B"|"4"|77|"6"|45|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.21|"Slight"|"2"|0.68|"344599"
"57A"|"Attewan loam, 1 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.18|7.89|11.56|13.82|"Well drained"|"Well drained"|"B"|"3"|82|"3"|82|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.22|"Slight"|"0"|0.87|"344600"
"57B"|"Attewan cobbly loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.47|6.82|9.97|11.69|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.131|"Slight"|"0"|0.9|"344601"
"57C"|"Attewan-Niart loams, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.32|8.23|12.04|14.54|"Well drained"|"Well drained"|"B"|"4"|50|"3"|50|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.173|"Slight"|"0"|0.55|"344602"
"58A"|"Verson clay loam, 1 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.18|7.86|11.41|14.39|"Well drained"|"Well drained"|"C"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.275|"Slight"|"0"|0.97|"344603"
"5A"|"Harlake silty clay, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|3.96|7.88|15.7|23.52|"Well drained"|"Well drained"|"C"|"4"|78|"4"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.452|"Slight"|"3"|0.93|"344604"
"60B"|"Abor silty clay, 1 to 8 percent slopes"||5|4.9|89|||"None"|"None"|"0"|3.68|7.08|11.78|12.39|"Well drained"|"Well drained"|"D"|"6"|90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.486|"Moderate"|"0"|1|"344605"
"60C"|"Abor-Neldore silty clays, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|3.66|6.12|9.03|9.43|"Well drained"|"Well drained"|"D"|"7"|45|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.491|"Moderate"|"0"|1|"344606"
"60D"|"Neldore-Abor silty clays, 4 to 15 percent slopes"||14|12.6|30|||"None"|"None"|"0"|3.66|5.7|7.67|7.67|"Well drained"|"Well drained"|"D"||100|"7"|57|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.526|"Severe"|"0"|1|"344607"
"61D"|"Neldore-Neldore, saline, silty clays, 4 to 25 percent slopes"||15|13.1|36|||"None"|"None"|"0"|3.41|5.34|5.68|5.68|"Well drained"|"Well drained"|"D"||100|"7"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.526|"Severe"|"0"|1|"344608"
"61E"|"Neldore-Volborg silty clays, 4 to 25 percent slopes"||10|11.9|30|||"None"|"None"|"7"|3.58|5.56|6.88|7.29|"Well drained"|"Well drained"|"D"||93|"7"|82|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.547|"Severe"|"0"|1|"344609"
"62C"|"Neldore silty clay, 4 to 25 percent slopes"||15|14.8|43|||"None"|"None"|"0"|3.62|6.24|6.82|6.82|"Well drained"|"Well drained"|"D"||95|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.487|"Severe"|"0"|1|"344610"
"62D"|"Neldore-Yawdim silty clays, 4 to 25 percent slopes"||15|15.3|28|||"None"|"None"|"0"|3.88|5.18|5.32|5.32|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.7|"Severe"|"0"|1|"344611"
"63A"|"Marias silty clay, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.64|7.09|13.84|20.59|"Well drained"|"Well drained"|"D"||87|"4"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344613"
"64A"|"Marvan-Vanda silty clays, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|3.33|6.42|11.62|16.82|"Well drained"|"Well drained"|"D"|"4"|52|"4"|57|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.491|"Slight"|"0"|1|"344614"
"64B"|"Marvan silty clay, 0 to 8 percent slopes"||4|3.8||||"None"|"None"|"0"|3.72|7.08|12.28|17.48|"Well drained"|"Well drained"|"D"|"4"|82|"4"|87|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.491|"Moderate"|"0"|1|"344615"
"68C"|"Megonot-Yawdim silty clay loams, 4 to 15 percent slopes"||10|9.7|41|||"None"|"None"|"0"|4.25|7.28|10.03|10.52|"Well drained"|"Well drained"|"D"||94|"4"|51|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.581|"Severe"|"0"|1|"344617"
"6A"|"Harlake silty clay, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.01|7.98|15.91|23.81|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.482|"Slight"|"5"|0.98|"344619"
"73E"|"Yawdim-Abor complex, 15 to 60 percent slopes"||38|31.4|28|||"None"|"None"|"0"|4.06|6.13|7.4|7.4|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344621"
"74D"|"Abor-Crago complex, 2 to 15 percent slopes"||10|8.7|81|||"None"|"None"|"0"|3.2|6.15|9.47|10.6|"Well drained"|"Well drained"|"D"||50|"4"|53|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.408|"Severe"|"0"|1|"344622"
"7A"|"Lostriver silty clay, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|3.73|7.31|14.46|21.61|"Well drained"|"Well drained"|"C"||83|"6"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.476|"Slight"|"3"|0.95|"344624"
"80E"|"Blacksheep-Rock outcrop-Twilight complex, 8 to 45 percent slopes"||27|22.9|46|||"None"|"None"|"0"|3.86|6.7|7.28|7.47|"Well drained"|"Well drained"|"D"||98|"7"|58|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.783|"Severe"|"0"|0.961|"344626"
"81B"|"Delpoint-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4|7.44|10.51|10.75|"Well drained"|"Well drained"|"C"|"3"|63|"3"|63|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.201|"Moderate"|"0"|0.638|"344627"
"82C"|"Cabbart-Delpoint, calcareous-Rock outcrop complex, 4 to 15 percent slopes"||10|9.9|41|||"None"|"None"|"0"|3.75|6.59|7.08|7.26|"Well drained"|"Well drained"|"D"||98|"6"|83|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.283|"Severe"|"0"|0.976|"344631"
"82E"|"Cabbart-Delpoint, calcareous-Rock outcrop complex, 8 to 45 percent slopes"||27|24|41|||"None"|"None"|"0"|3.74|6.52|6.99|7.18|"Well drained"|"Well drained"|"D"||100|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.768|"Severe"|"0"|0.976|"344632"
"83D"|"Cabbart-Rock outcrop-Blacksheep complex, 8 to 45 percent slopes"||27|25.2|41|||"None"|"None"|"0"|3.46|5.74|6.22|6.51|"Well drained"|"Well drained"|"D"||97|"7"|63|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.904|"Severe"|"0"|0.968|"344633"
"84C"|"Cabbart-Yawdim-Delpoint complex, 4 to 15 percent slopes"||10|9.6|38|||"None"|"None"|"0"|3.55|6.07|7.04|7.42|"Well drained"|"Well drained"|"D"||92|"6"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.367|"Severe"|"0"|0.95|"344634"
"84D"|"Cabbart-Yawdim-Badland complex, 4 to 35 percent slopes"||20|17.4|41|||"None"|"None"|"0"|3.6|6.26|7.13|7.81|"Well drained"|"Well drained"|"D"||91|"7"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.686|"Severe"|"0"|1|"344635"
"85A"|"Cabbart clay loam, 0 to 2 percent slopes"||1|1.5|41|||"None"|"None"|"0"|4.04|6.78|6.83|6.83|"Well drained"|"Well drained"|"D"||95|"6"|90|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Slight"|"0"|0.999|"344637"
"86E"|"Cabbart-Rock outcrop complex, 4 to 35 percent slopes"||20|19|30|||"None"|"None"|"0"|4.35|5.54|5.6|5.6|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.481|"Severe"|"0"|0.998|"344639"
"87B"|"Delpoint, calcareous-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|3.01|5.28|6.09|6.23|"Well drained"|"Well drained"|"C"|"4"|55|"6"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.282|"Moderate"|"0"|0.98|"344640"
"89C"|"Rentsac fine sandy loam, 2 to 8 percent slopes"||5|5.3|30|||"None"|"None"|"0"|2.49|3.34|3.51|3.51|"Well drained"|"Well drained"|"D"||97|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.033|"Slight"|"0"|0.984|"344642"
"8A"|"Harlake-Havre complex, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4|7.93|15.7|23.48|"Well drained"|"Well drained"|"C"|"4"|55|"4"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.336|"Slight"|"4"|0.784|"344643"
"93A"|"Crago-Musselshell complex, 1 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.25|6.22|9.22|11.76|"Well drained"|"Well drained"|"B"|"4"|90|"6"|50|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.201|"Slight"|"0"|0.574|"344649"
"93B"|"Crago cobbly loam, 1 to 8 percent slopes"||4|4||||"None"|"None"|"0"|3.07|5.55|8.45|10.43|"Well drained"|"Well drained"|"B"|"6"|85|"6"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.2|"Slight"|"3"|0.922|"344650"
"94A"|"Crago gravelly loam, 1 to 4 percent slopes"||2|2||||"None"|"None"|"0"|2.71|5.12|7.57|9.42|"Well drained"|"Well drained"|"B"|"4"|95|"6"|80|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.207|"Slight"|"0"|0.85|"344651"
"94E"|"Crago gravelly loam, 8 to 35 percent slopes"||22|19.4||||"None"|"None"|"0"|2.63|4.93|7.48|9.48|"Well drained"|"Well drained"|"B"|"4"|95|"6"|85|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.74|"Severe"|"5"|0.9|"344652"
"95A"|"Crago-Musselshell cobbly loams, 1 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.41|6.41|9.73|12.4|"Well drained"|"Well drained"|"B"|"6"|55|"6"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.198|"Slight"|"2"|0.808|"344653"
"95E"|"Yawdim-Crago complex, 4 to 35 percent slopes"||20|18.8|28|||"None"|"None"|"0"|3.45|4.92|6.2|7.03|"Well drained"|"Well drained"|"D"||55|"7"|47|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.716|"Severe"|"0"|0.948|"344656"
"97B"|"Musselshell-Crago complex, 4 to 8 percent slopes"||6|6.1||||"None"|"None"|"0"|3.47|6.48|9.64|12.44|"Well drained"|"Well drained"|"B"|"4"|95|"4"|55|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.151|"Moderate"|"0"|0.508|"344659"
"98A"|"Niart cobbly loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.51|8.8|13.46|17.08|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.193|"Slight"|"0"|0.065|"344660"
"98B"|"Niart-Crago complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.64|6.86|10.34|13.17|"Well drained"|"Well drained"|"B"|"4"|90|"4"|50|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.181|"Slight"|"0"|0.465|"344661"
"98C"|"Niart-Crago complex, 4 to 15 percent slopes"||10|9.6||||"None"|"None"|"0"|3.66|7.07|10.76|13.57|"Well drained"|"Well drained"|"B"|"4"|93|"4"|53|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.212|"Severe"|"2"|0.56|"344662"
"9A"|"Havre loam, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.15|8.1|15.93|23.76|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.226|"Slight"|"3"|0.112|"344664"
"9B"|"Havre, occasionally flooded-Yamacall loams, 0 to 4 percent slopes"||1|1.3||||"Occasional"|"Occasional"|"0"|4.1|8.05|15.88|23.71|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.219|"Slight"|"3"|0.452|"344665"
"DA"|"Denied access"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344666"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344668"
"UL"|"Urban land"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"360746"
"130B"|"Busby-Twilight fine sandy loams, 2 to 8 percent slopes"||5|5|64|||"None"|"None"|"0"|3.69|7.3|12.37|16.46|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.595|"360767"
"60E"|"Neldore-Abor silty clays, 15 to 45 percent slopes"||30|27|30|||"None"|"None"|"0"|3.78|5.58|7.67|7.67|"Well drained"|"Well drained"|"D"|"7"|85|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.833|"Severe"|"0"|1|"360789"
"425E"|"Maiden-Tibs-Whitecow complex, 2 to 25 percent slopes"||14|14.1|61|||"None"|"None"|"0"|3.61|6.03|9.09|11.63|"Well drained"|"Well drained"|"C"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.038|"Moderate"|"0"|0.99|"1710900"
"356A"|"Crago-Musselshell-Attewan complex, 1 to 4 percent slopes, fan"||1|1.3||||"None"|"None"|"0"|3.38|6.41|9.51|11.93|"Well drained"|"Well drained"|"B"|"4"|77|"6"|45|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.21|"Slight"|"2"|0.68|"1713818"
"460E"|"Yawdim-Abor complex, 8 to 35 percent slopes"||21|18.1|46|||"None"|"None"|"0"|4.16|7.53|9.32|9.68|"Well drained"|"Well drained"|"D"||95|"7"|64|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.821|"Severe"|"0"|1|"1713819"
"780F"|"Cabbart-Yamacall-Havre, rarely flooded, loams, 2 to 60 percent slopes"||34|13.5|30|||"None"|"Rare"|"0"|4.2|7.09|11.89|16.64|"Well drained"|"Well drained"|"B"||45|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.464|"Severe"|"0"|0.483|"1713820"
"880D"|"Delpoint-Cabbart loams, dry, 4 to 15 percent slopes"||10|9.9|41|||"None"|"None"|"0"|4.25|7.61|8.5|8.9|"Well drained"|"Well drained"|"D"||95|"6"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.191|"Severe"|"0"|0.932|"1713821"
"880F"|"Cabbart-Delpoint loams, moist, 4 to 45 percent slopes"||25|21.4|41|||"None"|"None"|"0"|3.76|6.7|7.48|7.87|"Well drained"|"Well drained"|"D"||95|"7"|50|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.672|"Severe"|"0"|0.947|"1713822"
"881F"|"Cabbart, dry-Delpoint, dry-Rock outcrop complex, 8 to 65 percent slopes"||40|32|41|||"None"|"None"|"0"|3.75|6.59|6.9|6.9|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.936|"Severe"|"0"|1|"1713823"
"354C"|"Bonfri-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.95|"1715945"
"354D"|"Cabbart-Bonfri loams, 4 to 15 percent slopes"||10|7.8|41|||"None"|"None"|"0"|3.93|7.07|9.7|9.7|"Well drained"|"Well drained"|"D"||55|"6"|55|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Severe"|"0"|0.807|"1715946"
"107A"|"Lostriver-Bullhook complex, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|3.85|7.43|14.56|21.69|"Well drained"|"Well drained"|"C"||85|"6"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.343|"Slight"|"5"|0.92|"1717985"
"108A"|"Harlake-Havre complex, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.04|7.97|15.74|23.51|"Well drained"|"Well drained"|"C"|"4"|56|"4"|53|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.333|"Slight"|"4"|0.556|"1717986"
"111A"|"Havre-Glendive complex, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|3.8|7.6|14.81|22.01|"Well drained"|"Well drained"|"B"|"2"|50|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.162|"Slight"|"5"|0.653|"1717987"
"182D"|"Cabbart-Delpoint loams, 4 to 15 percent slopes"||10|8.1|41|||"None"|"None"|"0"|3.84|6.95|8.79|9.21|"Well drained"|"Well drained"|"D"||55|"6"|50|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.23|"Severe"|"0"|0.799|"1717988"
"598B"|"Niart-Rothiemay loams, 1 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|4.33|8.43|13.97|18.8|"Well drained"|"Well drained"|"B"|"4"|95|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.202|"Slight"|"2"|0.204|"1717989"
"354B"|"Bonfri-Cabbart loams, 0 to 4 percent slopes"||2|2.9|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.95|"1887082"
"282F"|"Cabba-Doney loams, 8 to 45 percent slopes"||30|24.3|43|||"None"|"None"|"0"|4.13|7.51|8.45|8.45|"Well drained"|"Well drained"|"D"||100|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.823|"Severe"|"0"|0.976|"1910243"
"83E"|"Blacksheep-Twilight complex, 4 to 25 percent slopes"||15|14.2|46|||"None"|"None"|"0"|3.71|6.89|7.65|7.79|"Well drained"|"Well drained"|"D"||98|"7"|54|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.037|"Moderate"|"0"|0.992|"1913584"
"285C"|"Doney-Cabba loams, 2 to 8 percent slopes"||5|5.1|46|||"None"|"None"|"0"|4.16|7.9|9.98|10.36|"Well drained"|"Well drained"|"C"|"3"|55|"4"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.08|"Moderate"|"0"|0.925|"1913585"
"183E"|"Cabbart-Blacksheep, dry- complex, 8 to 25 percent slopes"||17|18.3|30|||"None"|"None"|"0"|3.56|5.27|5.5|5.68|"Well drained"|"Well drained"|"D"||98|"7"|83|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.417|"Severe"|"0"|0.99|"1913586"
"73D"|"Abor-Yawdim complex, 4 to 15 percent slopes"||10|9.6|46|||"None"|"None"|"0"|3.96|7.38|10.55|10.8|"Well drained"|"Well drained"|"D"||97|"6"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.69|"Severe"|"0"|1|"2617157"
"62E"|"Neldore-Rock outcrop complex, 15 to 60 percent slopes"||35|32.1|38|||"None"|"None"|"0"|3.67|5.72|6.4|6.72|"Well drained"|"Well drained"|"D"||100|"7"|58|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.954|"Severe"|"0"|1|"2986031"
"30D"|"Busby fine sandy loam, warm, 8 to 15 percent slopes"||12|12.3||||"None"|"None"|"0"|3.34|6.63|13.03|19.01|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.027|"Severe"|"0"|0.672|"3040417"
"30C"|"Busby fine sandy loam, warm,  2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.37|6.73|13.44|19.65|"Well drained"|"Well drained"|"A"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.043|"Moderate"|"0"|0.459|"3040505"
