"1"|"Abor silty clay, 1 to 8 percent slopes"||5|4.9|89|||"None"|"None"|"0"|3.68|7.08|11.78|12.39|"Well drained"|"Well drained"|"D"|"6"|90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.486|"Moderate"|"0"|1|"344669"
"10"|"Blackhall-Rock outcrop-Twilight complex, 8 to 45 percent slopes"||27|22.4|33|||"None"|"None"|"0"|3.75|5.67|6.7|6.7|"Well drained"|"Well drained"|"D"||100|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.698|"Severe"|"0"|0.892|"344670"
"100"|"Yawdim-Crago complex, 4 to 35 percent slopes"||20|20|41|||"None"|"None"|"0"|3.4|5.69|6.4|7.1|"Well drained"|"Well drained"|"D"||100|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"344671"
"101"|"Yawdim-Orinoco complex, 4 to 15 percent slopes"||10|10|41|||"None"|"None"|"0"|4.06|7.11|8.87|8.87|"Well drained"|"Well drained"|"D"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.408|"Severe"|"0"|1|"344672"
"102"|"Yawdim-Orinoco complex, 15 to 35 percent slopes"||25|23.2|38|||"None"|"None"|"0"|4.07|6.74|7.67|7.67|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.824|"Severe"|"0"|1|"344673"
"103"|"Zatoville silty clay loam, 1 to 6 percent slopes"||4|4.6||||"None"|"None"|"0"|4.12|7.95|13.92|19.32|"Well drained"|"Well drained"|"C"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.277|"Moderate"|"0"|1|"344674"
"104"|"Zatoville-Orinoco silty clay loams, 2 to 8 percent slopes"||5|5.8|43|||"None"|"None"|"0"|3.93|7.45|11.94|14.64|"Well drained"|"Well drained"|"D"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.31|"Moderate"|"0"|1|"344675"
"11"|"Busby fine sandy loam, 8 to 15 percent slopes"||12|11.7||||"None"|"None"|"0"|3.35|6.74|13.5|19.81|"Well drained"|"Well drained"|"A"|"3"|85|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.046|"Severe"|"0"|0.654|"344676"
"12"|"Busby-Blackhall fine sandy loams, 8 to 15 percent slopes"||12|12.4|33|||"None"|"None"|"0"|3.54|6.07|10.03|14|"Well drained"|"Well drained"|"A"||100|"4"|55|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.014|"Moderate"|"0"|0.792|"344677"
"13"|"Busby-Twilight fine sandy loams, 2 to 8 percent slopes"||5|5|64|||"None"|"None"|"0"|3.69|7.3|12.37|16.46|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.595|"344678"
"14"|"Cabbart loam, 8 to 15 percent slopes"||12|12|43|||"None"|"None"|"0"|4.39|7.42|7.42|7.42|"Well drained"|"Well drained"|"D"||100|"6"|100|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.208|"Severe"|"0"|1|"344679"
"15"|"Cabbart, calcareous-Crago-Delpoint, calcareous complex, 8 to 35 percent slopes"||25|24.1|41|||"None"|"None"|"0"|3.41|5.99|7.17|7.88|"Well drained"|"Well drained"|"D"||98|"6"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.979|"Severe"|"0"|1|"344680"
"16"|"Cabbart-Delpoint loams, 4 to 15 percent slopes"||10|8.1|41|||"None"|"None"|"0"|3.84|6.95|8.79|9.21|"Well drained"|"Well drained"|"D"||55|"6"|50|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.23|"Severe"|"0"|0.799|"344681"
"17"|"Cabbart-Delpoint-Cabbart, moist, loams, calcareous 4 to 35 percent slopes"||13|11.8|41|||"None"|"None"|"0"|3.74|6.51|6.93|6.93|"Well drained"|"Well drained"|"D"||100|"7"|65|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.253|"Severe"|"0"|1|"344682"
"18"|"Cabbart-Delpoint, calcareous-Rock outcrop complex, 8 to 45 percent slopes"||27|24|41|||"None"|"None"|"0"|3.74|6.52|6.99|7.18|"Well drained"|"Well drained"|"D"||100|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.768|"Severe"|"0"|0.976|"344683"
"19"|"Cabbart-Rock outcrop-Blacksheep complex, 8 to 45 percent slopes"||27|25.2|41|||"None"|"None"|"0"|3.46|5.74|6.22|6.51|"Well drained"|"Well drained"|"D"||97|"7"|63|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.904|"Severe"|"0"|0.968|"344684"
"2"|"Abor-Neldore silty clays, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|3.66|6.12|9.03|9.43|"Well drained"|"Well drained"|"D"|"7"|45|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.491|"Moderate"|"0"|1|"344685"
"20"|"Cabbart-Yawdim-Delpoint complex, 15 to 35 percent slopes"||25|24.1|38|||"None"|"None"|"0"|3.56|5.93|6.11|6.11|"Well drained"|"Well drained"|"D"||100|"7"|73|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.892|"Severe"|"0"|1|"344686"
"22"|"Cabbart, high precipitation-Cabbart, moist, complex, 15 to 60 percent slopes"||38|38|41|||"None"|"None"|"0"|4.43|7.15|7.15|7.15|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344688"
"23"|"Cabbart, moist-Blacksheep-Delpoint, calcareous complex, 6 to 60 percent slopes"||38|30.6|41|||"None"|"None"|"0"|3.6|6.16|6.36|6.36|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.827|"Severe"|"0"|1|"344689"
"24"|"Chinook fine sandy loam, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.62|7.12|13.75|20.05|"Well drained"|"Well drained"|"A"||100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.016|"Moderate"|"0"|0.47|"344690"
"25"|"Crago gravelly loam, 0 to 8 percent slopes"||4|4||||"None"|"None"|"0"|2.47|4.24|5.75|7.25|"Well drained"|"Well drained"|"B"||95|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.153|"Slight"|"0"|1|"344691"
"26"|"Crago gravelly loam, 8 to 35 percent slopes"||22|22.8||||"None"|"None"|"0"|2.45|4.25|5.75|7.25|"Well drained"|"Well drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.838|"Severe"|"0"|1|"344692"
"27"|"Crago-Musselshell complex, 0 to 4 percent slopes"||2|1.8||||"None"|"None"|"0"|3.47|5.55|8.18|10.45|"Well drained"|"Well drained"|"B"||97|"6"|70|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.105|"Slight"|"0"|0.7|"344693"
"28"|"Crago-Musselshell-Attewan complex, 0 to 2 percent slopes"||1|1.4||||"None"|"None"|"0"|3.32|6.18|9.56|11.91|"Well drained"|"Well drained"|"B"||100|"6"|50|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.124|"Slight"|"0"|0.7|"344694"
"29"|"Creed-Gerdrum complex, 1 to 6 percent slopes"||4|3.8||||"None"|"None"|"0"|3.42|6.18|10.87|15.54|"Well drained"|"Well drained"|"C"||100|"4"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.299|"Moderate"|"0"|1|"344695"
"3"|"Amherst clay loam, 1 to 6 percent slopes"||4|4.1|30|||"None"|"None"|"0"|3.81|4.52|4.52|4.52|"Well drained"|"Well drained"|"D"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.196|"Moderate"|"0"|1|"344696"
"30"|"Delpoint loam, 2 to 8 percent slopes"||5|5.5|56|||"None"|"None"|"0"|4.18|8.03|9.45|9.69|"Well drained"|"Well drained"|"C"|"3"|83|"3"|85|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.201|"Moderate"|"0"|0.912|"344697"
"31"|"Delpoint-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4|7.44|10.51|10.75|"Well drained"|"Well drained"|"C"|"3"|63|"3"|63|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.201|"Moderate"|"0"|0.638|"344698"
"32"|"Delpoint-Cabbart-Yamac loams, 4 to 15 percent slopes"||10|10.3|41|||"None"|"None"|"0"|4.2|7.72|10.75|12.01|"Well drained"|"Well drained"|"C"||100|"4"|50|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.176|"Moderate"|"0"|0.656|"344699"
"33"|"Ethridge clay loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.3|8.47|16.47|24.3|"Well drained"|"Well drained"|"C"|"3"|95|"3"|95|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.28|"Slight"|"0"|1|"344700"
"34"|"Ethridge clay loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.28|8.44|16.3|23.73|"Well drained"|"Well drained"|"C"||100|"3"|90|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.292|"Moderate"|"0"|1|"344701"
"35"|"Evanston loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.19|8.18|16.08|23.9|"Well drained"|"Well drained"|"B"|"2"|90|"3"|96|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.121|"Slight"|"0"|0.06|"344702"
"36"|"Evanston loam, 2 to 8 percent slopes"||5|4.8||||"None"|"None"|"0"|4.19|8.18|16.08|23.9|"Well drained"|"Well drained"|"B"||94|"3"|96|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.121|"Moderate"|"0"|0.06|"344703"
"37"|"Evanston-Attewan loams, 0 to 2 percent slopes"||1|1.4||||"None"|"None"|"0"|4.01|7.6|13.3|17.72|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.109|"Slight"|"0"|0.55|"344704"
"38"|"Gerdrum-Bascovy clays, 2 to 15 percent slopes"||9|9.1|77|||"None"|"None"|"0"|3.46|6.35|10.82|13.67|"Well drained"|"Well drained"|"D"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.8|"Severe"|"0"|1|"344705"
"39"|"Gerdrum-Creed complex, 1 to 6 percent slopes"||4|3.8||||"None"|"None"|"0"|3.41|6.1|10.67|15.24|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.299|"Moderate"|"0"|1|"344706"
"4"|"Amherst clay loam, 6 to 25 percent slopes"||16|16|30|||"None"|"None"|"0"|3.9|4.6|4.6|4.6|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.201|"Severe"|"0"|1|"344707"
"40"|"Gerdrum-Vanda complex, 1 to 6 percent slopes"||4|4||||"None"|"None"|"0"|3.09|5.63|10|14.15|"Well drained"|"Well drained"|"D"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.355|"Moderate"|"0"|1|"344708"
"41"|"Gerdrum-Vanda-Creed complex, 0 to 8 percent slopes"||5|4.1||||"None"|"None"|"0"|3.8|7.44|14.73|21.96|"Well drained"|"Well drained"|"D"|"6"|42|"6"|62|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.349|"Moderate"|"0"|1|"344709"
"42"|"Harlem silty clay, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|3.95|7.83|15.58|23.33|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344710"
"43"|"Harlem silty clay, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|3.97|7.88|15.7|23.53|"Well drained"|"Well drained"|"C"||97|"4"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.493|"Slight"|"0"|1|"344711"
"44"|"Harlem silty clay, saline, 0 to 2 percent slopes"||1|1.2||||"Rare"|"Rare"|"0"|3.52|6.34|11.98|17.58|"Well drained"|"Well drained"|"C"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.489|"Slight"|"5"|1|"344712"
"45"|"Harlem-Havre complex, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.05|7.86|15.48|23.11|"Well drained"|"Well drained"|"C"|"4"|45|"4"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.335|"Slight"|"0"|0.6|"344713"
"46"|"Harlem-Havre complex, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.05|7.86|15.48|23.11|"Well drained"|"Well drained"|"C"||100|"4"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.344|"Slight"|"0"|0.84|"344714"
"47"|"Harlem-Havre complex, saline, 0 to 2 percent slopes"||1|1.2||||"Rare"|"Rare"|"0"|3.51|6.23|11.65|17.08|"Well drained"|"Well drained"|"C"||100|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.342|"Slight"|"0"|0.911|"344715"
"48"|"Havre loam, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.25|8.2|16.1|23.91|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.073|"Slight"|"0"|0.111|"344716"
"49"|"Havre loam, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.26|8.27|16.29|24.23|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.197|"Slight"|"0"|0.62|"344717"
"5"|"Amherst-Delplain complex, 2 to 15 percent slopes"||9|9.6|30|||"None"|"None"|"0"|3.2|3.82|3.82|3.82|"Well drained"|"Well drained"|"D"||100|"6"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.237|"Severe"|"0"|1|"344718"
"50"|"Havre-Glendive complex, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.07|8.03|15.96|23.16|"Well drained"|"Well drained"|"B"|"4"|50|"4"|45|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.124|"Slight"|"0"|0.319|"344719"
"51"|"Havre-Glendive complex, 0 to 2 percent slopes, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.03|8.06|16.11|23.42|"Well drained"|"Well drained"|"B"||100|"4"|47|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.162|"Slight"|"0"|0.639|"344720"
"52"|"Havre-Harlem complex, 0 to 2 percent slopes, occasionally flooded, channeled"||1|1||||"Occasional"|"Occasional"|"0"|4.1|7.98|15.72|23.47|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.305|"Slight"|"0"|0.8|"344721"
"53"|"Havre-Yamac loams, 0 to 4 percent slopes"||1|1.6||||"Occasional"|"Occasional"|"0"|4.23|8.18|16.09|24|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.15|"Slight"|"0"|0.437|"344722"
"54"|"Kobar-Zatoville silty clay loams, 1 to 6 percent slopes"||4|4.8|77|||"None"|"None"|"0"|4.2|8.16|15.31|21.61|"Well drained"|"Well drained"|"C"|"3"|60|"3"|60|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.31|"Moderate"|"0"|1|"344723"
"55"|"Kremlin loam, 0 to 2 percent slopes"||1|1.4||||"None"|"None"|"0"|4.41|8.81|17.61|26.41|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.154|"Slight"|"0"|0.045|"344724"
"56"|"Kremlin loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.35|8.33|16.28|24.23|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.179|"Moderate"|"0"|0.023|"344725"
"57"|"Marias silty clay, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|3.57|6.99|13.74|20.49|"Well drained"|"Well drained"|"D"||100|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344726"
"58"|"Marmarth fine sandy loam, 1 to 8 percent slopes"||5|5.2|69|||"None"|"None"|"0"|3.85|7.8|10.96|11.21|"Well drained"|"Well drained"|"C"||100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.063|"Moderate"|"0"|0.722|"344727"
"59"|"Marvan silty clay, 1 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.38|6.45|12.16|16.66|"Well drained"|"Well drained"|"D"|"4"|85|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"344728"
"6"|"Attewan loam, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|4|7.36|11.43|12.93|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.105|"Slight"|"0"|1|"344729"
"60"|"Marvan-Vanda silty clays, 0 to 8 percent slopes"||4|4.3||||"None"|"None"|"0"|3.04|5.85|11.14|15.6|"Well drained"|"Well drained"|"D"||100|"4"|58|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"344730"
"61"|"Neldore silty clay, 4 to 25 percent slopes"||15|14.8|43|||"None"|"None"|"0"|3.62|6.24|6.82|6.82|"Well drained"|"Well drained"|"D"||95|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.487|"Severe"|"0"|1|"344731"
"62"|"Neldore-Abor silty clays, 4 to 15 percent slopes"||14|12.6|30|||"None"|"None"|"0"|3.66|5.7|7.67|7.67|"Well drained"|"Well drained"|"D"||100|"7"|57|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.526|"Severe"|"0"|1|"344732"
"63"|"Neldore-Abor silty clays, 15 to 45 percent slopes"||30|27|30|||"None"|"None"|"0"|3.78|5.58|7.67|7.67|"Well drained"|"Well drained"|"D"|"7"|85|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.833|"Severe"|"0"|1|"344733"
"64"|"Neldore-Bascovy-Rock outcrop complex, 6 to 60 percent slopes"||33|24.8|30|||"None"|"None"|"0"|3.45|5.15|6.64|7.18|"Well drained"|"Well drained"|"D"||95|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.787|"Severe"|"0"|1|"344734"
"65"|"Neldore-Neldore, saline, silty clays, 4 to 25 percent slopes"||15|15|43|||"None"|"None"|"0"|3.6|5.66|5.66|5.66|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"344735"
"67"|"Neldore-Volborg silty clays, 4 to 25 percent slopes"||10|11.9|30|||"None"|"None"|"7"|3.58|5.56|6.88|7.29|"Well drained"|"Well drained"|"D"||93|"7"|82|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.547|"Severe"|"0"|1|"344737"
"68"|"Neldore-Weingart complex, 2 to 15 percent slopes"||10|8.2|43|||"None"|"None"|"0"|3.64|6.13|7.14|7.3|"Well drained"|"Well drained"|"D"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.413|"Severe"|"0"|1|"344738"
"69"|"Neldore-Yawdim complex, 4 to 25 percent slopes"||15|14.7|41|||"None"|"None"|"0"|3.93|6.54|6.61|6.61|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.708|"Severe"|"0"|1|"344739"
"7"|"Badland"||42|39.6||||||"0"|3.71|6.26|7.34|7.34|||||100||90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.639|"Not rated"|"0"|1|"344740"
"70"|"Neldore, moist-Bascovy-Neldore, dry, silty clays, 6 to 60 percent slopes"||33|27.3|30|||"None"|"None"|"0"|3.82|5.34|6.47|6.86|"Well drained"|"Well drained"|"D"||95|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.861|"Severe"|"0"|1|"344741"
"71"|"Nobe-Absher silty clays, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|2.6|4.43|7.95|11.47|"Moderately well drained"|"Moderately well drained"|"D"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344742"
"72"|"Pinebreaks-Neldore, moist, silty clays, 15 to 60 percent slopes"||38|36.3|38|||"None"|"None"|"0"|3.43|5.13|5.43|5.7|"Well drained"|"Well drained"|"D"||95|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.974|"Severe"|"0"|1|"344743"
"73"|"Riverwash"||1|1||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344744"
"74"|"Rock outcrop"|||27||||||"0"|4.41|6.62|6.62|6.62|||||100||95|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"344745"
"75"|"Tanna clay loam, 1 to 6 percent slopes"||4|4.1|81|||"None"|"None"|"0"|4|7.9|12.62|12.87|"Well drained"|"Well drained"|"D"|"3"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.212|"Moderate"|"0"|1|"344746"
"76"|"Tanna-Weingart complex, 2 to 8 percent slopes"||5|5.4|74|||"None"|"None"|"0"|4.15|7.55|11.21|11.36|"Well drained"|"Well drained"|"D"||100|"3"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.234|"Moderate"|"0"|1|"344747"
"77"|"Teigen silty clay loam, 1 to 6 percent slopes"||4|4.3||||"None"|"None"|"0"|4.2|8.37|16.38|24.03|"Well drained"|"Well drained"|"C"||100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.299|"Moderate"|"0"|1|"344748"
"78"|"Twilight sandy loam, 2 to 8 percent slopes"||5|5.5|74|||"None"|"None"|"0"|3.75|7.16|10.19|10.19|"Well drained"|"Well drained"|"B"||100|"4"|90|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.018|"Moderate"|"0"|0.685|"344749"
"79"|"Twilight-Blacksheep sandy loams, 2 to 8 percent slopes"||8|7.5|46|||"None"|"None"|"0"|3.42|6.38|9.16|9.61|"Well drained"|"Well drained"|"B"|"4"|54|"4"|52|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.962|"344750"
"8"|"Bascovy-Neldore silty clays, 2 to 15 percent slopes"||9|8.9|30|||"None"|"None"|"0"|3.4|5.66|7.7|7.93|"Well drained"|"Well drained"|"D"||94|"4"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.491|"Severe"|"0"|0.99|"344751"
"80"|"Twilight-Blackhall-Rock outcrop complex, 4 to 25 percent slopes"||10|10|41|||"None"|"None"|"0"|3.73|6.83|8.89|8.89|"Well drained"|"Well drained"|"B"||100|"6"|40|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.015|"Moderate"|"0"|0.785|"344752"
"81"|"Ustic Torriorthents, 15 to 45 percent slopes"||30|30||||"None"|"None"|"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344753"
"82"|"Ustic Torriorthents, moderately saline, 15 to 45 percent slopes"||30|30||||"None"|"None"|"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344754"
"83"|"Ustic Torriorthents, strongly saline, 0 to 8 percent slopes"||4|4||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344755"
"84"|"Vaeda silty clay, 0 to 6 percent slopes"||3|3.1||||"None"|"None"|"0"|3.08|5.81|11.26|16.71|"Well drained"|"Well drained"|"D"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"344756"
"85"|"Vanda silty clay, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|2.51|4.97|9.87|14.77|"Well drained"|"Well drained"|"D"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344757"
"86"|"Vanda-Harlem-Marvan silty clays, 0 to 4 percent slopes"||2|2||||"None"|"Occasional"|"0"|3.13|6.1|11.95|17.66|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344758"
"87"|"Verson clay loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|4.29|7.99|12.71|15.64|"Well drained"|"Well drained"|"C"|"3"|95|"3"|95|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.271|"Slight"|"0"|1|"344759"
"88"|"Volborg silty clay, moist, 2 to 25 percent slopes"||14|14|46|||"None"|"None"|"0"|3.15|5.46|5.46|5.46|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"344760"
"89"|"Volborg-Volborg, eroded-Julin silty clays, 4 to 25 percent slopes"||15|13.9|28|||"None"|"None"|"0"|3.2|4.68|5.49|5.49|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"344761"
"9"|"Bascovy-Neldore-Neldore, moist, silty clays, 6 to 60 percent slopes"||11|22.2|30|||"None"|"None"|"0"|3.47|5.41|7.24|7.89|"Well drained"|"Well drained"|"D"||97|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.747|"Severe"|"0"|1|"344762"
"90"|"Volborg, eroded-Rock outcrop-Julin complex, 4 to 25 percent slopes"||15|12.7|28|||"None"|"None"|"0"|3.16|4.53|5.57|5.57|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"344763"
"91"|"Weingart silty clay loam, 1 to 8 percent slopes"||5|5.5|74|||"None"|"None"|"0"|3.81|6.37|8.39|8.39|"Well drained"|"Well drained"|"D"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.31|"Moderate"|"0"|1|"344764"
"92"|"Weingart-Warhorse complex, 1 to 8 percent slopes"||5|5|46|||"None"|"None"|"0"|4.03|6.49|8.12|8.12|"Well drained"|"Well drained"|"D"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.306|"Moderate"|"0"|1|"344765"
"93"|"Yamacall loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.09|7.54|14.19|20.71|"Well drained"|"Well drained"|"B"|"2"|85|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.197|"Slight"|"0"|0.15|"344766"
"94"|"Yamacall loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.06|8.02|15.7|23.13|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.198|"Moderate"|"0"|0.132|"344767"
"95"|"Yamac clay loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.16|8.16|16.16|24.16|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.194|"Slight"|"0"|0|"344768"
"96"|"Yamac clay loam, 2 to 8 percent slopes"||5|5.5||||"None"|"None"|"0"|4.16|8.16|15.7|22.9|"Well drained"|"Well drained"|"B"|"3"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.193|"Moderate"|"0"|0.065|"344769"
"97"|"Yamac-Busby complex, 2 to 8 percent slopes"||5|5.7||||"None"|"None"|"0"|3.91|7.71|14.66|21.11|"Well drained"|"Well drained"|"B"||100|"4"|50|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.118|"Moderate"|"0"|0.255|"344770"
"98"|"Yamacall-Delpoint loams, 2 to 8 percent slopes"||5|5.2|71|||"None"|"None"|"0"|3.76|7.34|12.36|16|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Moderate"|"0"|0.359|"344771"
"99"|"Yawdim silty clay, 8 to 15 percent slopes"||12|12|41|||"None"|"None"|"0"|4.25|6.97|6.97|6.97|"Well drained"|"Well drained"|"D"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"344772"
"105"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"360711"
"106"|"McKenzie silty clay, 0 to 2 percent slopes"||1|1.1||0|0|"None"|"None"|"90"|3.75|7.45|14.68|21.87|"Poorly drained"|"Poorly drained"|"D"||90|"5"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.948|"Slight"|"90"|1|"360712"
"107"|"Havre and Glendive soils, channeled, frequently flooded"||1|1||||"Frequent"|"Frequent"|"0"|3.74|7.18|13.95|20.67|"Well drained"|"Well drained"|"B"||90|"6"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.404|"Slight"|"3"|0.98|"361680"
"21"|"Cabbart-Yawdim-Rock outcrop complex, 4 to 35 percent slopes"||20|22|38|||"None"|"None"|"0"|3.51|5.57|5.57|5.57|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.563|"Severe"|"0"|1|"2837652"
"66"|"Neldore-Rock outcrop complex, 15 to 60 percent slopes"||35|32.1|38|||"None"|"None"|"0"|3.67|5.72|6.4|6.72|"Well drained"|"Well drained"|"D"||100|"7"|58|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.954|"Severe"|"0"|1|"2986034"
