08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21129514"|"21337544"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129515"|"21337545"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yetull soil is a minor component."|"21129516"|"21337546"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129517"|"21337547"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129559"|"21337589"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129560"|"21337590"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129561"|"21337591"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129562"|"21337592"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21129563"|"21337593"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129564"|"21337594"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist, calcareous component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129586"|"21337616"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129587"|"21337617"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21129588"|"21337618"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21129589"|"21337619"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21129590"|"21337620"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129591"|"21337621"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, calcareous component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129592"|"21337622"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129593"|"21337623"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129594"|"21337624"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21129595"|"21337625"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129596"|"21337626"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, calcareous component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129597"|"21337627"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129598"|"21337628"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129518"|"21337548"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21129519"|"21337549"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of sandy residuum weathered from calcareous sandstone over semiconsolidated residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129520"|"21337550"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21129521"|"21337551"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129522"|"21337552"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129523"|"21337553"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129524"|"21337554"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore, saline soil is a minor component."|"21129525"|"21337555"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129526"|"21337556"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129527"|"21337557"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21129528"|"21337558"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills on plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129529"|"21337559"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills on plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129530"|"21337560"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129604"|"21337634"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, calcareous component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129603"|"21337633"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129602"|"21337632"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonview soil is a minor component."|"21129601"|"21337631"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bascovy soil is a minor component."|"21129600"|"21337630"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129599"|"21337629"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129263"|"21337293"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129262"|"21337292"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackhall component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129261"|"21337291"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 55 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129260"|"21337290"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"21129259"|"21337289"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129258"|"21337288"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Orinoco component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"21129470"|"21337500"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21129469"|"21337499"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129468"|"21337498"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129467"|"21337497"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on fan remnants, terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC055MT Gravel (gr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129466"|"21337496"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129257"|"21337287"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129256"|"21337286"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129255"|"21337285"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackhall component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129254"|"21337284"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore, saline soil is a minor component."|"21129229"|"21337259"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21129228"|"21337258"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129227"|"21337257"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21129226"|"21337256"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129225"|"21337255"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 75 percent of the map unit. Slopes are 1 to 8 percent. This component is on alluvial fans on sedimentary plains.  Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21129224"|"21337254"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, calcareous component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on stream terraces on plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC613MT Silty-limy (sily)   Rru 58a-c  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129605"|"21337635"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Orinoco component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"21129480"|"21337510"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zatoville component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans, plains. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 24 within 30 inches of the soil surface."|"21129479"|"21337509"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Orinoco soil is a minor component."|"21129478"|"21337508"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zatoville component makes up 90 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, plains. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 24 within 30 inches of the soil surface."|"21129477"|"21337507"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21129476"|"21337506"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129475"|"21337505"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129474"|"21337504"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Orinoco component makes up 30 percent of the map unit. Slopes are 15 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 23 within 30 inches of the soil surface."|"21129473"|"21337503"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21129472"|"21337502"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129471"|"21337501"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129496"|"21337526"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains, swales on plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129495"|"21337525"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129494"|"21337524"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21129493"|"21337523"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21129492"|"21337522"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21129491"|"21337521"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21129481"|"21337511"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129201"|"21337231"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 20 percent of the map unit. Slopes are 15 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC049MT Silty-Steep (SiStp)   RRU 58A-C  11-14"" p.z. (combined R058AC046MT, R058AC047MT & R058AC048MT into this site) ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129202"|"21337232"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21129203"|"21337233"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (SwC)    RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129204"|"21337234"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129205"|"21337235"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129264"|"21337294"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129265"|"21337295"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129266"|"21337296"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129267"|"21337297"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist, calcareous component makes up 35 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129579"|"21337609"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, hard soil is a minor component."|"21129580"|"21337610"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21129581"|"21337611"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 25 percent of the map unit. Slopes are 6 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of sandy residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129582"|"21337612"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129583"|"21337613"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 20 percent of the map unit. Slopes are 6 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129584"|"21337614"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart, calcareous soil is a minor component."|"21129585"|"21337615"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21129268"|"21337298"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills, terraces, plains. The parent material consists of alluvium and/or eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129269"|"21337299"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21129270"|"21337300"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 95 percent of the map unit. Slopes are 0 to 8 percent. This component is on fan remnants, terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC055MT Gravel (gr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129271"|"21337301"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21129272"|"21337302"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 90 percent of the map unit. Slopes are 8 to 35 percent. This component is on fan remnants, terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC055MT Gravel (gr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129273"|"21337303"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21129274"|"21337304"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21129275"|"21337305"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC055MT Gravel (gr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129276"|"21337306"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC613MT Silty-limy (sily)   Rru 58a-c  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129277"|"21337307"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC055MT Gravel (gr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent.  "|"21129278"|"21337308"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC613MT Silty-limy (sily)   Rru 58a-c  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129279"|"21337309"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21129280"|"21337310"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants, terraces, plains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC055MT Gravel (gr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129281"|"21337311"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, fan remnants, foothills. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129282"|"21337312"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nobe soil is a minor component."|"21129283"|"21337313"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Creed component makes up 60 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 17 within 30 inches of the soil surface."|"21129284"|"21337314"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129285"|"21337315"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerdrum component makes up 30 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 2 to 4 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129286"|"21337316"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"21129239"|"21337269"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 90 percent of the map unit. Slopes are 1 to 6 percent. This component is on hills, plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21129240"|"21337270"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129241"|"21337271"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 80 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of semiconsolidated loamy residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129497"|"21337527"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cabbart soil is a minor component."|"21129498"|"21337528"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Twilight soil is a minor component."|"21129499"|"21337529"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Yamacall soil is a minor component."|"21129500"|"21337530"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bonfri soil is a minor component."|"21129501"|"21337531"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129565"|"21337595"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129566"|"21337596"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21129567"|"21337597"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129568"|"21337598"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129569"|"21337599"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 15 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129287"|"21337317"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129288"|"21337318"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129289"|"21337319"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129290"|"21337320"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackhall soil is a minor component."|"21129291"|"21337321"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gerdrum soil is a minor component."|"21129292"|"21337322"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129293"|"21337323"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gerdrum soil is a minor component."|"21129294"|"21337324"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129295"|"21337325"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bascovy soil is a minor component."|"21129296"|"21337326"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobar soil is a minor component."|"21129297"|"21337327"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evanston soil is a minor component."|"21129298"|"21337328"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evanston component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129299"|"21337329"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21129300"|"21337330"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobar soil is a minor component."|"21129301"|"21337331"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evanston soil is a minor component."|"21129302"|"21337332"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evanston component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129303"|"21337333"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"21129304"|"21337334"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evanston component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129305"|"21337335"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"21129306"|"21337336"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gravelly surface layer soil is a minor component."|"21129307"|"21337337"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, fan remnants, foothills. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129308"|"21337338"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bascovy component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 13 within 30 inches of the soil surface."|"21129309"|"21337339"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129310"|"21337340"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21129311"|"21337341"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerdrum component makes up 60 percent of the map unit. Slopes are 2 to 15 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 2 to 4 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129312"|"21337342"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nobe soil is a minor component."|"21129313"|"21337343"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Creed component makes up 40 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 17 within 30 inches of the soil surface."|"21129314"|"21337344"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129315"|"21337345"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerdrum component makes up 50 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 2 to 4 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129316"|"21337346"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 90 percent of the map unit. Slopes are 6 to 25 percent. This component is on hills, plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21129242"|"21337272"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils with channery loam surf soil is a minor component."|"21129243"|"21337273"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129244"|"21337274"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nobe soil is a minor component."|"21129317"|"21337347"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129318"|"21337348"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 30 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"21129319"|"21337349"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerdrum component makes up 55 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 2 to 4 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129320"|"21337350"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"21129505"|"21337535"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerdrum component makes up 40 percent of the map unit. Slopes are 0 to 8 percent. This component is on alluvial fans on plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 2 to 7 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R060BE565MT Claypan (cp)   Rru 60b-e  10-14"" P.z.  Lega ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129506"|"21337536"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129507"|"21337537"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 25 percent of the map unit. Slopes are 0 to 8 percent. This component is on alluvial fans on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R060BE568MT Dense Clay (dc)   Rru 60b-e  10-14"" P.z. Legac ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129508"|"21337538"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"21129509"|"21337539"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Creed component makes up 20 percent of the map unit. Slopes are 0 to 8 percent. This component is on alluvial flats alluvial fans on sedimentary plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer, natric, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R060BE565MT Claypan (cp)   Rru 60b-e  10-14"" P.z.  Lega ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 17 within 30 inches of the soil surface."|"21129510"|"21337540"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, saline soil is a minor component."|"21129321"|"21337351"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129322"|"21337352"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, wet soil is a minor component."|"21129323"|"21337353"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, saline soil is a minor component."|"21129324"|"21337354"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129325"|"21337355"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129326"|"21337356"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, wet soil is a minor component."|"21129327"|"21337357"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129328"|"21337358"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlake component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129329"|"21337359"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake, saline soil is a minor component."|"21129330"|"21337360"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129331"|"21337361"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129332"|"21337362"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, saline soil is a minor component."|"21129333"|"21337363"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129334"|"21337364"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21129335"|"21337365"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129336"|"21337366"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129337"|"21337367"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, saline soil is a minor component."|"21129338"|"21337368"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129339"|"21337369"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem soil is a minor component."|"21129340"|"21337370"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21129341"|"21337371"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"21129342"|"21337372"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21129343"|"21337373"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129344"|"21337374"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delplain soil is a minor component."|"21129245"|"21337275"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delplain component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills, plains. The parent material consists of colluvium derived from sandstone and shale and/or residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21129246"|"21337276"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 55 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills, plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21129247"|"21337277"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129248"|"21337278"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, saline soil is a minor component."|"21129345"|"21337375"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"21129346"|"21337376"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanly soil is a minor component."|"21129347"|"21337377"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129348"|"21337378"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129349"|"21337379"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"21129350"|"21337380"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, SALINE soil is a minor component."|"21129351"|"21337381"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"21129352"|"21337382"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129353"|"21337383"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129354"|"21337384"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129355"|"21337385"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem, saline soil is a minor component."|"21129356"|"21337386"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129357"|"21337387"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 30 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129358"|"21337388"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, wet soil is a minor component."|"21129359"|"21337389"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, saline soil is a minor component."|"21129360"|"21337390"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129361"|"21337391"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem soil is a minor component."|"21129362"|"21337392"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zatoville component makes up 25 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, plains. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 24 within 30 inches of the soil surface."|"21129363"|"21337393"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobar component makes up 60 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"21129364"|"21337394"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bascovy soil is a minor component."|"21129365"|"21337395"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129366"|"21337396"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21129367"|"21337397"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129511"|"21337541"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kremlin component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains. The parent material consists of loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129512"|"21337542"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21129513"|"21337543"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marias component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21129368"|"21337398"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gerdrum soil is a minor component."|"21129369"|"21337399"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Creed soil is a minor component."|"21129370"|"21337400"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21129371"|"21337401"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marmarth component makes up 90 percent of the map unit. Slopes are 1 to 8 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21129372"|"21337402"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bascovy soil is a minor component."|"21129373"|"21337403"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marvan component makes up 85 percent of the map unit. Slopes are 1 to 8 percent. This component is on fans, terraces, hillslopes, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21129374"|"21337404"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan, saline soil is a minor component."|"21129375"|"21337405"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"21129249"|"21337279"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, fan remnants, foothills. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129250"|"21337280"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 35 percent of the map unit. Slopes are 0 to 8 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"21129376"|"21337406"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marvan component makes up 50 percent of the map unit. Slopes are 0 to 8 percent. This component is on fans, terraces, hillslopes, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21129377"|"21337407"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bascovy soil is a minor component."|"21129378"|"21337408"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129379"|"21337409"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 85 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129570"|"21337600"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21129571"|"21337601"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, soft soil is a minor component."|"21129572"|"21337602"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129573"|"21337603"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129543"|"21337573"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129544"|"21337574"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21129545"|"21337575"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129546"|"21337576"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore, saline soil is a minor component."|"21129547"|"21337577"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129531"|"21337561"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129532"|"21337562"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 55 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R060BE577MT Shallow Clay Mlra 60b-e, 10-14 P.z. ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129533"|"21337563"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R060BE566MT Clayey, Mlra 60b-e, 10-14 P.z. ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129534"|"21337564"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129535"|"21337565"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 45 percent of the map unit. Slopes are 6 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129606"|"21337636"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bascovy component makes up 25 percent of the map unit. Slopes are 6 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129607"|"21337637"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129608"|"21337638"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129609"|"21337639"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21129610"|"21337640"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129380"|"21337410"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129381"|"21337411"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 40 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC053MT Dense Clay (dc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129382"|"21337412"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 45 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129383"|"21337413"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullock soil is a minor component."|"21129536"|"21337566"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129537"|"21337567"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vaeda soil is a minor component."|"21129538"|"21337568"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21129539"|"21337569"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129540"|"21337570"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Volborg component makes up 35 percent of the map unit. Slopes are 4 to 25 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC614MT Coarse Clay (cc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129541"|"21337571"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 35 percent of the map unit. Slopes are 4 to 25 percent. This component is on low hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129542"|"21337572"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Weingart component makes up 35 percent of the map unit. Slopes are 2 to 10 percent. This component is on low hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129384"|"21337414"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129385"|"21337415"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129386"|"21337416"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129387"|"21337417"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129388"|"21337418"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 50 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129389"|"21337419"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129390"|"21337420"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 40 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21129391"|"21337421"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129392"|"21337422"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129393"|"21337423"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129251"|"21337281"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21129252"|"21337282"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"21129253"|"21337283"
06/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore, MOIST component makes up 50 percent of the map unit. Slopes are 6 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AY730MT Ponderosa Pine 15-19 ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129611"|"21337641"
06/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore, DRY component makes up 15 percent of the map unit. Slopes are 6 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129612"|"21337642"
06/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bascovy component makes up 20 percent of the map unit. Slopes are 6 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129613"|"21337643"
06/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129614"|"21337644"
06/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129615"|"21337645"
06/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129616"|"21337646"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21129394"|"21337424"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nobe component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21129395"|"21337425"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absher component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 1 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"21129396"|"21337426"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinebreaks component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129397"|"21337427"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129398"|"21337428"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129399"|"21337429"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129400"|"21337430"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21129401"|"21337431"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129402"|"21337432"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21129403"|"21337433"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 90 percent of the map unit. Slopes are 1 to 6 percent. This component is on low hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129404"|"21337434"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Creed soil is a minor component."|"21129405"|"21337435"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21129406"|"21337436"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129407"|"21337437"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21129408"|"21337438"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129409"|"21337439"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Weingart component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129410"|"21337440"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teigen component makes up 90 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, plains. The parent material consists of alluvium derived from acid shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21129411"|"21337441"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Julin soil is a minor component."|"21129412"|"21337442"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackhall soil is a minor component."|"21129413"|"21337443"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129414"|"21337444"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21129230"|"21337260"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21129231"|"21337261"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21129232"|"21337262"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21129233"|"21337263"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129234"|"21337264"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 14 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129235"|"21337265"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129211"|"21337241"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129212"|"21337242"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129213"|"21337243"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"21129214"|"21337244"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sunburst, gravelly surface soil is a minor component."|"21129215"|"21337245"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bascovy component makes up 55 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129216"|"21337246"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129217"|"21337247"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackhall component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129415"|"21337445"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129416"|"21337446"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129417"|"21337447"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129418"|"21337448"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129419"|"21337449"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Frequently flooded soils soil is a minor component."|"21129420"|"21337450"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustic Torriorthents component makes up 85 percent of the map unit. Slopes are 15 to 45 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"21129421"|"21337451"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils that are strongly saline soil is a minor component."|"21129422"|"21337452"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Frequently flooded soils soil is a minor component."|"21129423"|"21337453"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustic Torriorthents component makes up 85 percent of the map unit. Slopes are 15 to 45 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"21129424"|"21337454"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129425"|"21337455"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderately saline soils soil is a minor component."|"21129426"|"21337456"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustic Torriorthents component makes up 90 percent of the map unit. Slopes are 0 to 8 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"21129427"|"21337457"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"21129428"|"21337458"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vaeda component makes up 90 percent of the map unit. Slopes are 0 to 6 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC053MT Dense Clay (dc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21129429"|"21337459"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 95 percent of the map unit. Slopes are 0 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC053MT Dense Clay (dc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"21129430"|"21337460"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129431"|"21337461"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanda component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC053MT Dense Clay (dc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"21129432"|"21337462"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marvan component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on fans, terraces, hillslopes, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC615MT Clayey-saline (cys)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21129433"|"21337463"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129434"|"21337464"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"21129435"|"21337465"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Verson component makes up 95 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129436"|"21337466"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21129437"|"21337467"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Volborg component makes up 85 percent of the map unit. Slopes are 2 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from acid shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129438"|"21337468"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129439"|"21337469"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129440"|"21337470"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Volborg component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from acid shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC052MT Shale (sh)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129441"|"21337471"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Volborg component makes up 45 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from acid shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC614MT Coarse Clay (cc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129442"|"21337472"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129443"|"21337473"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Julin component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from acid shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC614MT Coarse Clay (cc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21129444"|"21337474"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore, moist component makes up 25 percent of the map unit. Slopes are 6 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129218"|"21337248"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 25 percent of the map unit. Slopes are 6 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129219"|"21337249"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bascovy component makes up 40 percent of the map unit. Slopes are 6 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129220"|"21337250"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21129221"|"21337251"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129222"|"21337252"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129223"|"21337253"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Volborg soil is a minor component."|"21129445"|"21337475"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Volborg component makes up 40 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from acid shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC052MT Shale (sh)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21129446"|"21337476"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129447"|"21337477"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Julin component makes up 20 percent of the map unit. Slopes are 4 to 10 percent. This component is on hills, plains. The parent material consists of residuum weathered from acid shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC614MT Coarse Clay (cc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21129448"|"21337478"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129449"|"21337479"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Weingart component makes up 85 percent of the map unit. Slopes are 1 to 8 percent. This component is on low hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129450"|"21337480"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21129451"|"21337481"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21129452"|"21337482"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Weingart component makes up 50 percent of the map unit. Slopes are 1 to 8 percent. This component is on low hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (cp)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21129453"|"21337483"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Warhorse component makes up 35 percent of the map unit. Slopes are 1 to 8 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129454"|"21337484"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on sedimentary plains. The parent material consists of alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129502"|"21337532"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21129503"|"21337533"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21129504"|"21337534"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129548"|"21337578"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21129549"|"21337579"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21129550"|"21337580"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"21129551"|"21337581"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21129552"|"21337582"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"21129455"|"21337485"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129456"|"21337486"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129457"|"21337487"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21129458"|"21337488"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21129459"|"21337489"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129460"|"21337490"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129461"|"21337491"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21129462"|"21337492"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129553"|"21337583"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"21129554"|"21337584"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21129555"|"21337585"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21129556"|"21337586"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21129557"|"21337587"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129558"|"21337588"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129463"|"21337493"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21129464"|"21337494"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21129465"|"21337495"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21129482"|"21337512"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Gerdrum soil is a minor component."|"21129236"|"21337266"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Marvan soil is a minor component."|"21129237"|"21337267"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenzie component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on depressions on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 0 inches during March, April, May, June. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE007MT Overflow (ov)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21129238"|"21337268"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways on plains, flood plains on valleys. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE007MT Overflow (ov)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21129483"|"21337513"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways on plains, flood plains on valleys. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE007MT Overflow (ov)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129484"|"21337514"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21129485"|"21337515"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanly soil is a minor component."|"21129486"|"21337516"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"21129487"|"21337517"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21129488"|"21337518"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"21129489"|"21337519"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21129490"|"21337520"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129206"|"21337236"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (SwC)    RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21129207"|"21337237"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21129208"|"21337238"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21129209"|"21337239"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very shallow soils soil is a minor component."|"21129210"|"21337240"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 55 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills on plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21129574"|"21337604"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21129575"|"21337605"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore, saline soil is a minor component."|"21129576"|"21337606"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marias soil is a minor component."|"21129577"|"21337607"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21129578"|"21337608"
