07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Dooley component makes up 90 percent of the map unit. Slopes are 0 to 6 percent. This component is on till plains. The parent material consists of sandy alluvium and/or eolian sands over till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130951"|"21338982"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"21130952"|"21338983"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130953"|"21338984"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21130954"|"21338985"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"21130955"|"21338986"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Dooley component makes up 90 percent of the map unit. Slopes are 6 to 12 percent. This component is on till plains. The parent material consists of sandy alluvium and/or eolian sands over till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130956"|"21338987"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"21130957"|"21338988"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130958"|"21338989"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130959"|"21338990"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farnuf component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130960"|"21338991"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"21130961"|"21338992"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130962"|"21338993"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"21130963"|"21338994"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farnuf component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans, terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130964"|"21338995"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130965"|"21338996"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130966"|"21338997"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"21130967"|"21338998"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farnuf component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans, hillslopes. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130968"|"21338999"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130969"|"21339000"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130970"|"21339001"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"21130971"|"21339002"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farnuf component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on flood plains, fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130972"|"21339003"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"21130973"|"21339004"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130974"|"21339005"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 45 percent of the map unit. Slopes are 0 to 6 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"21130975"|"21339006"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"21130976"|"21339007"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21130977"|"21339008"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130978"|"21339009"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dimmick soil is a minor component."|"21130979"|"21339010"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Grail component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on swales, drainageways. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"21130980"|"21339011"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"21130981"|"21339012"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130982"|"21339013"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cherry component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of alluvium derived from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21130950"|"21338981"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Shambo soil is a minor component."|"21130949"|"21338980"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21130948"|"21338979"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lambert soil is a minor component."|"21130947"|"21338978"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cherry component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans, stream terraces. The parent material consists of alluvium derived from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21130946"|"21338977"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Shambo soil is a minor component."|"21130945"|"21338976"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130944"|"21338975"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21130943"|"21338974"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lambert soil is a minor component."|"21130942"|"21338973"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The McKenzie soil is a minor component."|"21130941"|"21338972"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130940"|"21338971"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"21130939"|"21338970"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130938"|"21338969"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Bowdoin component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE073MT Dense Clay (dc) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. "|"21130937"|"21338968"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21130936"|"21338967"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130935"|"21338966"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130934"|"21338965"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Bowbells component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on drainageways, swales. The parent material consists of alluvium over till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130933"|"21338964"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21130932"|"21338963"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130931"|"21338962"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21130930"|"21338961"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Bowbells component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways. The parent material consists of alluvium over till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21130929"|"21338960"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"21130928"|"21338959"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130927"|"21338958"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"21130926"|"21338957"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21130925"|"21338956"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Blanchard component makes up 90 percent of the map unit. Slopes are 4 to 12 percent. This component is on dunes. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21130924"|"21338955"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"21130923"|"21338954"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130922"|"21338953"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"21130921"|"21338952"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21130920"|"21338951"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Blanchard component makes up 90 percent of the map unit. Slopes are 4 to 20 percent. This component is on dunes. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21130919"|"21338950"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adger soil is a minor component."|"21130910"|"21338941"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21130909"|"21338940"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McKenzie soil is a minor component."|"21130908"|"21338939"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21130907"|"21338938"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimmick component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions on till plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is very high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R053AY711MT Recharge Closed Depression (cdr) ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21130906"|"21338937"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"21130983"|"21339014"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Trembles soil is a minor component."|"21130984"|"21339015"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"21130985"|"21339016"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havrelon component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21130986"|"21339017"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"21130987"|"21339018"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130988"|"21339019"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"21130989"|"21339020"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"21130990"|"21339021"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havrelon component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21130991"|"21339022"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lambert component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans, pediments. The parent material consists of alluvium derived from shale and siltstone and/or residuum weathered from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21130992"|"21339023"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130993"|"21339024"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"21130994"|"21339025"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"21130995"|"21339026"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lambert component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans, pediments. The parent material consists of alluvium derived from shale and siltstone and/or residuum weathered from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21130996"|"21339027"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21130997"|"21339028"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21130998"|"21339029"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"21130999"|"21339030"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lambert component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on fans, pediments. The parent material consists of alluvium derived from shale and siltstone and/or residuum weathered from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131000"|"21339031"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21131001"|"21339032"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21131002"|"21339033"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"21131003"|"21339034"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lambert component makes up 50 percent of the map unit. Slopes are 15 to 65 percent. This component is on fans, pediments. The parent material consists of alluvium derived from shale and siltstone and/or residuum weathered from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE065MT Clayey-steep (cystp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131004"|"21339035"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21131005"|"21339036"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lambert component makes up 65 percent of the map unit. Slopes are 20 to 50 percent. This component is on fans, pediments. The parent material consists of alluvium derived from shale and siltstone and/or residuum weathered from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE065MT Clayey-steep (cystp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131006"|"21339037"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 35 percent of the map unit. Slopes are 20 to 50 percent. This component is on escarpments. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE065MT Clayey-steep (cystp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"21131007"|"21339038"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lihen component makes up 90 percent of the map unit. Slopes are 0 to 6 percent. This component is on outwash terraces. The parent material consists of sandy alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21131008"|"21339039"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Blanchard soil is a minor component."|"21131009"|"21339040"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"21131010"|"21339041"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21131011"|"21339042"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Manning soil is a minor component."|"21131012"|"21339043"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"21131013"|"21339044"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21131014"|"21339045"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"21131015"|"21339046"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lohler component makes up 95 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131016"|"21339047"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lohler component makes up 95 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. "|"21131017"|"21339048"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"21131018"|"21339049"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21131019"|"21339050"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"21131020"|"21339051"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131021"|"21339052"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"21131022"|"21339053"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"21131023"|"21339054"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Manning component makes up 90 percent of the map unit. Slopes are 0 to 6 percent. This component is on stream terraces. The parent material consists of sandy alluvium over gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE079MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  "|"21131024"|"21339055"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lambert soil is a minor component."|"21131025"|"21339056"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Savage soil is a minor component."|"21131026"|"21339057"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Marias component makes up 95 percent of the map unit. Slopes are 2 to 4 percent. This component is on lake plains. The parent material consists of clayey glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21131027"|"21339058"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenzie component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions on till plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is very high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY703MT Discharge Closed Depression (cdd) ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21130911"|"21338942"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimmick soil is a minor component."|"21130912"|"21338943"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21130913"|"21338944"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adger soil is a minor component."|"21130914"|"21338945"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimmick soil is a minor component."|"21130902"|"21338933"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adger soil is a minor component."|"21130903"|"21338934"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nishon component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions on till plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is very high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY711MT Recharge Closed Depression (cdr) ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21130904"|"21338935"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21130905"|"21338936"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Nobe component makes up 95 percent of the map unit. Slopes are 0 to 6 percent. This component is on flood plains. The parent material consists of salty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE072MT Saline Overflow (sov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. "|"21131028"|"21339059"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"21131029"|"21339060"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Parshall component makes up 90 percent of the map unit. Slopes are 2 to 6 percent. This component is on dunes, outwash terraces. The parent material consists of alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21131030"|"21339061"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Blanchard soil is a minor component."|"21131031"|"21339062"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21131032"|"21339063"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"21131033"|"21339064"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131034"|"21339065"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Savage component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21131035"|"21339066"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131036"|"21339067"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131037"|"21339068"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Marias soil is a minor component."|"21131038"|"21339069"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Savage component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans, terraces. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21131039"|"21339070"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131040"|"21339071"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131041"|"21339072"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Marias soil is a minor component."|"21131042"|"21339073"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Savage component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21131043"|"21339074"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131044"|"21339075"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131045"|"21339076"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21131046"|"21339077"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Marias soil is a minor component."|"21131047"|"21339078"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131048"|"21339079"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131049"|"21339080"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"21131050"|"21339081"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Shambo component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces, till plains, fans. The parent material consists of alluvium and/or calcareous loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"21131051"|"21339082"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tally component makes up 90 percent of the map unit. Slopes are 2 to 6 percent. This component is on outwash terraces, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21131052"|"21339083"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21131053"|"21339084"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131054"|"21339085"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131055"|"21339086"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Trembles component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131056"|"21339087"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"21131057"|"21339088"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Trembles soil is a minor component."|"21131058"|"21339089"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"21131059"|"21339090"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21131060"|"21339091"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131061"|"21339092"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"21131062"|"21339093"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21131063"|"21339094"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131064"|"21339095"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, outwash plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"21131065"|"21339096"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21131066"|"21339097"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"21131067"|"21339098"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"21131068"|"21339099"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131069"|"21339100"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on terraces, outwash plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"21131070"|"21339101"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"21131071"|"21339102"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131072"|"21339103"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Savage soil is a minor component."|"21131073"|"21339104"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Marias soil is a minor component."|"21131074"|"21339105"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Ustifluvents component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil meets hydric criteria.   "|"21131075"|"21339106"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21131076"|"21339107"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Wabek component makes up 90 percent of the map unit. Slopes are 0 to 35 percent. This component is on outwash plains. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131077"|"21339108"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"21131078"|"21339109"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"21131079"|"21339110"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Manning soil is a minor component."|"21131080"|"21339111"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"21131081"|"21339112"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Wabek component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131082"|"21339113"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lambert component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on fans, pediments. The parent material consists of alluvium derived from shale and siltstone and/or residuum weathered from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21131083"|"21339114"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21131089"|"21339120"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21131090"|"21339121"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21131091"|"21339122"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"21131092"|"21339123"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"21131093"|"21339124"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131094"|"21339125"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21131095"|"21339126"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21131096"|"21339127"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21131097"|"21339128"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21131098"|"21339129"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"21131099"|"21339130"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"21131100"|"21339131"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131101"|"21339132"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131102"|"21339133"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21131103"|"21339134"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Williams component makes up 65 percent of the map unit. Slopes are 0 to 4 percent. This component is on till plains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21131084"|"21339115"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on till plains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"21131085"|"21339116"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131110"|"21339141"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131111"|"21339142"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"21131112"|"21339143"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21131113"|"21339144"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"21131114"|"21339145"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"21131115"|"21339146"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21131116"|"21339147"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21131117"|"21339148"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131118"|"21339149"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131119"|"21339150"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"21131120"|"21339151"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21131121"|"21339152"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"21131122"|"21339153"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"21131123"|"21339154"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"21131124"|"21339155"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 75 percent of the map unit. Slopes are 15 to 60 percent. This component is on hillslopes on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY040MT Loamy Steep (lostp)   Lru 53a-y ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21131104"|"21339135"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21131105"|"21339136"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"21131106"|"21339137"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"21131107"|"21339138"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahl soil is a minor component."|"21131108"|"21339139"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arnegard soil is a minor component."|"21131109"|"21339140"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 60 percent of the map unit. Slopes are 15 to 25 percent. This component is on terminal moraines. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE065MT Clayey-steep (cystp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"21131086"|"21339117"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Williams component makes up 35 percent of the map unit. Slopes are 15 to 25 percent. This component is on terminal moraines. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21131087"|"21339118"
07/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dimmick soil is a minor component."|"21131088"|"21339119"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"21130915"|"21338946"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"21130916"|"21338947"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"21130917"|"21338948"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Manning soil is a minor component."|"21130918"|"21338949"
