08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanstel soil is a minor component."|"21134989"|"21343112"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134990"|"21343113"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21134991"|"21343114"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Floweree component makes up 10 percent of the map unit. Slopes are 8 to 15 percent. This component is on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134992"|"21343115"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 75 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134993"|"21343116"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanstel soil is a minor component."|"21134994"|"21343117"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21134995"|"21343118"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134996"|"21343119"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21134988"|"21343111"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanstel component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134987"|"21343110"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21134986"|"21343109"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 70 percent of the map unit. Slopes are 0 to 4 percent. This component is on low hills on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134985"|"21343108"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Allentine component makes up 30 percent of the map unit. Slopes are 2 to 7 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 3 to  inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134500"|"21342623"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21134499"|"21342622"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gilt Edge component makes up 60 percent of the map unit. Slopes are 2 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, natric, is 5 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134498"|"21342621"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134497"|"21342620"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134496"|"21342619"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, fans, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134495"|"21342618"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, fans, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134494"|"21342617"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134493"|"21342616"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134492"|"21342615"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21134491"|"21342614"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134490"|"21342613"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 20 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134489"|"21342612"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 70 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, fans, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134488"|"21342611"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 70 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, fans, foothills. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134487"|"21342610"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21134486"|"21342609"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 20 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134485"|"21342608"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134484"|"21342607"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fattig component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134483"|"21342606"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"21134482"|"21342605"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134481"|"21342604"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21135001"|"21343124"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21135000"|"21343123"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambeth soil is a minor component."|"21134999"|"21343122"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on low hills on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134998"|"21343121"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brushton component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on paleoterraces on sedimentary plains. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134997"|"21343120"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134480"|"21342603"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134479"|"21342602"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC047MT Clayey-steep (cystp)   Rru 58a-c  11-14"" P.z.      Deleted.  Refer To Site: R058a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134478"|"21342601"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 30 percent of the map unit. Slopes are 15 to 25 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134477"|"21342600"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, shale soil is a minor component."|"21134476"|"21342599"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134475"|"21342598"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134474"|"21342597"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 80 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC047MT Clayey-steep (cystp)   Rru 58a-c  11-14"" P.z.      Deleted.  Refer To Site: R058a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134473"|"21342596"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134472"|"21342595"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134471"|"21342594"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134470"|"21342593"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134469"|"21342592"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Razor soil is a minor component."|"21134468"|"21342591"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 80 percent of the map unit. Slopes are 7 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134467"|"21342590"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134466"|"21342589"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Razor soil is a minor component."|"21134465"|"21342588"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134464"|"21342587"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134463"|"21342586"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 60 percent of the map unit. Slopes are 7 to 15 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134462"|"21342585"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21134461"|"21342584"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shaak component makes up 30 percent of the map unit. Slopes are 7 to 15 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134460"|"21342583"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oburn soil is a minor component."|"21134459"|"21342582"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 70 percent of the map unit. Slopes are 7 to 12 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134458"|"21342581"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21134457"|"21342580"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judith component makes up 20 percent of the map unit. Slopes are 10 to 15 percent. This component is on terraces, fans, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134456"|"21342579"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shaak soil is a minor component."|"21134455"|"21342578"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21134454"|"21342577"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 80 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134453"|"21342576"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shaak soil is a minor component."|"21134452"|"21342575"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oburn soil is a minor component."|"21134451"|"21342574"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oburn soil is a minor component."|"21134450"|"21342573"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shaak soil is a minor component."|"21134449"|"21342572"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21134448"|"21342571"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134447"|"21342570"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134446"|"21342569"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134445"|"21342568"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clapper component makes up 80 percent of the map unit. Slopes are 7 to 15 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC046MT Silty-steep 11-14"" P.z.     Deleted.  Refer To Site:  R058ac049mt ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134444"|"21342567"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134443"|"21342566"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134442"|"21342565"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134441"|"21342564"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clapper component makes up 80 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XC516MT Draft Silty-steep (sistp)   Rru 46-c  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134440"|"21342563"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134439"|"21342562"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134438"|"21342561"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shorey soil is a minor component."|"21134437"|"21342560"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134436"|"21342559"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21134435"|"21342558"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, lakebeds (relict), plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21134434"|"21342557"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134433"|"21342556"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 85 percent of the map unit. Slopes are 1 to 6 percent. This component is on fans, terraces, lakebeds (relict), plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21134432"|"21342555"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134431"|"21342554"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21134430"|"21342553"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, lakebeds (relict), plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21134429"|"21342552"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21134428"|"21342551"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134427"|"21342550"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134426"|"21342549"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Big Horn component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on hills, plains. The parent material consists of residuum. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3c.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134425"|"21342548"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21134424"|"21342547"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Allentine component makes up 35 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 3 to  inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134423"|"21342546"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 55 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134422"|"21342545"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134421"|"21342544"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Allentine soil is a minor component."|"21134420"|"21342543"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134419"|"21342542"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134418"|"21342541"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134417"|"21342540"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21134416"|"21342539"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134415"|"21342538"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134414"|"21342537"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134413"|"21342536"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21134412"|"21342535"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134411"|"21342534"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134410"|"21342533"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134409"|"21342532"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134408"|"21342531"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134407"|"21342530"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bainville component makes up 65 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134406"|"21342529"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worland component makes up 25 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134405"|"21342528"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bainville component makes up 40 percent of the map unit. Slopes are 7 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC046MT Silty-steep 11-14"" P.z.     Deleted.  Refer To Site:  R058ac049mt ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134404"|"21342527"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21134403"|"21342526"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134402"|"21342525"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Razor soil is a minor component."|"21134401"|"21342524"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134400"|"21342523"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 40 percent of the map unit. Slopes are 7 to 25 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC046MT Silty-steep 11-14"" P.z.     Deleted.  Refer To Site:  R058ac049mt ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134399"|"21342522"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134398"|"21342521"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC046MT Silty-steep 11-14"" P.z.     Deleted.  Refer To Site:  R058ac049mt ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134397"|"21342520"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bainville component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC046MT Silty-steep 11-14"" P.z.     Deleted.  Refer To Site:  R058ac049mt ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134396"|"21342519"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134395"|"21342518"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134394"|"21342517"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134393"|"21342516"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 70 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134392"|"21342515"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 20 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, lakebeds (relict), plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21134391"|"21342514"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134390"|"21342513"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134389"|"21342512"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, lakebeds (relict), plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21134388"|"21342511"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 60 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134387"|"21342510"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134386"|"21342509"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134385"|"21342508"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134384"|"21342507"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134383"|"21342506"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134382"|"21342505"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134381"|"21342504"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134380"|"21342503"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134379"|"21342502"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 80 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134378"|"21342501"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134377"|"21342500"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134376"|"21342499"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134375"|"21342498"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Apron component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills. The parent material consists of alluvium derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134374"|"21342497"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134373"|"21342496"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134372"|"21342495"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"21134371"|"21342494"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134370"|"21342493"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134369"|"21342492"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"21134368"|"21342491"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Apron component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills. The parent material consists of alluvium derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC056MT Sands (sa)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134367"|"21342490"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 65 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21134366"|"21342489"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134365"|"21342488"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 25 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21134364"|"21342487"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 80 percent of the map unit. Slopes are 7 to 15 percent. This component is on hills, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21134363"|"21342486"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134362"|"21342485"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"21134361"|"21342484"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134360"|"21342483"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134359"|"21342482"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alluvial land component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on channels, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC043MT Wet Meadow (wm)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134358"|"21342481"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134357"|"21342480"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alluvial land component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 6 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21134356"|"21342479"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134355"|"21342478"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21134354"|"21342477"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alluvial land component makes up 98 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 21 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21134353"|"21342476"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21135040"|"21343163"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135041"|"21343164"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135042"|"21343165"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135043"|"21343166"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Alluvial land component makes up 98 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 21 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21134352"|"21342475"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21134351"|"21342474"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amherst soil is a minor component."|"21134350"|"21342473"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, foothills. The parent material consists of colluvium derived from sandstone and shale and/or residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134349"|"21342472"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"21134348"|"21342471"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135038"|"21343161"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"21135049"|"21343172"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21135050"|"21343173"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135051"|"21343174"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 4 percent. This component is on pediments on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135052"|"21343175"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on pediments on sedimentary plains. The parent material consists of interbedded residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135053"|"21343176"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135044"|"21343167"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21135045"|"21343168"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135046"|"21343169"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"21135047"|"21343170"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21135048"|"21343171"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"21134347"|"21342470"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on hills, foothills. The parent material consists of colluvium derived from sandstone and shale and/or residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134346"|"21342469"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amherst soil is a minor component."|"21134345"|"21342468"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134735"|"21342858"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pierre component makes up 55 percent of the map unit. Slopes are 7 to 10 percent. This component is on hills, plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21134734"|"21342857"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lismas component makes up 35 percent of the map unit. Slopes are 10 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC052MT Shale (sh)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21134733"|"21342856"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134732"|"21342855"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21134731"|"21342854"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134953"|"21343076"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"21134954"|"21343077"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134955"|"21343078"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21134730"|"21342853"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"21134729"|"21342852"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pierre component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21134728"|"21342851"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134727"|"21342850"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oburn component makes up 40 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134726"|"21342849"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134725"|"21342848"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shaak component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134724"|"21342847"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shonkin soil is a minor component."|"21134723"|"21342846"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134722"|"21342845"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134721"|"21342844"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shaak component makes up 40 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134720"|"21342843"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oburn component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134719"|"21342842"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shonkin soil is a minor component."|"21134718"|"21342841"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21134717"|"21342840"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134716"|"21342839"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134715"|"21342838"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"21134956"|"21343079"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beenom component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on structural benches on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21134957"|"21343080"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 1 to 4 percent. This component is on low hills on sedimentary plains, structural benches on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134958"|"21343081"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134959"|"21343082"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135069"|"21343192"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135070"|"21343193"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21135071"|"21343194"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135072"|"21343195"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom, calcareous soil is a minor component."|"21135073"|"21343196"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135074"|"21343197"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"21134960"|"21343083"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134961"|"21343084"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21134962"|"21343085"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134963"|"21343086"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 70 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134964"|"21343087"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21134965"|"21343088"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 30 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of colluvium derived from sandstone and/or residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134966"|"21343089"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21134967"|"21343090"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134968"|"21343091"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134969"|"21343092"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 50 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134970"|"21343093"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21134971"|"21343094"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"21134972"|"21343095"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21134973"|"21343096"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cohagen component makes up 50 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134974"|"21343097"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridge soil is a minor component."|"21134975"|"21343098"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134976"|"21343099"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tally soil is a minor component."|"21134977"|"21343100"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 30 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134978"|"21343101"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 65 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of clayey residuum. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.   The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21134714"|"21342837"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Razor component makes up 25 percent of the map unit. Slopes are 4 to 6 percent. This component is on hills, plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134713"|"21342836"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 65 percent of the map unit. Slopes are 3 to 6 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134712"|"21342835"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134711"|"21342834"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 25 percent of the map unit. Slopes are 3 to 6 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134710"|"21342833"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 15 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134709"|"21342832"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134979"|"21343102"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"21134980"|"21343103"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ridge component makes up 35 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134981"|"21343104"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"21134982"|"21343105"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134983"|"21343106"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134984"|"21343107"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135081"|"21343204"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep, dry component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135082"|"21343205"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135083"|"21343206"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21135084"|"21343207"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21135085"|"21343208"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135086"|"21343209"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 60 percent of the map unit. Slopes are 1 to 3 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134708"|"21342831"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep, dry soil is a minor component."|"21135008"|"21343131"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135009"|"21343132"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of sandy residuum weathered from calcareous sandstone over semiconsolidated residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135010"|"21343133"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21135011"|"21343134"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21135012"|"21343135"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135013"|"21343136"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135059"|"21343182"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, dry component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135060"|"21343183"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21135061"|"21343184"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21135062"|"21343185"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135063"|"21343186"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 25 percent of the map unit. Slopes are 1 to 3 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134707"|"21342830"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134706"|"21342829"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134705"|"21342828"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 65 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134704"|"21342827"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 45 percent of the map unit. Slopes are 7 to 10 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134703"|"21342826"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134702"|"21342825"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134701"|"21342824"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of sandy residuum weathered from calcareous sandstone over semiconsolidated residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135020"|"21343143"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135021"|"21343144"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135022"|"21343145"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135023"|"21343146"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21135024"|"21343147"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21135025"|"21343148"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bainville component makes up 35 percent of the map unit. Slopes are 10 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134700"|"21342823"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134699"|"21342822"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134698"|"21342821"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 85 percent of the map unit. Slopes are 7 to 15 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134697"|"21342820"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134696"|"21342819"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134695"|"21342818"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134694"|"21342817"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134693"|"21342816"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134692"|"21342815"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134691"|"21342814"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134690"|"21342813"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134689"|"21342812"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hysham soil is a minor component."|"21134688"|"21342811"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134687"|"21342810"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21134686"|"21342809"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134278"|"21342401"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21134279"|"21342402"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21134280"|"21342403"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21134281"|"21342404"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134282"|"21342405"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"21134290"|"21342413"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134291"|"21342414"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macar component makes up 90 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134292"|"21342415"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21134293"|"21342416"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134294"|"21342417"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134295"|"21342418"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134296"|"21342419"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ridge component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134297"|"21342420"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"21134298"|"21342421"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ridge component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134299"|"21342422"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21134300"|"21342423"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134301"|"21342424"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"21134302"|"21342425"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134303"|"21342426"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21134304"|"21342427"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134305"|"21342428"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dast component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134306"|"21342429"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134307"|"21342430"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ridge component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134308"|"21342431"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21134309"|"21342432"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 40 percent of the map unit. Slopes are 4 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21134310"|"21342433"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Birney soil is a minor component."|"21134311"|"21342434"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lamedeer component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on plains. The parent material consists of alluvium derived from porcellanite and/or colluvium derived from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134312"|"21342435"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21134313"|"21342436"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lamedeer component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on plains. The parent material consists of alluvium derived from porcellanite and/or colluvium derived from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134314"|"21342437"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 40 percent of the map unit. Slopes are 4 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21134315"|"21342438"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Birney soil is a minor component."|"21134316"|"21342439"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134685"|"21342808"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenzie component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on depressions, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during March, April, May, June. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil meets hydric criteria.  The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134684"|"21342807"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 35 percent of the map unit. Slopes are 35 to 50 percent. This component is on hills, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21134683"|"21342806"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"21134682"|"21342805"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134681"|"21342804"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134680"|"21342803"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"21134679"|"21342802"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 80 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21134678"|"21342801"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134677"|"21342800"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21134676"|"21342799"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maginnis component makes up 80 percent of the map unit. Slopes are 7 to 15 percent. This component is on hills, foothills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21134675"|"21342798"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"21134674"|"21342797"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 18 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134673"|"21342796"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134672"|"21342795"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 50 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"21134671"|"21342794"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134670"|"21342793"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134669"|"21342792"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 45 percent of the map unit. Slopes are 4 to 10 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134668"|"21342791"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134667"|"21342790"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134666"|"21342789"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134665"|"21342788"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21134664"|"21342787"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134663"|"21342786"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"21134662"|"21342785"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134661"|"21342784"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during June, July, August, September. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134660"|"21342783"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134659"|"21342782"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hysham soil is a minor component."|"21134658"|"21342781"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134657"|"21342780"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134656"|"21342779"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134655"|"21342778"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 85 percent of the map unit. Slopes are 3 to 7 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134654"|"21342777"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134653"|"21342776"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lismas component makes up 80 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC052MT Shale (sh)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21134652"|"21342775"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21134651"|"21342774"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134650"|"21342773"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McKenzie soil is a minor component."|"21134649"|"21342772"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lavina component makes up 80 percent of the map unit. Slopes are 2 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC641MT Shallow Limy (swly)   Rru 58a-c  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134648"|"21342771"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134647"|"21342770"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134646"|"21342769"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 80 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21134645"|"21342768"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134644"|"21342767"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134643"|"21342766"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clapper soil is a minor component."|"21134642"|"21342765"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134641"|"21342764"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 80 percent of the map unit. Slopes are 4 to 7 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134640"|"21342763"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134639"|"21342762"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134638"|"21342761"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134637"|"21342760"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134636"|"21342759"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134635"|"21342758"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134634"|"21342757"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McKenzie soil is a minor component."|"21134633"|"21342756"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134632"|"21342755"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134631"|"21342754"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134630"|"21342753"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambert component makes up 80 percent of the map unit. Slopes are 7 to 35 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134629"|"21342752"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Razor component makes up 80 percent of the map unit. Slopes are 2 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134736"|"21342859"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21134737"|"21342860"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134738"|"21342861"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134739"|"21342862"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kyle component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of colluvium derived from clayey shale and/or residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134628"|"21342751"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134627"|"21342750"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kyle component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on hills, plains. The parent material consists of colluvium derived from clayey shale and/or residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134626"|"21342749"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"21134625"|"21342748"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134624"|"21342747"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134623"|"21342746"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kyle component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, fans, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134622"|"21342745"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134621"|"21342744"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21134620"|"21342743"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on low hills, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134619"|"21342742"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clapper soil is a minor component."|"21134618"|"21342741"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134617"|"21342740"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"21134616"|"21342739"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 45 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134615"|"21342738"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clapper soil is a minor component."|"21134614"|"21342737"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"21134613"|"21342736"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on low hills, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134612"|"21342735"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21134611"|"21342734"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134610"|"21342733"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on low hills, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134609"|"21342732"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134608"|"21342731"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"21134607"|"21342730"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21134606"|"21342729"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134605"|"21342728"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on low hills, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134604"|"21342727"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shonkin soil is a minor component."|"21134603"|"21342726"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134602"|"21342725"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134601"|"21342724"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134600"|"21342723"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134599"|"21342722"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134598"|"21342721"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134597"|"21342720"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Laurel component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134596"|"21342719"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134595"|"21342718"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134594"|"21342717"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134593"|"21342716"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"21134592"|"21342715"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Laurel component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134591"|"21342714"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Allentine soil is a minor component."|"21134590"|"21342713"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134589"|"21342712"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134588"|"21342711"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 70 percent of the map unit. Slopes are 0 to 2 percent. This component is on low hills, fans, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134587"|"21342710"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Allentine component makes up 30 percent of the map unit. Slopes are 2 to 7 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 3 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134586"|"21342709"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21134585"|"21342708"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 60 percent of the map unit. Slopes are 2 to 7 percent. This component is on low hills, fans, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3s. Irrigated land capability classification is 3s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134584"|"21342707"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134583"|"21342706"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hovert component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on depressions, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer, natric, is 1 to 5 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during February, March, April, May. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134582"|"21342705"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Razor soil is a minor component."|"21134581"|"21342704"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21134580"|"21342703"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134579"|"21342702"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hopley component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134578"|"21342701"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134577"|"21342700"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"21134576"|"21342699"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134575"|"21342698"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134574"|"21342697"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134573"|"21342696"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134572"|"21342695"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hilly component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21134571"|"21342694"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134570"|"21342693"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21134569"|"21342692"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134568"|"21342691"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134567"|"21342690"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shonkin soil is a minor component."|"21134566"|"21342689"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134565"|"21342688"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134564"|"21342687"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134563"|"21342686"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134562"|"21342685"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shonkin soil is a minor component."|"21134561"|"21342684"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Heldt component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"21134560"|"21342683"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21134559"|"21342682"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134558"|"21342681"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during April, May, June. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134557"|"21342680"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134556"|"21342679"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134555"|"21342678"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21134554"|"21342677"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134553"|"21342676"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hysham soil is a minor component."|"21134552"|"21342675"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134551"|"21342674"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 40 percent of the map unit. Slopes are 25 to 35 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134550"|"21342673"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134549"|"21342672"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hysham soil is a minor component."|"21134548"|"21342671"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohmiller component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134547"|"21342670"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134546"|"21342669"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21134545"|"21342668"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 60 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134544"|"21342667"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hysham component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, terraces, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21134543"|"21342666"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134542"|"21342665"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134541"|"21342664"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134540"|"21342663"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21134539"|"21342662"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 85 percent of the map unit. Slopes are 1 to 3 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134538"|"21342661"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134537"|"21342660"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134536"|"21342659"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134535"|"21342658"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134534"|"21342657"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"21134533"|"21342656"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134532"|"21342655"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134531"|"21342654"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134530"|"21342653"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134529"|"21342652"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134528"|"21342651"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"21134527"|"21342650"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134526"|"21342649"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134525"|"21342648"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134524"|"21342647"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134523"|"21342646"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21134522"|"21342645"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134521"|"21342644"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134520"|"21342643"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"21134519"|"21342642"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134518"|"21342641"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Grail component makes up 60 percent of the map unit. Slopes are 2 to 15 percent. This component is on fans, terraces, hills, foothills. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134517"|"21342640"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Grail component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, hills, foothills. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134516"|"21342639"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134515"|"21342638"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"21134514"|"21342637"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134513"|"21342636"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amherst soil is a minor component."|"21134512"|"21342635"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maginnis soil is a minor component."|"21134511"|"21342634"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Grail component makes up 80 percent of the map unit. Slopes are 2 to 4 percent. This component is on fans, terraces, hills, foothills. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134510"|"21342633"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glenberg component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134509"|"21342632"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134508"|"21342631"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134507"|"21342630"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134506"|"21342629"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glenberg component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, flood plains, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134505"|"21342628"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134504"|"21342627"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21134503"|"21342626"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glenberg component makes up 80 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134502"|"21342625"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134501"|"21342624"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cushman component makes up 35 percent of the map unit. Slopes are 2 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.   The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134740"|"21342863"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134741"|"21342864"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Razor component makes up 55 percent of the map unit. Slopes are 2 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e.  The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134742"|"21342865"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21134743"|"21342866"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134744"|"21342867"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134745"|"21342868"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21134746"|"21342869"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134747"|"21342870"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134748"|"21342871"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134749"|"21342872"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134750"|"21342873"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ryegate component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134751"|"21342874"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worland soil is a minor component."|"21134752"|"21342875"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lavina soil is a minor component."|"21134753"|"21342876"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134754"|"21342877"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sage component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, fans, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during January, February, March, April, May, June, July, November, December. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134755"|"21342878"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134756"|"21342879"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pierre soil is a minor component."|"21134757"|"21342880"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"21134758"|"21342881"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oburn soil is a minor component."|"21134759"|"21342882"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shonkin soil is a minor component."|"21134760"|"21342883"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shaak component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134761"|"21342884"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oburn soil is a minor component."|"21134762"|"21342885"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shaak component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134763"|"21342886"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134764"|"21342887"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134765"|"21342888"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lismas soil is a minor component."|"21134766"|"21342889"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21134767"|"21342890"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, plains. The parent material consists of clayey residuum. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC047MT Clayey-steep (cystp)   Rru 58a-c  11-14"" P.z.      Deleted.  Refer To Site: R058a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21134768"|"21342891"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134769"|"21342892"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oburn soil is a minor component."|"21134770"|"21342893"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shonkin component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 0 inches during March, April, May, June, July, August, September. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134771"|"21342894"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shaak soil is a minor component."|"21134772"|"21342895"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134773"|"21342896"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134774"|"21342897"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134775"|"21342898"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134776"|"21342899"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shorey component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134777"|"21342900"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clapper soil is a minor component."|"21134778"|"21342901"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134779"|"21342902"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134780"|"21342903"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134781"|"21342904"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shorey component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134782"|"21342905"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clapper soil is a minor component."|"21134783"|"21342906"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134784"|"21342907"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134785"|"21342908"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134786"|"21342909"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134787"|"21342910"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134788"|"21342911"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134789"|"21342912"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134790"|"21342913"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Toluca component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134791"|"21342914"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134792"|"21342915"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134793"|"21342916"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Toluca component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134794"|"21342917"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"21134795"|"21342918"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Toluca component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134796"|"21342919"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambert soil is a minor component."|"21134797"|"21342920"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134798"|"21342921"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134799"|"21342922"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134800"|"21342923"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Keiser soil is a minor component."|"21134801"|"21342924"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134802"|"21342925"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Treasure component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134803"|"21342926"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21134804"|"21342927"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21134805"|"21342928"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21134806"|"21342929"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Treasure component makes up 85 percent of the map unit. Slopes are 4 to 10 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134807"|"21342930"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Apron soil is a minor component."|"21134808"|"21342931"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134809"|"21342932"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134810"|"21342933"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vananda component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, lakebeds (relict), terraces, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21134811"|"21342934"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McKenzie soil is a minor component."|"21134812"|"21342935"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vananda component makes up 90 percent of the map unit. Slopes are 1 to 7 percent. This component is on fans, lakebeds (relict), terraces, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21134813"|"21342936"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21134814"|"21342937"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vananda component makes up 50 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, lakebeds (relict), terraces, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21134815"|"21342938"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 15 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 0 to 8 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21134816"|"21342939"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 35 percent of the map unit. Slopes are 4 to 7 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134846"|"21342969"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134847"|"21342970"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134848"|"21342971"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134849"|"21342972"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134850"|"21342973"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21134851"|"21342974"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21134852"|"21342975"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134853"|"21342976"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21134854"|"21342977"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worland component makes up 85 percent of the map unit. Slopes are 2 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134855"|"21342978"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134856"|"21342979"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134857"|"21342980"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wormser component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134858"|"21342981"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21134859"|"21342982"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134860"|"21342983"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lavina soil is a minor component."|"21134861"|"21342984"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wormser component makes up 85 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134862"|"21342985"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryegate soil is a minor component."|"21134863"|"21342986"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21134864"|"21342987"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lavina soil is a minor component."|"21134865"|"21342988"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134866"|"21342989"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wormser component makes up 70 percent of the map unit. Slopes are 2 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134867"|"21342990"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lavina component makes up 25 percent of the map unit. Slopes are 2 to 4 percent. This component is on hills, plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC641MT Shallow Limy (swly)   Rru 58a-c  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134868"|"21342991"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Travessilla soil is a minor component."|"21134869"|"21342992"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21134870"|"21342993"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21134871"|"21342994"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wormser component makes up 55 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134872"|"21342995"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worland component makes up 35 percent of the map unit. Slopes are 4 to 7 percent. This component is on hills, plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134873"|"21342996"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134874"|"21342997"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134875"|"21342998"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"21134876"|"21342999"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yegen component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on fans, hills, terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134877"|"21343000"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yegen component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on fans, hills, terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134878"|"21343001"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134879"|"21343002"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"21134880"|"21343003"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"21134881"|"21343004"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yegen component makes up 80 percent of the map unit. Slopes are 4 to 10 percent. This component is on fans, hills, terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134882"|"21343005"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"21134883"|"21343006"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134884"|"21343007"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"21134885"|"21343008"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yegen component makes up 45 percent of the map unit. Slopes are 7 to 15 percent. This component is on fans, hills, terraces, foothills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134886"|"21343009"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Toluca component makes up 45 percent of the map unit. Slopes are 7 to 15 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134887"|"21343010"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clapper soil is a minor component."|"21134888"|"21343011"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"21134931"|"21343054"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135039"|"21343162"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135033"|"21343156"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21135034"|"21343157"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135035"|"21343158"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135036"|"21343159"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21135037"|"21343160"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134949"|"21343072"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21134950"|"21343073"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134951"|"21343074"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dast soil is a minor component."|"21134952"|"21343075"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barvon soil is a minor component."|"21134330"|"21342453"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"21134331"|"21342454"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 45 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134332"|"21342455"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"21134333"|"21342456"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134334"|"21342457"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 60 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134325"|"21342448"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridge soil is a minor component."|"21134326"|"21342449"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"21134327"|"21342450"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134328"|"21342451"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134329"|"21342452"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, dry component makes up 30 percent of the map unit. Slopes are 8 to 60 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135075"|"21343198"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21135076"|"21343199"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep, dry component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135077"|"21343200"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135078"|"21343201"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21135079"|"21343202"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135080"|"21343203"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135014"|"21343137"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21135015"|"21343138"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21135016"|"21343139"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of sandy residuum weathered from calcareous sandstone over semiconsolidated residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135017"|"21343140"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135018"|"21343141"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135019"|"21343142"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135007"|"21343130"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21134902"|"21343025"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 30 percent of the map unit. Slopes are 4 to 25 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134903"|"21343026"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21134904"|"21343027"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"21134905"|"21343028"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"21134906"|"21343029"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (Sy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134907"|"21343030"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21134908"|"21343031"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (SwC)    RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134263"|"21342386"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134264"|"21342387"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134265"|"21342388"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21134266"|"21342389"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21134267"|"21342390"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21134268"|"21342391"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134269"|"21342392"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"21134270"|"21342393"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21134271"|"21342394"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21134272"|"21342395"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullhook soil is a minor component."|"21134273"|"21342396"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"21134274"|"21342397"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134275"|"21342398"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Orinoco soil is a minor component."|"21134276"|"21342399"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21134277"|"21342400"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 35 percent of the map unit. Slopes are 4 to 7 percent. This component is on fans, terraces, lakebeds (relict), plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21134817"|"21342940"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21134818"|"21342941"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134819"|"21342942"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134820"|"21342943"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134821"|"21342944"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134822"|"21342945"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134823"|"21342946"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134824"|"21342947"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134825"|"21342948"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134826"|"21342949"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134827"|"21342950"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wanetta soil is a minor component."|"21134828"|"21342951"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134829"|"21342952"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134830"|"21342953"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toluca soil is a minor component."|"21134831"|"21342954"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134832"|"21342955"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134833"|"21342956"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134834"|"21342957"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134835"|"21342958"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134836"|"21342959"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 65 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134837"|"21342960"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134838"|"21342961"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134839"|"21342962"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21134840"|"21342963"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 70 percent of the map unit. Slopes are 1 to 2 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134841"|"21342964"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Larim component makes up 25 percent of the map unit. Slopes are 3 to 4 percent. This component is on terraces, terraces, plains. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134842"|"21342965"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134843"|"21342966"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larim soil is a minor component."|"21134844"|"21342967"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wanetta component makes up 55 percent of the map unit. Slopes are 4 to 7 percent. This component is on terraces, plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134845"|"21342968"
09/09/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Urban land is a miscellaneous area."|"21134283"|"21342406"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tusler component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges on sedimentary plains. The parent material consists of sandy eolian deposits derived from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC056MT Sands (sa)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134945"|"21343068"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21134946"|"21343069"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134947"|"21343070"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blown-out land soil is a minor component."|"21134948"|"21343071"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 35 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134317"|"21342440"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barvon component makes up 30 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134318"|"21342441"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Korchea component makes up 30 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE389MT Overflow (ov)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134319"|"21342442"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Savage soil is a minor component."|"21134320"|"21342443"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barvon soil is a minor component."|"21134321"|"21342444"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macar component makes up 30 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134322"|"21342445"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134323"|"21342446"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134324"|"21342447"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barvon soil is a minor component."|"21134335"|"21342458"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridge soil is a minor component."|"21134336"|"21342459"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21134337"|"21342460"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134338"|"21342461"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on plains. The parent material consists of colluvium derived from sedimentary rock and/or residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134339"|"21342462"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"21134258"|"21342381"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist, calcareous component makes up 65 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on plains. The parent material consists of loamy residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134259"|"21342382"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134260"|"21342383"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridge, moist soil is a minor component."|"21134261"|"21342384"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sandstone and shale is a miscellaneous area."|"21134262"|"21342385"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist component makes up 45 percent of the map unit. Slopes are 25 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135064"|"21343187"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, dry component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135065"|"21343188"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21135066"|"21343189"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21135067"|"21343190"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135068"|"21343191"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barvon component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134340"|"21342463"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"21134341"|"21342464"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 45 percent of the map unit. Slopes are 25 to 65 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134342"|"21342465"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21134343"|"21342466"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134344"|"21342467"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Twilight soil is a minor component."|"21134926"|"21343049"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cabbart soil is a minor component."|"21134927"|"21343050"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains, fans on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134928"|"21343051"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Busby soil is a minor component."|"21134929"|"21343052"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134930"|"21343053"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on pediments on sedimentary plains. The parent material consists of interbedded residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135054"|"21343177"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21135055"|"21343178"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"21135056"|"21343179"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on pediments on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21135057"|"21343180"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"21135058"|"21343181"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 30 percent of the map unit. Slopes are 6 to 12 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134889"|"21343012"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Assinniboine component makes up 60 percent of the map unit. Slopes are 6 to 12 percent. This component is on low hills. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134890"|"21343013"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134891"|"21343014"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"21134892"|"21343015"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"21134893"|"21343016"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134897"|"21343020"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bonfri soil is a minor component."|"21134898"|"21343021"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Busby soil is a minor component."|"21134899"|"21343022"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Yamacall soil is a minor component."|"21134900"|"21343023"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blacksheep soil is a minor component."|"21134901"|"21343024"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134284"|"21342407"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21134285"|"21342408"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134286"|"21342409"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"21134287"|"21342410"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21134288"|"21342411"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hinterland soil is a minor component."|"21134289"|"21342412"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullhook soil is a minor component."|"21134932"|"21343055"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21134933"|"21343056"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 30 percent of the map unit. Slopes are 8 to 60 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134934"|"21343057"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134935"|"21343058"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans on plains, hills on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134936"|"21343059"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21134937"|"21343060"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21134938"|"21343061"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21134939"|"21343062"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, occasionally flooded soil is a minor component."|"21134940"|"21343063"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21134920"|"21343043"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Warhorse soil is a minor component."|"21134921"|"21343044"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21134922"|"21343045"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"21134923"|"21343046"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21134924"|"21343047"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 80 percent of the map unit. Slopes are 1 to 6 percent. This component is on low hills on plains. The parent material consists of alluvium derived from sandstone and shale and/or residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21134925"|"21343048"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21135026"|"21343149"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 55 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135027"|"21343150"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21135028"|"21343151"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatoville soil is a minor component."|"21135029"|"21343152"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"21135030"|"21343153"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Orinoco soil is a minor component."|"21135031"|"21343154"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21135032"|"21343155"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains, swales on plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21134909"|"21343032"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rominell soil is a minor component."|"21134910"|"21343033"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Eapa soil is a minor component."|"21134911"|"21343034"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Delpoint soil is a minor component."|"21134912"|"21343035"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Twilight soil is a minor component."|"21134913"|"21343036"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans on plains, stream terraces on plains, low hills on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134914"|"21343037"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenzie component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on depressions on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 12 inches during March, April, May, June. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21134941"|"21343064"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Vanda soil is a minor component."|"21134942"|"21343065"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Absher soil is a minor component."|"21134943"|"21343066"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Marvan soil is a minor component."|"21134944"|"21343067"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kobase soil is a minor component."|"21134915"|"21343038"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Busby soil is a minor component."|"21134916"|"21343039"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall, calcareous component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on plains, fans on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134917"|"21343040"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Yamacall soil is a minor component."|"21134918"|"21343041"
09/10/2014 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rominell soil is a minor component."|"21134919"|"21343042"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eapa, calcareous component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21134894"|"21343017"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21134895"|"21343018"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"21134896"|"21343019"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bainville soil is a minor component."|"21135002"|"21343125"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohmiller soil is a minor component."|"21135003"|"21343126"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21135004"|"21343127"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21135005"|"21343128"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 50 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills, plains. The parent material consists of clayey residuum. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE005MT Clayey-steep (cystp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21135006"|"21343129"
