"Aa"|"Absarokee clay loam, 1 to 4 percent slopes"||3|3.5|84|||"None"|"None"|"0"|3.85|7.12|8.43|8.43|"Well drained"|"Well drained"|"C"||100|"3"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.138|"Moderate"|"0"|1|"345670"
"Ab"|"Absarokee clay loam, 4 to 7 percent slopes"||6|6|84|||"None"|"None"|"0"|3.71|6.96|8.27|8.27|"Well drained"|"Well drained"|"C"||100|"3"|85|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.14|"Moderate"|"0"|1|"345671"
"Ag"|"Alluvial land, gravelly"||2|2||54|54|"Frequent"|"Frequent"|"0"|2.2|2.99|4.57|6.15|"Well drained"|"Well drained"|"A/D"||98|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.394|"Slight"|"2"|0.996|"345672"
"Al"|"Alluvial land, mixed"||1|1||54|54|"Occasional"|"Occasional"|"0"|2.06|2.85|4.43|6.01|"Well drained"|"Well drained"|"B/D"||98|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.08|"Slight"|"2"|0.996|"345673"
"Am"|"Alluvial land, seeped"||4|3.6||15|15|"None"|"None"|"0"|4.25|8.41|16.73|24.85|"Poorly drained"|"Poorly drained"|"C/D"||85|"5"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.857|"Slight"|"85"|0.968|"345674"
"An"|"Alluvial land, wet"||1|1||61|61|"Rare"|"Rare"|"0"|4.47|7.99|15.01|17.58|"Poorly drained"|"Poorly drained"|"C"|"3"|90|"3"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.158|"Slight"|"90"|0.98|"345675"
"Ao"|"Amherst clay loam, 7 to 15 percent slopes"||11|10.5|41|||"None"|"None"|"0"|3.55|5.71|5.86|5.86|"Well drained"|"Well drained"|"D"||100|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.139|"Severe"|"0"|1|"345676"
"Ap"|"Amherst-Maginnis channery clay loams, 4 to 7 percent slopes"||6|6|25|||"None"|"None"|"0"|3.05|4.87|5.02|5.02|"Well drained"|"Well drained"|"D"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.14|"Moderate"|"0"|1|"345677"
"Ar"|"Apron loamy fine sand, 4 to 7 percent slopes"||6|5.9||||"None"|"None"|"0"|1.84|3.5|6.6|9.18|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||92|"6"|86|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Not rated"|"Somewhat limited"|0.321|"Moderate"|"0"|1|"345678"
"As"|"Apron fine sandy loam, 4 to 7 percent slopes"||6|5.9||||"None"|"None"|"0"|3.5|6.86|12.04|15.93|"Well drained"|"Well drained"|"A"|"4"|87|"4"|87|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.007|"Moderate"|"0"|1|"345679"
"Au"|"Arvada clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.29|6.14|11.1|15.56|"Well drained"|"Well drained"|"D"|"6"|80|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.239|"Slight"|"0"|1|"345681"
"Av"|"Arvada clay loam, 1 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|3.33|6.25|11.37|15.99|"Well drained"|"Well drained"|"D"|"6"|80|"6"|80|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.227|"Moderate"|"0"|0.96|"345682"
"Aw"|"Arvada clay loam, 4 to 7 percent slopes"||6|5.7||||"None"|"None"|"0"|3.21|6.19|11.36|16.14|"Well drained"|"Well drained"|"D"|"6"|80|"6"|80|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.219|"Moderate"|"0"|0.92|"345683"
"Ax"|"Arvada-Bone silty clay loams, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.11|5.73|10.41|14.71|"Well drained"|"Well drained"|"D"|"7"|60|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.299|"Slight"|"0"|1|"345684"
"Ay"|"Arvada-Bone clays, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.17|5.89|10.69|15.05|"Well drained"|"Well drained"|"D"|"6"|70|"6"|70|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.273|"Slight"|"0"|1|"345685"
"Be"|"Bainville-Elso complex, 15 to 35 percent slopes"||25|22.3|30|||"None"|"None"|"0"|4.51|7.73|11.42|12.8|"Well drained"|"Well drained"|"C"||92|"6"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.876|"Severe"|"0"|0.947|"345688"
"Bf"|"Bainville-Elso-Shale outcrop complex, 7 to 25 percent slopes"||16|15.2|30|||"None"|"None"|"0"|4.45|7.32|9.95|10.23|"Well drained"|"Well drained"|"D"||99|"7"|41|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.576|"Severe"|"0"|0.979|"345689"
"Bl"|"Bainville-Worland complex, 4 to 7 percent slopes"||6|6|76|||"None"|"None"|"0"|4.37|8.7|14.27|14.87|"Well drained"|"Well drained"|"C"||69|"3"|71|"Not limited"|"Somewhat limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.306|"Moderate"|"0"|0.599|"345691"
"Bm"|"Bew silty clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.32|7.73|14.58|21.84|"Well drained"|"Well drained"|"C"|"3"|85|"3"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.475|"Slight"|"0"|0.883|"345692"
"Bn"|"Bew clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.58|6.83|13.36|20.33|"Well drained"|"Well drained"|"C"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.495|"Slight"|"0"|0.944|"345693"
"Bo"|"Bew clay, 1 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|3.49|6.62|12.83|19.58|"Well drained"|"Well drained"|"C"|"4"|91|"4"|91|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.5|"Slight"|"0"|1|"345694"
"Br"|"Bew-Allentine clays, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.38|6.36|12.01|17.87|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.5|"Slight"|"0"|1|"345695"
"Bs"|"Big Horn clay loam, 0 to 2 percent slopes"||1|1.3|140|||"None"|"None"|"0"|4.01|7.86|14.46|19.22|"Well drained"|"Well drained"|"C"||100|"3"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.293|"Slight"|"0"|0.965|"345696"
"Bt"|"Bone silty clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|2.49|4.38|8.09|11.74|"Well drained"|"Well drained"|"D"||85|"7"|91|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.492|"Slight"|"0"|1|"345697"
"Bu"|"Bone silty clay, 1 to 6 percent slopes"||4|3.9||||"None"|"None"|"0"|2.49|4.38|8.09|11.74|"Well drained"|"Well drained"|"D"||85|"7"|91|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.492|"Moderate"|"0"|1|"345698"
"Bv"|"Bone clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|2.49|4.38|8.09|11.74|"Well drained"|"Well drained"|"D"||85|"7"|91|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.492|"Slight"|"0"|1|"345699"
"Ca"|"Clapper clay loam, 15 to 35 percent slopes"||25|21.6||||"None"|"None"|"0"|3.6|6.02|9.55|12.91|"Well drained"|"Well drained"|"B"||90|"6"|80|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.843|"Severe"|"0"|0.919|"345700"
"Cg"|"Clapper gravelly loam, 7 to 15 percent slopes"||11|10.5||||"None"|"None"|"0"|3.47|5.89|9.38|12.74|"Well drained"|"Well drained"|"B"||91|"4"|89|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.271|"Moderate"|"0"|0.486|"345701"
"Da"|"Danvers silty clay loam, 2 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.21|7.98|15.48|22.81|"Well drained"|"Well drained"|"C"|"3"|85|"3"|97|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Moderate"|"0"|0.94|"345704"
"Dn"|"Danvers silty clay loam, 8 to 15 percent slopes"||12|10.7||||"None"|"None"|"0"|4.07|7.83|15.3|21.05|"Well drained"|"Well drained"|"C"||87|"4"|87|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.21|"Severe"|"0"|0.92|"345705"
"Dr"|"Danvers-Judith complex, 7 to 15 percent slopes"||10|10.1||||"None"|"None"|"0"|4.18|7.8|14.62|21.37|"Well drained"|"Well drained"|"C"||73|"4"|93|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.193|"Severe"|"0"|0.897|"345706"
"Ds"|"Danvers-Shaak clay loams, 7 to 15 percent slopes"||11|10.1||||"None"|"None"|"0"|3.84|7.58|15.17|22.02|"Well drained"|"Well drained"|"C"||90|"4"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.195|"Moderate"|"0"|0.94|"345707"
"Ec"|"Elso clay loam, 4 to 7 percent slopes"||6|5.8|30|||"None"|"None"|"0"|4.27|5.71|6.64|6.96|"Well drained"|"Well drained"|"D"||88|"6"|80|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.27|"Moderate"|"0"|0.96|"345708"
"El"|"Elso clay loam, 7 to 15 percent slopes"||11|10.2|30|||"None"|"None"|"0"|4.27|5.72|6.84|7.56|"Well drained"|"Well drained"|"D"||89|"6"|80|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.296|"Severe"|"0"|0.975|"345709"
"Eo"|"Elso clay loam, 15 to 60 percent slopes"||38|35|30|||"None"|"None"|"0"|4.31|5.65|6.54|7.06|"Well drained"|"Well drained"|"D"||94|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.95|"Severe"|"0"|1|"345710"
"Es"|"Elso-Lohmiller complex, 15 to 35 percent slopes"||25|21.9|30|||"None"|"None"|"0"|4.28|6.88|10.79|14.18|"Well drained"|"Well drained"|"C"||94|"7"|40|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.769|"Severe"|"0"|1|"345711"
"Fa"|"Brushton-Lonna silt loams, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.81|9.48|17.97|26.05|"Well drained"|"Well drained"|"B"|"2"|60|"3"|70|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.315|"Slight"|"0"|0.073|"345712"
"Fg"|"Fattig sandy clay loam, 4 to 7 percent slopes"||6|5.8|84|||"None"|"None"|"0"|4.09|7.93|13.16|14.03|"Well drained"|"Well drained"|"C"||85|"3"|95|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.173|"Moderate"|"0"|1|"345713"
"Fl"|"Fort Collins-Arvada clay loams, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.91|7.74|15.52|23.17|"Well drained"|"Well drained"|"B"|"2"|80|"3"|80|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.154|"Slight"|"0"|0.215|"345714"
"Fo"|"Fort Collins-Arvada clay loams, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.91|7.74|15.52|23.17|"Well drained"|"Well drained"|"B"|"2"|80|"3"|80|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.154|"Moderate"|"0"|0.215|"345715"
"Fr"|"Fort Collins and Thurlow clay loams, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.12|8.05|16.11|24.17|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.25|"Slight"|"0"|0.13|"345716"
"Ft"|"Fort Collins and Thurlow clay loams, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.12|8.05|16.11|24.17|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.25|"Moderate"|"0"|0.13|"345717"
"Ga"|"Gilt Edge-Allentine complex, 2 to 7 percent slopes"||5|4.8|94|||"None"|"None"|"0"|3.84|6.79|11.34|13.05|"Well drained"|"Well drained"|"D"||60|"6"|70|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.33|"Moderate"|"0"|1|"345718"
"Gh"|"Glenberg fine sandy loam, 1 to 4 percent slopes"||3|2.7||||"Rare"|"Rare"|"0"|3.67|7.07|13.76|16.57|"Well drained"|"Well drained"|"A"|"4"|80|"4"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.033|"Moderate"|"0"|0.9|"345719"
"Gl"|"Glenberg loam, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.47|7.82|14.52|18.98|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.033|"Slight"|"0"|0.9|"345720"
"Go"|"Glenberg loam, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.39|8.54|14.15|16.85|"Well drained"|"Well drained"|"B"|"3"|80|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.033|"Slight"|"0"|0.9|"345721"
"Gr"|"Grail clay loam, 2 to 4 percent slopes"||3|3.3||||"None"|"None"|"0"|3.67|7.01|11.09|14.28|"Well drained"|"Well drained"|"C"|"3"|87|"3"|87|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.218|"Moderate"|"0"|1|"345722"
"Gs"|"Grail silty clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.92|7.73|15.35|22.98|"Well drained"|"Well drained"|"C"|"4"|85|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.483|"Slight"|"5"|0.93|"345723"
"Gt"|"Grail soils, 2 to 15 percent slopes"||9|8.6||||"None"|"None"|"0"|3.8|7.36|11.98|15.29|"Well drained"|"Well drained"|"C"||91|"4"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.233|"Severe"|"0"|0.972|"345724"
"Ha"|"Haverson loam, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.3|8.18|15.93|23.4|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.071|"Slight"|"0"|0.2|"345725"
"Hb"|"Haverson loam, clay substratum, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.49|8.66|16.43|23.24|"Well drained"|"Well drained"|"B"|"2"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.105|"Slight"|"1"|1|"345726"
"Hc"|"Haverson clay loam, 0 to 1 percent slopes"||1|1||||"Occasional"|"Occasional"|"0"|4.04|7.99|15.89|23.8|"Well drained"|"Well drained"|"C"|"2"|87|"3"|87|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.122|"Slight"|"0"|0.61|"345727"
"Hd"|"Haverson silty clay loam, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.03|8|15.94|23.88|"Well drained"|"Well drained"|"C"|"2"|94|"3"|94|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.095|"Slight"|"0"|0.366|"345728"
"He"|"Haverson silty clay loam, 1 to 3 percent slopes"||2|2||||"Rare"|"Rare"|"0"|4.03|7.97|15.68|23.32|"Well drained"|"Well drained"|"C"|"2"|85|"3"|91|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.109|"Slight"|"0"|0.402|"345729"
"Hh"|"Haverson-Hysham loams, 0 to 1 percent slopes"||1|1||137|137|"Rare"|"Rare"|"0"|3.83|7.39|14.52|21.54|"Well drained"|"Moderately well drained"|"B"|"2"|64|"3"|64|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.065|"Slight"|"0"|0.333|"345730"
"Hl"|"Haverson and Lohmiller soils, 0 to 4 percent slopes"||2|2||||"Rare"|"Rare"|"0"|4.03|7.89|14.97|21.64|"Well drained"|"Well drained"|"B"|"3"|47|"3"|93|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.15|"Slight"|"0"|0.574|"345731"
"Hm"|"Haverson and Lohmiller soils, channeled, 0 to 35 percent slopes"||1|12.5||||"Rare"|"Rare"|"0"|4.26|8.12|15.63|22.85|"Well drained"|"Well drained"|"B"||80|"6"|85|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.43|"Slight"|"0"|0.579|"345732"
"Hn"|"Haverson loam, gravelly variant, 0 to 1 percent slopes"||1|1||137|137|"Rare"|"Rare"|"0"|4.38|8.54|14.02|16.24|"Well drained"|"Well drained"|"B"|"3"|85|"3"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Slight"|"0"|0.91|"345733"
"Ho"|"Heldt silty clay loam, 4 to 7 percent slopes"||6|6||||"None"|"None"|"0"|4.2|7.73|14.53|21.33|"Well drained"|"Well drained"|"C"|"3"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.241|"Moderate"|"0"|1|"345734"
"Hp"|"Hesper silty clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"5"|4.31|8.59|17.74|24.3|"Well drained"|"Well drained"|"C"|"2"|91|"3"|91|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.471|"Slight"|"0"|0.359|"345735"
"Hr"|"Hesper silty clay loam, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"5"|4.3|8.56|17.67|24.21|"Well drained"|"Well drained"|"C"|"2"|89|"3"|89|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.472|"Moderate"|"0"|0.373|"345736"
"Hs"|"Hilly, gravelly land"||25|23.3||||"None"|"None"|"0"|1.95|2.77|3.96|4.93|"Excessively drained"|"Excessively drained"|"A"||93|"7"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.925|"Severe"|"0"|1|"345737"
"Ht"|"Hopley loam, 4 to 7 percent slopes"||6|5.9|119|||"None"|"None"|"0"|4.26|8.04|15.35|18.31|"Well drained"|"Well drained"|"B"||95|"3"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.143|"Moderate"|"0"|1|"345738"
"Hu"|"Hovert clay, 0 to 1 percent slopes"||1|1.5||0|0|"None"|"None"|"85"|3.8|6.81|12.37|17.47|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"||96|"6"|89|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.894|"Slight"|"85"|0.98|"345739"
"Hv"|"Hydro-Allentine complex, 2 to 7 percent slopes"||5|5.1|81|||"None"|"None"|"0"|3.55|6.49|11.22|14.97|"Well drained"|"Well drained"|"C"|"3"|60|"3"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.415|"Moderate"|"0"|1|"345740"
"Hw"|"Hydro-Arvada clay loams, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.43|6.36|11.65|16.79|"Well drained"|"Well drained"|"C"|"3"|70|"3"|70|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.346|"Slight"|"0"|1|"345741"
"Hx"|"Hysham-Laurel loams, 0 to 2 percent slopes"||1|1||61|61|"None"|"None"|"0"|2.76|5.46|10.87|16.28|"Moderately well drained"|"Somewhat poorly drained"|"B"|"6"|60|"6"|60|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.14|"Slight"|"1"|0.827|"345742"
"Hy"|"Hysham-Laurel silty clay loams, 0 to 2 percent slopes"||1|1||61|61|"None"|"None"|"0"|2.73|5.41|10.76|16.11|"Moderately well drained"|"Somewhat poorly drained"|"B"|"6"|55|"6"|55|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.142|"Slight"|"0"|0.828|"345743"
"Hz"|"Hysham and Haverson soils, 0 to 4 percent slopes"||2|1.9||122|122|"Rare"|"Rare"|"0"|3.62|6.99|13.74|20.21|"Well drained"|"Moderately well drained"|"B"|"2"|56|"3"|56|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Slight"|"0"|0.442|"345744"
"Kc"|"Keiser silty clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"5"|4.1|8.25|16.55|24.74|"Well drained"|"Well drained"|"C"|"2"|89|"3"|89|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.478|"Slight"|"0"|0.373|"345745"
"Ke"|"Keiser silty clay loam, 1 to 4 percent slopes"||3|3.3||||"None"|"None"|"0"|4.36|8.66|17.11|25.23|"Well drained"|"Well drained"|"C"|"2"|91|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.423|"Moderate"|"0"|0.338|"345746"
"Kg"|"Keiser silty clay loam, 4 to 7 percent slopes"||6|6.2||||"None"|"None"|"0"|4.28|8.47|16.74|24.7|"Well drained"|"Well drained"|"C"|"3"|85|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.457|"Moderate"|"0"|0.332|"345747"
"Kh"|"Keiser and Hesper silty clay loams, 0 to 1 percent slopes"||1|1.1||||"None"|"None"|"0"|4.24|8.48|17.21|24.43|"Well drained"|"Well drained"|"C"|"2"|96|"3"|96|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.424|"Slight"|"0"|0.316|"345748"
"Kl"|"Kyle silty clay, 0 to 1 percent slopes"||1|1.3||||"None"|"None"|"0"|3.83|7.23|13.85|20.2|"Well drained"|"Well drained"|"D"|"4"|85|"4"|91|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"345749"
"Km"|"Kyle silty clay, 1 to 4 percent slopes"||3|3.7|127|||"None"|"None"|"0"|3.91|7.2|13.59|16.99|"Well drained"|"Well drained"|"D"|"4"|85|"4"|91|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"345750"
"Kn"|"Kyle silty clay, 4 to 7 percent slopes"||6|6|79|||"None"|"None"|"0"|3.94|7.48|14.08|17.3|"Well drained"|"Well drained"|"D"|"4"|85|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"345751"
"La"|"Lonna-Vanstel complex, 0 to 4 percent slopes"||2|1.8||||"None"|"None"|"0"|4.63|9.17|18.06|26.91|"Well drained"|"Well drained"|"B"|"4"|70|"4"|70|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.316|"Slight"|"0"|0|"345752"
"Lb"|"Lonna silt loam, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.63|9.14|18.03|26.7|"Well drained"|"Well drained"|"B"|"4"|88|"4"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.324|"Moderate"|"0"|0.03|"345753"
"Lc"|"Lonna silt loams, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|4.63|9.09|17.76|26.04|"Well drained"|"Well drained"|"B"|"4"|98|"4"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.984|"Severe"|"0"|0.659|"345754"
"Ws"|"Wormser clay loam, 1 to 4 percent slopes"||3|3.1|86|||"None"|"None"|"0"|3.79|7.4|12.15|12.32|"Well drained"|"Well drained"|"C"|"3"|88|"3"|88|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.321|"Moderate"|"0"|1|"345829"
"Wt"|"Wormser clay loam, 4 to 7 percent slopes"||6|5.8|86|||"None"|"None"|"0"|3.84|7.43|12.1|12.1|"Well drained"|"Well drained"|"C"|"3"|88|"3"|88|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.334|"Moderate"|"0"|1|"345830"
"Wv"|"Wormser-Lavina clay loams, 2 to 4 percent slopes"||3|3|48|||"None"|"None"|"0"|3.96|7.75|11.73|11.73|"Well drained"|"Well drained"|"C"|"3"|70|"3"|70|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.344|"Moderate"|"0"|1|"345831"
"Ww"|"Wormser-Worland sandy loams, 4 to 7 percent slopes"||6|6|86|||"None"|"None"|"0"|3.59|7.02|12.42|12.51|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.183|"Moderate"|"0"|0.985|"345832"
"Ya"|"Yegen sandy loam, 0 to 1 percent slopes"||1|1.3||||"None"|"None"|"0"|3.76|7.74|14.8|21.68|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.068|"Slight"|"0"|0.108|"345833"
"Yd"|"Yegen sandy loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.76|7.74|14.8|21.68|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.068|"Slight"|"0"|0.108|"345834"
"Ye"|"Yegen sandy loam, 4 to 10 percent slopes"||7|6.8||||"None"|"None"|"0"|3.75|7.71|14.34|20.59|"Well drained"|"Well drained"|"B"|"4"|80|"4"|80|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.066|"Moderate"|"0"|0.113|"345835"
"Yt"|"Yegen and Toluca soils, 7 to 15 percent slopes"||11|11||||"None"|"None"|"0"|3.88|7.53|13.3|18.58|"Well drained"|"Well drained"|"B"|"4"|90|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.181|"Moderate"|"0"|0.374|"345836"
"GP"|"Gravel pit"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"696354"
"UL"|"Urban land"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"696355"
"453C"|"Cabbart-Bonfri loams, 2 to 8 percent slopes"||5|5.5|41|||"None"|"None"|"0"|3.87|6.98|9.88|9.88|"Well drained"|"Well drained"|"D"|"6"|50|"6"|52|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.21|"Moderate"|"0"|1|"1883531"
"381D"|"Blacksheep-Tusler complex, 4 to 15 percent slopes"||10|9.9|46|||"None"|"None"|"0"|3.32|6.12|7.68|9.12|"Well drained"|"Well drained"|"D"||93|"6"|59|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.264|"Moderate"|"0"|0.96|"1896419"
"285C"|"Doney-Cabba loams, 2 to 8 percent slopes"||5|5.1|46|||"None"|"None"|"0"|4.16|7.9|9.98|10.36|"Well drained"|"Well drained"|"C"|"3"|55|"4"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.08|"Moderate"|"0"|0.925|"1896888"
"285D"|"Cabba-Doney loams, 4 to 15 percent slopes"||12|9.2|43|||"None"|"None"|"0"|4.15|7.59|9.19|9.57|"Well drained"|"Well drained"|"D"||100|"6"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.543|"Severe"|"0"|0.927|"1897360"
"283F"|"Cabba-Rock outcrop complex, 8 to 45 percent slopes"||27|24.2|30|||"None"|"None"|"0"|4.08|5.33|5.48|5.48|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.873|"Severe"|"0"|1|"1897372"
"285F"|"Blacksheep, dry-Cabbart, dry-Rock outcrop, complex, 8 to 60 percent slopes"||21|24.5|30|||"None"|"None"|"0"|3.59|5.6|6.33|6.94|"Well drained"|"Well drained"|"D"||93|"7"|68|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.713|"Severe"|"0"|0.944|"1897375"
"189B"|"Rentsac-Beenom complex, 1 to 4 percent slopes"||3|3.4|30|||"None"|"None"|"0"|3.24|5.12|5.59|5.59|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.155|"Moderate"|"0"|0.95|"1898078"
"189C"|"Rentsac-Cabbart complex, 2 to 15 percent slopes"||9|9.4|41|||"None"|"None"|"0"|2.84|4.58|4.73|4.73|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.109|"Slight"|"0"|1|"1898095"
"80D"|"Blacksheep sandy loam, 4 to 15 percent slopes"||10|9.9|46|||"None"|"None"|"0"|3.73|6.76|7|7|"Well drained"|"Well drained"|"D"||100|"6"|80|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.039|"Moderate"|"0"|0.985|"1898165"
"83E"|"Blacksheep-Twilight complex, 4 to 25 percent slopes"||15|14.2|46|||"None"|"None"|"0"|3.71|6.89|7.65|7.79|"Well drained"|"Well drained"|"D"||98|"7"|54|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.037|"Moderate"|"0"|0.992|"1899133"
"483E"|"Cohagen-Dast fine sandy loams, 4 to 25 percent slopes"||14|13.5|38|||"None"|"None"|"0"|3.81|6.43|8.38|8.51|"Well drained"|"Well drained"|"D"||100|"6"|63|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.085|"Severe"|"0"|0.975|"1899180"
"282D"|"Cabbart-Blacksheep complex, 4 to 15 percent slopes"||10|9.9|41|||"None"|"None"|"0"|3.55|5.97|6.25|6.42|"Well drained"|"Well drained"|"D"||100|"6"|95|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.149|"Severe"|"0"|0.976|"1901405"
"282E"|"Cabba-Ridge complex, 8 to 25 percent slopes"||16|15.9|30|||"None"|"None"|"0"|3.89|5.6|5.9|6.07|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.58|"Severe"|"0"|0.978|"1903775"
"183E"|"Cabbart-Blacksheep, dry- complex, 8 to 25 percent slopes"||17|18.3|30|||"None"|"None"|"0"|3.56|5.27|5.5|5.68|"Well drained"|"Well drained"|"D"||98|"7"|83|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.417|"Severe"|"0"|0.99|"1904087"
"383E"|"Cabbart-Blacksheep complex, 8 to 25 percent slopes"||20|20.2|41|||"None"|"None"|"0"|3.54|5.91|6.3|6.64|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.506|"Severe"|"0"|0.984|"1904088"
"280D"|"Cabbart, moist-Delpoint, dry loams, 4 to 15 percent slopes"||10|8.5|41|||"None"|"None"|"0"|3.74|6.69|7.66|8.03|"Well drained"|"Well drained"|"D"||55|"6"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.24|"Severe"|"0"|0.95|"1904531"
"32D"|"Twilight-Blacksheep-Rock outcrop, complex, 4 to 25 percent slopes"||12|12.2|46|||"None"|"None"|"0"|3.71|7.09|8.78|9.36|"Well drained"|"Well drained"|"B"||93|"4"|50|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.041|"Severe"|"0"|0.88|"1913542"
"83D"|"Cabbart-Rock outcrop-Blacksheep complex, 8 to 45 percent slopes"||27|25.2|41|||"None"|"None"|"0"|3.46|5.74|6.22|6.51|"Well drained"|"Well drained"|"D"||97|"7"|63|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.904|"Severe"|"0"|0.968|"1913559"
"84C"|"Cabbart-Yawdim-Delpoint complex, 4 to 15 percent slopes"||10|9.6|38|||"None"|"None"|"0"|3.55|6.07|7.04|7.42|"Well drained"|"Well drained"|"D"||92|"6"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.367|"Severe"|"0"|0.95|"1913560"
"84D"|"Cabbart-Yawdim-Badland complex, 4 to 35 percent slopes"||20|17.4|41|||"None"|"None"|"0"|3.6|6.26|7.13|7.81|"Well drained"|"Well drained"|"D"||91|"7"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.686|"Severe"|"0"|1|"1913561"
"87B"|"Delpoint, calcareous-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|3.01|5.28|6.09|6.23|"Well drained"|"Well drained"|"C"|"4"|55|"6"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.282|"Moderate"|"0"|0.98|"1913562"
"230C"|"Macar loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.29|8.31|15.84|23.04|"Well drained"|"Well drained"|"B"||95|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.085|"Moderate"|"0"|0.05|"1913563"
"240E"|"Ridge-Dast-Rock outcrop complex, 4 to 35 percent slopes"||10|15.9|41|||"None"|"None"|"0"|3.59|6.26|8.03|8.03|"Well drained"|"Well drained"|"D"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.366|"Severe"|"0"|1|"1913564"
"242D"|"Dast-Ridge sandy loams, 2 to 8 percent slopes"||5|6.5|46|||"None"|"None"|"0"|3.56|6.58|9.27|9.27|"Well drained"|"Well drained"|"D"||55|"4"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.114|"Moderate"|"0"|1|"1913565"
"242F"|"Ridge-Dast sandy loams, 8 to 45 percent slopes"||30|23.4|41|||"None"|"None"|"0"|3.52|6.2|8.2|8.2|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.565|"Severe"|"0"|1|"1913566"
"245F"|"Lamedeer-Ringling channery loams, 4 to 45 percent slopes"||30|26.8||||"None"|"None"|"0"|2.94|5.15|7.92|9.77|"Well drained"|"Well drained"|"B"||100|"6"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1913567"
"246F"|"Lamedeer-Ringling channery loams, moist, 4 to 45 percent slopes"||30|26.8||||"None"|"None"|"0"|2.94|5.15|7.92|9.77|"Well drained"|"Well drained"|"B"||100|"6"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1913568"
"255C"|"Shambo-Korchea-Barvon loams, 2 to 8 percent slopes"||3|4|74|||"None"|"Rare"|"0"|4.47|8.71|15.94|22.02|"Well drained"|"Well drained"|"B"|"3"|35|"3"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.076|"Moderate"|"0"|0.212|"1913569"
"281D"|"Doney-Cabba-Macar loams, 4 to 15 percent slopes"||12|9.9|43|||"None"|"None"|"0"|4.18|7.84|11.25|13.5|"Well drained"|"Well drained"|"C"||100|"4"|40|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.36|"Severe"|"0"|0.677|"1913570"
"282F"|"Cabba-Doney loams, 8 to 45 percent slopes"||30|24.3|43|||"None"|"None"|"0"|4.13|7.51|8.45|8.45|"Well drained"|"Well drained"|"D"||100|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.823|"Severe"|"0"|0.976|"1913571"
"286F"|"Cabbart, calcareous-Rock outcrop complex, 8 to 45 percent slopes"||27|24.4|0|||"None"|"None"|"0"|3.57|4.64|4.78|4.78|"Well drained"|"Well drained"|"D"|"7"|75|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.938|"Severe"|"0"|1|"1913572"
"287F"|"Cabbart, moist-Delpoint, dry loams, 8 to 45 percent slopes"||35|28.6|41|||"None"|"None"|"0"|3.77|6.7|7.08|7.08|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.924|"Severe"|"0"|1|"1913573"
"354B"|"Bonfri-Cabbart loams, 0 to 4 percent slopes"||2|2.9|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.95|"1869336"
"182D"|"Cabbart-Delpoint loams, 4 to 15 percent slopes"||10|8.1|41|||"None"|"None"|"0"|3.84|6.95|8.79|9.21|"Well drained"|"Well drained"|"D"||55|"6"|50|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.23|"Severe"|"0"|0.799|"1869328"
"81B"|"Delpoint-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4|7.44|10.51|10.75|"Well drained"|"Well drained"|"C"|"3"|63|"3"|63|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.201|"Moderate"|"0"|0.638|"1869303"
"Wo"|"Worland fine sandy loam, 2 to 7 percent slopes"||5|5.1|102|||"None"|"None"|"0"|3.5|6.78|12.75|12.97|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.07|"Moderate"|"0"|0.955|"345827"
"Wn"|"Work clay loam, 4 to 7 percent slopes"||6|5.7||||"None"|"None"|"0"|4.14|8.16|15.61|21.53|"Well drained"|"Well drained"|"C"|"3"|91|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.155|"Moderate"|"0"|0.312|"345826"
"Wm"|"Work clay loam, 1 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|4.13|8.15|16.18|24.21|"Well drained"|"Well drained"|"C"|"2"|94|"3"|100|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.149|"Moderate"|"0"|0.312|"345825"
"Wl"|"Wanetta-Larim clay loams, 4 to 7 percent slopes"||6|6||||"None"|"None"|"0"|3.9|7.35|10.54|12.37|"Well drained"|"Well drained"|"B"|"3"|60|"3"|60|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.239|"Moderate"|"0"|0.95|"345824"
"Wk"|"Wanetta-Larim clay loams, 1 to 4 percent slopes"||2|2.5||||"None"|"None"|"0"|4.02|7.79|11|12.65|"Well drained"|"Well drained"|"B"|"2"|70|"3"|70|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.256|"Slight"|"0"|1|"345823"
"Wh"|"Wanetta-Larim clay loams, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.98|7.65|10.92|12.75|"Well drained"|"Well drained"|"B"|"2"|65|"3"|65|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.259|"Slight"|"0"|1|"345822"
"Wg"|"Wanetta clay loam, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.2|8.52|12.41|14.45|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.311|"Slight"|"0"|1|"345821"
"Wf"|"Wanetta clay loam, 0 to 1 percent slopes"||1|1.1||||"None"|"None"|"0"|4.24|8.51|12.5|14.58|"Well drained"|"Well drained"|"B"|"2"|86|"3"|93|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.304|"Slight"|"0"|0.94|"345820"
"We"|"Wanetta gravelly loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.61|9.01|15.7|17.51|"Well drained"|"Well drained"|"B"|"3"|85|"3"|90|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.144|"Slight"|"0"|1|"345819"
"Wc"|"Wanetta loam, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|4.56|8.9|15.52|17.47|"Well drained"|"Well drained"|"B"|"2"|85|"3"|88|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.31|"Moderate"|"0"|0.97|"345818"
"Wa"|"Wanetta loam, 0 to 1 percent slopes"||1|1.1||||"None"|"None"|"0"|4.55|8.88|15.55|17.64|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.32|"Slight"|"0"|1|"345817"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"345816"
"Ve"|"Vananda-Bone clays, 4 to 7 percent slopes"||6|6||||"None"|"None"|"0"|2.6|4.79|9.01|13.16|"Well drained"|"Well drained"|"D"|"7"|50|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.454|"Moderate"|"0"|1|"345815"
"Vd"|"Vananda silty clay, 1 to 7 percent slopes"||4|4.2||||"None"|"None"|"0"|2.55|4.75|9.15|13.55|"Well drained"|"Well drained"|"D"|"7"|90|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"345814"
"Va"|"Vananda silty clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"5"|2.62|4.92|9.52|14.12|"Well drained"|"Well drained"|"D"|"7"|90|"7"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.525|"Slight"|"5"|1|"345813"
"Tw"|"Treasure fine sandy loam, 4 to 10 percent slopes"||7|6.9||||"None"|"None"|"0"|3.87|7.67|14.59|21.42|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Moderate"|"0"|0.1|"345812"
"Tu"|"Treasure fine sandy loam, 1 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|3.92|7.72|14.8|21.7|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.053|"Moderate"|"0"|0.069|"345811"
"To"|"Toluca and Wanetta clay loams, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.46|8.79|16.94|19.49|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.325|"Slight"|"0"|0.894|"345807"
"Tn"|"Toluca and Wanetta clay loams, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.43|8.77|15.01|17.56|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.334|"Slight"|"0"|0.894|"345806"
"Tm"|"Toluca clay loam, 4 to 7 percent slopes"||6|6||||"None"|"None"|"0"|4.21|8.1|15.09|19.17|"Well drained"|"Well drained"|"B"|"3"|85|"3"|94|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.342|"Moderate"|"0"|0.112|"345805"
"Th"|"Toluca clay loam, 1 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|4.21|8.1|15.09|19.17|"Well drained"|"Well drained"|"B"|"3"|91|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.299|"Moderate"|"0"|0.108|"345804"
"Te"|"Toluca clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.18|8.07|14.66|18.29|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.302|"Slight"|"0"|0.15|"345803"
"Tc"|"Thurlow clay loam, 4 to 7 percent slopes"||6|5.8||||"None"|"None"|"0"|4.16|7.97|15.62|23.27|"Well drained"|"Well drained"|"C"|"3"|92|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.351|"Moderate"|"0"|0.252|"345802"
"Ta"|"Thurlow clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.16|7.97|15.6|23.23|"Well drained"|"Well drained"|"C"|"2"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.346|"Slight"|"0"|0.252|"345801"
"Sr"|"Shorey gravelly loam, 4 to 7 percent slopes"||6|6||||"None"|"None"|"0"|3.98|7.9|13.84|17.83|"Well drained"|"Well drained"|"B"|"3"|96|"3"|96|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.12|"Moderate"|"0"|0.066|"345800"
"So"|"Shorey gravelly loam, 1 to 4 percent slopes"||3|3.3||||"None"|"None"|"0"|3.98|7.9|13.9|17.96|"Well drained"|"Well drained"|"B"|"2"|89|"3"|96|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.124|"Slight"|"0"|0.059|"345799"
"Sn"|"Shonkin loam, 0 to 1 percent slopes"||1|1.1||0|0|"None"|"None"|"85"|4.36|7.64|13.89|19.38|"Somewhat poorly drained"|"Somewhat poorly drained"|"C/D"||85|"6"|89|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.877|"Slight"|"85"|1|"345798"
"Sm"|"Shale outcrop-Midway complex, 15 to 35 percent slopes"|||25|30|||"None"|"None"|"0"|4.26|5.11|5.11|5.11|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"345797"
"Sl"|"Shale outcrop"|||25||||||"0"|4.25|4.25|4.25|4.25|||||100||90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"345796"
"Sk"|"Shaak silty clay loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.92|7.53|15.12|20.65|"Well drained"|"Well drained"|"C"|"2"|85|"3"|91|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.184|"Moderate"|"0"|1|"345795"
"Sh"|"Shaak silty clay loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"2"|3.93|7.54|15.25|20.7|"Well drained"|"Well drained"|"C"|"2"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.201|"Slight"|"2"|1|"345794"
"Sa"|"Sage clay, 0 to 1 percent slopes"||1|1.4||46|46|"None"|"None"|"0"|2.05|4.05|6.68|9.11|"Poorly drained"|"Poorly drained"|"C/D"||100|"7"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.95|"Slight"|"90"|1|"345793"
"Rn"|"Ryegate fine sandy loam, 2 to 4 percent slopes"||3|3.1|64|||"None"|"None"|"0"|3.53|7.24|9.65|9.67|"Well drained"|"Well drained"|"C"|"3"|85|"3"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.101|"Moderate"|"0"|1|"345790"
"Rk"|"Rock land"|||15.2||||||"0"|3.89|7.08|9.13|9.13|||||100||90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.614|"Not rated"|"0"|1|"345789"
"Re"|"Riverwash"|||1||||||"0"|3.33|6.53|12.88|19.23|||||90||90|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.147|"Not rated"|"5"|0.769|"345788"
"Rc"|"Razor-Cushman complex, 2 to 4 percent slopes"||3|3.2|71|||"None"|"None"|"0"|3.94|7.37|11.32|11.33|"Well drained"|"Well drained"|"D"|"3"|55|"3"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.231|"Moderate"|"0"|0.975|"345787"
"Ra"|"Razor clay loam, 2 to 7 percent slopes"||5|5.1|74|||"None"|"None"|"0"|3.9|6.83|9.63|9.63|"Well drained"|"Well drained"|"D"|"3"|80|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.226|"Moderate"|"0"|0.95|"345786"
"Pl"|"Pierre-Lismas clays, 7 to 15 percent slopes"||9|10.2|25|||"None"|"None"|"0"|4|6.38|9.35|9.63|"Well drained"|"Well drained"|"D"||93|"4"|62|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"345785"
"Pc"|"Pierre clay, 4 to 7 percent slopes"||6|6.5|79|||"None"|"None"|"0"|3.88|7.37|11.64|11.93|"Well drained"|"Well drained"|"D"||93|"4"|87|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"345784"
"Os"|"Oburn-Shaak complex, 1 to 4 percent slopes"||3|3||||"None"|"None"|"8"|4.02|7.29|13.22|17.45|"Well drained"|"Well drained"|"C"|"6"|40|"3"|52|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.259|"Moderate"|"0"|1|"345783"
"Oh"|"Oburn-Shaak complex, 0 to 1 percent slopes"||1|1||||"None"|"None"|"9"|4.08|7.31|13.58|17.61|"Well drained"|"Well drained"|"C"|"6"|45|"6"|54|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.265|"Slight"|"0"|1|"345782"
"Mw"|"Midway-Razor clay loams, 4 to 7 percent slopes"||6|5.7|30|||"None"|"None"|"0"|4.35|5.79|6.6|6.6|"Well drained"|"Well drained"|"D"||75|"6"|72|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.22|"Moderate"|"0"|0.985|"345780"
"Mv"|"McRae-Hysham loams, 3 to 6 percent slopes"||5|4.8||||"None"|"None"|"0"|4.2|8.05|15.8|23.55|"Well drained"|"Well drained"|"B"|"3"|65|"3"|75|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.242|"Moderate"|"0"|0.25|"345779"
"Mu"|"McRae-Hysham loams, 1 to 3 percent slopes"||2|1.9||||"None"|"Rare"|"0"|4.21|8.05|15.73|23.4|"Well drained"|"Well drained"|"B"|"2"|75|"3"|75|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.224|"Slight"|"0"|0.25|"345778"
"Mt"|"McRae-Hysham loams, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.19|7.96|15.48|23.01|"Well drained"|"Well drained"|"B"|"2"|65|"3"|65|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.253|"Slight"|"0"|0.35|"345777"
"Ms"|"McRae-Bainville loams, 7 to 15 percent slopes"||9|10.4|64|||"None"|"None"|"0"|4.39|8.66|14.85|19.1|"Well drained"|"Well drained"|"B"||95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.489|"Severe"|"0"|0.461|"345776"
"Mr"|"McRae loam, 7 to 15 percent slopes"||11|10.5||||"None"|"None"|"0"|4.5|8.78|16.96|24.7|"Well drained"|"Well drained"|"B"||94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.338|"Severe"|"0"|0.357|"345775"
"Mo"|"McRae loam, 4 to 7 percent slopes"||6|5.7||||"None"|"None"|"0"|4.49|8.75|17.01|24.91|"Well drained"|"Well drained"|"B"|"3"|85|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.279|"Moderate"|"0"|0.035|"345774"
"Mn"|"McRae loam, 1 to 4 percent slopes"||3|2.8||||"None"|"None"|"0"|4.46|8.67|17.13|25.58|"Well drained"|"Well drained"|"B"|"2"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.253|"Moderate"|"0"|0|"345773"
"Mm"|"McRae loam, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|4.36|8.5|16.82|25.14|"Well drained"|"Well drained"|"B"|"2"|94|"3"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.254|"Slight"|"0"|0.047|"345772"
"Mk"|"McKenzie clay, 0 to 1 percent slopes"||1|1.2||0|0|"None"|"None"|"85"|3.68|7.3|14.56|21.81|"Poorly drained"|"Poorly drained"|"D"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.917|"Slight"|"85"|1|"345771"
"Mg"|"Maginnis-Rock outcrop complex, 35 to 60 percent slopes"||53|46.7|5||||"None"|"0"|2.15|2.15|2.15|2.15||"Well drained"|||100|"8"|55|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"345770"
"Mc"|"Maginnis channery clay loam, 15 to 35 percent slopes"||25|25|25|||"None"|"None"|"0"|1.8|1.8|1.8|1.8|"Well drained"|"Well drained"|"D"||100|"7"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"345769"
"Ma"|"Maginnis channery clay loam, 7 to 15 percent slopes"||11|9.7|25|||"None"|"None"|"0"|2.02|2.75|3.37|3.72|"Well drained"|"Well drained"|"D"||90|"7"|80|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.149|"Moderate"|"0"|1|"345768"
"Lv"|"Lohmiller silty clay, gravelly variant, 0 to 1 percent slopes"||1|1||||"None"|"Rare"|"0"|4.01|8.02|15.33|20.15|"Well drained"|"Well drained"|"C"|"3"|80|"3"|98|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.435|"Slight"|"2"|0.873|"345767"
"Lu"|"Lohmiller-Hysham silty clay loams, 0 to 1 percent slopes"||1|1||122|122|"None"|"None"|"0"|3.65|6.84|13.21|19.59|"Well drained"|"Moderately well drained"|"C"||50|"4"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.167|"Slight"|"0"|0.865|"345766"
"Lt"|"Lohmiller-Elso complex, 4 to 15 percent slopes"||7|9.3|30|||"None"|"None"|"0"|4.38|6.98|11.42|15.87|"Well drained"|"Well drained"|"C"||95|"4"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.275|"Moderate"|"0"|1|"345765"
"Ls"|"Lohmiller soils, seeped, 0 to 2 percent slopes"||1|1||137|137|"Rare"|"Rare"|"0"|4.12|8.1|16.04|23.99|"Well drained"|"Well drained"|"C"|"4"|80|"4"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.265|"Slight"|"2"|0.894|"345764"
"Lr"|"Lohmiller silty clay, 0 to 1 percent slopes"||1|1||||"None"|"None"|"0"|3.96|7.87|15.68|22.29|"Well drained"|"Well drained"|"C"|"4"|90|"4"|85|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.433|"Slight"|"0"|0.947|"345763"
"Lo"|"Lohmiller silty clay, 3 to 7 percent slopes"||5|5.2||||"None"|"None"|"0"|4.45|8.47|16.51|24.56|"Well drained"|"Well drained"|"C"|"3"|100|"3"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.274|"Moderate"|"0"|0.91|"345762"
"Ln"|"Lismas clay, 15 to 35 percent slopes"||25|21.7|25|||"None"|"None"|"0"|4.18|4.91|5.92|6.1|"Well drained"|"Well drained"|"D"||95|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.9|"Severe"|"0"|1|"345761"
"Lm"|"Lavina loam, 2 to 4 percent slopes"||3|3|48|||"None"|"None"|"2"|4.47|8.2|8.9|9.17|"Well drained"|"Well drained"|"D"|"6"|80|"6"|92|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.346|"Moderate"|"2"|1|"345760"
"Ll"|"Larim gravelly loam, 15 to 35 percent slopes"||25|25||||"None"|"None"|"0"|3.43|4.41|5.84|6.88|"Excessively drained"|"Excessively drained"|"A"||100|"7"|84|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"345759"
"Lh"|"Larim gravelly loam, 4 to 7 percent slopes"||6|5.1||||"None"|"None"|"0"|3.14|5.14|7.27|9.22|"Well drained"|"Well drained"|"B"|"4"|90|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.14|"Moderate"|"0"|1|"345758"
"Lg"|"Larim gravelly loam, 0 to 4 percent slopes"||2|1.9||||"None"|"None"|"0"|3.14|5.14|7.27|9.22|"Well drained"|"Well drained"|"B"|"4"|90|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.14|"Slight"|"0"|1|"345757"
"Le"|"Larim loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"2"|3.49|5.69|8.45|10.49|"Well drained"|"Well drained"|"B"|"4"|85|"6"|87|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.184|"Slight"|"2"|1|"345756"
"Ld"|"Lambert soils, 7 to 35 percent slopes"||21|20.9||||"None"|"None"|"0"|4.78|9.03|17.05|24.68|"Well drained"|"Well drained"|"C"||95|"6"|88|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.972|"Severe"|"0"|0.965|"345755"
"289F"|"Cabba-Barvon loams, 15 to 65 percent slopes"||45|33.9|30|||"None"|"None"|"0"|4.03|6.49|8.35|8.35|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.942|"Severe"|"0"|1|"1913574"
"131C"|"Delpoint-Yamacall loams, 2 to 8 percent slopes"||5|5.3|56|||"None"|"None"|"0"|4.12|8.01|11.56|14.31|"Well drained"|"Well drained"|"C"|"3"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Moderate"|"0"|0.632|"1913843"
"354C"|"Bonfri-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.95|"1913844"
"10"|"Assinniboine-Rentsac complex, 6 to 12 percent slopes"||9|8.9|46|||"None"|"None"|"0"|3.64|6.89|11.41|13.81|"Well drained"|"Well drained"|"B"||97|"4"|63|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.104|"Severe"|"0"|0.407|"1946662"
"32B"|"Twilight sandy loam, 2 to 8 percent slopes"||5|5|89|||"None"|"None"|"0"|3.77|7.3|12.52|12.96|"Well drained"|"Well drained"|"B"|"4"|89|"4"|89|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Moderate"|"0"|0.519|"1946663"
"369D"|"Rentsac-Tanna complex, 2 to 15 percent slopes"||9|9|41|||"None"|"None"|"0"|3.01|5.42|6.56|6.64|"Well drained"|"Well drained"|"D"|"7"|52|"7"|52|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.184|"Slight"|"0"|1|"1946664"
"780F"|"Cabbart-Yamacall-Havre, rarely flooded, loams, 2 to 60 percent slopes"||34|13.5|30|||"None"|"Rare"|"0"|4.2|7.09|11.89|16.64|"Well drained"|"Well drained"|"B"||45|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.464|"Severe"|"0"|0.483|"1946665"
"53A"|"Tanna loam, 1 to 6 percent slopes"||4|4.3|64|||"None"|"None"|"0"|4.05|7.06|8.93|9.17|"Well drained"|"Well drained"|"D"|"3"|83|"3"|83|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.271|"Moderate"|"0"|1|"2396138"
"460E"|"Yawdim-Abor complex, 8 to 35 percent slopes"||21|18.1|46|||"None"|"None"|"0"|4.16|7.53|9.32|9.68|"Well drained"|"Well drained"|"D"||95|"7"|64|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.821|"Severe"|"0"|1|"2396559"
"35B"|"Yamacall-Busby complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.91|7.7|14.84|21.66|"Well drained"|"Well drained"|"B"|"3"|55|"3"|57|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.125|"Moderate"|"0"|0.261|"2396639"
"21A"|"McKenzie silty clay, 0 to 2 percent slopes"||1|1.1||30|30|"None"|"None"|"85"|3.6|7.13|14.11|21.08|"Poorly drained"|"Poorly drained"|"D"||90|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.925|"Slight"|"85"|1|"2396640"
"41A"|"Yamacall loam, calcareous, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.26|8.6|16.7|24.57|"Well drained"|"Well drained"|"B"|"4"|92|"4"|92|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.199|"Slight"|"0"|0.112|"2396641"
"152B"|"Eapa loam, calcareous, 0 to 8 percent slopes"||4|4||||"None"|"None"|"0"|4.22|8.61|17.53|26.7|"Well drained"|"Well drained"|"B"||90|"4"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.217|"Moderate"|"0"|0.05|"2396643"
"My"|"MLRA 58A Midway-Shale outcrop complex, 4 to 35 percent slopes"||15|15.9|30|||"None"|"None"|"0"|4.55|6.34|8.06|9.13|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.375|"Severe"|"0"|1|"2926231"
