"AbC"|"Abor silty clay, 3 to 9 percent slopes"||6|6.1|97|||"None"|"None"|"0"|3.88|7.62|14.29|14.66|"Well drained"|"Well drained"|"D"||95|"4"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.451|"Moderate"|"0"|0.91|"147476"
"Af"|"Aeric Fluvaquents"||3|3||99|99|"Frequent"|"Frequent"|"0"|4.29|8.04|15.54|20.51|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.4|"Moderate"|"25"|1|"147477"
"AmB"|"Amesha sandy loam, 1 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|3.37|7.37|15.3|22.49|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.061|"Slight"|"0"|0.05|"147478"
"AmC"|"Amesha sandy loam, 4 to 9 percent slopes"||7|7||||"None"|"None"|"0"|3.31|7.18|14.83|21.82|"Well drained"|"Well drained"|"B"|"4"|100|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.061|"Moderate"|"0"|0.095|"147479"
"AnB"|"Amesha cobbly sandy loam, 1 to 4 percent slopes"||3|3.5||||"None"|"None"|"0"|3.43|7.09|14.05|20.11|"Well drained"|"Well drained"|"B"|"4"|100|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.089|"Slight"|"0"|0.486|"147480"
"AoB"|"Amesha loam, 1 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|4.2|8.21|16.23|23.59|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.108|"Moderate"|"0"|0|"147481"
"AoC"|"Amesha loam, 4 to 9 percent slopes"||7|6.3||||"None"|"None"|"0"|3.9|7.63|14.9|21.57|"Well drained"|"Well drained"|"B"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.105|"Moderate"|"0"|0.168|"147482"
"BcE"|"Blaine-Cheadle cobbly loams, 10 to 25 percent slopes"||18|17.4|30|||"None"|"None"|"0"|2.71|4.31|4.89|4.89|"Well drained"|"Well drained"|"C"||100|"6"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.283|"Moderate"|"0"|0.995|"147483"
"BdC"|"Blanyon clay loam, 3 to 10 percent slopes"||7|7.6||||"None"|"None"|"0"|3.88|7.8|15.16|21.46|"Well drained"|"Well drained"|"C"|"3"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.121|"Moderate"|"0"|0.892|"147484"
"Bo"|"Borohemists"||1|1||0|0|"None"|"None"|"100"|8.5|16|30.01|37.9|"Very poorly drained"|"Very poorly drained"|"C/D"||100|"5"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Slight"|"100"|1|"147485"
"BpD"|"Bridger cobbly loam, 5 to 15 percent slopes"||10|13.3||||"None"|"None"|"0"|3.41|6.68|12.85|18.68|"Well drained"|"Well drained"|"C"||100|"4"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.207|"Moderate"|"0"|0.65|"147486"
"BrD"|"Bridger silt loam, 5 to 15 percent slopes"||10|10||||"None"|"None"|"0"|4.53|8.23|14.94|21.44|"Well drained"|"Well drained"|"C"||100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.803|"Severe"|"0"|0.5|"147487"
"BsA"|"Brocko silt loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|4.86|9.66|18.6|26.88|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.182|"Slight"|"0"|0.125|"147488"
"BsB"|"Brocko silt loam, 2 to 5 percent slopes"||4|4.1||||"None"|"None"|"0"|4.86|9.71|19.41|28.11|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.194|"Moderate"|"0"|0.038|"147489"
"BsC"|"Brocko silt loam, 5 to 9 percent slopes"||7|6.9||||"None"|"None"|"0"|4.87|9.71|18.51|26.94|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.192|"Moderate"|"0"|0|"147490"
"BsD"|"Brocko silt loam, 9 to 25 percent slopes"||17|17||||"None"|"None"|"0"|4.78|9.3|17.08|24.26|"Well drained"|"Well drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.912|"Severe"|"0"|0.996|"147491"
"BtA"|"Brocko silt loam, wet, 0 to 2 percent slopes"||1|1.8||122|122|"None"|"None"|"0"|4.39|8.64|17.14|24.89|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.188|"Slight"|"0"|0.375|"147492"
"CaE"|"Cabbart complex, 9 to 35 percent slopes"||22|19.5|38|||"None"|"None"|"0"|4.18|7.14|9.29|10.04|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.798|"Severe"|"0"|0.981|"147493"
"CdE"|"Cheadle stony loam, 9 to 35 percent slopes"||22|19.6|30|||"None"|"None"|"0"|2.55|3.5|3.74|3.74|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.671|"Moderate"|"0"|0.994|"147494"
"ChB"|"Chinook sandy loam, 1 to 4 percent slopes"||3|3.2||||"None"|"None"|"0"|3.51|7.08|13.96|20.21|"Well drained"|"Well drained"|"A"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.033|"Moderate"|"0"|0.36|"147495"
"ChC"|"Chinook sandy loam, 4 to 9 percent slopes"||7|6.8||||"None"|"None"|"0"|3.5|7.03|13.81|19.89|"Well drained"|"Well drained"|"A"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.031|"Moderate"|"0"|0.443|"147496"
"CkB"|"Chinook sandy loam, gravelly subsoil variant, 1 to 4 percent slopes"||3|3.3||||"None"|"None"|"0"|3.5|6.93|12.56|15.56|"Well drained"|"Well drained"|"A"|"4"|100|"4"|83|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.052|"Slight"|"0"|0.885|"147497"
"CmC"|"Chinook-Crago loamy sands, 1 to 9 percent slopes"||5|5||||"None"|"None"|"0"|2.47|4.54|8.49|11.79|"Well drained"|"Well drained"|"A"|"6"|90|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.715|"Moderate"|"0"|0.9|"147498"
"CnC"|"Chinook-Crago complex, 5 to 9 percent slopes"||7|7||||"None"|"None"|"0"|2.75|5.67|11.27|15.79|"Well drained"|"Well drained"|"A"|"4"|100|"4"|60|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.057|"Moderate"|"0"|0.58|"147499"
"CnE"|"Chinook-Crago complex, 9 to 35 percent slopes"||22|18.4||||"None"|"None"|"0"|2.87|5.67|10.41|14.05|"Well drained"|"Well drained"|"A"||95|"6"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.686|"Severe"|"0"|0.95|"147500"
"CrC"|"Crago complex, 4 to 9 percent slopes"||7|6.3||||"None"|"None"|"0"|3.43|6.57|11.64|14.77|"Well drained"|"Well drained"|"B"|"4"|100|"6"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.145|"Moderate"|"0"|0.75|"147501"
"DeB"|"Delphill loam, 2 to 5 percent slopes"||4|4.2|89|||"None"|"None"|"0"|4.17|8.17|14.72|15.38|"Well drained"|"Well drained"|"C"||90|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.245|"Moderate"|"0"|0.178|"147502"
"DhD"|"Delphill-Abor complex, 5 to 20 percent slopes"||13|13.4|38|||"None"|"None"|"0"|4.1|7.72|13.26|13.95|"Well drained"|"Well drained"|"C"||90|"6"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.434|"Severe"|"0"|0.931|"147503"
"Do"|"Dominic soils"||1|1||168|168|"Rare"|"Rare"|"0"|3.6|4.96|7.21|9.08|"Excessively drained"|"Excessively drained"|"B"|"7"|80|"7"|80|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.062|"Slight"|"0"|0.9|"147504"
"EcF"|"Ess-Cheadle complex, 35 to 60 percent slopes"||48|48|30|||"None"|"None"|"0"|2.55|3.82|6.04|8.01|"Well drained"|"Well drained"|"B"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147505"
"Fa"|"Fairdale silt loam"||1|1||122|122|"None"|"Rare"|"0"|4.73|9.11|17.66|25.12|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"|"3"|80|"3"|80|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.184|"Slight"|"5"|0.925|"147506"
"Fb"|"Fairdale-Lothair silty clays"||1|1||122|122|"None"|"None"|"0"|4.12|8.3|16.51|24.04|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|80|"4"|80|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.748|"Slight"|"20"|1|"147507"
"Fd"|"Fluvaquentic Haplaquolls"||1|1||31|31|"Occasional"|"Occasional"|"0"|4.7|9.27|18.77|26.62|"Poorly drained"|"Poorly drained"|"B/D"|"5"|100|"5"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.998|"Slight"|"100"|1|"147508"
"Ha"|"Havre loam"||1|1||||"Rare"|"Rare"|"0"|4.35|8.44|16.46|23.81|"Well drained"|"Well drained"|"B"|"2"|80|"3"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.08|"Slight"|"0"|0.15|"147509"
"HgE"|"Hilger extremely stony loam, 8 to 25 percent slopes"||17|15.3||||"None"|"None"|"0"|2.25|4.16|7.85|11.13|"Well drained"|"Well drained"|"B"||90|"7"|80|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.171|"Moderate"|"0"|0.85|"147510"
"LaF"|"Lake creek channery loam, 20 to 50 percent slopes"||35|35.5|36|||"None"|"None"|"0"|2.97|5.42|8.43|8.43|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147511"
"LoE"|"Loberg very stony loam, 10 to 35 percent slopes"||23|23.3||||"None"|"None"|"0"|1.94|4.28|8.47|12.1|"Well drained"|"Well drained"|"C"||100|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.927|"Moderate"|"0"|1|"147512"
"Lt"|"Lothair silty clay"||1|1||||"None"|"None"|"0"|4.03|8.04|16.07|24.08|"Well drained"|"Well drained"|"C"||80|"4"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.483|"Slight"|"0"|0.971|"147513"
"MaB"|"Martinsdale loam, 2 to 5 percent slopes"||4|4.2||||"None"|"None"|"0"|4.28|7.41|11.51|15.61|"Well drained"|"Well drained"|"C"|"3"|80|"3"|80|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.078|"Moderate"|"0"|0.567|"147514"
"MaC"|"Martinsdale loam, 5 to 9 percent slopes"||7|7.7||||"None"|"None"|"0"|4.33|7.54|11.7|15.82|"Well drained"|"Well drained"|"C"|"3"|80|"3"|80|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.103|"Moderate"|"0"|0.555|"147515"
"McC"|"Martinsdale cobbly loam, 2 to 9 percent slopes"||6|5.6||||"None"|"None"|"0"|3.91|7.37|13.89|20.03|"Well drained"|"Well drained"|"C"|"3"|80|"3"|80|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.099|"Moderate"|"0"|0.6|"147516"
"Md"|"Mine dumps"||38|38||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"147517"
"MsA"|"Mussel loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.22|8.44|16.79|23.34|"Well drained"|"Well drained"|"B"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.119|"Slight"|"0"|0.05|"147518"
"MsB"|"Mussel loam, 2 to 5 percent slopes"||4|3.8||||"None"|"None"|"0"|4.12|8.17|16.25|22.77|"Well drained"|"Well drained"|"B"|"4"|100|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.117|"Moderate"|"0"|0.05|"147519"
"Mt"|"Mussel-Crago complex"||4|4.1||||"None"|"None"|"0"|3.75|7.36|14.17|19.36|"Well drained"|"Well drained"|"B"|"4"|75|"4"|70|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.128|"Moderate"|"0"|0.3|"147520"
"MuB"|"Mussel-Musselshell complex, 2 to 5 percent slopes"||4|4.3||||"None"|"None"|"0"|4.07|8.01|15.75|21.25|"Well drained"|"Well drained"|"B"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.126|"Moderate"|"0"|0.138|"147521"
"MuC"|"Mussel-Musselshell complex, 5 to 9 percent slopes"||7|6.6||||"None"|"None"|"0"|3.97|7.87|15.55|21.02|"Well drained"|"Well drained"|"B"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.13|"Moderate"|"0"|0.394|"147522"
"MvB"|"Musselshell gravelly loam, 2 to 5 percent slopes"||4|4||||"None"|"None"|"0"|3.82|7.59|14.63|18.38|"Well drained"|"Well drained"|"B"|"4"|100|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.13|"Slight"|"0"|0.3|"147523"
"MvC"|"Musselshell gravelly loam, 5 to 9 percent slopes"||7|6.9||||"None"|"None"|"0"|3.76|7.54|14.57|18.33|"Well drained"|"Well drained"|"B"|"4"|100|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.13|"Moderate"|"0"|0.3|"147524"
"MwE"|"Musselshell-Crago channery loams, 15 to 35 percent slopes"||25|24||||"None"|"None"|"0"|3.33|6.47|12.08|15.44|"Well drained"|"Well drained"|"B"||95|"6"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.955|"Severe"|"0"|0.949|"147525"
"MxE"|"Musselshell-Crago cobbly loams, 8 to 20 percent slopes"||14|12.5||||"None"|"None"|"0"|3.66|7.16|13.52|17.04|"Well drained"|"Well drained"|"B"||90|"6"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.124|"Moderate"|"0"|0.927|"147526"
"MyC"|"Musselshell-Thess cobbly loams, 3 to 8 percent slopes"||6|6.1||||"None"|"None"|"0"|3.92|7.89|15.07|18.5|"Well drained"|"Well drained"|"B"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.118|"Moderate"|"0"|0.852|"147527"
"NeF"|"Nielsen channery loam, 15 to 60 percent slopes"||38|34.6|36|||"None"|"None"|"0"|3.69|5.38|5.99|5.99|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"147528"
"PaD"|"Passcreek channery silt loam, 6 to 15 percent slopes"||11|18.4|97|||"None"|"None"|"0"|3.8|7.13|12.11|12.46|"Well drained"|"Well drained"|"C"||100|"4"|75|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.292|"Moderate"|"0"|0.525|"147529"
"PcE"|"Passcreek-Lake Creek channery loams, 15 to 35 percent slopes"||25|27.6|36|||"None"|"None"|"0"|3.52|6.46|10.35|10.35|"Well drained"|"Well drained"|"C"||100|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"147530"
"Pm"|"Perma very cobbly loam"||4|4.7||||"None"|"None"|"0"|3.22|6.04|9.8|12.68|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||85|"6"|75|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.12|"Slight"|"0"|0.896|"147531"
"Pr"|"Perma very cobbly loam, wet"||4|4.8||122|122|"None"|"None"|"0"|3.19|5.95|9.58|12.3|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"||90|"6"|70|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.115|"Slight"|"0"|0.853|"147532"
"Ra"|"Radersburg very cobbly loam"||4|3.7||||"None"|"None"|"0"|2.86|6.3|13.21|18.8|"Well drained"|"Well drained"|"C"||72|"6"|72|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.267|"Slight"|"0"|0.82|"147533"
"ReE"|"Rencot channery loam, 15 to 35 percent slopes"||25|24.1|46|||"None"|"None"|"0"|2.92|4.9|5.04|5.04|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.902|"Severe"|"0"|0.994|"147534"
"Rr"|"Rivra gravelly loam"||3|2.5||137|137|"Occasional"|"Occasional"|"0"|2.06|3.18|5.36|7.21|"Moderately well drained"|"Moderately well drained"|"B"||85|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Not limited"|0.093|"Slight"|"5"|1|"147535"
"RsE"|"Rooset extremely stony loam, 9 to 35 percent slopes"||22|22.6||||"None"|"None"|"0"|2.34|4.64|8.87|12.68|"Well drained"|"Well drained"|"C"||100|"7"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.856|"Moderate"|"0"|1|"147536"
"RtC"|"Rootel channery loam, 3 to 9 percent slopes"||6|7.6|58|||"None"|"None"|"0"|3.83|7.62|10.11|11.33|"Well drained"|"Well drained"|"C"||80|"3"|70|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.26|"Moderate"|"0"|0.84|"147537"
"SaB"|"Sappington clay loam, 2 to 5 percent slopes"||4|4.2||||"None"|"None"|"0"|3.8|7.36|14.32|20.53|"Well drained"|"Well drained"|"B"|"2"|80|"3"|80|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.19|"Moderate"|"0"|0.05|"147538"
"SaC"|"Sappington clay loam, 5 to 9 percent slopes"||7|7||||"None"|"None"|"0"|3.74|7.23|14.06|20.13|"Well drained"|"Well drained"|"B"|"3"|85|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.186|"Moderate"|"0"|0.05|"147539"
"SgB"|"Sappington gravelly clay loam, 2 to 5 percent slopes"||4|4.2||||"None"|"None"|"0"|3.27|6.74|13.55|19.62|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.187|"Slight"|"0"|0.05|"147540"
"SgC"|"Sappington gravelly clay loam, 5 to 9 percent slopes"||7|7||||"None"|"None"|"0"|3.29|6.78|13.61|19.68|"Well drained"|"Well drained"|"B"|"3"|85|"3"|85|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.183|"Moderate"|"0"|0.05|"147541"
"Sv"|"Scravo cobbly loam"||1|1.4||||"None"|"None"|"0"|2.97|4.89|7.39|8.95|"Well drained"|"Well drained"|"B"|"4"|100|"6"|85|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.082|"Slight"|"0"|1|"147542"
"Sw"|"Scravo very cobbly loam"||3|2.7||||"None"|"None"|"0"|2.31|3.9|5.94|7.44|"Well drained"|"Well drained"|"B"||75|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.151|"Slight"|"0"|1|"147543"
"Te"|"Thess silt loam"||2|2.5||||"None"|"None"|"0"|4.57|8.83|11.95|14.33|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.14|"Slight"|"0"|0.95|"147544"
"Ts"|"Thess-Scravo complex"||1|1.2||||"None"|"None"|"0"|3.75|6.97|11.71|13.21|"Well drained"|"Well drained"|"B"|"4"|90|"4"|60|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.099|"Slight"|"0"|1|"147545"
"TtE"|"Tolman channery loam, 10 to 35 percent slopes"||23|21.5|46|||"None"|"None"|"0"|3.1|5.06|5.19|5.19|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.856|"Severe"|"0"|0.995|"147546"
"Tu"|"Toston silty clay loam"||3|2.7||137|137|"Rare"|"Rare"|"0"|4.1|8.13|14.62|20.85|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"6"|70|"6"|75|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.27|"Moderate"|"5"|0.9|"147547"
"TvF"|"Tropal-Rock outcrop complex, 15 to 60 percent slopes"||38|37.8|48|||"None"|"None"|"0"|2.34|4.14|4.58|4.94|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147548"
"Uf"|"Ustic Torrifluvents"||2|2||||"Frequent"|"Frequent"|"0"|4.4|8.4|16.4|24.4|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.4|"Slight"|"0"|1|"147549"
"Ut"|"Ustic Torriorthents, saline"||3|3||114|114|"Rare"|"Rare"|"0"|2.75|5.5|11|16.5|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"|"4"|95|"6"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.07|"Moderate"|"0"|0.778|"147550"
"Va"|"Villy silty clay loam"||1|1||31|31|"Rare"|"Rare"|"0"|4.57|9.32|18.82|27.36|"Poorly drained"|"Poorly drained"|"C/D"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.998|"Slight"|"100"|1|"147551"
"Vd"|"Villy silty clay loam, drained"||1|1||99|99|"Rare"|"Rare"|"0"|4.57|9.32|18.82|27.36|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"3"|90|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.478|"Slight"|"10"|0.55|"147552"
"WhF"|"Whitore channery silt loam, 25 to 60 percent slopes"||43|43|48|||"None"|"None"|"0"|2.05|3.7|6.65|9.6|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147553"
"WnE"|"Windham cobbly loam, 9 to 35 percent slopes"||22|17.3||||"None"|"None"|"0"|3.07|4.9|8.26|11.27|"Well drained"|"Well drained"|"B"||80|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.556|"Severe"|"0"|0.868|"147554"
"WoF"|"Woodrock-Loberg complex, 15 to 60 percent slopes"||38|38|81|||"None"|"None"|"0"|2.04|4.79|8.35|9.68|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147555"
"WrE"|"Woodrock-Rock outcrop complex, 15 to 35 percent slopes"||25|25.4|71|||"None"|"None"|"0"|2.4|5.16|8.26|8.69|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.978|"Severe"|"0"|1|"147556"
"4"|"Bronec, Clunton, Channeled, and Amesha soils, 0 to 8 percent slopes"||5|3.9||15|15|"None"|"Frequent"|"30"|3.67|7.21|14.03|19.45|"Well drained"|"Very poorly drained"|"B"|"4"|60|"4"|60|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.425|"Moderate"|"32"|0.376|"147557"
"11C"|"Amesha silt loam, 4 to 8 percent slopes"||6|6.1||||"None"|"None"|"0"|4.37|8.33|15.71|22.43|"Well drained"|"Well drained"|"B"|"4"|97|"4"|98|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.128|"Moderate"|"0"|0.032|"147558"
"11D"|"Amesha silt loam, 8 to 15 percent slopes"||12|12.8||||"None"|"None"|"0"|4.36|8.33|15.87|22.78|"Well drained"|"Well drained"|"B"|"4"|92|"4"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.188|"Severe"|"0"|0.655|"147559"
"13A"|"Anamac loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.38|8.65|16.82|24.69|"Well drained"|"Well drained"|"B"|"3"|94|"3"|94|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.132|"Slight"|"0"|0.036|"147560"
"13C"|"Anamac loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.35|8.53|16.58|24.33|"Well drained"|"Well drained"|"B"|"3"|94|"3"|92|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.139|"Moderate"|"0"|0.039|"147561"
"18A"|"Brocko silt loam, 0 to 2 percent slopes"||1|1.2||||"None"|"None"|"0"|4.99|9.97|19.92|29.86|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.206|"Slight"|"0"|0|"147562"
"18C"|"Brocko silt loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.95|9.88|19.63|29.35|"Well drained"|"Well drained"|"B"|"4"|98|"4"|99|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.214|"Moderate"|"0"|0.021|"147563"
"18E"|"Brocko silt loam, 15 to 35 percent slopes"||25|25.5||||"None"|"None"|"0"|4.7|9.35|18.54|27.64|"Well drained"|"Well drained"|"B"||100|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.988|"Severe"|"0"|1|"147564"
"20C"|"Windham gravelly loam, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.01|5.48|8.32|10.36|"Well drained"|"Well drained"|"B"|"4"|97|"6"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.042|"Moderate"|"0"|0.69|"147565"
"20D"|"Windham gravelly loam, 8 to 15 percent slopes"||12|11.9||||"None"|"None"|"0"|3.03|5.5|8.36|10.44|"Well drained"|"Well drained"|"B"|"4"|94|"6"|89|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.042|"Moderate"|"0"|0.709|"147566"
"26C"|"Crago gravelly loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|2.7|4.87|7.33|9.51|"Well drained"|"Well drained"|"B"|"4"|98|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.199|"Moderate"|"0"|0.934|"147567"
"26E"|"Crago gravelly loam, 15 to 25 percent slopes"||20|20.1||||"None"|"None"|"0"|2.76|5.01|7.64|9.93|"Well drained"|"Well drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.531|"Severe"|"0"|0.982|"147568"
"27D"|"Bronec gravelly loam, 8 to 15 percent slopes"||12|11.8||||"None"|"None"|"0"|3.8|6.6|12.09|16.1|"Well drained"|"Well drained"|"B"|"4"|95|"4"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.192|"Moderate"|"0"|0.612|"147569"
"37A"|"Pieriver silt loam, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.28|8.27|15.83|22.46|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|90|"4"|88|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.226|"Slight"|"2"|0.709|"147570"
"41"|"Bronec, Amesha, and Riverrun, channeled soils, 0 to 35 percent slopes"||18|15.6||130|130|"None"|"Occasional"|"0"|2.88|5.46|10.43|14.83|"Well drained"|"Moderately well drained"|"B"||73|"6"|92|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.229|"Severe"|"3"|0.981|"147571"
"64C"|"Varney sandy clay loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.81|7.25|12.79|17.61|"Well drained"|"Well drained"|"B"|"3"|91|"3"|91|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.099|"Moderate"|"0"|0.041|"147572"
"74D"|"Shawmut gravelly loam, 4 to 15 percent slopes, bouldery"||10|10.6||||"None"|"None"|"0"|3.88|6.83|10.88|13.92|"Well drained"|"Well drained"|"B"||90|"7"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.108|"Moderate"|"0"|0.225|"147573"
"76A"|"Absay silty clay loam, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|3.3|5.68|10.25|14.8|"Well drained"|"Well drained"|"D"|"7"|90|"7"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.207|"Slight"|"0"|0.976|"147574"
"77F"|"Rock outcrop-Pensore-Crago association, 25 to 60 percent slopes, stony"|||41.4|43|||"None"|"None"|"0"|2.48|4.49|5.76|6.79|"Well drained"|"Well drained"|||100|"7"|54|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|0.983|"Severe"|"0"|1|"147575"
"80C"|"Floweree silt loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.44|8.7|17.21|25.71|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.329|"Moderate"|"0"|0.006|"147576"
"81C"|"Ethridge clay loam, 2 to 8 percent slopes"||5|5.5||||"None"|"None"|"0"|4.36|8.39|15.87|23.22|"Well drained"|"Well drained"|"C"|"3"|89|"3"|89|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.293|"Moderate"|"0"|0.953|"147577"
"83C"|"Shoddy silty clay loam, 2 to 8 percent slopes"||5|5.2|41|||"None"|"None"|"0"|4.54|7.55|8.08|8.59|"Well drained"|"Well drained"|"D"||94|"6"|94|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.317|"Moderate"|"0"|0.94|"147578"
"87C"|"Kobarter clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.35|8.51|16.19|22.8|"Well drained"|"Well drained"|"C"|"3"|96|"3"|96|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.327|"Moderate"|"0"|0.98|"147579"
"87D"|"Kobarter clay loam, 8 to 15 percent slopes"||12|11.7||||"None"|"None"|"0"|4.34|8.48|15.99|22.44|"Well drained"|"Well drained"|"C"|"4"|91|"4"|92|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.336|"Severe"|"0"|0.975|"147580"
"92D"|"Clunton, Cometcrik, and Perma, stony soils, 0 to 15 percent slopes"||2|3.2||15|15|"Frequent"|"Frequent"|"40"|4.48|8.74|16.86|21.41|"Very poorly drained"|"Very poorly drained"|"C/D"|"5"|75|"5"|75|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.567|"Slight"|"75"|0.875|"147581"
"113D"|"Amesha-Amesha, stony complex, 8 to 15 percent slopes"||12|14.3||||"None"|"None"|"0"|3.53|6.91|13.51|20.06|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.27|"Moderate"|"0"|0.665|"147582"
"114D"|"Amesha-Crago-Shoddy complex, 4 to 15 percent slopes"||10|10.1|41|||"None"|"None"|"0"|3.77|6.82|10.45|13.78|"Well drained"|"Well drained"|"B"|"4"|60|"6"|57|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.208|"Severe"|"0"|0.676|"147583"
"115C"|"Amesha gravelly loam, 2 to 8 percent slopes"||5|5.5||||"None"|"None"|"0"|3.56|7.02|13.94|20.77|"Well drained"|"Well drained"|"B"|"4"|93|"4"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.125|"Moderate"|"0"|0.041|"147584"
"115D"|"Amesha gravelly loam, 8 to 15 percent slopes"||12|12.8||||"None"|"None"|"0"|3.48|6.85|13.4|19.89|"Well drained"|"Well drained"|"B"|"4"|92|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.147|"Moderate"|"0"|0.658|"147585"
"116C"|"Amesha loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.16|8.09|15.43|22.13|"Well drained"|"Well drained"|"B"|"4"|96|"4"|97|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.112|"Moderate"|"0"|0.034|"147586"
"118C"|"Amesha cobbly loam, 2 to 8 percent slopes"||5|5.5||||"None"|"None"|"0"|3.6|7.06|13.96|20.8|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.115|"Moderate"|"0"|0.337|"147587"
"122F"|"Maiden-Lap-Windham complex, 35 to 60 percent slopes"||48|47.8|46|||"None"|"None"|"0"|2.42|4.12|5.17|5.59|"Well drained"|"Well drained"|"C"||100|"7"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147588"
"123E"|"Maiden-Rock outcrop-Lap complex, 8 to 35 percent slopes, very stony"||12|16.4|41|||"None"|"None"|"0"|2.39|3.87|4.53|4.72|"Well drained"|"Well drained"|"C"||55|"6"|52|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.612|"Moderate"|"0"|1|"147589"
"123F"|"Maiden-Rock outcrop-Lap complex, 35 to 60 percent slopes, very stony"||48|48.4|41|||"None"|"None"|"0"|2.36|3.84|4.5|4.69|"Well drained"|"Well drained"|"C"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147590"
"151D"|"Delpoint-Abor complex, 4 to 15 percent slopes"||10|8.8|64|||"None"|"None"|"0"|4.13|8.03|10.81|12.03|"Well drained"|"Well drained"|"C"|"4"|83|"4"|83|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.316|"Moderate"|"0"|0.849|"147591"
"191C"|"Cabbart-Shoddy-Amesha complex, 2 to 8 percent slopes"||5|5.3|41|||"None"|"None"|"0"|4.22|7.61|10.32|12.93|"Well drained"|"Well drained"|"D"||63|"6"|63|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.234|"Moderate"|"0"|0.667|"147592"
"191D"|"Cabbart-Shoddy-Amesha complex, 8 to 15 percent slopes"||12|11.7|41|||"None"|"None"|"0"|4.23|7.57|10.16|12.6|"Well drained"|"Well drained"|"D"||67|"6"|63|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.245|"Severe"|"0"|0.853|"147593"
"191E"|"Cabbart-Shoddy-Amesha complex, 15 to 45 percent slopes"||30|29.5|41|||"None"|"None"|"0"|3.93|7.27|9.15|10.85|"Well drained"|"Well drained"|"D"||97|"7"|66|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.943|"Severe"|"0"|0.98|"147594"
"201F"|"Windham-Rock outcrop-Lap complex, 35 to 70 percent slopes, very stony"||53|51|41|||"None"|"None"|"0"|2.44|4.35|6.17|7.44|"Well drained"|"Well drained"|"B"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147595"
"203D"|"Windham gravelly loam, 4 to 15 percent slopes, stony"||10|10.3||||"None"|"None"|"0"|3.02|5.5|8.39|10.49|"Well drained"|"Well drained"|"B"|"4"|93|"6"|91|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.058|"Moderate"|"0"|0.715|"147596"
"231A"|"Ledger-Moltoner-McKenton complex, 0 to 2 percent slopes"||1|1||15|15|"Rare"|"Rare"|"0"|2.96|5.68|10.85|15.51|"Somewhat poorly drained"|"Very poorly drained"|"D"|"6"|80|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.476|"Slight"|"44"|1|"147597"
"263F"|"Crago-Rock outcrop-Pensore complex, 25 to 60 percent slopes, stony"||43|42.1|43|||"None"|"None"|"0"|2.4|4.48|6.4|8.03|"Well drained"|"Well drained"|"B"||100|"7"|64|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147598"
"264C"|"Crago-Amesha complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.34|6.25|10.75|14.87|"Well drained"|"Well drained"|"B"|"4"|97|"4"|53|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.141|"Moderate"|"0"|0.562|"147599"
"264F"|"Crago-Amesha complex, 35 to 60 percent slopes"||48|46.1||||"None"|"None"|"0"|3.25|6.02|10.3|14.22|"Well drained"|"Well drained"|"B"||97|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.973|"Severe"|"0"|1|"147600"
"265E"|"Crago very cobbly loam, 15 to 45 percent slopes, very stony"||30|29.2||||"None"|"None"|"0"|2.51|4.76|7.47|9.86|"Well drained"|"Well drained"|"B"||100|"7"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.982|"Severe"|"0"|0.993|"147601"
"271C"|"Bronec-Amesha complex, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.86|7.01|13.06|17.89|"Well drained"|"Well drained"|"B"|"4"|91|"4"|89|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.173|"Moderate"|"0"|0.063|"147602"
"271E"|"Bronec-Amesha complex, 15 to 35 percent slopes"||25|26||||"None"|"None"|"0"|3.3|6.3|12.04|17.05|"Well drained"|"Well drained"|"B"||98|"6"|92|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.96|"Severe"|"0"|0.987|"147603"
"273D"|"Bronec-Shoddy-Amesha complex, 4 to 15 percent slopes"||10|9.8|41|||"None"|"None"|"0"|4.19|7.33|11.32|14.53|"Well drained"|"Well drained"|"B"|"4"|62|"4"|62|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.221|"Severe"|"0"|0.498|"147604"
"273E"|"Bronec-Shoddy-Amesha complex, 15 to 35 percent slopes"||25|22.9|41|||"None"|"None"|"0"|4.14|7.33|11.69|15.23|"Well drained"|"Well drained"|"B"||93|"6"|59|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.904|"Severe"|"0"|0.934|"147605"
"274C"|"Bronec complex, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|2.83|5.64|11.09|15.2|"Well drained"|"Well drained"|"B"|"4"|89|"4"|89|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.203|"Moderate"|"0"|0.246|"147606"
"275D"|"Bronec very gravelly loam, 4 to 15 percent slopes, very stony"||10|10.5||||"None"|"None"|"0"|2.79|5.54|10.98|14.84|"Well drained"|"Well drained"|"B"|"6"|90|"6"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.431|"Moderate"|"0"|0.448|"147607"
"294C"|"Sieben, stony-Sieberell, very stony complex, 2 to 15 percent slopes"||9|10||||"None"|"None"|"0"|2.99|5.09|8.25|10.72|"Well drained"|"Well drained"|"B"|"4"|86|"4"|50|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.339|"Moderate"|"0"|0.591|"147608"
"362C"|"Udecide-Varney sandy clay loams, 2 to 8 percent slopes"||5|5.8|71|||"None"|"None"|"0"|4.04|7.69|11.92|14.32|"Well drained"|"Well drained"|"C"|"3"|84|"3"|84|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.113|"Moderate"|"0"|0.367|"147609"
"371A"|"Havre-Ryell-Handke complex, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|3.88|7.37|13.16|18.82|"Well drained"|"Somewhat poorly drained"|"C"|"4"|65|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.054|"Slight"|"0"|0.77|"147610"
"422F"|"Perma-Whitlash-Rock outcrop complex, 15 to 45 percent slopes, very stony, moist"||30|31.1|28|||"None"|"None"|"0"|2.86|4.5|6.98|8.24|"Somewhat excessively drained"|"Well drained"|"B"||93|"6"|43|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.963|"Severe"|"0"|0.979|"147611"
"423C"|"Wimper loam, 2 to 8 percent slopes"||5|5.3||||"None"|"None"|"0"|3.87|6.35|10.43|14.48|"Well drained"|"Well drained"|"B"|"4"|99|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.038|"Moderate"|"0"|0.036|"147612"
"482A"|"Riverrun-Cardwell complex, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|3.32|5.64|8.7|10.69|"Moderately well drained"|"Somewhat poorly drained"|"C"|"6"|55|"6"|57|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.131|"Slight"|"2"|0.981|"147613"
"492D"|"Roto-Pensore-Crago complex, 4 to 15 percent slopes"||10|11.6|48|||"None"|"None"|"0"|2.45|4.46|6.06|6.63|"Well drained"|"Well drained"|"C"|"4"|55|"6"|64|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.256|"Moderate"|"0"|0.974|"147614"
"492F"|"Roto-Pensore-Crago complex, 35 to 60 percent slopes, stony"||48|44.7|43|||"None"|"None"|"0"|2.31|4.31|5.9|6.49|"Well drained"|"Well drained"|"C"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147615"
"532C"|"Sappington-Amesha complex, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.92|7.65|14.8|21.59|"Well drained"|"Well drained"|"B"|"3"|55|"3"|55|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.161|"Moderate"|"0"|0.035|"147616"
"533A"|"Sappington clay loam, 0 to 2 percent slopes"||1|1.6||||"None"|"None"|"0"|3.69|7.18|13.81|20.2|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Slight"|"0"|0.037|"147617"
"533C"|"Sappington clay loam, 2 to 8 percent slopes"||5|5.5||||"None"|"None"|"0"|3.69|7.18|13.81|20.2|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Moderate"|"0"|0.042|"147618"
"631D"|"Rencot-Rock outcrop-Rencot, stony complex, 8 to 25 percent slopes"||17|16.1|48|||"None"|"None"|"0"|2.63|4.81|5.3|5.6|"Well drained"|"Well drained"|"D"||90|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.201|"Severe"|"0"|0.957|"147619"
"631E"|"Rencot-Rencot, very stony-Rock outcrop complex, 25 to 60 percent slopes"||43|41.2|48|||"None"|"None"|"0"|2.44|4.57|5.13|5.47|"Well drained"|"Well drained"|"D"||100|"7"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147620"
"631F"|"Rencot-Bronec-Rock outcrop complex, 35 to 70 percent slopes"||53|50.5|48|||"None"|"None"|"0"|2.53|4.82|6.59|7.84|"Well drained"|"Well drained"|"D"||100|"7"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147621"
"642D"|"Varney clay loam, 8 to 15 percent slopes"||12|10.9||||"None"|"None"|"0"|3.99|7.5|13.17|18.06|"Well drained"|"Well drained"|"B"|"4"|88|"4"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.149|"Moderate"|"0"|0.624|"147622"
"643C"|"Varney cobbly loam, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.63|6.81|12.29|17.16|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.196|"Moderate"|"0"|0.025|"147623"
"662B"|"Judell gravelly loam, 1 to 4 percent slopes, very stony"||3|3.4||||"None"|"None"|"0"|3.69|7.55|15.13|22.65|"Well drained"|"Well drained"|"B"|"6"|90|"6"|97|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.394|"Slight"|"0"|0.447|"147624"
"734D"|"Martinsdale loam, 4 to 15 percent slopes, very stony"||10|10.2||||"None"|"None"|"0"|4.09|7.83|14.54|19.78|"Well drained"|"Well drained"|"C"|"6"|85|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.397|"Severe"|"0"|0.507|"147625"
"851D"|"Walbert-Shoddy-Cabbart complex, 2 to 15 percent slopes"||9|9.1|41|||"None"|"None"|"0"|3.5|6.06|7.1|7.89|"Well drained"|"Well drained"|"D"||80|"6"|80|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.166|"Severe"|"0"|0.877|"147626"
"971F"|"Cowood, rubbly-Rock outcrop association, 25 to 60 percent slopes"||43|43|48|||"None"|"None"|"0"|1.67|2.92|3.37|3.75|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147627"
"1120E"|"Quaint channery loam, 8 to 35 percent slopes, very stony"||22|21.1|36|||"None"|"None"|"0"|3.05|4.23|4.37|4.37|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||93|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.765|"Severe"|"0"|1|"147628"
"1121E"|"Quaint-Rock outcrop-Redfist complex, 4 to 25 percent slopes"||15|13|36|||"None"|"None"|"0"|3.19|4.87|6.05|6.53|"Somewhat excessively drained"|"Well drained"|"D"||71|"7"|43|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.12|"Moderate"|"0"|0.972|"147629"
"1121F"|"Quaint-Rock outcrop complex, 15 to 45 percent slopes"||30|24.4|36|||"None"|"None"|"0"|3.06|4.42|4.89|4.89|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||86|"7"|44|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.784|"Severe"|"0"|0.999|"147630"
"1131C"|"Redfist-Quaint channery loams, 2 to 8 percent slopes"||5|5.2|36|||"None"|"None"|"0"|3.23|5.12|6.58|6.8|"Well drained"|"Well drained"|"C"|"4"|58|"4"|50|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.072|"Moderate"|"0"|0.978|"147631"
"1132D"|"Redfist-Perma-Rock outcrop complex, 2 to 35 percent slopes, bouldery"||19|19|74|||"None"|"None"|"0"|3.16|5.22|7.69|8.49|"Well drained"|"Well drained"|"C"||94|"7"|79|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.411|"Severe"|"0"|0.984|"147632"
"1142E"|"Devilfence-Rock outcrop-Wilspring complex, 8 to 35 percent slopes"||22|20.2|36|||"None"|"None"|"0"|2.57|3.77|4.49|4.78|"Somewhat excessively drained"|"Well drained"|"D"||91|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.727|"Severe"|"0"|0.955|"147633"
"1142F"|"Devilfence-Rock outcrop complex, 35 to 60 percent slopes"||48|39.5|36|||"None"|"None"|"0"|2.57|3.7|4.26|4.34|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||91|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.852|"Severe"|"0"|1|"147634"
"1741F"|"Tropal-Rock outcrop-Whitore complex, 15 to 45 percent slopes, bouldery"||30|32.1|41|||"None"|"None"|"0"|2|3.47|5.16|6.29|"Well drained"|"Well drained"|"D"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.986|"Severe"|"0"|1|"147635"
"1790F"|"Sigbird, very bouldery-Sigbird, stony-Rock outcrop complex, 25 to 70 percent slopes"||53|44.2|36|||"None"|"None"|"0"|2.49|3.62|3.9|4.05|"Somewhat excessively drained"|"Somewhat excessively drained"|"D"||100|"7"|76|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.991|"Severe"|"0"|1|"147636"
"3033B"|"Sappington-Amesha loams, 1 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|4.01|7.69|14.6|21.22|"Well drained"|"Well drained"|"B"|"3"|63|"3"|63|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.151|"Slight"|"0"|0|"147637"
"2"|"Rubble land-Rock outcrop association"|||40||||||"0"|2.3|4.16|5.65|6.87|||||100||75|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"147638"
"1E"|"Gnojek, dry-Wickes-Gnojek, moist complex, 15 to 45 percent slopes"||30|29.5|41|||"None"|"None"|"0"|2.31|3.83|4.69|5.04|"Well drained"|"Well drained"|"D"||98|"7"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.98|"Severe"|"0"|1|"147639"
"2F"|"Pensore, very stony-Rock outcrop-Crago, stony complex, 15 to 60 percent slopes"||35|32.9|41|||"None"|"None"|"0"|2.28|3.8|4.95|5.66|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147640"
"3F"|"Lap, very stony-Rock outcrop-Windham, stony complex, 15 to 60 percent slopes"||45|39.6|41|||"None"|"None"|"0"|2.54|4.21|5.97|7.69|"Well drained"|"Well drained"|"D"||100|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147641"
"4D"|"Crago gravelly loam, stony, 4 to 15 percent slopes"||10|10.1||||"None"|"None"|"0"|2|3.39|5.82|7.37|"Well drained"|"Well drained"|"B"|"4"|90|"6"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.242|"Moderate"|"0"|0.95|"147642"
"5F"|"Whitecow, stony-Lap, very stony-Rock outcrop complex, 15 to 60 percent slopes"||48|46|41|||"None"|"None"|"0"|2.34|4.31|7.26|10.2|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147643"
"6E"|"Gnojek, stony-Gnojek, very stony-Wickes, stony complex, 15 to 45 percent slopes"||30|29.3|41|||"None"|"None"|"0"|2.21|3.65|4.42|4.42|"Well drained"|"Well drained"|"D"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.982|"Severe"|"0"|1|"147644"
"7D"|"Circleville family-Gnojek, stony complex, 4 to 15 percent slopes"||6|8.6|41|||"None"|"None"|"0"|3.16|4.36|5.66|5.66|"Well drained"|"Well drained"|"C"||100|"7"|95|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.249|"Moderate"|"0"|1|"147645"
"8D"|"Crago, stony-Musselshell complex, 8 to 15 percent slopes"||12|13.3||||"None"|"None"|"0"|2.44|4.52|8.16|10.41|"Well drained"|"Well drained"|"B"|"4"|98|"6"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.3|"Moderate"|"0"|0.89|"147646"
"10D"|"Rootel-Skein-Whitesage complex, 4 to 15 percent slopes"||10|10.7|36|||"None"|"None"|"0"|3.72|6.8|9.76|11.1|"Well drained"|"Well drained"|"C"||80|"6"|47|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.249|"Severe"|"0"|0.682|"147647"
"11E"|"Skein-Rootel complex, 8 to 25 percent slopes"||17|16.8|36|||"None"|"None"|"0"|3.54|5.86|7.18|7.45|"Well drained"|"Well drained"|"D"||96|"7"|62|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.226|"Severe"|"0"|0.985|"147648"
"12E"|"Gnojek-Duffson complex, 15 to 45 percent slopes"||30|27.9|41|||"None"|"None"|"0"|2.6|4.64|6.12|6.81|"Well drained"|"Well drained"|"D"||89|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.906|"Severe"|"0"|1|"147649"
"13D"|"Gnojek-Duffson complex, 4 to 15 percent slopes"||12|11.8|41|||"None"|"None"|"0"|2.52|4.46|5.72|6.17|"Well drained"|"Well drained"|"D"||95|"7"|90|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.25|"Moderate"|"0"|0.947|"147650"
"14E"|"Rencot-Rock outcrop-Birney complex, very stony, 15 to 45 percent slopes"||30|30|46|||"None"|"None"|"0"|2.71|4.51|5.54|6.34|"Well drained"|"Well drained"|"D"||80|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147651"
"15E"|"Rencot-Rootel complex, 15 to 45 percent slopes"||30|29.5|46|||"None"|"None"|"0"|2.48|4.7|5.48|5.7|"Well drained"|"Well drained"|"D"||97|"7"|72|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.974|"Severe"|"0"|1|"147652"
"16C"|"Varney loam, 2 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|3.65|7.05|13.27|19.39|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.244|"Moderate"|"0"|0.023|"147653"
"23B"|"Patouza clay, 0 to 6 percent slopes"||3|3.1||||"None"|"None"|"0"|4.11|8.26|15.81|23.16|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.469|"Slight"|"0"|0.9|"147654"
"32C"|"Amesha loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.31|8.29|15.43|22.11|"Well drained"|"Well drained"|"B"|"4"|97|"4"|97|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.146|"Moderate"|"0"|0.027|"147655"
"32D"|"Amesha loam, 8 to 15 percent slopes"||12|12.6||||"None"|"None"|"0"|4.3|8.23|15.27|21.92|"Well drained"|"Well drained"|"B"||90|"4"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Severe"|"0"|0.62|"147656"
"32E"|"Amesha-Trimad complex, 15 to 45 percent slopes"||30|28.6||||"None"|"None"|"0"|4.08|7.87|14.32|20.69|"Well drained"|"Well drained"|"B"||98|"7"|93|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.937|"Severe"|"0"|0.986|"147657"
"35D"|"Kalsted sandy loam, 8 to 15 percent slopes"||12|12.7||||"None"|"None"|"0"|3.04|6.07|10.69|15.09|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"|"4"|95|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.124|"Moderate"|"0"|0.651|"147658"
"42B"|"Trimad loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.51|6.16|9.27|12.24|"Well drained"|"Well drained"|"B"|"3"|90|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.176|"Slight"|"0"|0.287|"147659"
"52E"|"Martinsdale loam, 15 to 35 percent slopes"||25|25.9||||"None"|"None"|"0"|4.49|8.47|14.74|20.34|"Well drained"|"Well drained"|"C"||93|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"147660"
"71D"|"Quigley loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.76|6.99|13.37|19.72|"Well drained"|"Well drained"|"B"|"4"|95|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.046|"Severe"|"0"|0.633|"147661"
"83D"|"Shoddy silty clay loam, 8 to 15 percent slopes"||12|11.6|41|||"None"|"None"|"0"|4.48|7.45|8.15|8.8|"Well drained"|"Well drained"|"D"||90|"6"|92|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.319|"Severe"|"0"|0.96|"147662"
"91F"|"Whitore gravelly loam, 35 to 60 percent slopes, stony"||48|48.9||||"None"|"None"|"0"|3.86|6.45|9.91|13.23|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147663"
"113C"|"Amesha-Amesha, stony complex, 2 to 8 percent slopes"||5|5.7||||"None"|"None"|"0"|3.59|7.04|13.94|20.73|"Well drained"|"Well drained"|"B"|"4"|94|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.146|"Moderate"|"0"|0.249|"147664"
"163C"|"Beanlake gravelly loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.46|6.85|13.6|20.35|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.072|"Moderate"|"0"|0.05|"147665"
"301A"|"Rivra-Ryell-Bonebasin complex, 0 to 2 percent slopes"||1|1.1||122|122|"Rare"|"Rare"|"0"|4.09|6.29|9.25|10.85|"Well drained"|"Well drained"|"A"|"6"|50|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Not limited"|0.138|"Slight"|"15"|1|"147666"
"366E"|"Windham cobbly loam, 15 to 35 percent slopes, stony"||25|26.2||||"None"|"None"|"0"|2.85|4.1|6.1|8.1|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"147667"
"425E"|"Musselshell-Pensore, stony complex, 15 to 35 percent slopes"||25|26.2|41|||"None"|"None"|"0"|3.45|6.17|10.19|12.6|"Well drained"|"Well drained"|"B"||100|"6"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147668"
"466E"|"Windham cobbly loam, 15 to 45 percent slopes, stony"||30|31.1||||"None"|"None"|"0"|2.78|4.01|5.85|7.69|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147669"
"512D"|"Enbar-Bowery-Nythar complex, 4 to 15 percent slopes"||6|6.4||15|15|"Rare"|"Rare"|"0"|4.74|9.44|17.59|24.2|"Somewhat poorly drained"|"Very poorly drained"|"C"|"3"|65|"3"|65|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.207|"Moderate"|"20"|0.605|"147670"
"614D"|"Adel loam, cool, 4 to 15 percent slopes"||10|10.2||||"None"|"None"|"0"|4.63|9.08|17.89|26.69|"Well drained"|"Well drained"|"B"||95|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Not limited"|0.026|"Severe"|"5"|0.27|"147671"
"701A"|"Rivra-Mccabe-Bonebasin complex, 0 to 2 percent slopes"||1|1||46|46|"Occasional"|"Occasional"|"0"|4.2|6.5|8.54|10.17|"Well drained"|"Poorly drained"|"C"||70|"6"|48|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Not limited"|0.287|"Slight"|"49"|1|"147672"
"710E"|"Cabbart-Amesha-Trimad complex, 15 to 45 percent slopes"||30|30|48|||"None"|"None"|"0"|3.91|7.56|9.95|12.26|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147673"
"752B"|"Sixbeacon-Vendome complex, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.15|4.93|7.1|9.09|"Well drained"|"Well drained"|"B"|"3"|45|"4"|60|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.095|"Slight"|"0"|0.921|"147674"
"774F"|"Rock outcrop-Whitlash, bouldery association, 35 to 70 percent slopes"|||46.1|28||||"None"|"0"|2.58|3.84|5.46|6.36|"Well drained"|"Well drained"|||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147675"
"786F"|"Whitecow, stony-Lap, very stony-Rock outcrop complex, 35 to 60 percent slopes"||48|48|41|||"None"|"None"|"0"|3.56|5.64|8.86|11.75|"Well drained"|"Well drained"|"B"||100|"7"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147676"
"811E"|"Blacksheep, moist-Kalsted-Scravo complex, 15 to 45 percent slopes"||30|30|41|||"None"|"None"|"0"|2.7|4.71|6|7.26|"Well drained"|"Well drained"|"D"||100|"6"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147677"
"816E"|"Pensore-Rock outcrop complex, 15 to 45 percent slopes"||30|32|41|||"None"|"None"|"0"|2.64|4|4.22|4.37|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147678"
"816G"|"Pensore-Rock outcrop complex, 45 to 70 percent slopes"||58|58|41|||"None"|"None"|"0"|2.32|3.72|3.94|4.15|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"147679"
"GP"|"Gravel pit"|||||||||"0"|||||||||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"147680"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"147681"
