09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delphill soil is a minor component."|"21148251"|"21356374"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21148252"|"21356375"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blanyon soil is a minor component."|"21148253"|"21356376"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 80 percent of the map unit. Slopes are 3 to 9 percent. This component is on low hills. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC446MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21148254"|"21356377"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"21147948"|"21356071"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Aeric Fluvaquents component makes up 75 percent of the map unit. Slopes are 0 to 5 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 39 inches during March, April, May, June, July, August, September. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147949"|"21356072"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21148255"|"21356378"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148256"|"21356379"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148257"|"21356380"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21148258"|"21356381"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21147950"|"21356073"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21147951"|"21356074"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 80 percent of the map unit. Slopes are 4 to 9 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147952"|"21356075"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147953"|"21356076"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 70 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147746"|"21355869"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21147747"|"21355870"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147748"|"21355871"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147749"|"21355872"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21147750"|"21355873"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21147751"|"21355874"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 90 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147752"|"21355875"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 60 percent of the map unit. Slopes are 4 to 9 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147753"|"21355876"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147754"|"21355877"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21147755"|"21355878"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147756"|"21355879"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 40 percent of the map unit. Slopes are 10 to 25 percent.   Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147757"|"21355880"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21147758"|"21355881"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 10 to 25 percent.  The parent material consists of residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC469MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147759"|"21355882"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21147760"|"21355883"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blaine soil is a minor component."|"21147761"|"21355884"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21147954"|"21356077"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delphill soil is a minor component."|"21147955"|"21356078"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147956"|"21356079"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blanyon component makes up 75 percent of the map unit. Slopes are 3 to 10 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044XC446MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21147957"|"21356080"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Borohemists component makes up 100 percent of the map unit. Slopes are 0 to 2 percent. This component is on depressions. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 40 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148259"|"21356382"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 70 percent of the map unit. Slopes are 5 to 15 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147958"|"21356081"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21147959"|"21356082"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset soil is a minor component."|"21147960"|"21356083"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 80 percent of the map unit. Slopes are 5 to 15 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148260"|"21356383"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21148261"|"21356384"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21148493"|"21356616"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21148494"|"21356617"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148495"|"21356618"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 75 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of silty loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148496"|"21356619"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148497"|"21356620"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148498"|"21356621"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 85 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of silty loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148499"|"21356622"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148500"|"21356623"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148501"|"21356624"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148502"|"21356625"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 80 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of silty loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148503"|"21356626"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148504"|"21356627"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Small areas with surface stone soil is a minor component."|"21148505"|"21356628"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148506"|"21356629"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148507"|"21356630"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148508"|"21356631"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 70 percent of the map unit. Slopes are 9 to 25 percent.  The parent material consists of silty loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148509"|"21356632"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21148510"|"21356633"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 75 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of silty loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148511"|"21356634"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 25 percent of the map unit. Slopes are 9 to 35 percent.  The parent material consists of soft residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC452MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21147961"|"21356084"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21147962"|"21356085"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21147963"|"21356086"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21147964"|"21356087"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147965"|"21356088"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21147966"|"21356089"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delphill soil is a minor component."|"21147967"|"21356090"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 25 percent of the map unit. Slopes are 9 to 35 percent.  The parent material consists of soft residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC452MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21147968"|"21356091"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 65 percent of the map unit. Slopes are 9 to 35 percent.  The parent material consists of residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 8 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC469MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148262"|"21356385"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148263"|"21356386"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blaine soil is a minor component."|"21148264"|"21356387"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21148265"|"21356388"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Assinniboine soil is a minor component."|"21147969"|"21356092"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147970"|"21356093"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 80 percent of the map unit. Slopes are 1 to 4 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147971"|"21356094"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148266"|"21356389"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 95 percent of the map unit. Slopes are 4 to 9 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148267"|"21356390"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147762"|"21355885"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21147763"|"21355886"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 70 percent of the map unit. Slopes are 1 to 4 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147764"|"21355887"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147765"|"21355888"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147766"|"21355889"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Assinniboine soil is a minor component."|"21147767"|"21355890"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 50 percent of the map unit. Slopes are 1 to 9 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC450MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147768"|"21355891"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 40 percent of the map unit. Slopes are 1 to 9 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC450MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147769"|"21355892"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147770"|"21355893"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 35 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147771"|"21355894"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147772"|"21355895"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook, cobbly component makes up 20 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147773"|"21355896"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 20 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147774"|"21355897"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147775"|"21355898"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21147776"|"21355899"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chinook component makes up 40 percent of the map unit. Slopes are 9 to 35 percent.  The parent material consists of alluvium and/or loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC451MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147777"|"21355900"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 40 percent of the map unit. Slopes are 9 to 35 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147778"|"21355901"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148268"|"21356391"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 30 percent of the map unit. Slopes are 4 to 9 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148269"|"21356392"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148270"|"21356393"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 25 percent of the map unit. Slopes are 4 to 9 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148271"|"21356394"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148272"|"21356395"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21147972"|"21356095"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delphill component makes up 80 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of soft siltstone and/or soft clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147973"|"21356096"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21147974"|"21356097"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delphill component makes up 40 percent of the map unit. Slopes are 5 to 20 percent.  The parent material consists of soft siltstone and/or soft clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148273"|"21356396"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toston soil is a minor component."|"21148274"|"21356397"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148275"|"21356398"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148276"|"21356399"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 30 percent of the map unit. Slopes are 5 to 20 percent. This component is on low hills. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC446MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21148277"|"21356400"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dominic component makes up 30 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 66 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC454MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"21147975"|"21356098"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dominic component makes up 20 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 66 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC454MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"21147976"|"21356099"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairdale soil is a minor component."|"21147977"|"21356100"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dominic component makes up 30 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 66 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC454MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"21147978"|"21356101"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"21147979"|"21356102"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 40 percent of the map unit. Slopes are 35 to 60 percent.  The parent material consists of residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC469MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148512"|"21356635"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148513"|"21356636"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ess component makes up 50 percent of the map unit. Slopes are 35 to 60 percent.  The parent material consists of cobbly and stony alluvium and/or cobbly and stony colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC474MT Silty-stony (sist) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21148514"|"21356637"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villy soil is a minor component."|"21148515"|"21356638"
09/16/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21148516"|"21356639"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairdale component makes up 80 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148517"|"21356640"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villy soil is a minor component."|"21148518"|"21356641"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lothair component makes up 39 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during June, July, August, September. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148519"|"21356642"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairdale component makes up 41 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148520"|"21356643"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"21148521"|"21356644"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquentic haplaqu component makes up 100 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21148522"|"21356645"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21147980"|"21356103"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21147981"|"21356104"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147982"|"21356105"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 70 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of Loamy Alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2c. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147983"|"21356106"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"21147984"|"21356107"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hilger component makes up 80 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of calcareous gravelly and cobbly colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC474MT Silty-stony (sist) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148278"|"21356401"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148279"|"21356402"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148280"|"21356403"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148281"|"21356404"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake creek component makes up 80 percent of the map unit. Slopes are 20 to 50 percent.  The parent material consists of residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21147985"|"21356108"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21147986"|"21356109"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nielsen soil is a minor component."|"21147987"|"21356110"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 80 percent of the map unit. Slopes are 10 to 35 percent.  The parent material consists of alluvium derived from igneous and sedimentary rock and/or colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21148282"|"21356405"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset soil is a minor component."|"21148283"|"21356406"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lake creek soil is a minor component."|"21148284"|"21356407"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21148285"|"21356408"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lothair component makes up 80 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC446MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147988"|"21356111"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147989"|"21356112"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 80 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147779"|"21355902"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21147780"|"21355903"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"21147781"|"21355904"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 80 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147782"|"21355905"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"21147783"|"21355906"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"21147784"|"21355907"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21147785"|"21355908"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 80 percent of the map unit. Slopes are 2 to 9 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147786"|"21355909"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"21147787"|"21355910"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21147788"|"21355911"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dumps is a miscellaneous area."|"21147789"|"21355912"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147990"|"21356113"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussel component makes up 80 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147991"|"21356114"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21147992"|"21356115"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147993"|"21356116"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21147994"|"21356117"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21148286"|"21356409"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussel component makes up 80 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148287"|"21356410"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148288"|"21356411"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148289"|"21356412"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 25 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147995"|"21356118"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147996"|"21356119"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussel component makes up 60 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147997"|"21356120"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147998"|"21356121"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147999"|"21356122"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148290"|"21356413"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148291"|"21356414"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148292"|"21356415"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148293"|"21356416"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussel component makes up 50 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148294"|"21356417"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 30 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148295"|"21356418"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mussel component makes up 40 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148523"|"21356646"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148524"|"21356647"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 40 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148525"|"21356648"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148526"|"21356649"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148527"|"21356650"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148528"|"21356651"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 70 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148529"|"21356652"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 70 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148530"|"21356653"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148531"|"21356654"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148532"|"21356655"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148533"|"21356656"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148534"|"21356657"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21148535"|"21356658"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 40 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (Ly)   LRU 44B-A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148536"|"21356659"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 50 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148537"|"21356660"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148296"|"21356419"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148297"|"21356420"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148298"|"21356421"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 30 percent of the map unit. Slopes are 8 to 20 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148299"|"21356422"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 55 percent of the map unit. Slopes are 8 to 20 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148300"|"21356423"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148000"|"21356123"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 30 percent of the map unit. Slopes are 3 to 8 percent.  The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148001"|"21356124"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 60 percent of the map unit. Slopes are 3 to 8 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148002"|"21356125"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"21148301"|"21356424"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"21148302"|"21356425"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nielsen component makes up 75 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of loamy shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP810MT Shallow Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148303"|"21356426"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Passcreek soil is a minor component."|"21148304"|"21356427"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"21148003"|"21356126"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ess soil is a minor component."|"21148004"|"21356127"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nielsen soil is a minor component."|"21148005"|"21356128"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Passcreek component makes up 75 percent of the map unit. Slopes are 6 to 15 percent.  The parent material consists of loamy shale and/or loamy argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148006"|"21356129"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lake Creek component makes up 40 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21147790"|"21355913"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nielsen soil is a minor component."|"21147791"|"21355914"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Passcreek component makes up 41 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of loamy shale and/or loamy argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147792"|"21355915"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21147793"|"21355916"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 75 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC474MT Silty-stony (sist) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21147794"|"21355917"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21147795"|"21355918"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"21147796"|"21355919"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21147797"|"21355920"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 70 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during March, April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.   "|"21147798"|"21355921"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"21147799"|"21355922"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"21147800"|"21355923"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mussel soil is a minor component."|"21147801"|"21355924"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147802"|"21355925"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147803"|"21355926"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Radersburg component makes up 70 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of gravelly and cobbly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC458MT Silty-stony (sist) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147804"|"21355927"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21147805"|"21355928"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148007"|"21356130"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolman soil is a minor component."|"21148008"|"21356131"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21148009"|"21356132"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 60 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of calcareous loamy residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC452MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148010"|"21356133"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"21148011"|"21356134"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21148305"|"21356428"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villy soil is a minor component."|"21148306"|"21356429"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra component makes up 70 percent of the map unit. Slopes are 0 to 5 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XC448MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21148307"|"21356430"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21148308"|"21356431"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"21148309"|"21356432"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 80 percent of the map unit. Slopes are 9 to 35 percent.  The parent material consists of calcareous clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC474MT Silty-stony (sist) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148012"|"21356135"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21148013"|"21356136"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148310"|"21356433"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rootel component makes up 70 percent of the map unit. Slopes are 3 to 9 percent.  The parent material consists of calcareous residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21148311"|"21356434"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148312"|"21356435"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"21148313"|"21356436"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148014"|"21356137"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148015"|"21356138"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 80 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148016"|"21356139"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148017"|"21356140"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 80 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of calcareous loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148538"|"21356661"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148539"|"21356662"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148540"|"21356663"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148541"|"21356664"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148542"|"21356665"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 80 percent of the map unit. Slopes are 2 to 5 percent.  The parent material consists of calcareous loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"21148543"|"21356666"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148544"|"21356667"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148545"|"21356668"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 80 percent of the map unit. Slopes are 5 to 9 percent.  The parent material consists of calcareous loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC455MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"21148546"|"21356669"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148547"|"21356670"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148548"|"21356671"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148549"|"21356672"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 65 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC454MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148550"|"21356673"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148551"|"21356674"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148552"|"21356675"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148553"|"21356676"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 75 percent of the map unit. Slopes are 0 to 5 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC454MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148018"|"21356141"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21148019"|"21356142"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21148020"|"21356143"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toston soil is a minor component."|"21148314"|"21356437"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lothair soil is a minor component."|"21148315"|"21356438"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21148316"|"21356439"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148317"|"21356440"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 80 percent of the map unit. Slopes are 1 to 3 percent.  The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148318"|"21356441"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 30 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC454MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148021"|"21356144"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thess component makes up 60 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XC457MT Silty-limy (sily) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148022"|"21356145"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21148023"|"21356146"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148319"|"21356442"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21148320"|"21356443"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"21148321"|"21356444"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 70 percent of the map unit. Slopes are 10 to 35 percent.  The parent material consists of calcareous loamy residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA136MT Shallow Loamy (SwLo)   LRU 44B-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148322"|"21356445"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147806"|"21355929"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thess soil is a minor component."|"21147807"|"21355930"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villy soil is a minor component."|"21147808"|"21355931"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Toston component makes up 70 percent of the map unit. Slopes are 0 to 5 percent.  The parent material consists of strongly alkaline alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 54 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21147809"|"21355932"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairdale soil is a minor component."|"21147810"|"21355933"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal soil is a minor component."|"21147811"|"21355934"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21147812"|"21355935"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21147813"|"21355936"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal component makes up 55 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of calcareous gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147814"|"21355937"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"21147815"|"21355938"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustic Torrifluvents component makes up 100 percent of the map unit. Slopes are 1 to 3 percent.   Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XC448MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147816"|"21355939"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gravelly loamy sand surface soil is a minor component."|"21147817"|"21355940"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustic Torriorthents component makes up 95 percent of the map unit. Slopes are 0 to 5 percent.   Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 45 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21147818"|"21355941"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Very poorly drained soils soil is a minor component."|"21148323"|"21356446"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Villy component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during April, May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148324"|"21356447"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Villy component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 39 inches during April, May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148024"|"21356147"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villy soil is a minor component."|"21148025"|"21356148"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore component makes up 80 percent of the map unit. Slopes are 25 to 60 percent.   Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148325"|"21356448"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148326"|"21356449"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal soil is a minor component."|"21148327"|"21356450"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148026"|"21356149"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 60 percent of the map unit. Slopes are 9 to 35 percent.   Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XC471MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"21148027"|"21356150"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21148028"|"21356151"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148029"|"21356152"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21148030"|"21356153"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 30 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21148554"|"21356677"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148555"|"21356678"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodrock component makes up 60 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of loamy residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148556"|"21356679"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148557"|"21356680"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodrock component makes up 65 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of loamy residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21148558"|"21356681"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"21148559"|"21356682"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset soil is a minor component."|"21148560"|"21356683"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148184"|"21356307"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148185"|"21356308"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"21148186"|"21356309"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 20 percent of the map unit. Slopes are 1 to 8 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148187"|"21356310"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, cobbly soil is a minor component."|"21148188"|"21356311"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clunton component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps. The parent material consists of fine-loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is rarely ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21148189"|"21356312"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 35 percent of the map unit. Slopes are 1 to 8 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148190"|"21356313"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"21148191"|"21356314"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"21148192"|"21356315"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147678"|"21355801"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147679"|"21355802"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21147680"|"21355803"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147681"|"21355804"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, greater slope soil is a minor component."|"21147682"|"21355805"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21147683"|"21355806"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21147892"|"21356015"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147893"|"21356016"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147894"|"21356017"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, greater slope soil is a minor component."|"21147895"|"21356018"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21147896"|"21356019"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cozberg soil is a minor component."|"21148193"|"21356316"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148194"|"21356317"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21148195"|"21356318"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"21148196"|"21356319"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Anamac component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, hillsides, terraces. The parent material consists of calcareous fine-loamy alluvium or tertiary valley fill. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148197"|"21356320"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anamac, greater slope soil is a minor component."|"21148198"|"21356321"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, stony soil is a minor component."|"21147897"|"21356020"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147898"|"21356021"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21147899"|"21356022"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"21147900"|"21356023"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anamac, cobbly soil is a minor component."|"21147901"|"21356024"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Anamac component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, hillsides, terraces. The parent material consists of calcareous fine-loamy alluvium or tertiary valley fill. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147902"|"21356025"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on ridges, hillsides, alluvial fans. The parent material consists of coarse-silty calcareous loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148439"|"21356562"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko, greater slope soil is a minor component."|"21148440"|"21356563"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148441"|"21356564"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 95 percent of the map unit. Slopes are 2 to 8 percent. This component is on ridges, hillsides, alluvial fans. The parent material consists of coarse-silty calcareous loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148442"|"21356565"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148443"|"21356566"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148444"|"21356567"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko, greater slope soil is a minor component."|"21148445"|"21356568"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21148446"|"21356569"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Brocko component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on ridges, hillsides, alluvial fans. The parent material consists of coarse-silty calcareous loess. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA040MT Loamy Steep (lostp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148447"|"21356570"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zbart soil is a minor component."|"21148448"|"21356571"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, volcanic, sandstone soil is a minor component."|"21148449"|"21356572"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148450"|"21356573"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148451"|"21356574"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148452"|"21356575"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"21148453"|"21356576"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden soil is a minor component."|"21148454"|"21356577"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap soil is a minor component."|"21148455"|"21356578"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148456"|"21356579"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell soil is a minor component."|"21148457"|"21356580"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21147903"|"21356026"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper soil is a minor component."|"21147904"|"21356027"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap soil is a minor component."|"21147905"|"21356028"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Limy Sagebrush Shrubland, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147906"|"21356029"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden soil is a minor component."|"21147907"|"21356030"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell soil is a minor component."|"21147908"|"21356031"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148199"|"21356322"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, escarpments, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148200"|"21356323"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148201"|"21356324"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148202"|"21356325"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148203"|"21356326"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21148204"|"21356327"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148205"|"21356328"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148206"|"21356329"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148207"|"21356330"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148208"|"21356331"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 85 percent of the map unit. Slopes are 15 to 25 percent. This component is on escarpments, hillsides, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148209"|"21356332"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148210"|"21356333"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"21148458"|"21356581"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148459"|"21356582"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148460"|"21356583"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148461"|"21356584"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148462"|"21356585"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nestley soil is a minor component."|"21147684"|"21355807"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Handke soil is a minor component."|"21147685"|"21355808"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairway soil is a minor component."|"21147686"|"21355809"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pieriver component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood plains, flood-plain steps. The parent material consists of fine-loamy recent alluvium from mixed rock sources. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21147687"|"21355810"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"21147688"|"21355811"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cardwell soil is a minor component."|"21147689"|"21355812"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverrun soil is a minor component."|"21147690"|"21355813"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, flood-plain steps, drainageways. The parent material consists of sandy and gravelly recent alluvium from mixed igneous, sedimentary and metamorphic rocks. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA060MT Overflow (ov)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21148211"|"21356334"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, cobbly soil is a minor component."|"21148212"|"21356335"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 29 percent of the map unit. Slopes are 1 to 35 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148213"|"21356336"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 31 percent of the map unit. Slopes are 1 to 35 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148214"|"21356337"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148215"|"21356338"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148216"|"21356339"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"21148217"|"21356340"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148218"|"21356341"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21147909"|"21356032"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sieben, stony soil is a minor component."|"21147910"|"21356033"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21147911"|"21356034"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces, knolls, hillsides, alluvial fans. The parent material consists of fine-loamy slope alluvium from semiconsolidated sandstone, siltstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147912"|"21356035"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raghorn soil is a minor component."|"21147913"|"21356036"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anamac soil is a minor component."|"21147914"|"21356037"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut, bouldery component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, escarpments, hillsides. The parent material consists of gravelly colluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent.  "|"21148219"|"21356342"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wickes, stony soil is a minor component."|"21148220"|"21356343"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, very stony soil is a minor component."|"21148221"|"21356344"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper soil is a minor component."|"21148222"|"21356345"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absay component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of saline, sodic, clayey alluvium derived from shale-siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 27 within 30 inches of the soil surface."|"21147691"|"21355814"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147692"|"21355815"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21147693"|"21355816"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatony soil is a minor component."|"21147694"|"21355817"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trudau soil is a minor component."|"21147695"|"21355818"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21147696"|"21355819"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147697"|"21355820"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, lesser slope soil is a minor component."|"21147698"|"21355821"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore, stony component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillsides, escarpments, ridges, knolls, strath terraces. The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147699"|"21355822"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roto, stony soil is a minor component."|"21147700"|"21355823"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21147701"|"21355824"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, stony component makes up 20 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillsides, escarpments, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21147702"|"21355825"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148463"|"21356586"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Floweree component makes up 95 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces, knolls, alluvial fans. The parent material consists of fine-silty loess, calcareous. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148464"|"21356587"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21148465"|"21356588"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148466"|"21356589"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21147915"|"21356038"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, terraces, hillsides, escarpments. The parent material consists of clayey slope alluvium derived from semiconsolidated shale, clayey. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21147916"|"21356039"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147917"|"21356040"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21147918"|"21356041"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shoddy soil is a minor component."|"21147919"|"21356042"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21147920"|"21356043"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147921"|"21356044"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147922"|"21356045"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21147923"|"21356046"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21147924"|"21356047"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147703"|"21355826"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21147704"|"21355827"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shoddy soil is a minor component."|"21147705"|"21355828"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21147706"|"21355829"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobarter component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls, hillsides, alluvial fans. The parent material consists of clayey slope alluvium derived from semiconsolidated shale-siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS330MT Clayey (cy) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21147707"|"21355830"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147708"|"21355831"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21147709"|"21355832"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobarter component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, alluvial fans, knolls. The parent material consists of clayey slope alluvium derived from semiconsolidated shale-siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21147710"|"21355833"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21147711"|"21355834"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147712"|"21355835"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shoddy soil is a minor component."|"21147713"|"21355836"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clunton component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood-plain steps. The parent material consists of fine-loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is rarely ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21148228"|"21356351"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"21148229"|"21356352"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium and/or colluvium derived from basalt and/or metavolcanics. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21148230"|"21356353"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Faith soil is a minor component."|"21148231"|"21356354"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cometcrik component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood-plain steps, flood plains. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21148232"|"21356355"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 41 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148240"|"21356363"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, stony soil is a minor component."|"21148241"|"21356364"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, stony soil is a minor component."|"21148242"|"21356365"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, steeper slopes soil is a minor component."|"21148243"|"21356366"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha, stony component makes up 39 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148244"|"21356367"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21147934"|"21356057"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 29 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillsides, escarpments, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21147935"|"21356058"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21147936"|"21356059"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walbert soil is a minor component."|"21147937"|"21356060"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 31 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, hillsides, knolls, plains. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147938"|"21356061"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147939"|"21356062"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147940"|"21356063"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anamac soil is a minor component."|"21147941"|"21356064"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148479"|"21356602"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148480"|"21356603"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, steeper slopes soil is a minor component."|"21148481"|"21356604"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148482"|"21356605"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148483"|"21356606"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, stony soil is a minor component."|"21148484"|"21356607"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148485"|"21356608"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, stony soil is a minor component."|"21148486"|"21356609"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148487"|"21356610"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, stony soil is a minor component."|"21148488"|"21356611"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21147733"|"21355856"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, greater slope soil is a minor component."|"21147734"|"21355857"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21147735"|"21355858"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147736"|"21355859"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147737"|"21355860"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21147738"|"21355861"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21147739"|"21355862"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, hillsides, knolls, plains. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148489"|"21356612"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, greater slope soil is a minor component."|"21148490"|"21356613"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, stony soil is a minor component."|"21148491"|"21356614"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21148492"|"21356615"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, very stony soil is a minor component."|"21147740"|"21355863"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147741"|"21355864"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21147742"|"21355865"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, very stony soil is a minor component."|"21147743"|"21355866"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly residuum weathered from limestone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147744"|"21355867"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147745"|"21355868"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148245"|"21356368"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap, cool, very stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly residuum weathered from limestone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148246"|"21356369"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148247"|"21356370"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, stony soil is a minor component."|"21148248"|"21356371"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, moist, very stony soil is a minor component."|"21148249"|"21356372"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden, very stony component makes up 45 percent of the map unit. Slopes are 8 to 15 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148250"|"21356373"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, very stony soil is a minor component."|"21147942"|"21356065"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, moist, very stony soil is a minor component."|"21147943"|"21356066"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21147944"|"21356067"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21147945"|"21356068"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap, cool, very stony component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly residuum weathered from limestone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147946"|"21356069"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maiden, very stony component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147947"|"21356070"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148031"|"21356154"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148032"|"21356155"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21148033"|"21356156"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21148034"|"21356157"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21148035"|"21356158"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148036"|"21356159"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shoddy soil is a minor component."|"21148037"|"21356160"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on escarpments, hills, knolls. The parent material consists of fine-loamy slope alluvium over loamy residuum weathered from semiconsolidated sandstone-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148038"|"21356161"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148045"|"21356168"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148046"|"21356169"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21148047"|"21356170"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 29 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148048"|"21356171"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walbert soil is a minor component."|"21148049"|"21356172"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 31 percent of the map unit. Slopes are 2 to 8 percent. This component is on escarpments, hills, knolls. The parent material consists of loamy residuum weathered from semiconsolidated siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21148050"|"21356173"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21148051"|"21356174"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on escarpments, hills, knolls. The parent material consists of loamy residuum weathered from semiconsolidated siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21148334"|"21356457"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21148335"|"21356458"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148336"|"21356459"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21148337"|"21356460"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walbert soil is a minor component."|"21148338"|"21356461"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148339"|"21356462"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148340"|"21356463"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21148341"|"21356464"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart, very stony soil is a minor component."|"21148052"|"21356175"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor, stony soil is a minor component."|"21148053"|"21356176"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary beds soil is a minor component."|"21148054"|"21356177"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, hills, knolls. The parent material consists of loamy residuum weathered from semiconsolidated siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21148055"|"21356178"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148056"|"21356179"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148057"|"21356180"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA040MT Loamy Steep (lostp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148058"|"21356181"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21148059"|"21356182"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap, very stony component makes up 20 percent of the map unit. Slopes are 35 to 70 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly residuum weathered from limestone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP913MT Limy Warm Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148060"|"21356183"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"21148061"|"21356184"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham, very stony component makes up 40 percent of the map unit. Slopes are 35 to 70 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP912MT Limy Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148062"|"21356185"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden, very stony soil is a minor component."|"21148063"|"21356186"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148064"|"21356187"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Warneke soil is a minor component."|"21148065"|"21356188"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham, stony component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on divides, escarpments, hillsides, ridges. The parent material consists of gravelly slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148342"|"21356465"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell soil is a minor component."|"21148343"|"21356466"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21148344"|"21356467"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden soil is a minor component."|"21148345"|"21356468"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap soil is a minor component."|"21148346"|"21356469"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148347"|"21356470"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverrun soil is a minor component."|"21148348"|"21356471"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wetsand soil is a minor component."|"21148349"|"21356472"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cardwell soil is a minor component."|"21148350"|"21356473"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ledger component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood plains, flood-plain steps. The parent material consists of saline and sodic clayey alluvium derived from shale-siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21148351"|"21356474"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenton component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood plains, flood-plain steps. The parent material consists of saline and sodic clayey recent alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"21148352"|"21356475"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moltoner component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood plains, flood-plain steps. The parent material consists of saline and sodic fine-loamy stratified recent alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 6s. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21148353"|"21356476"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148066"|"21356189"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148067"|"21356190"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148068"|"21356191"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148069"|"21356192"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roto, stony soil is a minor component."|"21148070"|"21356193"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore, stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillsides, escarpments, ridges, knolls, strath terraces. The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148071"|"21356194"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, stony component makes up 40 percent of the map unit. Slopes are 25 to 60 percent. This component is on hillsides, escarpments, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148072"|"21356195"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148073"|"21356196"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cozberg, stony soil is a minor component."|"21148561"|"21356684"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, cobbly soil is a minor component."|"21148562"|"21356685"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"21148563"|"21356686"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, stony soil is a minor component."|"21148564"|"21356687"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 41 percent of the map unit. Slopes are 2 to 8 percent. This component is on escarpments, hillsides, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148565"|"21356688"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148566"|"21356689"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 39 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148567"|"21356690"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21148568"|"21356691"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, cobbly soil is a minor component."|"21148569"|"21356692"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA040MT Loamy Steep (lostp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148570"|"21356693"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, very stony soil is a minor component."|"21148571"|"21356694"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on escarpments, hillsides, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148572"|"21356695"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore, stony soil is a minor component."|"21148573"|"21356696"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"21148574"|"21356697"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21148074"|"21356197"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148075"|"21356198"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148076"|"21356199"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, very stony component makes up 85 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillsides, escarpments, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148077"|"21356200"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21148078"|"21356201"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148079"|"21356202"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147819"|"21355942"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147820"|"21355943"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147821"|"21355944"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21147822"|"21355945"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21147823"|"21355946"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"21147824"|"21355947"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfist soil is a minor component."|"21147825"|"21355948"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA040MT Loamy Steep (lostp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147826"|"21355949"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, greater slope soil is a minor component."|"21147827"|"21355950"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, very cobbly component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21147828"|"21355951"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21147829"|"21355952"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart, very stony soil is a minor component."|"21147830"|"21355953"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147831"|"21355954"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21147832"|"21355955"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"21147833"|"21355956"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148354"|"21356477"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 36 percent of the map unit. Slopes are 4 to 15 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148355"|"21356478"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walbert soil is a minor component."|"21148356"|"21356479"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148357"|"21356480"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21148358"|"21356481"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21148359"|"21356482"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148360"|"21356483"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 34 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148361"|"21356484"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA040MT Loamy Steep (lostp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148080"|"21356203"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148081"|"21356204"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148082"|"21356205"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148083"|"21356206"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21148084"|"21356207"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Walbert soil is a minor component."|"21148085"|"21356208"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21148086"|"21356209"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21148087"|"21356210"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21148088"|"21356211"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"21148089"|"21356212"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148090"|"21356213"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, very cobbly component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148091"|"21356214"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148092"|"21356215"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148093"|"21356216"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148094"|"21356217"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, greater slope, very stony soil is a minor component."|"21148575"|"21356698"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sieben, bouldery soil is a minor component."|"21148576"|"21356699"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148577"|"21356700"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, very stony component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on valley floors, escarpments, hillsides, alluvial fans. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148578"|"21356701"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148579"|"21356702"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21148362"|"21356485"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sieben, bouldery soil is a minor component."|"21148363"|"21356486"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148364"|"21356487"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148365"|"21356488"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sieben, very stony soil is a minor component."|"21148366"|"21356489"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell, very stony soil is a minor component."|"21148367"|"21356490"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sieben, stony component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillsides, terraces, alluvial fans. The parent material consists of calcareous gravelly tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148368"|"21356491"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sieberell, very stony component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillsides, terraces, alluvial fans. The parent material consists of calcareous gravelly slope alluvium over sandy and gravelly slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21148369"|"21356492"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148580"|"21356703"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces, hillsides, knolls, alluvial fans. The parent material consists of fine-loamy slope alluvium from semiconsolidated sandstone, siltstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148581"|"21356704"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, greater slope soil is a minor component."|"21148582"|"21356705"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide, greater slope soil is a minor component."|"21148583"|"21356706"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21148584"|"21356707"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21148585"|"21356708"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Udecide component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls, hillsides, interfluves. The parent material consists of calcareous fine-loamy slope alluvium over residuum weathered from semiconsolidated sandstone-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21148586"|"21356709"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood-plain steps, flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148587"|"21356710"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ryell component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, drainageways, flood-plain steps. The parent material consists of coarse-loamy over sandy and gravelly recent alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148588"|"21356711"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverrun soil is a minor component."|"21148589"|"21356712"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Handke component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood plains, flood-plain steps. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA110MT Sandy (sy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21148590"|"21356713"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Faith soil is a minor component."|"21148591"|"21356714"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, very stony component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on alluvial fans, escarpments, hillsides, ridges. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148592"|"21356715"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148593"|"21356716"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, very stony component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on alluvial fans, escarpments, hillsides, ridges. The parent material consists of gravelly colluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21148594"|"21356717"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Connieo, very bouldery soil is a minor component."|"21148595"|"21356718"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Breeton soil is a minor component."|"21148596"|"21356719"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, stony soil is a minor component."|"21148597"|"21356720"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baxton, bouldery soil is a minor component."|"21148598"|"21356721"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"21148599"|"21356722"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148600"|"21356723"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quaint soil is a minor component."|"21148601"|"21356724"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, stony soil is a minor component."|"21148602"|"21356725"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clasoil soil is a minor component."|"21148603"|"21356726"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, hillsides, terraces. The parent material consists of calcareous gravelly slope alluvium derived from fine-grained sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148604"|"21356727"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cardwell component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, flood-plain steps. The parent material consists of fine-silty alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148605"|"21356728"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Handke soil is a minor component."|"21148606"|"21356729"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nestley soil is a minor component."|"21148607"|"21356730"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clunton soil is a minor component."|"21148608"|"21356731"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pieriver soil is a minor component."|"21148609"|"21356732"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, flood-plain steps, drainageways. The parent material consists of sandy and gravelly recent alluvium from mixed igneous, sedimentary and metamorphic rocks. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA134MT Shallow To Gravel (swgr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21148610"|"21356733"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillsides, escarpments, ridges, knolls, strath terraces. The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148611"|"21356734"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on escarpments, hillsides, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148612"|"21356735"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, stony soil is a minor component."|"21148613"|"21356736"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roto, greater slope soil is a minor component."|"21148614"|"21356737"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148615"|"21356738"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roto component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillsides, ridges, escarpments. The parent material consists of gravelly slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148616"|"21356739"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21148617"|"21356740"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148095"|"21356218"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago, lesser slope soil is a minor component."|"21148096"|"21356219"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148097"|"21356220"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roto, lesser slope soil is a minor component."|"21148098"|"21356221"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore, stony component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on hillsides, escarpments, ridges, knolls, strath terraces. The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148099"|"21356222"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21148100"|"21356223"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, stony component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on hillsides, escarpments, plains, alluvial fans. The parent material consists of calcareous gravelly slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 55 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21148101"|"21356224"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roto, stony component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on hillsides, ridges, escarpments. The parent material consists of gravelly slope alluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148102"|"21356225"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148370"|"21356493"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, cobbly soil is a minor component."|"21148371"|"21356494"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148372"|"21356495"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, greater slope soil is a minor component."|"21148373"|"21356496"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148374"|"21356497"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21148375"|"21356498"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Floweree soil is a minor component."|"21148376"|"21356499"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, greater slope soil is a minor component."|"21148618"|"21356741"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21148619"|"21356742"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148620"|"21356743"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock soil is a minor component."|"21148621"|"21356744"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148622"|"21356745"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, hillsides, knolls, plains. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148623"|"21356746"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, greater slope soil is a minor component."|"21148624"|"21356747"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21148625"|"21356748"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148626"|"21356749"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148627"|"21356750"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148377"|"21356500"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on escarpments, hillsides, strath terraces. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148378"|"21356501"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148379"|"21356502"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot, stony component makes up 20 percent of the map unit. Slopes are 8 to 25 percent. This component is on escarpments, hillsides, strath terraces. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148380"|"21356503"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lahood soil is a minor component."|"21148381"|"21356504"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148382"|"21356505"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lahood, stony soil is a minor component."|"21148103"|"21356226"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 40 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments, hillsides, strath terraces. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148104"|"21356227"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot, very stony component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments, hillsides, strath terraces. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148105"|"21356228"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148106"|"21356229"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148107"|"21356230"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21148108"|"21356231"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148383"|"21356506"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 55 percent of the map unit. Slopes are 35 to 70 percent. This component is on escarpments, hillsides, strath terraces. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148384"|"21356507"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec component makes up 20 percent of the map unit. Slopes are 35 to 70 percent. This component is on valley floors, alluvial fans, escarpments, hillsides. The parent material consists of sandy and gravelly calcareous tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA038MT Droughty Steep (drstp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148385"|"21356508"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148386"|"21356509"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Geohrock, stony soil is a minor component."|"21148387"|"21356510"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roto, stony soil is a minor component."|"21148388"|"21356511"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, lesser slope soil is a minor component."|"21148389"|"21356512"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21148109"|"21356232"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21148110"|"21356233"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces, knolls, hillsides, alluvial fans. The parent material consists of fine-loamy slope alluvium from semiconsolidated sandstone, siltstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA001MT Clayey (cy)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148111"|"21356234"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"21148112"|"21356235"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anamac soil is a minor component."|"21148113"|"21356236"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces, knolls, hillsides, alluvial fans. The parent material consists of fine-loamy slope alluvium from semiconsolidated sandstone, siltstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147834"|"21355957"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21147835"|"21355958"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington soil is a minor component."|"21147836"|"21355959"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, stony soil is a minor component."|"21147837"|"21355960"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raghorn soil is a minor component."|"21147838"|"21355961"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sieben, stony soil is a minor component."|"21147839"|"21355962"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Judell, very stony component makes up 90 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, hillsides, terraces. The parent material consists of fine-loamy slope alluvium derived from limestone, unspecified. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148628"|"21356751"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148629"|"21356752"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judell, L soil is a minor component."|"21148630"|"21356753"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maiden soil is a minor component."|"21148631"|"21356754"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale, very stony component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, hillsides, terraces. The parent material consists of calcareous fine-loamy slope alluvium derived from fine-grained sandstone, siltstone and metamorphic rocks. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148390"|"21356513"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21148391"|"21356514"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, stony soil is a minor component."|"21148392"|"21356515"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert soil is a minor component."|"21148393"|"21356516"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work, stony soil is a minor component."|"21148394"|"21356517"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147846"|"21355969"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21147847"|"21355970"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 25 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21147848"|"21355971"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Walbert component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on interfluves, ridges, hillsides. The parent material consists of sandy residuum weathered from semiconsolidated coarse-grained sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21147849"|"21355972"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21147850"|"21355973"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21147851"|"21355974"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on escarpments, hills, knolls. The parent material consists of loamy residuum weathered from semiconsolidated siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21147852"|"21355975"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Udecide soil is a minor component."|"21147853"|"21355976"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21147854"|"21355977"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, rubbly component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountainsides, ridges, escarpments. The parent material consists of gravelly residuum weathered from sandstone, unspecified. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP902MT Shallow Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148114"|"21356237"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148115"|"21356238"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tigeron, very stony soil is a minor component."|"21148116"|"21356239"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve, very stony soil is a minor component."|"21148117"|"21356240"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sigbird, bouldery soil is a minor component."|"21148118"|"21356241"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfern, rubbly soil is a minor component."|"21148119"|"21356242"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arrowpeak, very stony soil is a minor component."|"21148120"|"21356243"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quaint, very stony component makes up 90 percent of the map unit. Slopes are 8 to 35 percent. This component is on ridges, hillsides, plateaus. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21147925"|"21356048"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfist soil is a minor component."|"21147926"|"21356049"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, shale soil is a minor component."|"21147927"|"21356050"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quincreek soil is a minor component."|"21147928"|"21356051"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilspring soil is a minor component."|"21147714"|"21355837"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21147715"|"21355838"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quaint component makes up 40 percent of the map unit. Slopes are 4 to 25 percent. This component is on ridges, hillsides, plateaus. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21147716"|"21355839"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redfist component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, hillsides, knolls. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21147717"|"21355840"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quincreek soil is a minor component."|"21147718"|"21355841"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ferball soil is a minor component."|"21147719"|"21355842"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Devilfence soil is a minor component."|"21147720"|"21355843"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilspring soil is a minor component."|"21147721"|"21355844"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quaint component makes up 41 percent of the map unit. Slopes are 15 to 45 percent. This component is on ridges, hillsides, plateaus. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21147722"|"21355845"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Devilfence soil is a minor component."|"21147723"|"21355846"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfist soil is a minor component."|"21147724"|"21355847"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quincreek soil is a minor component."|"21147725"|"21355848"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21147726"|"21355849"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redfist component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, hillsides, knolls. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21147727"|"21355850"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, very stony soil is a minor component."|"21147728"|"21355851"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quaint component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on ridges, hillsides, plateaus. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21147729"|"21355852"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quincreek soil is a minor component."|"21147730"|"21355853"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Devilfence soil is a minor component."|"21147731"|"21355854"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilspring soil is a minor component."|"21147732"|"21355855"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, bouldery component makes up 25 percent of the map unit. Slopes are 2 to 35 percent. This component is on alluvial fans, hillsides, escarpments, ridges. The parent material consists of gravelly colluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21148233"|"21356356"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148234"|"21356357"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redfist, bouldery component makes up 40 percent of the map unit. Slopes are 2 to 35 percent. This component is on alluvial fans, hillsides, knolls. The parent material consists of calcareous gravelly slope alluvium over residuum weathered from hard red shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21148235"|"21356358"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, very stony soil is a minor component."|"21148236"|"21356359"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitlash, very stony soil is a minor component."|"21148237"|"21356360"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, very bouldery soil is a minor component."|"21148238"|"21356361"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quaint, very stony soil is a minor component."|"21148239"|"21356362"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quincreek soil is a minor component."|"21148467"|"21356590"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Devilfence component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on ridges, escarpments, hillsides. The parent material consists of gravelly residuum weathered from shale-siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148468"|"21356591"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilspring component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on escarpments, hillsides, ridges. The parent material consists of calcareous gravelly colluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.   The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148469"|"21356592"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148470"|"21356593"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vigilante soil is a minor component."|"21148471"|"21356594"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper, stony soil is a minor component."|"21148472"|"21356595"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Devilfence component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on ridges, escarpments, hillsides. The parent material consists of gravelly residuum weathered from shale-siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148473"|"21356596"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfist soil is a minor component."|"21148474"|"21356597"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148475"|"21356598"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quincreek soil is a minor component."|"21148476"|"21356599"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilspring soil is a minor component."|"21148477"|"21356600"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vigilante soil is a minor component."|"21148478"|"21356601"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore, bouldery component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, alluvial fans. The parent material consists of gravelly colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148328"|"21356451"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Firada, very stony soil is a minor component."|"21148329"|"21356452"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, bouldery component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on ridges, mountain slopes. The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP912MT Limy Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21148330"|"21356453"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville, rubbly soil is a minor component."|"21148331"|"21356454"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148332"|"21356455"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanson, stony soil is a minor component."|"21148333"|"21356456"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sigbird, stony component makes up 30 percent of the map unit. Slopes are 25 to 50 percent. This component is on escarpments, ridges, mountain slopes. The parent material consists of gravelly slope alluvium derived from hard shale over residuum weathered from hard shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148039"|"21356162"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle, very bouldery soil is a minor component."|"21148040"|"21356163"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sigbird, very bouldery component makes up 40 percent of the map unit. Slopes are 35 to 70 percent. This component is on escarpments, ridges, mountain slopes. The parent material consists of gravelly slope alluvium derived from hard shale over residuum weathered from hard shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148041"|"21356164"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kimpton, very bouldery soil is a minor component."|"21148042"|"21356165"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hanson, stony soil is a minor component."|"21148043"|"21356166"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148044"|"21356167"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sappington component makes up 60 percent of the map unit. Slopes are 1 to 4 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148172"|"21356295"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, greater slope soil is a minor component."|"21148173"|"21356296"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148174"|"21356297"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 35 percent of the map unit. Slopes are 1 to 4 percent. This component is on hillsides, plains, alluvial fans, knolls. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148175"|"21356298"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tigeron, very bouldery soil is a minor component."|"21148176"|"21356299"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve, rubbly soil is a minor component."|"21148177"|"21356300"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, very bouldery soil is a minor component."|"21148178"|"21356301"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle, very bouldery soil is a minor component."|"21148179"|"21356302"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redfern, rubbly soil is a minor component."|"21148180"|"21356303"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot, very stony soil is a minor component."|"21148181"|"21356304"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21148182"|"21356305"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148183"|"21356306"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek, Dry component makes up 50 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly residuum weathered from argillite gravelly residuum weathered from metaquartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21147879"|"21356002"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wickes component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of gravelly colluvium over residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21147880"|"21356003"
08/07/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek component makes up 10 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly residuum weathered from argillite gravelly residuum weathered from metaquartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21147881"|"21356004"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holter soil is a minor component."|"21147882"|"21356005"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21147883"|"21356006"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21147884"|"21356007"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert soil is a minor component."|"21147885"|"21356008"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 40 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA132MT Shallow Limy (SwLy)   LRU 44B-A ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"21148652"|"21356775"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 20 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148653"|"21356776"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148654"|"21356777"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148655"|"21356778"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"21148656"|"21356779"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"21148423"|"21356546"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Judith soil is a minor component."|"21148424"|"21356547"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 20 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS356MT Silty-droughty-steep (sidrstp) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"21148425"|"21356548"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 40 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS353MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148426"|"21356549"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148427"|"21356550"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"21148661"|"21356784"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 90 percent of the map unit. Slopes are 4 to 15 percent.  The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148662"|"21356785"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148663"|"21356786"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 50 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of gravelly colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148155"|"21356278"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148156"|"21356279"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148157"|"21356280"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 30 percent of the map unit. Slopes are 15 to 60 percent.  The parent material consists of gravelly residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS353MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148158"|"21356281"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148159"|"21356282"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wickes component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of gravelly colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21147886"|"21356009"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Circleville soil is a minor component."|"21147887"|"21356010"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek, Dry component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of gravelly residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21147888"|"21356011"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21147889"|"21356012"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of gravelly residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS353MT Shallow (sw) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21147890"|"21356013"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wickes soil is a minor component."|"21147891"|"21356014"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148163"|"21356286"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek, Dry component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of gravelly residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21148164"|"21356287"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gnojek soil is a minor component."|"21148165"|"21356288"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Circleville component makes up 60 percent of the map unit. Slopes are 4 to 8 percent. This component is on plains. The parent material consists of gravelly colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 30 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21148166"|"21356289"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148657"|"21356780"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of calcareous gravelly alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148658"|"21356781"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of coarse-loamy alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148659"|"21356782"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148660"|"21356783"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148428"|"21356551"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skein component makes up 25 percent of the map unit. Slopes are 4 to 15 percent.  The parent material consists of loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (SwLo)   LRU 44B-A ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148429"|"21356552"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"21148430"|"21356553"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21148431"|"21356554"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rootel component makes up 40 percent of the map unit. Slopes are 4 to 15 percent.  The parent material consists of fine-loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21148432"|"21356555"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitesage component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, alluvial fans. The parent material consists of fine-loamy slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148433"|"21356556"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Skein component makes up 60 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills. The parent material consists of loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (SwLo)   LRU 44B-A ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 22 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148167"|"21356290"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rootel component makes up 30 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of fine-loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21148168"|"21356291"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148169"|"21356292"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitesage soil is a minor component."|"21148170"|"21356293"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rencot soil is a minor component."|"21148171"|"21356294"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek, Dry component makes up 60 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly residuum weathered from argillite gravelly residuum weathered from metaquartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21148434"|"21356557"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148435"|"21356558"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21148436"|"21356559"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evanston soil is a minor component."|"21148437"|"21356560"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duffson component makes up 25 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly residuum weathered from metaquartzite gravelly residuum weathered from argillite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS347MT Silty-steep (sistp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148438"|"21356561"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"21148664"|"21356787"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148665"|"21356788"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gnojek, Dry component makes up 60 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of gravelly residuum weathered from argillite gravelly residuum weathered from metaquartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21148666"|"21356789"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evanston soil is a minor component."|"21148667"|"21356790"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Duffson component makes up 25 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of gravelly residuum weathered from argillite gravelly residuum weathered from metaquartzite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148668"|"21356791"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Birney component makes up 20 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148669"|"21356792"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rootel soil is a minor component."|"21148670"|"21356793"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"21148671"|"21356794"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148672"|"21356795"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gnojek soil is a minor component."|"21148673"|"21356796"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 40 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly residuum weathered from metaquartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148674"|"21356797"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rencot component makes up 65 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of gravelly residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"21148675"|"21356798"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148676"|"21356799"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitesage soil is a minor component."|"21148677"|"21356800"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gnojek soil is a minor component."|"21148678"|"21356801"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rootel component makes up 15 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of fine-loamy colluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XS347MT Silty-steep (sistp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21148679"|"21356802"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"21148160"|"21356283"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148161"|"21356284"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of fine-loamy alluvium derived from mixed sources. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148162"|"21356285"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147860"|"21355983"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147861"|"21355984"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Patouza component makes up 90 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS330MT Clayey (cy) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147862"|"21355985"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21148121"|"21356244"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Headwaters soil is a minor component."|"21148122"|"21356245"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148123"|"21356246"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148124"|"21356247"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148125"|"21356248"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148403"|"21356526"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on stream terraces. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS341MT Limy (ly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148404"|"21356527"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"21148405"|"21356528"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148406"|"21356529"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowery soil is a minor component."|"21147855"|"21355978"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21147856"|"21355979"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"21147857"|"21355980"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS346MT Sandy-steep (systp) 9-14"" P.z.   Deleted.  Refer To R044xs347mt. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147858"|"21355981"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 70 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS347MT Silty-steep (sistp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147859"|"21355982"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21147863"|"21355986"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21147864"|"21355987"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"21147865"|"21355988"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on stream terraces, alluvial fans. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS335MT Sandy (sy) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147866"|"21355989"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148126"|"21356249"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148127"|"21356250"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148128"|"21356251"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"21148129"|"21356252"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meagher soil is a minor component."|"21148130"|"21356253"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments. The parent material consists of loamy alluvium colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS363MT Thin Silty (tsi) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148131"|"21356254"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowery soil is a minor component."|"21148132"|"21356255"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beanlake soil is a minor component."|"21148133"|"21356256"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21148134"|"21356257"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale soil is a minor component."|"21147867"|"21355990"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beanlake soil is a minor component."|"21147868"|"21355991"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anceney soil is a minor component."|"21147869"|"21355992"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on stream terraces. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044XS355MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147870"|"21355993"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brocko soil is a minor component."|"21148223"|"21356346"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobarter soil is a minor component."|"21148224"|"21356347"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shoddy component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, knolls. The parent material consists of calcareous clayey slope alluvium over residuum weathered from semiconsolidated shale-siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA131MT Shallow Clay (swc)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21148225"|"21356348"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21148226"|"21356349"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148227"|"21356350"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148407"|"21356530"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"21148408"|"21356531"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"21148409"|"21356532"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148410"|"21356533"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sappington, stony soil is a minor component."|"21147929"|"21356052"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha, stony component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillsides, knolls, plains, alluvial fans. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147930"|"21356053"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, hillsides, plains, knolls. The parent material consists of calcareous coarse-loamy tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21147931"|"21356054"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha, steeper slopes soil is a minor component."|"21147932"|"21356055"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, very stony soil is a minor component."|"21147933"|"21356056"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21147871"|"21355994"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beanlake component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS357MT Limy (ly) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147872"|"21355995"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beanlake soil is a minor component."|"21147873"|"21355996"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS338MT Shallow To Gravel (swgr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21148411"|"21356534"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ryell component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during April, May, June. Organic matter content in the surface horizon is about 1 percent. This component is in the R044XS339MT Silty (si) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21148412"|"21356535"
08/07/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonebasin component makes up 10 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 40 percent. This component is in the R043BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148413"|"21356536"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"21148414"|"21356537"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"21148415"|"21356538"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans, stream terraces. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS356MT Silty-droughty-steep (sidrstp) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148632"|"21356755"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148633"|"21356756"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"21148634"|"21356757"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148135"|"21356258"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148136"|"21356259"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Musselshell component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of loamy alluvium loamy colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS347MT Silty-steep (sistp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148137"|"21356260"
01/21/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA132MT Shallow Limy (SwLy)   LRU 44B-A ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"21148138"|"21356261"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Musselshell soil is a minor component."|"21148139"|"21356262"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham, stony component makes up 85 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148140"|"21356263"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, greater slopes soil is a minor component."|"21148141"|"21356264"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap, stony soil is a minor component."|"21148142"|"21356265"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148143"|"21356266"
05/15/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Enbar component makes up 55 percent of the map unit. Slopes are 4 to 8 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148144"|"21356267"
05/15/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowery component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BB060MT Overflow (ov)   Lru 44b-b ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21148145"|"21356268"
05/15/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"21148146"|"21356269"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nythar component makes up 15 percent of the map unit. Slopes are 4 to 6 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21148147"|"21356270"
05/15/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"21148148"|"21356271"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on drainageways. The parent material consists of loamy alluvium loamy colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the F044BP908MT Upland Aspen Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21148635"|"21356758"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"21148636"|"21356759"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"21148637"|"21356760"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redlodge soil is a minor component."|"21148638"|"21356761"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonebasin component makes up 10 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 40 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148416"|"21356539"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mccabe component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during May, June. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21148417"|"21356540"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"21148418"|"21356541"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rivra component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21148419"|"21356542"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21148420"|"21356543"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21148421"|"21356544"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"21148422"|"21356545"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21147874"|"21355997"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21147875"|"21355998"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS336MT Shallow (sw) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147876"|"21355999"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments. The parent material consists of alluvium colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS346MT Sandy-steep (systp) 9-14"" P.z.   Deleted.  Refer To R044xs347mt. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147877"|"21356000"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amesha component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments. The parent material consists of loamy alluvium loamy colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS347MT Silty-steep (sistp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147878"|"21356001"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cozberg soil is a minor component."|"21147840"|"21355963"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"21147841"|"21355964"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sieben soil is a minor component."|"21147842"|"21355965"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, terraces, valley floors. The parent material consists of calcareous gravelly alluvium over sandy and gravelly tertiary valley fill alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21147843"|"21355966"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vendome component makes up 40 percent of the map unit. Slopes are 1 to 4 percent. This component is on plains, knolls, terraces, alluvial fans. The parent material consists of calcareous gravelly alluvium over sandy and gravelly alluvium from mixed igneous, sedimentary and metamorphic rocks. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA134MT Shallow To Gravel (swgr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21147844"|"21355967"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, stony soil is a minor component."|"21147845"|"21355968"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blaincreek, very stony soil is a minor component."|"21148395"|"21356518"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wickes, very stony soil is a minor component."|"21148396"|"21356519"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sawicki, very stony soil is a minor component."|"21148397"|"21356520"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148398"|"21356521"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Brickner, very bouldery soil is a minor component."|"21148399"|"21356522"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mocmont, stony soil is a minor component."|"21148400"|"21356523"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, bouldery component makes up 20 percent of the map unit. Slopes are 35 to 70 percent. This component is on alluvial fans, hillsides, escarpments, ridges. The parent material consists of gravelly residuum weathered from fine-grained sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21148401"|"21356524"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, very stony soil is a minor component."|"21148402"|"21356525"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow, stony component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148639"|"21356762"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21148640"|"21356763"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap, very stony component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of loamy residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS353MT Shallow (sw) 15-19"" P.z., Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148641"|"21356764"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148642"|"21356765"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow, moderately deep soil is a minor component."|"21148643"|"21356766"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments. The parent material consists of sandy residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21148149"|"21356272"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments. The parent material consists of loamy alluvium loamy colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS346MT Sandy-steep (systp) 9-14"" P.z.   Deleted.  Refer To R044xs347mt. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148150"|"21356273"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21148151"|"21356274"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments. The parent material consists of sandy and gravelly alluvium sandy and gravelly colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS340MT Silty-droughty-steep (sidrstp) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21148152"|"21356275"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21148153"|"21356276"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pensore soil is a minor component."|"21148644"|"21356767"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 60 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"21148645"|"21356768"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148646"|"21356769"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148647"|"21356770"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crago soil is a minor component."|"21148648"|"21356771"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore component makes up 60 percent of the map unit. Slopes are 45 to 70 percent. This component is on hills. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044XS612MT Shallow Limy (swly) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent.  "|"21148649"|"21356772"
09/08/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21148650"|"21356773"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"21148651"|"21356774"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21148154"|"21356277"
