03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218516"|"21434179"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Medicinelodge soil is a minor component."|"21218517"|"21434180"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, extremely bouldery component makes up 25 percent of the map unit. Slopes are 15 to 50 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218518"|"21434181"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, stony component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, landslides. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218519"|"21434182"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, landslides. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218520"|"21434183"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bridger soil is a minor component."|"21218521"|"21434184"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cheadle soil is a minor component."|"21218522"|"21434185"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21218523"|"21434186"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21218238"|"21433901"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, stony component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218239"|"21433902"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bridger soil is a minor component."|"21218240"|"21433903"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, very bouldery component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218241"|"21433904"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218242"|"21433905"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cheadle soil is a minor component."|"21218243"|"21433906"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blaine soil is a minor component."|"21218244"|"21433907"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21217899"|"21433562"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21217900"|"21433563"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21217901"|"21433564"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 45 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217902"|"21433565"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21217903"|"21433566"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"21217904"|"21433567"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21217905"|"21433568"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21217906"|"21433569"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very stony component makes up 20 percent of the map unit. Slopes are 8 to 50 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218245"|"21433908"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21218246"|"21433909"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21218247"|"21433910"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cheadle soil is a minor component."|"21218248"|"21433911"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Philipsburg soil is a minor component."|"21218249"|"21433912"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Medicinelodge soil is a minor component."|"21218250"|"21433913"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 45 percent of the map unit. Slopes are 8 to 50 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218251"|"21433914"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218252"|"21433915"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 25 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217907"|"21433570"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217908"|"21433571"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Narrows soil is a minor component."|"21217909"|"21433572"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Doolittle soil is a minor component."|"21217910"|"21433573"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21217911"|"21433574"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218253"|"21433916"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21218254"|"21433917"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doolittle soil is a minor component."|"21218255"|"21433918"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"21218256"|"21433919"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218257"|"21433920"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently flooded component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218258"|"21433921"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218259"|"21433922"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently ponded soil is a minor component."|"21218260"|"21433923"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218261"|"21433924"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows, saline soil is a minor component."|"21218262"|"21433925"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Matsingale, frequently ponded soil is a minor component."|"21218786"|"21434449"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218787"|"21434450"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truaxcreek component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218788"|"21434451"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently ponded component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218789"|"21434452"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"21218790"|"21434453"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dutchhollow soil is a minor component."|"21217919"|"21433582"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lehunt, saline component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches during April, May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 70 within 30 inches of the soil surface."|"21217920"|"21433583"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Matsingale soil is a minor component."|"21217921"|"21433584"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21217922"|"21433585"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crookedrun soil is a minor component."|"21217923"|"21433586"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodtick component makes up 40 percent of the map unit. Slopes are 8 to 45 percent. This component is on dunes, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218915"|"21434578"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jackrabbit component makes up 60 percent of the map unit. Slopes are 4 to 12 percent. This component is on dunes, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218916"|"21434579"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodtick component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on dunes, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218080"|"21433743"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jackrabbit component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on dunes, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218081"|"21433744"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sandrift, frequently ponded component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on dune slacks, intermontane basins. The parent material consists of eolian sands over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 33 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218082"|"21433745"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodtick component makes up 55 percent of the map unit. Slopes are 4 to 35 percent. This component is on dunes, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218386"|"21434049"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jackrabbit soil is a minor component."|"21218387"|"21434050"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Branham component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on ridges, intermontane basins. The parent material consists of eolian influenced colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218388"|"21434051"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218389"|"21434052"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jackrabbit component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on dunes on fan remnants, intermontane basins. The parent material consists of eolian sands over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218917"|"21434580"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218918"|"21434581"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bighole component makes up 25 percent of the map unit. Slopes are 1 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218919"|"21434582"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, swales. The parent material consists of slope alluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BD060MT Overflow (ov)   Lru 44b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218920"|"21434583"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218921"|"21434584"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"21218922"|"21434585"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"21218923"|"21434586"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218924"|"21434587"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullrey soil is a minor component."|"21218925"|"21434588"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on swales, mountains. The parent material consists of colluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218926"|"21434589"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal soil is a minor component."|"21218927"|"21434590"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 45 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218928"|"21434591"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bullrey component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218929"|"21434592"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218930"|"21434593"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"21218931"|"21434594"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218390"|"21434053"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on ridges, mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from volcanic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218391"|"21434054"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"21218392"|"21434055"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Surdal, stony soil is a minor component."|"21218393"|"21434056"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218394"|"21434057"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during March, April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218083"|"21433746"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete, frequently ponded component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on bogs on lakebeds, intermontane basins. The parent material consists of mucky peat organic material over alluvium and/or lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218084"|"21433747"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218085"|"21433748"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218395"|"21434058"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lehunt soil is a minor component."|"21218396"|"21434059"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Regulus, frequently ponded component makes up 75 percent of the map unit. Slopes are 0 to 1 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21218397"|"21434060"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sandrift component makes up 20 percent of the map unit. Slopes are 0 to 1 percent. This component is on lakebeds, intermontane basins. The parent material consists of eolian sands over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218398"|"21434061"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sandrift soil is a minor component."|"21218086"|"21433749"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218087"|"21433750"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zufelt component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer, strongly contrasting textural stratification, is 20 to 40 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21218088"|"21433751"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21218946"|"21434609"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Philipsburg soil is a minor component."|"21218417"|"21434080"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218418"|"21434081"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, stony component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218419"|"21434082"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21218420"|"21434083"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hooligan soil is a minor component."|"21218421"|"21434084"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cheadle soil is a minor component."|"21218422"|"21434085"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, very stony component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218423"|"21434086"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finn soil is a minor component."|"21218424"|"21434087"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bridger soil is a minor component."|"21218155"|"21433818"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finn soil is a minor component."|"21218156"|"21433819"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, stony component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218157"|"21433820"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hooligan soil is a minor component."|"21218158"|"21433821"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Ratiopeak soil is a minor component."|"21218159"|"21433822"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218160"|"21433823"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, very stony component makes up 31 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218161"|"21433824"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"21218962"|"21434625"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zufelt soil is a minor component."|"21218963"|"21434626"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218964"|"21434627"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-c, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218965"|"21434628"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218966"|"21434629"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset soil is a minor component."|"21218967"|"21434630"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dutchhollow soil is a minor component."|"21218968"|"21434631"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218969"|"21434632"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Narrows soil is a minor component."|"21218970"|"21434633"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Foolhen soil is a minor component."|"21218971"|"21434634"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218972"|"21434635"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trailhollow component makes up 15 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218973"|"21434636"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Woodtick component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on dunes on dune fields, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218974"|"21434637"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lyonsbridge soil is a minor component."|"21218975"|"21434638"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Woodtick soil is a minor component."|"21218976"|"21434639"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sandrift soil is a minor component."|"21218977"|"21434640"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Denied access is a miscellaneous area."|"21218211"|"21433874"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jackrabbit component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on dunes on dune fields, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218978"|"21434641"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beancreek component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, dunes on lakebeds. The parent material consists of eolian deposits over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD110MT Sandy (sy)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21218979"|"21434642"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dutchhollow soil is a minor component."|"21218980"|"21434643"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete, frequently flooded soil is a minor component."|"21218425"|"21434088"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hellroaring soil is a minor component."|"21218426"|"21434089"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 20 percent of the map unit. Slopes are 1 to 3 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218427"|"21434090"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently flooded component makes up 55 percent of the map unit. Slopes are 1 to 3 percent. This component is on flood plains on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218428"|"21434091"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218429"|"21434092"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regulus, frequently flooded soil is a minor component."|"21218430"|"21434093"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, stony component makes up 15 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountains, hills. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218162"|"21433825"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Babb component makes up 35 percent of the map unit. Slopes are 4 to 25 percent. This component is on hills, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218163"|"21433826"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 20 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountains, hills. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218164"|"21433827"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218165"|"21433828"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Doolittle soil is a minor component."|"21218166"|"21433829"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Knep soil is a minor component."|"21218167"|"21433830"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crookedrun soil is a minor component."|"21218168"|"21433831"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Narrows soil is a minor component."|"21218169"|"21433832"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beancreek component makes up 50 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, fan remnants on lakebeds. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD110MT Sandy (sy)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21218431"|"21434094"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lehunt soil is a minor component."|"21218432"|"21434095"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hellroaring soil is a minor component."|"21218433"|"21434096"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 25 percent of the map unit. Slopes are 1 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218434"|"21434097"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Truaxcreek soil is a minor component."|"21218435"|"21434098"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doolittle component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BE001MT Clayey (cy)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218170"|"21433833"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Babb soil is a minor component."|"21218171"|"21433834"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rooset soil is a minor component."|"21218172"|"21433835"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shineberger soil is a minor component."|"21218173"|"21433836"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dutchhollow soil is a minor component."|"21218174"|"21433837"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, swales on mountain slopes. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE001MT Clayey (cy)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218175"|"21433838"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dutchhollow soil is a minor component."|"21218706"|"21434369"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doolittle component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BE161MT Thin Clayey (tcy)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218707"|"21434370"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Babb soil is a minor component."|"21218708"|"21434371"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shineberger soil is a minor component."|"21218709"|"21434372"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rooset soil is a minor component."|"21218710"|"21434373"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, swales on mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE005MT Clayey Steep (cystp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218711"|"21434374"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Raynesford soil is a minor component."|"21218179"|"21433842"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bellcanyon component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE030MT Limy (ly)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218180"|"21433843"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat, stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD031MT Limy Droughty (lydr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218181"|"21433844"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218182"|"21433845"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hardhart soil is a minor component."|"21218183"|"21433846"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE135MT Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218184"|"21433847"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tropal soil is a minor component."|"21218712"|"21434375"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, swales on mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"21218713"|"21434376"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bellcanyon soil is a minor component."|"21218714"|"21434377"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hardhart soil is a minor component."|"21218715"|"21434378"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218716"|"21434379"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD031MT Limy Droughty (lydr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218717"|"21434380"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Regulus soil is a minor component."|"21218718"|"21434381"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Woodtick soil is a minor component."|"21218913"|"21434576"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jackrabbit component makes up 90 percent of the map unit. Slopes are 1 to 6 percent. This component is on dunes on dune fields, intermontane basins. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218914"|"21434577"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge, occasionally flooded soil is a minor component."|"21218572"|"21434235"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on escarpments, hills, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218573"|"21434236"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21218574"|"21434237"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leavitt soil is a minor component."|"21218575"|"21434238"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doolittle component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on escarpments, hills, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Thin Clayey (tcy)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218576"|"21434239"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Knep component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on escarpments, hills, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 43b-e, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent.  The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21218577"|"21434240"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21218578"|"21434241"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit, stony soil is a minor component."|"21218579"|"21434242"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21218293"|"21433956"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21218294"|"21433957"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leavitt component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218295"|"21433958"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge, occasionally flooded soil is a minor component."|"21218296"|"21433959"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doolittle soil is a minor component."|"21218297"|"21433960"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Knep component makes up 15 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, landslides on escarpments. The parent material consists of slide deposits. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE030MT Limy (ly)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent.  The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21218298"|"21433961"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tongue River component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218299"|"21433962"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit, very stony soil is a minor component."|"21218300"|"21433963"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21217976"|"21433639"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit, stony soil is a minor component."|"21217977"|"21433640"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge, occasionally flooded soil is a minor component."|"21217978"|"21433641"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21217979"|"21433642"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tongue River component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on escarpments, hills, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21217980"|"21433643"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on escarpments, hills, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21217981"|"21433644"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doolittle soil is a minor component."|"21217982"|"21433645"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leavitt component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, swales on hills. The parent material consists of slope alluvium and/or colluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21217983"|"21433646"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete, ponded component makes up 25 percent of the map unit. Slopes are 0 to 1 percent. This component is on intermontane basins, bogs on lakebeds. The parent material consists of mucky peat organic material over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during March, April, May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218831"|"21434494"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete component makes up 40 percent of the map unit. Slopes are 0 to 1 percent. This component is on intermontane basins, bogs on lakebeds. The parent material consists of mucky peat organic material over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during March, April, May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218832"|"21434495"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21218833"|"21434496"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dunkleber, frequently ponded component makes up 15 percent of the map unit. Slopes are 0 to 1 percent. This component is on bogs on lakebeds, intermontane basins. The parent material consists of mucky peat organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during March, April, May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 50 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218834"|"21434497"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, landslides. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218301"|"21433964"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218302"|"21433965"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218303"|"21433966"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218304"|"21433967"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"21218305"|"21433968"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218306"|"21433969"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21218593"|"21434256"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leavitt soil is a minor component."|"21218594"|"21434257"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218595"|"21434258"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle, very stony soil is a minor component."|"21218596"|"21434259"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very stony component makes up 40 percent of the map unit. Slopes are 20 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218597"|"21434260"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 30 percent of the map unit. Slopes are 20 to 50 percent. This component is on mountains, swales on mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"21218598"|"21434261"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, stony component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, ridges. The parent material consists of colluvium. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217984"|"21433647"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 35 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21217985"|"21433648"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"21217986"|"21433649"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21217987"|"21433650"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21217988"|"21433651"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21217989"|"21433652"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, very stony component makes up 20 percent of the map unit. Slopes are 15 to 60 percent. This component is on ridges, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217990"|"21433653"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218992"|"21434655"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21218993"|"21434656"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218994"|"21434657"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218995"|"21434658"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218996"|"21434659"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 80 percent of the map unit. Slopes are 2 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of slope alluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218997"|"21434660"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"21218399"|"21434062"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218400"|"21434063"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Henneberry, very stony component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, ridges. The parent material consists of residuum weathered from calcareous conglomerate. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218401"|"21434064"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nikat soil is a minor component."|"21218402"|"21434065"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elispring component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, swales on mountain slopes. The parent material consists of colluvium derived from calcareous conglomerate. Depth to a root restrictive layer, bedrock, lithic, is 21 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218403"|"21434066"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, very stony component makes up 25 percent of the map unit. Slopes are 15 to 50 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21218404"|"21434067"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, calcareous conglomerate soil is a minor component."|"21218791"|"21434454"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg, very stony component makes up 20 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from volcanic breccia. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21218792"|"21434455"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"21218793"|"21434456"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, very stony component makes up 15 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218794"|"21434457"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slagamelt soil is a minor component."|"21218795"|"21434458"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218796"|"21434459"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sicklesteets, very stony component makes up 35 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from calcareous conglomerate. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218797"|"21434460"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, extremely stony soil is a minor component."|"21218798"|"21434461"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Limadam soil is a minor component."|"21218350"|"21434013"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"21218351"|"21434014"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yacreek component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants on lakebeds, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218352"|"21434015"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 60 percent of the map unit. Slopes are 0 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218353"|"21434016"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hellroaring soil is a minor component."|"21218354"|"21434017"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockisland soil is a minor component."|"21218355"|"21434018"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lyonsbridge soil is a minor component."|"21218681"|"21434344"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockisland soil is a minor component."|"21218682"|"21434345"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truaxcreek soil is a minor component."|"21218683"|"21434346"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Littletable soil is a minor component."|"21218684"|"21434347"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants on lakebeds, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218685"|"21434348"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beancreek component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants on lakebeds, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Sandy (sy)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21218686"|"21434349"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Owenspring soil is a minor component."|"21218147"|"21433810"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"21218148"|"21433811"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218149"|"21433812"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218150"|"21433813"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, landslides on mountain valleys. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218151"|"21433814"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218152"|"21433815"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218153"|"21433816"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin, frequently ponded soil is a minor component."|"21218154"|"21433817"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scudder, stony component makes up 25 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218368"|"21434031"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, extremely stony component makes up 25 percent of the map unit. Slopes are 15 to 60 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218369"|"21434032"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal, extremely stony soil is a minor component."|"21218370"|"21434033"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218371"|"21434034"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sicklesteets, very bouldery component makes up 30 percent of the map unit. Slopes are 15 to 60 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218372"|"21434035"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"21218373"|"21434036"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218374"|"21434037"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"21218599"|"21434262"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"21218600"|"21434263"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218601"|"21434264"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"21218602"|"21434265"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218603"|"21434266"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218604"|"21434267"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218605"|"21434268"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, occasionally flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on mountains, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland, Riparian Meadow (rm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218379"|"21434042"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mooseflat, occasionally flooded component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 2 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP801MT Bottomland, Riparian Meadow (rm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218380"|"21434043"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regulus, occasionally flooded soil is a minor component."|"21218381"|"21434044"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Medicinelodge, occasionally flooded component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood-plain steps, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches (depth from the mineral surface is 8 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland, Riparian Meadow (rm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218382"|"21434045"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218383"|"21434046"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slagamelt soil is a minor component."|"21218384"|"21434047"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wisdom soil is a minor component."|"21218385"|"21434048"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218755"|"21434418"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218756"|"21434419"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Regulus, occasionally flooded soil is a minor component."|"21218757"|"21434420"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson, very stony soil is a minor component."|"21218758"|"21434421"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bearmouth, stony soil is a minor component."|"21218759"|"21434422"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218760"|"21434423"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants on lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218185"|"21433848"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lehunt soil is a minor component."|"21218186"|"21433849"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Foolhen soil is a minor component."|"21218187"|"21433850"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beancreek component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants on lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD110MT Sandy (sy)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21218188"|"21433851"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lyonsbridge component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants on lakebeds, intermontane basins. The parent material consists of alluvium over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21218189"|"21433852"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lehunt soil is a minor component."|"21218988"|"21434651"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218989"|"21434652"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218990"|"21434653"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218991"|"21434654"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela, stony component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218548"|"21434211"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, extremely stony component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains, ridges. The parent material consists of colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218549"|"21434212"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"21218550"|"21434213"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very stony component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218551"|"21434214"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss soil is a minor component."|"21218552"|"21434215"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 65 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, ridges. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217961"|"21433624"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges, mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21217962"|"21433625"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"21217963"|"21433626"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21217964"|"21433627"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218287"|"21433950"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 40 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218288"|"21433951"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, very stony component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218289"|"21433952"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle, extremely stony soil is a minor component."|"21218290"|"21433953"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218291"|"21433954"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218292"|"21433955"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218700"|"21434363"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy (lo)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218701"|"21434364"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218702"|"21434365"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218703"|"21434366"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218704"|"21434367"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218705"|"21434368"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP819MT Alpine, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218499"|"21434162"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver, lesser slopes soil is a minor component."|"21218500"|"21434163"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218501"|"21434164"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, stony surface component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hillslopes, hills. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Alpine, Upland Alpine ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218502"|"21434165"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, very stony component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21217942"|"21433605"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin, stony soil is a minor component."|"21217943"|"21433606"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy (lo)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21217944"|"21433607"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, stony component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21217945"|"21433608"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21217946"|"21433609"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218744"|"21434407"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan, stony soil is a minor component."|"21218745"|"21434408"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very stony component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Droughty Steep (drstp)   Lru 43b-d, Upland Alpine ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218746"|"21434409"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218747"|"21434410"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, very stony component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, mountains. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Droughty Steep (drstp)   Lru 43b-d, Upland Alpine ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218748"|"21434411"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver, extremely stony soil is a minor component."|"21218749"|"21434412"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin, stony soil is a minor component."|"21218750"|"21434413"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 70 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-c, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218807"|"21434470"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crookedrun soil is a minor component."|"21218808"|"21434471"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218809"|"21434472"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson, extremely stony soil is a minor component."|"21218810"|"21434473"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on drainageways, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP816MT Subirrigated Sagebrush Shrubland, Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21218811"|"21434474"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, quartzite, limestone soil is a minor component."|"21218096"|"21433759"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, extremely stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218097"|"21433760"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very bouldery component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218098"|"21433761"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, ridges. The parent material consists of slope alluvium and/or colluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218099"|"21433762"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218100"|"21433763"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21218101"|"21433764"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218102"|"21433765"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218275"|"21433938"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, extremely stony component makes up 26 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Unspecified ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218276"|"21433939"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218277"|"21433940"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very stony component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on ridges, mountains, escarpments. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218278"|"21433941"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, stony component makes up 24 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments, ridges, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Unspecified ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218279"|"21433942"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21218280"|"21433943"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle, stony soil is a minor component."|"21218281"|"21433944"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, extremely stony component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218533"|"21434196"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218534"|"21434197"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218535"|"21434198"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, very stony component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218536"|"21434199"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal, stony soil is a minor component."|"21218537"|"21434200"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sicklesteets, very stony soil is a minor component."|"21218538"|"21434201"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21218539"|"21434202"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218540"|"21434203"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218541"|"21434204"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218733"|"21434396"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 85 percent of the map unit. Slopes are 1 to 8 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218734"|"21434397"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, frequently flooded soil is a minor component."|"21218735"|"21434398"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21218736"|"21434399"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"21218737"|"21434400"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scudder, stony component makes up 70 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218488"|"21434151"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin, very stony soil is a minor component."|"21218489"|"21434152"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal soil is a minor component."|"21218490"|"21434153"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218491"|"21434154"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scudder, stony component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21217924"|"21433587"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21217925"|"21433588"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21217926"|"21433589"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hardhart soil is a minor component."|"21217927"|"21433590"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal component makes up 45 percent of the map unit. Slopes are 8 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from limestone and dolomite over calcareous residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21217928"|"21433591"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leavitt soil is a minor component."|"21218606"|"21434269"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218607"|"21434270"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, stony component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, ridges. The parent material consists of slope alluvium and/or colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218608"|"21434271"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218609"|"21434272"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bridger soil is a minor component."|"21218610"|"21434273"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21218307"|"21433970"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"21218308"|"21433971"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218309"|"21433972"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, stony component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218310"|"21433973"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218311"|"21433974"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle, stony soil is a minor component."|"21218312"|"21433975"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, stony component makes up 30 percent of the map unit. Slopes are 20 to 50 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218313"|"21433976"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, very stony component makes up 20 percent of the map unit. Slopes are 25 to 60 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP819MT Limy Droughty (lydr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21218932"|"21434595"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elispring soil is a minor component."|"21218933"|"21434596"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218934"|"21434597"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Briggsranch, extremely bouldery soil is a minor component."|"21218935"|"21434598"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Henneberry, very stony component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on ridges, mountains. The parent material consists of residuum weathered from calcareous conglomerate. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218936"|"21434599"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nikat soil is a minor component."|"21218937"|"21434600"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218216"|"21433879"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 35 percent of the map unit. Slopes are 1 to 8 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218217"|"21433880"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows, saline soil is a minor component."|"21218218"|"21433881"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21218219"|"21433882"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 50 percent of the map unit. Slopes are 1 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218220"|"21433883"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dutchhollow, frequently flooded soil is a minor component."|"21218529"|"21434192"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows, saline soil is a minor component."|"21218530"|"21434193"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 55 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218531"|"21434194"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218532"|"21434195"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hellroaring component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218668"|"21434331"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways on lakebeds, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218669"|"21434332"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Littletable component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, lakebeds. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Saline Upland (su)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218670"|"21434333"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218671"|"21434334"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218672"|"21434335"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Matsingale, frequently ponded soil is a minor component."|"21218673"|"21434336"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Levengood soil is a minor component."|"21218314"|"21433977"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shineberger, extremely stony component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on ridges, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BC135MT Shallow Limy Droughty (swlydr)   Lru 43b-c ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218315"|"21433978"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BC031MT Limy Droughty (lydr)   Lru 43b-c ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218316"|"21433979"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218317"|"21433980"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beancreek, stony component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of loess over slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"21218318"|"21433981"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218413"|"21434076"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218414"|"21434077"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218415"|"21434078"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockisland soil is a minor component."|"21218416"|"21434079"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan soil is a minor component."|"21217888"|"21433551"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban, stony soil is a minor component."|"21217889"|"21433552"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217890"|"21433553"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, very stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217891"|"21433554"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21217892"|"21433555"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21217893"|"21433556"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Briggsranch, very stony soil is a minor component."|"21218492"|"21434155"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madigan soil is a minor component."|"21218493"|"21434156"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21218494"|"21434157"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dalys component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on escarpments, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 3 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland, Very Shallow (vsw)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218495"|"21434158"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, hills. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218496"|"21434159"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, volcanic soil is a minor component."|"21218497"|"21434160"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218498"|"21434161"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21217991"|"21433654"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, extremely bouldery component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21217992"|"21433655"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, stony component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21217993"|"21433656"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on landslides, mountains. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217994"|"21433657"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"21217995"|"21433658"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"21217996"|"21433659"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21217997"|"21433660"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently flooded component makes up 35 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains on drainageways, mountains. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218835"|"21434498"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crookedrun soil is a minor component."|"21218836"|"21434499"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truaxcreek soil is a minor component."|"21218837"|"21434500"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Medicinelodge, frequently flooded component makes up 25 percent of the map unit. Slopes are 1 to 6 percent. This component is on flood plains on drainageways, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 14 inches) during May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland, Meadow (m)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21218838"|"21434501"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 20 percent of the map unit. Slopes are 1 to 4 percent. This component is on mountains, flood plains on drainageways. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland, Meadow (m)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218839"|"21434502"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hardhart, very stony soil is a minor component."|"21218282"|"21433945"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scudder, stony component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218283"|"21433946"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, extremely stony component makes up 35 percent of the map unit. Slopes are 25 to 80 percent. This component is on mountains, mountain slopes, canyon walls. The parent material consists of colluvium derived from limestone and dolomite over calcareous residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE135MT Shallow Cool Woodland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218284"|"21433947"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218285"|"21433948"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"21218286"|"21433949"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scudder, stony soil is a minor component."|"21218767"|"21434430"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218768"|"21434431"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, extremely stony component makes up 25 percent of the map unit. Slopes are 45 to 80 percent. This component is on mountains, mountain slopes, canyon walls. The parent material consists of colluvium derived from limestone and dolomite over calcareous residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE135MT Shallow Cool Woodland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218769"|"21434432"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21218770"|"21434433"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21217914"|"21433577"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford, very stony soil is a minor component."|"21217915"|"21433578"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, very stony component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains, ridges on mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP820MT Droughty Steep (drstp)   Lru 43b-a, Upland Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21217916"|"21433579"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood, extremely stony soil is a minor component."|"21217917"|"21433580"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains, ridges on mountain slopes. The parent material consists of slope alluvium and/or colluvium over residuum weathered from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE135MT Shallow Cool Woodland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21217918"|"21433581"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Briggsranch component makes up 25 percent of the map unit. Slopes are 30 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of residuum weathered from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 4 to 10 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland, Very Shallow (vsw)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 27 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218129"|"21433792"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218130"|"21433793"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shineberger component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, escarpments, mountain slopes. The parent material consists of colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-c, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218131"|"21433794"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218132"|"21433795"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beancreek soil is a minor component."|"21218133"|"21433796"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockisland soil is a minor component."|"21218176"|"21433839"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon soil is a minor component."|"21218177"|"21433840"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on stream terraces, alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218178"|"21433841"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg, greater slopes soil is a minor component."|"21218568"|"21434231"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 25 percent of the map unit. Slopes are 2 to 4 percent. This component is on drainageways, depressions, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218569"|"21434232"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 65 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218570"|"21434233"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Limadam soil is a minor component."|"21218571"|"21434234"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Limadam, silty clay loam soil is a minor component."|"21218559"|"21434222"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Limadam component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043AP811MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218560"|"21434223"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hellroaring soil is a minor component."|"21218561"|"21434224"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Narrows soil is a minor component."|"21218562"|"21434225"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Matsingale, frequently ponded component makes up 25 percent of the map unit. Slopes are 0 to 1 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP814MT Subirrigated Saline-sodic Shrubland ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218840"|"21434503"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hellroaring, frequently ponded component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 31 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218841"|"21434504"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Limadam component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043AP811MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218842"|"21434505"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Narrows soil is a minor component."|"21218843"|"21434506"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Philipsburg soil is a minor component."|"21218844"|"21434507"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Matsingale, frequently ponded component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP814MT Subirrigated Saline-sodic Shrubland ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218845"|"21434508"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Philipsburg soil is a minor component."|"21218846"|"21434509"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218847"|"21434510"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Limadam component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043AP811MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218848"|"21434511"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hellroaring soil is a minor component."|"21218849"|"21434512"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finn soil is a minor component."|"21218850"|"21434513"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218851"|"21434514"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"21218852"|"21434515"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, very stony component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218853"|"21434516"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tibson soil is a minor component."|"21218854"|"21434517"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun, frequently flooded component makes up 20 percent of the map unit. Slopes are 1 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21217998"|"21433661"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21217999"|"21433662"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently flooded component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218000"|"21433663"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Regulus, frequently flooded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 16 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218001"|"21433664"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Foolhen soil is a minor component."|"21218002"|"21433665"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tepete soil is a minor component."|"21218003"|"21433666"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218319"|"21433982"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218320"|"21433983"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tepete soil is a minor component."|"21218321"|"21433984"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Regulus, frequently flooded component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, strongly contrasting textural stratification, is 40 to 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 16 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218322"|"21433985"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dutchhollow soil is a minor component."|"21218323"|"21433986"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bearmouth, very stony component makes up 15 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21218004"|"21433667"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218005"|"21433668"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, stony component makes up 15 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218006"|"21433669"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, frequently flooded soil is a minor component."|"21218007"|"21433670"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218008"|"21433671"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"21218009"|"21433672"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218324"|"21433987"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bearmouth soil is a minor component."|"21218325"|"21433988"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Houlihan soil is a minor component."|"21218326"|"21433989"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 65 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218327"|"21433990"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barbarela, stony soil is a minor component."|"21218010"|"21433673"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 20 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from volcanic and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218011"|"21433674"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very stony component makes up 45 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from volcanic and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218012"|"21433675"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, extremely stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, ridges on mountain slopes. The parent material consists of colluvium over residuum weathered from volcanic and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BD138MT Shallow Cool Woodland, Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218013"|"21433676"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, volcanic soil is a minor component."|"21218014"|"21433677"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullrey soil is a minor component."|"21218015"|"21433678"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Slidemountain soil is a minor component."|"21218611"|"21434274"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville, very bouldery component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218612"|"21434275"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Adel soil is a minor component."|"21218613"|"21434276"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218614"|"21434277"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Elkpeak soil is a minor component."|"21218615"|"21434278"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218616"|"21434279"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Arrowpeak soil is a minor component."|"21218617"|"21434280"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkpeak, stony component makes up 45 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218618"|"21434281"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 20 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountains, swales on mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218619"|"21434282"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218620"|"21434283"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Booneville component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218621"|"21434284"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Booneville soil is a minor component."|"21218622"|"21434285"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arrowpeak, very stony component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218623"|"21434286"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218624"|"21434287"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Boatman soil is a minor component."|"21218625"|"21434288"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Adel soil is a minor component."|"21218626"|"21434289"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkpeak, stony component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218627"|"21434290"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Adel soil is a minor component."|"21218628"|"21434291"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkpeak, stony component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218629"|"21434292"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arrowpeak, very stony component makes up 15 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218630"|"21434293"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Booneville soil is a minor component."|"21218631"|"21434294"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218632"|"21434295"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boatman component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218633"|"21434296"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales, mountains. The parent material consists of alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218016"|"21433679"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218017"|"21433680"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leavitt component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of alluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218018"|"21433681"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Philipsburg soil is a minor component."|"21218019"|"21433682"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sebud soil is a minor component."|"21218020"|"21433683"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"21218328"|"21433991"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218329"|"21433992"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, extremely stony component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on ridges, mountain slopes, mountains. The parent material consists of slope alluvium over residuum weathered from volcanic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"21218330"|"21433993"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium derived from volcanic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218331"|"21433994"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Surdal, stony component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium over residuum weathered from volcanic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218332"|"21433995"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21218021"|"21433684"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, stony component makes up 20 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218022"|"21433685"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, ridges. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218023"|"21433686"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218024"|"21433687"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tiban soil is a minor component."|"21218025"|"21433688"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville, stony component makes up 40 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous, metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218026"|"21433689"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"21218333"|"21433996"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, very stony component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, ridges. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218334"|"21433997"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Ratiopeak soil is a minor component."|"21218335"|"21433998"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland, stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21218336"|"21433999"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218337"|"21434000"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tiban soil is a minor component."|"21218338"|"21434001"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finn soil is a minor component."|"21218339"|"21434002"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Ratiopeak soil is a minor component."|"21218855"|"21434518"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tiban soil is a minor component."|"21218856"|"21434519"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218857"|"21434520"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, very stony component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, ridges. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218858"|"21434521"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Levengood soil is a minor component."|"21218859"|"21434522"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland, stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21218860"|"21434523"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Cheadle soil is a minor component."|"21218861"|"21434524"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doolittle component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BE161MT Thin Clayey (tcy)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218862"|"21434525"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21218863"|"21434526"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218864"|"21434527"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnette soil is a minor component."|"21218865"|"21434528"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Medicinelodge soil is a minor component."|"21218866"|"21434529"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Knep component makes up 20 percent of the map unit. Slopes are 4 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE030MT Limy (ly)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"21218867"|"21434530"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leavitt soil is a minor component."|"21218868"|"21434531"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218674"|"21434337"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218675"|"21434338"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on marshes, intermontane basins. The parent material consists of organic material over  alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during January, February, March, April, May, June, July, August, September, October, November, December. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218676"|"21434339"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hellroaring soil is a minor component."|"21218677"|"21434340"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Limadam soil is a minor component."|"21218678"|"21434341"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yacreek soil is a minor component."|"21218679"|"21434342"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways on lakebeds, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218680"|"21434343"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Matsingale, frequently ponded component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218869"|"21434532"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hellroaring soil is a minor component."|"21218870"|"21434533"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218871"|"21434534"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218872"|"21434535"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete, frequently ponded component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on marshes on lakebeds, intermontane basins. The parent material consists of mucky peat organic material over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during March, April, May, June, July, August, September. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218873"|"21434536"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bellcanyon component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE030MT Limy (ly)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218874"|"21434537"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Trailhollow soil is a minor component."|"21218875"|"21434538"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rockisland soil is a minor component."|"21218876"|"21434539"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 15 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218877"|"21434540"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 20 percent of the map unit. Slopes are 1 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218878"|"21434541"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Regulus, frequently ponded component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21218340"|"21434003"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tepete soil is a minor component."|"21218341"|"21434004"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218342"|"21434005"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Narrows soil is a minor component."|"21218343"|"21434006"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leavitt component makes up 35 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218027"|"21433690"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finn soil is a minor component."|"21218028"|"21433691"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Levengood soil is a minor component."|"21218029"|"21433692"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tiban soil is a minor component."|"21218030"|"21433693"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak component makes up 40 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218031"|"21433694"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leavitt soil is a minor component."|"21218344"|"21434007"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tepete soil is a minor component."|"21218345"|"21434008"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bighole component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218346"|"21434009"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crookedrun component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218347"|"21434010"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Beancreek soil is a minor component."|"21218348"|"21434011"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Foolhen soil is a minor component."|"21218349"|"21434012"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bighole component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218634"|"21434297"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218635"|"21434298"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crookedrun soil is a minor component."|"21218636"|"21434299"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Medicinelodge, frequently flooded component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 14 inches) during May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218637"|"21434300"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tepete soil is a minor component."|"21218638"|"21434301"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finn soil is a minor component."|"21218032"|"21433695"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farlin, very stony component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218033"|"21433696"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland, very bouldery component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21218034"|"21433697"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"21218035"|"21433698"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Philipsburg soil is a minor component."|"21218036"|"21433699"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218812"|"21434475"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218813"|"21434476"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, extremely stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, plateaus on mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218814"|"21434477"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, plateaus on mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218815"|"21434478"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"21218816"|"21434479"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, very stony component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, plateaus on mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE036MT Droughty (dr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21218817"|"21434480"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218268"|"21433931"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, extremely stony soil is a minor component."|"21218269"|"21433932"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218270"|"21433933"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hairpin component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, low hills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Argillic (loa)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218271"|"21433934"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"21218272"|"21433935"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218273"|"21433936"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"21218274"|"21433937"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon soil is a minor component."|"21218212"|"21433875"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin, stony soil is a minor component."|"21218213"|"21433876"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Raynesford soil is a minor component."|"21218214"|"21433877"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat, very stony component makes up 80 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-d, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218215"|"21433878"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bellcanyon component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP805MT Limy (ly)   Lru 43b-e, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218694"|"21434357"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21218695"|"21434358"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Truaxcreek soil is a minor component."|"21218696"|"21434359"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218697"|"21434360"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow component makes up 15 percent of the map unit. Slopes are 1 to 4 percent. This component is on stream terraces, mountains. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218698"|"21434361"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-d, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218699"|"21434362"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218799"|"21434462"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218800"|"21434463"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218801"|"21434464"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"21218802"|"21434465"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, very stony component makes up 30 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountains, mountain slopes, ridges. The parent material consists of colluvium over residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218803"|"21434466"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, extremely bouldery soil is a minor component."|"21218804"|"21434467"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"21218805"|"21434468"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, very stony component makes up 45 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218806"|"21434469"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218751"|"21434414"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madigan soil is a minor component."|"21218752"|"21434415"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, stony component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218753"|"21434416"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely stony component makes up 40 percent of the map unit. Slopes are 8 to 50 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218754"|"21434417"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, hills. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21218123"|"21433786"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shineberger, stony soil is a minor component."|"21218124"|"21433787"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218125"|"21433788"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21218126"|"21433789"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218127"|"21433790"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, mountains. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218128"|"21433791"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"21218503"|"21434166"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak, very stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218504"|"21434167"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218505"|"21434168"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218506"|"21434169"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218507"|"21434170"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218508"|"21434171"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, very stony soil is a minor component."|"21218509"|"21434172"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gullied land soil is a minor component."|"21218140"|"21433803"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockisland, stony, lesser slopes soil is a minor component."|"21218141"|"21433804"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218142"|"21433805"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland, stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21218143"|"21433806"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218144"|"21433807"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218145"|"21433808"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver, very stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218146"|"21433809"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21218117"|"21433780"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Briggsranch soil is a minor component."|"21218118"|"21433781"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 50 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218119"|"21433782"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, conglomerate soil is a minor component."|"21218120"|"21433783"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal soil is a minor component."|"21218121"|"21433784"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218122"|"21433785"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21217885"|"21433548"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crookedrun soil is a minor component."|"21217886"|"21433549"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trailhollow component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces, drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217887"|"21433550"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset, extremely stony soil is a minor component."|"21218909"|"21434572"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger, stony soil is a minor component."|"21218910"|"21434573"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218911"|"21434574"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218912"|"21434575"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, mountains. The parent material consists of slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-d, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218221"|"21433884"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nikat, greater slopes soil is a minor component."|"21218222"|"21433885"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bellcanyon component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, mountains. The parent material consists of slope alluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP805MT Limy (ly)   Lru 43b-e, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218223"|"21433886"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon, greater slopes soil is a minor component."|"21218224"|"21433887"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford, stony component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218455"|"21434118"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat, stony component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD031MT Limy Droughty (lydr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218456"|"21434119"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon soil is a minor component."|"21218457"|"21434120"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin, very stony soil is a minor component."|"21218458"|"21434121"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21218076"|"21433739"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crago, stony component makes up 65 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Droughty (lydr)   Lru 43b-a, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218077"|"21433740"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amesha soil is a minor component."|"21218078"|"21433741"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pensore, extremely stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills, mountains. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland, Shallow Limy Droughty (swlydr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218079"|"21433742"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218513"|"21434176"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Droughty (dr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218514"|"21434177"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218515"|"21434178"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg, greater slopes soil is a minor component."|"21218234"|"21433897"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 75 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, hills. The parent material consists of colluvium derived from metamorphic rock and/or sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BY021ID MOUNTAIN LOAMY 22+ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218235"|"21433898"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver, lesser slopes soil is a minor component."|"21218236"|"21433899"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21218237"|"21433900"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin, extremely stony soil is a minor component."|"21218553"|"21434216"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat, occasionally flooded soil is a minor component."|"21218554"|"21434217"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss soil is a minor component."|"21218555"|"21434218"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21218556"|"21434219"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, extremely stony component makes up 40 percent of the map unit. Slopes are 35 to 75 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21218557"|"21434220"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very stony component makes up 15 percent of the map unit. Slopes are 35 to 75 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21218558"|"21434221"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss soil is a minor component."|"21217954"|"21433617"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21217955"|"21433618"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redchief soil is a minor component."|"21217956"|"21433619"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oro Fino, stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21217957"|"21433620"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, very stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21217958"|"21433621"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely bouldery component makes up 15 percent of the map unit. Slopes are 15 to 25 percent. This component is on mountains, ridges. The parent material consists of colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21217959"|"21433622"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bavdark soil is a minor component."|"21217960"|"21433623"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, very stony component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, low hills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21218818"|"21434481"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, mountains. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218819"|"21434482"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218820"|"21434483"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss soil is a minor component."|"21218821"|"21434484"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oro Fino, stony component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, low hills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD032MT Loamy (lo)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218822"|"21434485"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, extremely stony soil is a minor component."|"21218823"|"21434486"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218824"|"21434487"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes, ridges. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218825"|"21434488"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beechcreek, very stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, paralithic, is 22 to 37 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218826"|"21434489"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eastridge, very stony soil is a minor component."|"21218827"|"21434490"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ermont, extremely stony component makes up 15 percent of the map unit. Slopes are 15 to 25 percent. This component is on ridges, mountains, escarpments. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218828"|"21434491"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218829"|"21434492"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, rhyolite soil is a minor component."|"21218830"|"21434493"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, limestone soil is a minor component."|"21218134"|"21433797"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nikat component makes up 50 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP805MT Limy Droughty (lydr)   Lru 43b-d, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218135"|"21433798"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon soil is a minor component."|"21218136"|"21433799"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountain slopes, ridges, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218137"|"21433800"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21218138"|"21433801"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21218139"|"21433802"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nikat soil is a minor component."|"21218436"|"21434099"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Raynesford component makes up 75 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, hills. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218437"|"21434100"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bellcanyon soil is a minor component."|"21218438"|"21434101"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trailhollow soil is a minor component."|"21218439"|"21434102"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21217929"|"21433592"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverslide soil is a minor component."|"21217930"|"21433593"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21217931"|"21433594"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowcamp soil is a minor component."|"21217932"|"21433595"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bighole soil is a minor component."|"21217933"|"21433596"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn, frequently flooded component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21217934"|"21433597"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eastridge, very stony component makes up 20 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash influenced colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218771"|"21434434"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ermont, extremely stony component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on ridges, mountains, escarpments. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP810MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Grassland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218772"|"21434435"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Euell, very stony soil is a minor component."|"21218773"|"21434436"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218774"|"21434437"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"21218775"|"21434438"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218776"|"21434439"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"21218687"|"21434350"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, frequently ponded, stony soil is a minor component."|"21218688"|"21434351"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bullrey component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE040MT Loamy Steep (lostp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218689"|"21434352"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copperbasin, occasionally flooded soil is a minor component."|"21218690"|"21434353"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, gneiss soil is a minor component."|"21218691"|"21434354"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barbarela component makes up 20 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218692"|"21434355"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, very stony component makes up 20 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountain slopes, mountains, ridges on mountain slopes. The parent material consists of colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218693"|"21434356"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218103"|"21433766"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely stony component makes up 25 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountains, ridges. The parent material consists of slope alluvium and/or colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218104"|"21433767"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, very stony soil is a minor component."|"21218105"|"21433768"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barbarela soil is a minor component."|"21218106"|"21433769"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullrey soil is a minor component."|"21218107"|"21433770"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud, stony component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218108"|"21433771"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scudder, rubbly component makes up 20 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountains, debris avalanches. The parent material consists of debris avalanche deposits derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"21217912"|"21433575"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21217913"|"21433576"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21218954"|"21434617"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218955"|"21434618"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, extremely bouldery component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218956"|"21434619"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218957"|"21434620"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rooset, very stony component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218958"|"21434621"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218959"|"21434622"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Henneberry, very stony soil is a minor component."|"21218960"|"21434623"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Owenspring,  soil is a minor component."|"21218961"|"21434624"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, volcanic soil is a minor component."|"21218580"|"21434243"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218581"|"21434244"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tongue River component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218582"|"21434245"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"21218583"|"21434246"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218584"|"21434247"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Stemple, stony component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218585"|"21434248"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hooligan component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on escarpments, hills, mountains. The parent material consists of slope alluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218586"|"21434249"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Knep soil is a minor component."|"21218587"|"21434250"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doolittle soil is a minor component."|"21218588"|"21434251"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Burnette soil is a minor component."|"21218589"|"21434252"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit, stony soil is a minor component."|"21218590"|"21434253"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leavitt component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, swales on hills. The parent material consists of slope alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218591"|"21434254"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge, occasionally flooded soil is a minor component."|"21218592"|"21434255"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hooligan soil is a minor component."|"21218981"|"21434644"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doolittle component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments, mountains. The parent material consists of colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BE161MT Thin Clayey (tcy)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218982"|"21434645"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Briggsranch, very stony soil is a minor component."|"21218983"|"21434646"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Inabnit, very stony component makes up 20 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218984"|"21434647"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tongue River component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218985"|"21434648"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leavitt soil is a minor component."|"21218986"|"21434649"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21218987"|"21434650"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Taylorspring, very stony component makes up 20 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, hills. The parent material consists of colluvium derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD038MT Droughty Steep (drstp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent.  "|"21218542"|"21434205"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21218543"|"21434206"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copenhaver, extremely stony component makes up 55 percent of the map unit. Slopes are 15 to 50 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD138MT Shallow Droughty (swdr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218544"|"21434207"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218545"|"21434208"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218546"|"21434209"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Comad, extremely stony soil is a minor component."|"21218547"|"21434210"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shineberger, extremely stony soil is a minor component."|"21217894"|"21433557"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21217895"|"21433558"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beancreek, stony component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, escarpments, mountains. The parent material consists of loess over colluvium derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21217896"|"21433559"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sandstone, mudstone soil is a minor component."|"21217897"|"21433560"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-c, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21217898"|"21433561"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hardhart, very stony soil is a minor component."|"21218263"|"21433926"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218264"|"21433927"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21218265"|"21433928"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tropal, very stony soil is a minor component."|"21218266"|"21433929"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Briggsranch component makes up 30 percent of the map unit. Slopes are 35 to 80 percent. This component is on canyons, mountains. The parent material consists of residuum weathered from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 4 to 10 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Sagebrush Shrubland, Very Shallow (vsw)   Lru 43b-d ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 27 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218267"|"21433930"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218375"|"21434038"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 75 percent of the map unit. Slopes are 1 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21218376"|"21434039"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ratiopeak soil is a minor component."|"21218377"|"21434040"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver, very stony soil is a minor component."|"21218378"|"21434041"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy (lo)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218062"|"21433725"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson, rubbly soil is a minor component."|"21218063"|"21433726"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver, very stony soil is a minor component."|"21218064"|"21433727"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson, extremely stony component makes up 55 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-c, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218065"|"21433728"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Briggsranch, very stony soil is a minor component."|"21218761"|"21434424"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hardhart, very stony component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21218762"|"21434425"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farlin, very stony soil is a minor component."|"21218763"|"21434426"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP811MT Shallow Limy Droughty (swlydr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218764"|"21434427"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218765"|"21434428"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scudder soil is a minor component."|"21218766"|"21434429"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crookedrun soil is a minor component."|"21218639"|"21434302"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218640"|"21434303"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truaxcreek component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218641"|"21434304"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218642"|"21434305"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218649"|"21434312"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete, ponded component makes up 30 percent of the map unit. Slopes are 1 to 6 percent. This component is on intermontane basins, raised bogs on lakebeds. The parent material consists of mucky peat organic material over debris avalanche deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21218650"|"21434313"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dunkleber component makes up 60 percent of the map unit. Slopes are 1 to 3 percent. This component is on raised bogs, intermontane basins. The parent material consists of woody organic material over debris avalanche deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during March, April, May, June, July, August, September, October, November. Organic matter content in the surface horizon is about 50 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218651"|"21434314"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete, ponded component makes up 20 percent of the map unit. Slopes are 0 to 1 percent. This component is on intermontane basins, fens on alluvial fans. The parent material consists of mucky peat organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218643"|"21434306"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crookedrun soil is a minor component."|"21218644"|"21434307"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Regulus component makes up 25 percent of the map unit. Slopes are 1 to 3 percent. This component is on fens on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21218645"|"21434308"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete component makes up 35 percent of the map unit. Slopes are 1 to 3 percent. This component is on fens on alluvial fans, intermontane basins. The parent material consists of mucky peat organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218646"|"21434309"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218647"|"21434310"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dunkleber soil is a minor component."|"21218648"|"21434311"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Matsingale, frequently ponded component makes up 20 percent of the map unit. Slopes are 0 to 1 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 1 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 30 within 30 inches of the soil surface."|"21218037"|"21433700"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows, saline component makes up 20 percent of the map unit. Slopes are 1 to 4 percent. This component is on lakebeds, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP813MT Subirrigated Saline-sodic Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21218038"|"21433701"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Narrows soil is a minor component."|"21218039"|"21433702"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tepete, ponded component makes up 40 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, marshes on lakebeds. The parent material consists of mucky peat organic material over lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218040"|"21433703"
03/29/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21218041"|"21433704"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218728"|"21434391"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218729"|"21434392"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"21218730"|"21434393"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218731"|"21434394"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Maciver component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218732"|"21434395"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218205"|"21433868"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"21218206"|"21433869"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21218207"|"21433870"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044XS705MT Silty-droughty (sidr) 9-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218208"|"21433871"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kalsted soil is a minor component."|"21218209"|"21433872"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"21218210"|"21433873"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218197"|"21433860"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218198"|"21433861"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218199"|"21433862"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218200"|"21433863"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on swales on hills, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218201"|"21433864"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21218202"|"21433865"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"21218203"|"21433866"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218204"|"21433867"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shineberger component makes up 10 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium and/or colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BC135MT Shallow Limy Droughty (swlydr)   Lru 43b-c ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218719"|"21434382"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218720"|"21434383"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"21218721"|"21434384"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21218722"|"21434385"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218723"|"21434386"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21218724"|"21434387"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218725"|"21434388"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on intermontane basins, hillslopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BD040MT Loamy Steep (lostp)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218726"|"21434389"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, escarpments, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218727"|"21434390"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashbough, rarely flooded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218459"|"21434122"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neen soil is a minor component."|"21218460"|"21434123"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairway soil is a minor component."|"21218461"|"21434124"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dillon soil is a minor component."|"21218462"|"21434125"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218463"|"21434126"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Threeriv soil is a minor component."|"21218464"|"21434127"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Madbeaver soil is a minor component."|"21218465"|"21434128"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218466"|"21434129"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Newtman soil is a minor component."|"21218467"|"21434130"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rivra soil is a minor component."|"21218474"|"21434137"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sieberell component makes up 25 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (dr)   Lru 44b-a ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21218475"|"21434138"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scravo soil is a minor component."|"21218476"|"21434139"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavwan component makes up 55 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (lo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21218477"|"21434140"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beavwan soil is a minor component."|"21218478"|"21434141"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, very stony soil is a minor component."|"21218479"|"21434142"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 50 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218480"|"21434143"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, very stony component makes up 15 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218481"|"21434144"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"21218482"|"21434145"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, very stony soil is a minor component."|"21218483"|"21434146"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bavdark soil is a minor component."|"21218484"|"21434147"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218485"|"21434148"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218486"|"21434149"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"21218487"|"21434150"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scravo, stony component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments. The parent material consists of colluvium over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA137MT Shallow To Gravel Limy (swgrly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218738"|"21434401"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218739"|"21434402"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trimad soil is a minor component."|"21218740"|"21434403"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21218741"|"21434404"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments. The parent material consists of residuum weathered from calcareous siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA136MT Shallow Loamy (swlo)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218742"|"21434405"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kalsted component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA030MT Limy (ly)   Lru 44b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218743"|"21434406"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fourmile component makes up 65 percent of the map unit. Slopes are 8 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218450"|"21434113"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fourmile, extremely bouldery component makes up 15 percent of the map unit. Slopes are 8 to 25 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21218451"|"21434114"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban, very stony soil is a minor component."|"21218452"|"21434115"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, rarely flooded soil is a minor component."|"21218453"|"21434116"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218454"|"21434117"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, very stony component makes up 35 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218443"|"21434106"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218444"|"21434107"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow, stony component makes up 20 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218445"|"21434108"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibkey soil is a minor component."|"21218446"|"21434109"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shadow component makes up 15 percent of the map unit. Slopes are 15 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R043BE038MT Droughty Steep (drstp)   Lru 43b-e, Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218447"|"21434110"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poin soil is a minor component."|"21218448"|"21434111"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, very stony soil is a minor component."|"21218449"|"21434112"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Newtman soil is a minor component."|"21218468"|"21434131"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21218469"|"21434132"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairway soil is a minor component."|"21218470"|"21434133"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Threeriv, frequently flooded component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BY080MT Riparian Meadow (rm)   Lru 44b-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218471"|"21434134"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beavrock, occasionally flooded component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches (depth from the mineral surface is 21 inches) during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218472"|"21434135"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashbough soil is a minor component."|"21218473"|"21434136"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218225"|"21433888"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely bouldery component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP811MT Shallow Droughty (swdr)   Lru 43b-d, Shallow Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218226"|"21433889"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21218227"|"21433890"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, extremely stony component makes up 41 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218510"|"21434173"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, stony component makes up 39 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218511"|"21434174"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ratiopeak component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218512"|"21434175"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218089"|"21433752"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Slagamelt component makes up 25 percent of the map unit. Slopes are 0 to 8 percent. This component is on intermontane basins, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP907MT Subirrigated Cool Woodland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"21218090"|"21433753"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21218091"|"21433754"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mooseflat, occasionally flooded soil is a minor component."|"21218092"|"21433755"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hairpin, stony component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium and/or lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218093"|"21433756"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tepete soil is a minor component."|"21218094"|"21433757"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin, frequently ponded, stony soil is a minor component."|"21218095"|"21433758"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21217935"|"21433598"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on swales on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21217936"|"21433599"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foolhen, frequently flooded component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21217937"|"21433600"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn, frequently flooded soil is a minor component."|"21217938"|"21433601"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger soil is a minor component."|"21217939"|"21433602"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"21217940"|"21433603"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowcamp component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21217941"|"21433604"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bronec, stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP819MT Limy Droughty (lydr)   Lru 43b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21217947"|"21433610"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gullied land soil is a minor component."|"21217948"|"21433611"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Polaris, stony soil is a minor component."|"21217949"|"21433612"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21217950"|"21433613"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson, stony soil is a minor component."|"21217951"|"21433614"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Levengood soil is a minor component."|"21217952"|"21433615"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec, extremely stony soil is a minor component."|"21217953"|"21433616"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson, stony soil is a minor component."|"21218409"|"21434072"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tibson component makes up 70 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, fan remnants. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Limy Droughty (lydr)   Lru 43b-c, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218410"|"21434073"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218411"|"21434074"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockisland soil is a minor component."|"21218412"|"21434075"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, basalt, rhyolite tuff soil is a minor component."|"21218109"|"21433772"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nieman, extremely stony component makes up 15 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from volcanic breccia. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP810MT Shallow Droughty (swdr)   Lru 43b-e, Shallow Grassland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218110"|"21433773"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"21218111"|"21433774"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin, very stony soil is a minor component."|"21218112"|"21433775"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Droughty Steep (drstp)   Lru 43b-e, Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218113"|"21433776"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218114"|"21433777"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Butchhill, very stony component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from volcanic breccia. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Droughty Steep (drstp)   Lru 43b-e, Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218115"|"21433778"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"21218116"|"21433779"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Maciver soil is a minor component."|"21218524"|"21434187"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Truaxcreek component makes up 60 percent of the map unit. Slopes are 1 to 8 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 31 inches (depth from the mineral surface is 30 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218525"|"21434188"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tiban soil is a minor component."|"21218526"|"21434189"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dutchhollow, frequently flooded component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer, abrupt textural change, is 20 to 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218527"|"21434190"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crookedrun soil is a minor component."|"21218528"|"21434191"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218066"|"21433729"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald, frequently ponded, stony soil is a minor component."|"21218067"|"21433730"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Butchhill, very stony component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on mountains, low hills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty (dr)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21218068"|"21433731"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218069"|"21433732"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Donald, stony component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, low hills. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Argillic (loa)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218070"|"21433733"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, stony soil is a minor component."|"21218071"|"21433734"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, extremely bouldery soil is a minor component."|"21218901"|"21434564"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, very stony soil is a minor component."|"21218902"|"21434565"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218903"|"21434566"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218904"|"21434567"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218905"|"21434568"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Donald, stony component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218906"|"21434569"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Butchhill, very stony component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218907"|"21434570"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Donald, frequently ponded, stony soil is a minor component."|"21218908"|"21434571"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rocko, stony component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218057"|"21433720"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dalys soil is a minor component."|"21218058"|"21433721"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218059"|"21433722"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, extremely stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE138MT Shallow Droughty (swdr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218060"|"21433723"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"21218061"|"21433724"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shineberger, extremely stony soil is a minor component."|"21217965"|"21433628"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Knep, stony component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP805MT Limy (ly)   Lru 43b-e, Limy Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 16 percent.  The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21217966"|"21433629"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21217967"|"21433630"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset soil is a minor component."|"21217968"|"21433631"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Loamy Argillic (loa)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21217969"|"21433632"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21217970"|"21433633"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sandstone soil is a minor component."|"21217971"|"21433634"
08/26/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Narrows component makes up 65 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP817MT Subirrigated Shrubland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 24 percent.  "|"21218563"|"21434226"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Limadam component makes up 20 percent of the map unit. Slopes are 4 to 8 percent. This component is on intermontane basins, lakebeds. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP819MT Limy (ly)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218564"|"21434227"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Limadam, silty clay soil is a minor component."|"21218565"|"21434228"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hellroaring soil is a minor component."|"21218566"|"21434229"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21218567"|"21434230"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shineberger, very stony component makes up 15 percent of the map unit. Slopes are 4 to 8 percent. This component is on ridges, mountains. The parent material consists of slope alluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BD133MT Shallow Sandy (swsy)   Lru 43b-d ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21217972"|"21433635"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Philipsburg soil is a minor component."|"21217973"|"21433636"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tibson soil is a minor component."|"21217974"|"21433637"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockisland component makes up 70 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BD036MT Droughty (dr)   Lru 43b-d ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 32 percent.  "|"21217975"|"21433638"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule, very stony component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, ridges, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21218879"|"21434542"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Currycreek component makes up 30 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218880"|"21434543"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville soil is a minor component."|"21218881"|"21434544"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water, sag ponds soil is a minor component."|"21218882"|"21434545"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pricepeet component makes up 15 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218883"|"21434546"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218884"|"21434547"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tophat soil is a minor component."|"21218885"|"21434548"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slidemountain, extremely bouldery soil is a minor component."|"21218886"|"21434549"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule, very stony component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountain slopes, ridges, mountains. The parent material consists of slope alluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21218887"|"21434550"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Currycreek component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218888"|"21434551"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowmule, very stony, greater slopes soil is a minor component."|"21218889"|"21434552"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218890"|"21434553"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water, sag ponds soil is a minor component."|"21218891"|"21434554"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como, stony component makes up 75 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218892"|"21434555"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boatman soil is a minor component."|"21218893"|"21434556"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, extremely stony soil is a minor component."|"21218894"|"21434557"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sedimentary soil is a minor component."|"21218895"|"21434558"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water, sag ponds soil is a minor component."|"21218356"|"21434019"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218357"|"21434020"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Medicinelodge soil is a minor component."|"21218358"|"21434021"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slidemountain, extremely bouldery soil is a minor component."|"21218359"|"21434022"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chicken,  component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218360"|"21434023"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pricepeet, very stony component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218361"|"21434024"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Currycreek soil is a minor component."|"21218362"|"21434025"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Como soil is a minor component."|"21218652"|"21434315"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville, very bouldery component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218653"|"21434316"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boatman, very stony component makes up 35 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218654"|"21434317"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Currycreek soil is a minor component."|"21218655"|"21434318"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tophat soil is a minor component."|"21218656"|"21434319"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Como component makes up 15 percent of the map unit. Slopes are 35 to 80 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21218657"|"21434320"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boatman, very stony component makes up 45 percent of the map unit. Slopes are 35 to 80 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21218658"|"21434321"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, extremely stony soil is a minor component."|"21218659"|"21434322"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville, very bouldery component makes up 25 percent of the map unit. Slopes are 35 to 80 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218660"|"21434323"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218661"|"21434324"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chutes soil is a minor component."|"21218662"|"21434325"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21218663"|"21434326"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree, talus soil is a minor component."|"21218664"|"21434327"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nemesis, extremely bouldery component makes up 20 percent of the map unit. Slopes are 45 to 80 percent. This component is on mountains, mountain slopes, avalanche chutes. The parent material consists of slide deposits and/or colluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21218665"|"21434328"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chutes is a miscellaneous area."|"21218666"|"21434329"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boatman, very stony soil is a minor component."|"21218667"|"21434330"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"21218896"|"21434559"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218897"|"21434560"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chicken,  soil is a minor component."|"21218898"|"21434561"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boatman component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from igneous and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218899"|"21434562"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Targhee, bouldery component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218900"|"21434563"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wesdy,  component makes up 70 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21218405"|"21434068"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wesdy, greater slopes soil is a minor component."|"21218406"|"21434069"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218407"|"21434070"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wesdy, extremely bouldery component makes up 15 percent of the map unit. Slopes are 4 to 12 percent. This component is on ridges, mountains. The parent material consists of slope alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21218408"|"21434071"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, extremely stony soil is a minor component."|"21218047"|"21433710"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Currycreek soil is a minor component."|"21218048"|"21433711"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218049"|"21433712"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yellowmule component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, landslides on mountain slopes. The parent material consists of slide deposits derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218050"|"21433713"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tongue River component makes up 45 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218051"|"21433714"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218052"|"21433715"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218363"|"21434026"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP821MT Loamy Steep (lostp)   Lru 43b-e, Upland Alpine ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218364"|"21434027"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Burnette component makes up 45 percent of the map unit. Slopes are 15 to 50 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP821MT Loamy Steep (lostp)   Lru 43b-e, Upland Alpine ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21218365"|"21434028"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boatman soil is a minor component."|"21218366"|"21434029"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, extremely stony soil is a minor component."|"21218367"|"21434030"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Adel component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BE032MT Loamy (lo)   Lru 43b-e ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218053"|"21433716"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boatman, stony component makes up 50 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of slope alluvium and/or colluvium derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218054"|"21433717"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, talus soil is a minor component."|"21218055"|"21433718"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chutes soil is a minor component."|"21218056"|"21433719"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, extremely stony soil is a minor component."|"21218228"|"21433891"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218229"|"21433892"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monaberg component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218230"|"21433893"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, stony component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills, intermontane basins. The parent material consists of slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218231"|"21433894"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218232"|"21433895"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hairpin soil is a minor component."|"21218233"|"21433896"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218042"|"21433705"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218043"|"21433706"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonniebee, stony component makes up 40 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from igneous rock over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 33 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218044"|"21433707"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tophat soil is a minor component."|"21218045"|"21433708"
09/01/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Slidemountain, extremely stony component makes up 15 percent of the map unit. Slopes are 25 to 45 percent. This component is on mountains, ridges. The parent material consists of colluvium over residuum weathered from igneous and sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21218046"|"21433709"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leavitt soil is a minor component."|"21218440"|"21434103"
09/08/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Houlihan soil is a minor component."|"21218441"|"21434104"
08/25/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridger component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218442"|"21434105"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21218947"|"21434610"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullrey, lesser slopes soil is a minor component."|"21218948"|"21434611"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rooset, greater slopes soil is a minor component."|"21218949"|"21434612"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Knep soil is a minor component."|"21218950"|"21434613"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blaine, very stony surface component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, hills. The parent material consists of colluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BY021ID MOUNTAIN LOAMY 22+ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21218951"|"21434614"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle, extremely stony surface component makes up 15 percent of the map unit. Slopes are 15 to 25 percent. This component is on ridges, hills. The parent material consists of colluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BY018ID Shallow Sagebrush Shrubland, SOUTH SLOPE STONY22+ PSSP6-FEID ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218952"|"21434615"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg, greater slopes component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hillslopes, hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BY021ID MOUNTAIN LOAMY 22+ FEID/POGR9-GEVI2, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218953"|"21434616"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, conglomerate soil is a minor component."|"21218777"|"21434440"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, scree soil is a minor component."|"21218778"|"21434441"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen soil is a minor component."|"21218779"|"21434442"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Houlihan component makes up 15 percent of the map unit. Slopes are 20 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from conglomerate. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Loamy Steep (lostp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218780"|"21434443"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"21218781"|"21434444"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, stony soil is a minor component."|"21218782"|"21434445"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nieman, very stony soil is a minor component."|"21218783"|"21434446"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, very stony component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on ridges, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Droughty Steep (drstp)   Lru 43b-e, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21218784"|"21434447"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tiban, extremely stony component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on escarpments, ridges, mountains. The parent material consists of colluvium derived from conglomerate. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21218785"|"21434448"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Levengood, extremely stony component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 21 percent.  "|"21218190"|"21433853"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tropal, rubbly component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from limestone and dolomite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP805MT Limy Sagebrush Shrubland, Shallow Limy Droughty (swlydr)   Lru 43b-e ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21218191"|"21433854"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Philipsburg, extremely stony component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on landslides on mountain slopes, mountains. The parent material consists of slide deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP819MT Loamy Steep (lostp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21218192"|"21433855"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Inabnit, very stony soil is a minor component."|"21218193"|"21433856"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger, very stony soil is a minor component."|"21218194"|"21433857"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doolittle, very stony soil is a minor component."|"21218195"|"21433858"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bridger, frequently ponded, stony soil is a minor component."|"21218196"|"21433859"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Butchhill, frequently ponded, stony soil is a minor component."|"21218938"|"21434601"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve, very stony soil is a minor component."|"21218939"|"21434602"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21218940"|"21434603"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Butchhill, very stony component makes up 15 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21218941"|"21434604"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monaberg soil is a minor component."|"21218942"|"21434605"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg, extremely stony component makes up 55 percent of the map unit. Slopes are 8 to 25 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP819MT Droughty Steep (drstp)   Lru 43b-d, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21218943"|"21434606"
02/11/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, quartzite soil is a minor component."|"21218944"|"21434607"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, stony soil is a minor component."|"21218945"|"21434608"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Droughty (dr)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218072"|"21433735"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bronec soil is a minor component."|"21218073"|"21433736"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trimad, extremely stony component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Droughty (dr)   Lru 44b-a, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 26 percent.  "|"21218074"|"21433737"
02/26/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Coyoteflats, rubbly component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Rubbly (ry)   Lru 43b-c, Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 19 percent.  "|"21218075"|"21433738"
