07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21226952"|"21442816"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226953"|"21442817"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"21226954"|"21442818"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226777"|"21442641"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"21226778"|"21442642"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21226779"|"21442643"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, intermontane basins. The parent material consists of alluvium and/or colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA036MT Droughty (Dr)   LRU 43A-A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21226780"|"21442644"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger soil is a minor component."|"21226781"|"21442645"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"21226782"|"21442646"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowlake component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB033MT Loamy Argillic (Loa)   LRU 44A-B ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21226783"|"21442647"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB036MT Droughty (Dr)   LRU 44A-B ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"21226784"|"21442648"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm, greater slope soil is a minor component."|"21226941"|"21442805"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226942"|"21442806"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226943"|"21442807"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills, intermontane basins. The parent material consists of colluvium over residuum weathered from argillite and/or quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (Swdr)   LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21226944"|"21442808"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm, greater slopes soil is a minor component."|"21226945"|"21442809"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills, intermontane basins. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA038MT Droughty Steep (Drstp)   LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226946"|"21442810"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"21226947"|"21442811"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226977"|"21442841"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tamarack soil is a minor component."|"21226978"|"21442842"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mitten soil is a minor component."|"21226979"|"21442843"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lozeau, deep component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on escarpments, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226980"|"21442844"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on escarpments, mountains. The parent material consists of volcanic ash over till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226981"|"21442845"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on escarpments, mountains. The parent material consists of till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227007"|"21442871"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226998"|"21442862"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Combest soil is a minor component."|"21226999"|"21442863"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21227000"|"21442864"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mitten soil is a minor component."|"21227001"|"21442865"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227002"|"21442866"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227003"|"21442867"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lozeau soil is a minor component."|"21227004"|"21442868"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lozeau soil is a minor component."|"21226934"|"21442798"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227005"|"21442869"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"21227006"|"21442870"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227032"|"21442896"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lozeau, deep soil is a minor component."|"21227033"|"21442897"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227034"|"21442898"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226935"|"21442799"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226936"|"21442800"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 90 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226937"|"21442801"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"21226938"|"21442802"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227035"|"21442899"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tevis soil is a minor component."|"21227036"|"21442900"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mitten soil is a minor component."|"21227037"|"21442901"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tevis soil is a minor component."|"21226939"|"21442803"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21226940"|"21442804"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mitten soil is a minor component."|"21226966"|"21442830"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21227038"|"21442902"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227039"|"21442903"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21227040"|"21442904"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227066"|"21442930"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig, greater slope soil is a minor component."|"21226958"|"21442822"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226959"|"21442823"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226967"|"21442831"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21226968"|"21442832"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Stevie soil is a minor component."|"21226969"|"21442833"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226970"|"21442834"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway, cool soil is a minor component."|"21227067"|"21442931"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227068"|"21442932"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from argillite or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227069"|"21442933"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"21227070"|"21442934"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from argillite or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227008"|"21442872"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21227009"|"21442873"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway, cool soil is a minor component."|"21227010"|"21442874"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227011"|"21442875"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"21227012"|"21442876"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21227396"|"21443260"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till and/or drift derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227397"|"21443261"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 35 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till and/or drift. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227398"|"21443262"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227399"|"21443263"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"21227400"|"21443264"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Winkler soil is a minor component."|"21226955"|"21442819"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, mountain slopes. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21226956"|"21442820"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21226957"|"21442821"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226971"|"21442835"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"21226972"|"21442836"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Combest soil is a minor component."|"21226973"|"21442837"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21226982"|"21442846"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21226983"|"21442847"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226984"|"21442848"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 20 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226985"|"21442849"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glaciercreek soil is a minor component."|"21226986"|"21442850"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226960"|"21442824"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"21226931"|"21442795"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Combest soil is a minor component."|"21226930"|"21442794"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226929"|"21442793"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Winkler soil is a minor component."|"21226928"|"21442792"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 40 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226933"|"21442797"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mitten soil is a minor component."|"21226932"|"21442796"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 30 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite and/or siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226897"|"21442761"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21226896"|"21442760"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Combest soil is a minor component."|"21226895"|"21442759"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226894"|"21442758"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226927"|"21442791"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigdraw component makes up 30 percent of the map unit. Slopes are 30 to 50 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21226926"|"21442790"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226925"|"21442789"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226924"|"21442788"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226902"|"21442766"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigdraw component makes up 35 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AB040MT Loamy Steep (lostp)   Lru 43a-b ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21226901"|"21442765"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 55 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (swdr)   Lru 43a-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226900"|"21442764"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226899"|"21442763"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bigdraw soil is a minor component."|"21226898"|"21442762"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (swdr)   Lru 43a-a ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226870"|"21442734"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigdraw component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB032MT Loamy (lo)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21226869"|"21442733"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226868"|"21442732"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bigarm soil is a minor component."|"21226920"|"21442784"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226919"|"21442783"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigdraw component makes up 20 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AB040MT Loamy Steep (lostp)   Lru 43a-b ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21226918"|"21442782"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 50 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (swdr)   Lru 43a-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226917"|"21442781"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226916"|"21442780"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hogsby component makes up 20 percent of the map unit. Slopes are 8 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from argillite and/or quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (Swdr)   LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21226915"|"21442779"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on hills. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA038MT Droughty Steep (Drstp)   LRU 43A-A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226914"|"21442778"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226913"|"21442777"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226912"|"21442776"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"21226888"|"21442752"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226887"|"21442751"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226886"|"21442750"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler, cool component makes up 40 percent of the map unit. Slopes are 8 to 40 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226885"|"21442749"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott, cool component makes up 25 percent of the map unit. Slopes are 8 to 40 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium or residuum derived from argillite or quartzite. Depth to a root restrictive layer, bedrock, lithic,  inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP906MT SHALLOW WARM WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226884"|"21442748"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McLangor component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on mountains, flood plains. The parent material consists of organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY182MT Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21226893"|"21442757"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Meadowpeak component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY080MT Riparian Meadow (rm)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.   "|"21226892"|"21442756"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21226891"|"21442755"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bowlake soil is a minor component."|"21226890"|"21442754"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Biglake soil is a minor component."|"21226889"|"21442753"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Biglake soil is a minor component."|"21226852"|"21442716"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Biglake component makes up 90 percent of the map unit. Slopes are 0 to 8 percent. This component is on drainageways, stream terraces, alluvial fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB134MT Shallow To Gravel (swgr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21226851"|"21442715"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lozeau soil is a minor component."|"21226850"|"21442714"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21226849"|"21442713"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pashua component makes up 90 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226848"|"21442712"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lozeau soil is a minor component."|"21226863"|"21442727"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lozeau soil is a minor component."|"21226862"|"21442726"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lozeau component makes up 85 percent of the map unit. Slopes are 30 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226817"|"21442681"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21226816"|"21442680"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226815"|"21442679"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lozeau soil is a minor component."|"21226847"|"21442711"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lozeau component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226846"|"21442710"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21226845"|"21442709"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226844"|"21442708"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Meadowpass soil is a minor component."|"21226822"|"21442686"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226821"|"21442685"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Meadowpass component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB033MT Loamy Argillic (loa)   Lru 44a-b ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21226820"|"21442684"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226880"|"21442744"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 90 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (swdr)   Lru 43a-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226861"|"21442725"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226860"|"21442724"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bigarm soil is a minor component."|"21226911"|"21442775"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Finleypoint soil is a minor component."|"21226910"|"21442774"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226909"|"21442773"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226908"|"21442772"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bowlake soil is a minor component."|"21226907"|"21442771"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Minesinger soil is a minor component."|"21226879"|"21442743"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger, stony component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, stream terraces, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB036MT Droughty (dr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"21226878"|"21442742"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowlake soil is a minor component."|"21226859"|"21442723"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger, greater slope soil is a minor component."|"21226858"|"21442722"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans, stream terraces, intermontane basins. The parent material consists of tertiary alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA036MT Droughty (Dr)   LRU 44A-A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"21226857"|"21442721"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Minesinger, stony soil is a minor component."|"21226819"|"21442683"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Camascreek soil is a minor component."|"21226818"|"21442682"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint soil is a minor component."|"21226856"|"21442720"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226855"|"21442719"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"21226854"|"21442718"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226853"|"21442717"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"21226877"|"21442741"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"21226876"|"21442740"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226875"|"21442739"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226874"|"21442738"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AB038MT Droughty Steep (Drstp)   LRU 43A-B ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226873"|"21442737"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bigarm soil is a minor component."|"21226872"|"21442736"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hogsby soil is a minor component."|"21226871"|"21442735"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Minesinger soil is a minor component."|"21226843"|"21442707"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, intermontane basins. The parent material consists of alluvium and/or colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AB036MT Droughty (dr)   Lru 43a-b ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21226842"|"21442706"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226841"|"21442705"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"21226834"|"21442698"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"21226833"|"21442697"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 90 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA038MT Droughty Steep (Drstp)   LRU 43A-A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226832"|"21442696"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226831"|"21442695"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226830"|"21442694"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bigarm soil is a minor component."|"21226829"|"21442693"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Minesinger soil is a minor component."|"21226828"|"21442692"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigarm component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills, intermontane basins. The parent material consists of alluvium and/or colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB036MT Droughty (dr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"21226827"|"21442691"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"21226814"|"21442678"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till and/or drift derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226813"|"21442677"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21226812"|"21442676"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21226811"|"21442675"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21226810"|"21442674"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"21226836"|"21442700"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"21226835"|"21442699"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226792"|"21442656"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21226791"|"21442655"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226826"|"21442690"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"21226800"|"21442664"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"21226799"|"21442663"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226798"|"21442662"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226809"|"21442673"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226808"|"21442672"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 90 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226807"|"21442671"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21226806"|"21442670"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"21226805"|"21442669"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226804"|"21442668"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from argillite and quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226803"|"21442667"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"21226802"|"21442666"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21226801"|"21442665"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21226961"|"21442825"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockhill soil is a minor component."|"21226962"|"21442826"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Stevie soil is a minor component."|"21226963"|"21442827"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 20 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226964"|"21442828"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 40 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21226965"|"21442829"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227071"|"21442935"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 55 percent of the map unit. Slopes are 15 to 50 percent. This component is on glacially scoured ridges on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP905MT Shallow Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227072"|"21442936"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on glacially scoured ridges on mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227073"|"21442937"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226987"|"21442851"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 15 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226988"|"21442852"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glaciercreek soil is a minor component."|"21226989"|"21442853"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Stevie component makes up 15 percent of the map unit. Slopes are 30 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP902MT Ashy Cool-moist Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227024"|"21442888"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 55 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227025"|"21442889"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21227026"|"21442890"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"21227027"|"21442891"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"21227028"|"21442892"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lynchlake soil is a minor component."|"21227029"|"21442893"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227030"|"21442894"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 55 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227031"|"21442895"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21227058"|"21442922"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227178"|"21443042"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 15 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines on mountain slopes, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227179"|"21443043"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"21227206"|"21443070"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Stevie soil is a minor component."|"21227207"|"21443071"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"21227208"|"21443072"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21227209"|"21443073"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 35 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines on mountain slopes, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227210"|"21443074"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 25 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines on mountain slopes, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227211"|"21443075"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227013"|"21442877"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 55 percent of the map unit. Slopes are 15 to 50 percent. This component is on glacially scoured ridges, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP905MT Shallow Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227014"|"21442878"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on glacially scoured ridges, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227015"|"21442879"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Glaciercreek soil is a minor component."|"21227074"|"21442938"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lynchlake soil is a minor component."|"21227100"|"21442964"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227101"|"21442965"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Courville soil is a minor component."|"21227102"|"21442966"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227103"|"21442967"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Meadowpeak soil is a minor component."|"21227104"|"21442968"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tallcreek soil is a minor component."|"21227105"|"21442969"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McGregor component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on closed depressions, intermontane basins. The parent material consists of volcanic ash over alluvium and/or lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y, Subirrigated Grassland 43a Lru P ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.   "|"21227106"|"21442970"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacklake component makes up 20 percent of the map unit. Slopes are 0 to 1 percent. This component is on depressions, intermontane basins. The parent material consists of organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY071MT Pothole (ph)   Lru 44a-y, Subirrigated Grassland 43a Lru P ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21227107"|"21442971"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Meadowpeak component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY080MT Bottomland 43a Lru P, Riparian Meadow (rm)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.   "|"21227132"|"21442996"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostprairie soil is a minor component."|"21227133"|"21442997"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barzee soil is a minor component."|"21227134"|"21442998"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McLangor soil is a minor component."|"21227059"|"21442923"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacklake soil is a minor component."|"21227060"|"21442924"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak soil is a minor component."|"21227061"|"21442925"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McGregor soil is a minor component."|"21227062"|"21442926"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barzee component makes up 80 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, intermontane basins. The parent material consists of organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AY182MT Bottomland 43a Lru P, Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21227063"|"21442927"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tallcreek component makes up 20 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces, intermontane basins. The parent material consists of volcanic ash over glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21226990"|"21442854"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackcreek component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 20 inches during April, May. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 4w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21226991"|"21442855"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McGregor component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, flood plains. The parent material consists of volcanic ash over alluvium and/or lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.   "|"21226992"|"21442856"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackcreek component makes up 80 percent of the map unit. Slopes are 0 to 8 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 20 inches during April, May. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AH003MT Wet Meadow ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227064"|"21442928"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tallcreek soil is a minor component."|"21227065"|"21442929"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak, occasionally flooded soil is a minor component."|"21227092"|"21442956"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tamarack soil is a minor component."|"21227093"|"21442957"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227041"|"21442905"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haskillpass component makes up 20 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AB040MT Loamy Steep (lostp)   Lru 43a-b ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227042"|"21442906"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227043"|"21442907"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21227044"|"21442908"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227045"|"21442909"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21227046"|"21442910"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McLangor component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, depressions, intermontane basins. The parent material consists of organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY182MT Bottomland 43a Lru P, Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21227076"|"21442940"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacklake soil is a minor component."|"21227077"|"21442941"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak soil is a minor component."|"21227078"|"21442942"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McGregor soil is a minor component."|"21227079"|"21442943"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barzee component makes up 30 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains, depressions, intermontane basins. The parent material consists of organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AY182MT Bottomland 43a Lru P, Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21227080"|"21442944"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak, occasionally flooded soil is a minor component."|"21227047"|"21442911"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barzee soil is a minor component."|"21227048"|"21442912"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacklake component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions, intermontane basins. The parent material consists of organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AH008MT POTHOLE ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21227049"|"21442913"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McLangor soil is a minor component."|"21227075"|"21442939"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dahlake component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on lake terraces, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AY092MT Bottomland 43a Lru P, Bottomland 44a Lru P, Saline Subirrigated (ssb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 7s.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 28 within 30 inches of the soil surface."|"21226993"|"21442857"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitebear component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on lake terraces, intermontane basins. The parent material consists of lacustrine deposits. Depth to a root restrictive layer, natric, is 8 to 18 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AY092MT Bottomland 43a Lru P, Bottomland 44a Lru P, Saline Subirrigated (ssb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 25 within 30 inches of the soil surface."|"21226994"|"21442858"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak soil is a minor component."|"21226995"|"21442859"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21226903"|"21442767"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226904"|"21442768"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigdraw component makes up 40 percent of the map unit. Slopes are 8 to 30 percent. This component is on hills. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"21226905"|"21442769"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226906"|"21442770"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lynchlake, dry component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on collapsed lake plains, intermontane basins. The parent material consists of volcanic ash over glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21226996"|"21442860"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lynchlake soil is a minor component."|"21226997"|"21442861"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pleasantvalley soil is a minor component."|"21227016"|"21442880"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Courville soil is a minor component."|"21227017"|"21442881"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on collapsed lake plains, intermontane basins. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21227018"|"21442882"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Half Moon soil is a minor component."|"21227019"|"21442883"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tallcreek soil is a minor component."|"21227020"|"21442884"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on collapsed lake plains, intermontane basins. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227110"|"21442974"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Auggie soil is a minor component."|"21227111"|"21442975"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crystalex soil is a minor component."|"21227112"|"21442976"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lynchlake component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on collapsed lake plains, intermontane basins. The parent material consists of volcanic ash over glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227113"|"21442977"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glaciercreek soil is a minor component."|"21227114"|"21442978"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis, dry soil is a minor component."|"21226837"|"21442701"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 90 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226838"|"21442702"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"21226839"|"21442703"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226840"|"21442704"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227021"|"21442885"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227022"|"21442886"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21227023"|"21442887"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pashua component makes up 55 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227050"|"21442914"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pashua soil is a minor component."|"21227051"|"21442915"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227135"|"21442999"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21227136"|"21443000"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21227137"|"21443001"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pashua component makes up 45 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227138"|"21443002"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pashua, deep component makes up 30 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227139"|"21443003"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"21227094"|"21442958"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227095"|"21442959"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227096"|"21442960"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 85 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from argillite or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227097"|"21442961"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway, cool soil is a minor component."|"21227098"|"21442962"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21227099"|"21442963"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227116"|"21442980"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills, intermontane basins. The parent material consists of colluvium over residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA136MT Shallow Loamy (swlo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227117"|"21442981"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21227081"|"21442945"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227082"|"21442946"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 45 percent of the map unit. Slopes are 15 to 60 percent. This component is on glacially scoured ridges, mountains. The parent material consists of colluvium over residuum weathered from quartzite and/or argillite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP905MT Shallow Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227083"|"21442947"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 20 percent of the map unit. Slopes are 15 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from quartzite and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227108"|"21442972"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pleasantvalley soil is a minor component."|"21227109"|"21442973"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haskillpass component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AB040MT Loamy Steep (lostp)   Lru 43a-b ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227052"|"21442916"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on moraines, mountains. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227053"|"21442917"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wimper soil is a minor component."|"21227054"|"21442918"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227055"|"21442919"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227056"|"21442920"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21227115"|"21442979"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Winkler soil is a minor component."|"21227156"|"21443020"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 30 percent of the map unit. Slopes are 40 to 70 percent. This component is on mountains, mountain slopes. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227157"|"21443021"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227158"|"21443022"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 30 percent of the map unit. Slopes are 40 to 85 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite and/or argillite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227159"|"21443023"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227164"|"21443028"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockhill soil is a minor component."|"21227165"|"21443029"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21227166"|"21443030"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 25 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227167"|"21443031"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 35 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227168"|"21443032"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crystalex component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, intermontane basins. The parent material consists of wind modified outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227118"|"21442982"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"21227119"|"21442983"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, intermontane basins. The parent material consists of volcanic ash over outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227120"|"21442984"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loonlake soil is a minor component."|"21227121"|"21442985"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Half Moon soil is a minor component."|"21227122"|"21442986"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tamarack component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, intermontane basins. The parent material consists of volcanic ash over outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227123"|"21442987"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crystalex soil is a minor component."|"21227057"|"21442921"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"21227084"|"21442948"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"21227085"|"21442949"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on kame terraces, mountains. The parent material consists of volcanic ash over outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227086"|"21442950"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 25 percent of the map unit. Slopes are 8 to 30 percent. This component is on kame terraces, moraines, mountains. The parent material consists of volcanic ash over outwash and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227087"|"21442951"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tamarack soil is a minor component."|"21227088"|"21442952"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitebear component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on lake terraces, intermontane basins. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer, natric, is 8 to 18 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AY092MT Saline Subirrigated (ssb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"21227169"|"21443033"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lostprairie component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on lake terraces, intermontane basins. The parent material consists of volcanic ash over glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 3w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"21227170"|"21443034"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dahlake soil is a minor component."|"21227171"|"21443035"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wimper soil is a minor component."|"21227198"|"21443062"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Half Moon soil is a minor component."|"21227199"|"21443063"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Half Moon soil is a minor component."|"21227200"|"21443064"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tallcreek soil is a minor component."|"21227201"|"21443065"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haskillpass component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AA032MT Loamy (lo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227140"|"21443004"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lostprairie soil is a minor component."|"21227141"|"21443005"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 20 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227142"|"21443006"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 50 percent of the map unit. Slopes are 8 to 30 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21227143"|"21443007"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Meadowpeak soil is a minor component."|"21227144"|"21443008"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haskillpass component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines, intermontane basins. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AA032MT Loamy (lo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227089"|"21442953"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lostprairie soil is a minor component."|"21227090"|"21442954"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Dahlake soil is a minor component."|"21227091"|"21442955"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227124"|"21442988"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21227125"|"21442989"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Meadowpeak soil is a minor component."|"21227126"|"21442990"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lynchlake, dry component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of volcanic ash over glaciolacustrine deposits and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227127"|"21442991"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Winfall soil is a minor component."|"21227128"|"21442992"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 15 percent of the map unit. Slopes are 8 to 20 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227129"|"21442993"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Courville soil is a minor component."|"21227130"|"21442994"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 40 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, intermontane basins. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227131"|"21442995"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Meadowpeak soil is a minor component."|"21227148"|"21443012"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227145"|"21443009"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges on mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227146"|"21443010"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on ridges on mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227147"|"21443011"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lynchlake, dry component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, moraines. The parent material consists of volcanic ash over glaciolacustrine deposits and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227202"|"21443066"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227203"|"21443067"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Courville soil is a minor component."|"21227204"|"21443068"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pleasantvalley component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines, intermontane basins. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227205"|"21443069"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Meadowpeak component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY080MT Riparian Meadow (rm)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.   "|"21227232"|"21443096"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The McGregor soil is a minor component."|"21227233"|"21443097"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tallcreek soil is a minor component."|"21227234"|"21443098"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quast component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on eskers, outwash terraces, intermontane basins. The parent material consists of outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044XW184MT Silty (si) 15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227149"|"21443013"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, outwash terraces, eskers. The parent material consists of outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB036MT Droughty (dr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227150"|"21443014"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wimper soil is a minor component."|"21227151"|"21443015"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on outwash terraces, intermontane basins. The parent material consists of outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227152"|"21443016"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227172"|"21443036"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, mountain slopes. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227173"|"21443037"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 35 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, moraines. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227174"|"21443038"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wimper soil is a minor component."|"21227175"|"21443039"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 25 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227176"|"21443040"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227177"|"21443041"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Haskillpass soil is a minor component."|"21227160"|"21443024"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lostprairie soil is a minor component."|"21227161"|"21443025"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21227162"|"21443026"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227163"|"21443027"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Meadowpeak soil is a minor component."|"21227189"|"21443053"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blackcreek soil is a minor component."|"21227190"|"21443054"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21227153"|"21443017"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowpeak soil is a minor component."|"21227154"|"21443018"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pleasantvalley soil is a minor component."|"21227155"|"21443019"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227180"|"21443044"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville, dry soil is a minor component."|"21227181"|"21443045"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21227182"|"21443046"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tallcreek soil is a minor component."|"21227183"|"21443047"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21227184"|"21443048"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227185"|"21443049"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21227186"|"21443050"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Combest soil is a minor component."|"21227187"|"21443051"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 30 percent of the map unit. Slopes are 40 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227188"|"21443052"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pleasantvalley soil is a minor component."|"21227214"|"21443078"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 20 percent of the map unit. Slopes are 40 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP905MT Shallow Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227215"|"21443079"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loonlake soil is a minor component."|"21226881"|"21442745"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 90 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces, outwash plains, valleys. The parent material consists of volcanic ash over alluvium or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21226882"|"21442746"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glaciercreek soil is a minor component."|"21226883"|"21442747"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sacheen soil is a minor component."|"21226921"|"21442785"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCollum component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT UPLAND GRASSLAND ESG 44A LRU P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21226922"|"21442786"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grantsdale soil is a minor component."|"21226923"|"21442787"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Horseplains, channeled soil is a minor component."|"21226950"|"21442814"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCollum soil is a minor component."|"21226951"|"21442815"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227212"|"21443076"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227213"|"21443077"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP805MT Shallow Droughty (swdr)   Lru 43a-a, Shallow Grassland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227240"|"21443104"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 55 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227241"|"21443105"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"21227242"|"21443106"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227226"|"21443090"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 15 percent of the map unit. Slopes are 8 to 30 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AP805MT Shallow Droughty (swdr)   Lru 43a-a, Shallow Grassland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227227"|"21443091"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227228"|"21443092"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 70 percent of the map unit. Slopes are 15 to 30 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227229"|"21443093"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227230"|"21443094"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227231"|"21443095"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227257"|"21443121"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Ashleylake soil is a minor component."|"21227219"|"21443083"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227220"|"21443084"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Foyslake soil is a minor component."|"21227221"|"21443085"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata component makes up 85 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountains, moraines. The parent material consists of volcanic ash over till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227222"|"21443086"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227248"|"21443112"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227249"|"21443113"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227250"|"21443114"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 75 percent of the map unit. Slopes are 20 to 50 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227251"|"21443115"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21227252"|"21443116"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227253"|"21443117"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227254"|"21443118"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227255"|"21443119"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake, greater slope soil is a minor component."|"21227256"|"21443120"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 80 percent of the map unit. Slopes are 30 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227281"|"21443145"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"21227265"|"21443129"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227266"|"21443130"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kila soil is a minor component."|"21227267"|"21443131"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake, greater slope soil is a minor component."|"21227268"|"21443132"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 80 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227269"|"21443133"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227196"|"21443060"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy, greater slope soil is a minor component."|"21227197"|"21443061"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227223"|"21443087"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McMannamy component makes up 80 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227224"|"21443088"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"21227225"|"21443089"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227191"|"21443055"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227192"|"21443056"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy, greater slope soil is a minor component."|"21227193"|"21443057"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McMannamy component makes up 85 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227194"|"21443058"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"21227195"|"21443059"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227243"|"21443107"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227244"|"21443108"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper soil is a minor component."|"21227245"|"21443109"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 80 percent of the map unit. Slopes are 30 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227246"|"21443110"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"21227247"|"21443111"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21227273"|"21443137"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227235"|"21443099"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper soil is a minor component."|"21227236"|"21443100"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227237"|"21443101"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21227238"|"21443102"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227239"|"21443103"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227216"|"21443080"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repp component makes up 50 percent of the map unit. Slopes are 40 to 80 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of colluvium derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227217"|"21443081"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 25 percent of the map unit. Slopes are 40 to 60 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227218"|"21443082"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227258"|"21443122"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227259"|"21443123"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"21227260"|"21443124"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"21227261"|"21443125"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 70 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227262"|"21443126"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, outwash terraces. The parent material consists of volcanic ash over outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227298"|"21443162"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 80 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent.  "|"21227299"|"21443163"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Idahocreek soil is a minor component."|"21227290"|"21443154"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"21227291"|"21443155"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kila component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on outwash terraces, stream terraces, mountains. The parent material consists of alluvium and/or outwash over till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches (depth from the mineral surface is 47 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP910MT Upland Cool-moist Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21227292"|"21443156"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Idahocreek component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash terraces, stream terraces, intermontane basins. The parent material consists of alluvium and/or outwash derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 20 inches during April. Organic matter content in the surface horizon is about 4 percent. This component is in the R043AP802MT Bottomland 43a Lru P ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent.  "|"21227263"|"21443127"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kila soil is a minor component."|"21227264"|"21443128"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Half Moon soil is a minor component."|"21227289"|"21443153"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 10 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, outwash terraces, moraines. The parent material consists of volcanic ash over outwash and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227310"|"21443174"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lesier soil is a minor component."|"21227311"|"21443175"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lesier, dry component makes up 65 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, intermontane basins, outwash terraces. The parent material consists of volcanic ash over outwash and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21227312"|"21443176"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on intermontane basins, moraines, outwash terraces. The parent material consists of outwash and/or till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent.  "|"21227337"|"21443201"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glaciercreek component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, intermontane basins. The parent material consists of volcanic ash over outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227274"|"21443138"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lesier component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, intermontane basins. The parent material consists of volcanic ash over outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21227275"|"21443139"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226864"|"21442728"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Battlebutte component makes up 65 percent of the map unit. Slopes are 30 to 60 percent. This component is on hills, mountains. The parent material consists of residuum weathered from welded tuff. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AA138MT Shallow Droughty (swdr)   Lru 43a-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226865"|"21442729"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Battlebutte soil is a minor component."|"21226866"|"21442730"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bigdraw soil is a minor component."|"21226867"|"21442731"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21227282"|"21443146"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashleylake, greater slope soil is a minor component."|"21227283"|"21443147"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashleylake component makes up 75 percent of the map unit. Slopes are 8 to 30 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from argillite and/or calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP910MT Upland Cool-moist Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21227284"|"21443148"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"21227285"|"21443149"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"21227286"|"21443150"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bendahl soil is a minor component."|"21227287"|"21443151"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Idahocreek soil is a minor component."|"21227288"|"21443152"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashleylake component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from argillite and/or calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP910MT Upland Cool-moist Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21227313"|"21443177"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kila component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash terraces, mountains. The parent material consists of outwash over till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches (depth from the mineral surface is 47 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP910MT Upland Cool-moist Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21227314"|"21443178"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227315"|"21443179"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashleylake, greater slope soil is a minor component."|"21227293"|"21443157"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227294"|"21443158"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashleylake component makes up 65 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from argillite and/or calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT UPLAND COOL-MOIST WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21227295"|"21443159"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"21227296"|"21443160"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"21227321"|"21443185"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bendahl soil is a minor component."|"21227322"|"21443186"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The McMannamy soil is a minor component."|"21227323"|"21443187"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 95 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"21227324"|"21443188"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227276"|"21443140"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227277"|"21443141"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 60 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227278"|"21443142"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"21227279"|"21443143"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on glacially scoured ridges, mountains. The parent material consists of colluvium over residuum weathered from quartzite and/or argillite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP905MT Shallow Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227280"|"21443144"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227270"|"21443134"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McMannamy component makes up 35 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21227271"|"21443135"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 55 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"21227272"|"21443136"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227297"|"21443161"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kingspoint soil is a minor component."|"21227325"|"21443189"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint, outwash substratum component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on mountains, outwash terraces, moraines. The parent material consists of till derived from calcareous siltstone over outwash derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"21227326"|"21443190"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Idahocreek soil is a minor component."|"21227305"|"21443169"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trumancreek component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R043AP802MT Bottomland 43a Lru P ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria.   "|"21227306"|"21443170"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blackcreek component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium and/or outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 20 inches during April, May. Organic matter content in the surface horizon is about 3 percent. This component is in the R043AP802MT Bottomland 43a Lru P ecological site. Nonirrigated land capability classification is 4w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227307"|"21443171"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kila soil is a minor component."|"21227308"|"21443172"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 25 percent of the map unit. Slopes are 2 to 12 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227309"|"21443173"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashleylake soil is a minor component."|"21227300"|"21443164"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McMannamy soil is a minor component."|"21227301"|"21443165"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kila soil is a minor component."|"21227302"|"21443166"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lesier soil is a minor component."|"21227303"|"21443167"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 80 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, mountains. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227304"|"21443168"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Trumancreek soil is a minor component."|"21227316"|"21443180"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The McGregor soil is a minor component."|"21227317"|"21443181"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lesier component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, mountains. The parent material consists of volcanic ash over outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"21227318"|"21443182"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Foyslake soil is a minor component."|"21227319"|"21443183"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, mountains. The parent material consists of outwash and/or glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21227320"|"21443184"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blackcreek soil is a minor component."|"21226823"|"21442687"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tallcreek component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of volcanic ash over glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21226824"|"21442688"
08/06/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tallcreek soil is a minor component."|"21226825"|"21442689"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bowlake component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on relict stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB033MT Loamy Argillic (Loa)   LRU 44A-B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21226793"|"21442657"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Minesinger component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on relict stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA032MT Loamy (Lo)   LRU 44A-A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"21226794"|"21442658"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kerl soil is a minor component."|"21226795"|"21442659"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Niarada soil is a minor component."|"21226796"|"21442660"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"21226797"|"21442661"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lynchlake soil is a minor component."|"21227329"|"21443193"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lynchlake soil is a minor component."|"21227330"|"21443194"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Pleasantvalley soil is a minor component."|"21227331"|"21443195"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blackcreek soil is a minor component."|"21227332"|"21443196"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon, cool component makes up 40 percent of the map unit. Slopes are 8 to 30 percent. This component is on collapsed lake plains, intermontane basins. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21227333"|"21443197"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Half Moon component makes up 30 percent of the map unit. Slopes are 8 to 30 percent. This component is on collapsed lake plains, intermontane basins. The parent material consists of glaciolacustrine deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21227334"|"21443198"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tallcreek soil is a minor component."|"21227335"|"21443199"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wimper, greater slope soil is a minor component."|"21227346"|"21443210"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 80 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227347"|"21443211"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227348"|"21443212"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kila soil is a minor component."|"21227349"|"21443213"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227338"|"21443202"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ashleylake component makes up 50 percent of the map unit. Slopes are 40 to 60 percent. This component is on glacially scoured ridges, mountains. The parent material consists of volcanic ash over till derived from argillite and/or calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT UPLAND COOL-MOIST WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21227339"|"21443203"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"21227340"|"21443204"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foyslake soil is a minor component."|"21227341"|"21443205"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 15 percent of the map unit. Slopes are 40 to 70 percent. This component is on glacially scoured ridges, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP905MT SHALLOW COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227342"|"21443206"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227327"|"21443191"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from quartzite and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227328"|"21443192"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Winkler soil is a minor component."|"21227354"|"21443218"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227355"|"21443219"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227356"|"21443220"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227336"|"21443200"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21227363"|"21443227"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from quartzite and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227364"|"21443228"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Winkler soil is a minor component."|"21227365"|"21443229"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227366"|"21443230"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Combest soil is a minor component."|"21227367"|"21443231"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227368"|"21443232"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21226785"|"21442649"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finleypoint component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226786"|"21442650"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226787"|"21442651"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigarm soil is a minor component."|"21226788"|"21442652"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hogsby soil is a minor component."|"21226789"|"21442653"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finleypoint, dry soil is a minor component."|"21226790"|"21442654"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eaglewing component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043AP910MT UPLAND COOL-MOIST WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227350"|"21443214"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eaglewing, stony silt loam soil is a minor component."|"21227351"|"21443215"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227352"|"21443216"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21227353"|"21443217"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"21227377"|"21443241"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227357"|"21443221"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McMannamy component makes up 35 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"21227358"|"21443222"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 55 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"21227359"|"21443223"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227360"|"21443224"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227361"|"21443225"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The McMannamy soil is a minor component."|"21227362"|"21443226"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 70 percent of the map unit. Slopes are 8 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"21227386"|"21443250"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Repp soil is a minor component."|"21227387"|"21443251"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227388"|"21443252"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21227343"|"21443207"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The McMannamy soil is a minor component."|"21227344"|"21443208"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kingspoint component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent.  "|"21227345"|"21443209"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wimper soil is a minor component."|"21227371"|"21443235"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21227372"|"21443236"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The McMannamy soil is a minor component."|"21227369"|"21443233"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blackcreek soil is a minor component."|"21227370"|"21443234"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foyslake component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on mountains, moraines. The parent material consists of till derived from calcareous siltstone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent.  "|"21227394"|"21443258"
07/26/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kila soil is a minor component."|"21227395"|"21443259"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21226948"|"21442812"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21226949"|"21442813"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 45 percent of the map unit. Slopes are 30 to 50 percent. This component is on moraines on mountain slopes, mountains. The parent material consists of volcanic ash over drift and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226974"|"21442838"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockhill component makes up 25 percent of the map unit. Slopes are 30 to 50 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP905MT Shallow Cool Woodland 43a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21226975"|"21442839"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"21226976"|"21442840"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21227378"|"21443242"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wimper component makes up 25 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of till derived from calcareous siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227379"|"21443243"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on glaciated mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AA138MT Shallow Droughty (Swdr)   LRU 43A-A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. There are no saline horizons within 30 inches of the soil surface. "|"21227380"|"21443244"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repp soil is a minor component."|"21227381"|"21443245"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kingspoint soil is a minor component."|"21227382"|"21443246"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten, very stony soil is a minor component."|"21227373"|"21443237"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larry soil is a minor component."|"21227374"|"21443238"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sol, very stony component makes up 35 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, mountains. The parent material consists of undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227375"|"21443239"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 50 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, mountains. The parent material consists of undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227376"|"21443240"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 55 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, colluvial aprons, mountains. The parent material consists of undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227389"|"21443253"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kadygulch, dry soil is a minor component."|"21227390"|"21443254"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Combest component makes up 40 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, colluvial aprons, mountains. The parent material consists of volcanic ash over undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227391"|"21443255"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 90 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, colluvial aprons, mountains. The parent material consists of volcanic ash over undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21227392"|"21443256"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"21227393"|"21443257"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"21227383"|"21443247"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCay soil is a minor component."|"21227384"|"21443248"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 90 percent of the map unit. Slopes are 35 to 55 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT UPLAND COOL WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227385"|"21443249"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"21227401"|"21443265"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"21227402"|"21443266"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCay component makes up 90 percent of the map unit. Slopes are 35 to 55 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP908MT UPLAND COLD WOODLAND ESG 43A LRU P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21227403"|"21443267"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"21227404"|"21443268"
