08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21333505"|"21572006"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21333506"|"21572007"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333507"|"21572008"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Heldt component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21333508"|"21572009"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333509"|"21572010"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333510"|"21572011"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Heldt component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21333511"|"21572012"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333512"|"21572013"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333513"|"21572014"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333514"|"21572015"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333515"|"21572016"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21333516"|"21572017"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333517"|"21572018"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333518"|"21572019"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333519"|"21572020"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333520"|"21572021"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333521"|"21572022"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333522"|"21572023"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333523"|"21572024"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333524"|"21572025"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333525"|"21572026"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333526"|"21572027"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hesper component makes up 85 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333527"|"21572028"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333528"|"21572029"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333529"|"21572030"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 45 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333530"|"21572031"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hopley component makes up 45 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333531"|"21572032"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333532"|"21572033"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21333533"|"21572034"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gilt Edge soil is a minor component."|"21333534"|"21572035"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333535"|"21572036"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3c. Irrigated land capability classification is 3c. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333536"|"21572037"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Heldt component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"21333504"|"21572005"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21333503"|"21572004"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333502"|"21572003"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bankard soil is a minor component."|"21333501"|"21572002"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333500"|"21572001"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 40 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21333499"|"21572000"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 45 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 48 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE012MT Saline Lowland (sl)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21333498"|"21571999"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21333497"|"21571998"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333496"|"21571997"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21333495"|"21571996"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bankard soil is a minor component."|"21333494"|"21571995"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 85 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333493"|"21571994"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21333492"|"21571993"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333491"|"21571992"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21333490"|"21571991"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333489"|"21571990"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21333488"|"21571989"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333487"|"21571988"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333486"|"21571987"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21333485"|"21571986"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21333484"|"21571985"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333483"|"21571984"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333482"|"21571983"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21333481"|"21571982"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverson component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333480"|"21571981"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21333479"|"21571980"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glenberg component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333478"|"21571979"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bankard soil is a minor component."|"21333477"|"21571978"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverson soil is a minor component."|"21333476"|"21571977"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21333475"|"21571976"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333474"|"21571975"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333473"|"21571974"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gilt Edge component makes up 85 percent of the map unit. Slopes are 2 to 6 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE013MT Claypan (cp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333472"|"21571973"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333471"|"21571972"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21333470"|"21571971"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333469"|"21571970"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gilt Edge component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE013MT Claypan (cp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333468"|"21571969"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bone soil is a minor component."|"21333467"|"21571968"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21333466"|"21571967"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rapelje soil is a minor component."|"21333465"|"21571966"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Galata component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE388MT Clayey (cy)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 17 within 30 inches of the soil surface."|"21333464"|"21571965"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333463"|"21571964"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333462"|"21571963"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333461"|"21571962"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333460"|"21571961"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333459"|"21571960"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333458"|"21571959"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333457"|"21571958"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333456"|"21571957"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333455"|"21571956"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 95 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333454"|"21571955"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333453"|"21571954"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333452"|"21571953"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"21333451"|"21571952"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 25 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333450"|"21571951"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 70 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21333449"|"21571950"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"21333448"|"21571949"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon component makes up 45 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333447"|"21571948"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 45 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333446"|"21571947"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21333445"|"21571946"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hopley soil is a minor component."|"21333444"|"21571945"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"21333443"|"21571944"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 65 percent of the map unit. Slopes are 0 to 6 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333442"|"21571943"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21333441"|"21571942"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rapelje soil is a minor component."|"21333440"|"21571941"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21333439"|"21571940"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21333438"|"21571939"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 70 percent of the map unit. Slopes are 8 to 20 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333437"|"21571938"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Galata soil is a minor component."|"21333436"|"21571937"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rapelje soil is a minor component."|"21333435"|"21571936"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 25 percent of the map unit. Slopes are 8 to 20 percent. This component is on hills. The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333434"|"21571935"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21333433"|"21571934"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 65 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333432"|"21571933"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Galata soil is a minor component."|"21333431"|"21571932"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rapelje soil is a minor component."|"21333430"|"21571931"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 30 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333429"|"21571930"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333428"|"21571929"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333427"|"21571928"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relan soil is a minor component."|"21333426"|"21571927"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21333425"|"21571926"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333424"|"21571925"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relan soil is a minor component."|"21333423"|"21571924"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333422"|"21571923"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relan soil is a minor component."|"21333421"|"21571922"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farland component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333420"|"21571921"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rapelje soil is a minor component."|"21333419"|"21571920"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333418"|"21571919"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relan soil is a minor component."|"21333417"|"21571918"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21333416"|"21571917"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21333415"|"21571916"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arvada soil is a minor component."|"21333414"|"21571915"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21333413"|"21571914"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Epsie component makes up 90 percent of the map unit. Slopes are 4 to 15 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. "|"21333412"|"21571913"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ocean lake component makes up 35 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21333411"|"21571912"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Remmit soil is a minor component."|"21333410"|"21571911"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333409"|"21571910"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vona soil is a minor component."|"21333408"|"21571909"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 45 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333407"|"21571908"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21333406"|"21571907"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Remmit soil is a minor component."|"21333405"|"21571906"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333404"|"21571905"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333403"|"21571904"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 85 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333402"|"21571903"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Remmit soil is a minor component."|"21333401"|"21571902"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333400"|"21571901"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333399"|"21571900"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333398"|"21571899"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 90 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333397"|"21571898"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333396"|"21571897"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333395"|"21571896"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333394"|"21571895"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 20 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333393"|"21571894"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cushman component makes up 70 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of loamy residuum. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333392"|"21571893"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333391"|"21571892"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333390"|"21571891"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 25 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333389"|"21571890"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cushman component makes up 70 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy residuum. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333388"|"21571889"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21333387"|"21571888"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Campspass component makes up 50 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of loamy colluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 11 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333386"|"21571887"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"21333385"|"21571886"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21333384"|"21571885"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Barvon component makes up 20 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of loamy residuum. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333383"|"21571884"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21333382"|"21571883"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333381"|"21571882"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 15 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE393MT Shallow Clay (swc)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21333380"|"21571881"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Campspass soil is a minor component."|"21333379"|"21571880"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barvon soil is a minor component."|"21333378"|"21571879"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 15 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333377"|"21571878"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 40 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333376"|"21571877"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333375"|"21571876"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333374"|"21571875"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333373"|"21571874"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333372"|"21571873"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333371"|"21571872"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333370"|"21571871"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333369"|"21571870"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333368"|"21571869"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bew component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333367"|"21571868"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333366"|"21571867"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333365"|"21571866"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333364"|"21571865"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21333363"|"21571864"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glenberg soil is a minor component."|"21333362"|"21571863"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bankard component makes up 90 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE018MT Sands (sa)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21333361"|"21571862"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 70 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE014MT Dense Clay (dc)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333360"|"21571861"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bone component makes up 30 percent of the map unit. Slopes are 0 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE014MT Dense Clay (dc)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"21333359"|"21571860"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333537"|"21572038"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gilt Edge soil is a minor component."|"21333538"|"21572039"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333539"|"21572040"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3c. Irrigated land capability classification is 3c. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333540"|"21572041"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333541"|"21572042"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gilt Edge soil is a minor component."|"21333542"|"21572043"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333543"|"21572044"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333544"|"21572045"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gilt Edge soil is a minor component."|"21333545"|"21572046"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 80 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333546"|"21572047"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arvada component makes up 15 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE014MT Dense Clay (dc)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333547"|"21572048"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333548"|"21572049"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 30 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333549"|"21572050"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333550"|"21572051"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333551"|"21572052"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 60 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333552"|"21572053"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hydro soil is a minor component."|"21333553"|"21572054"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333554"|"21572055"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333555"|"21572056"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hydro component makes up 70 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3c. Irrigated land capability classification is 3c. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"21333556"|"21572057"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fort Collins component makes up 25 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333557"|"21572058"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333558"|"21572059"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333559"|"21572060"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333560"|"21572061"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21333561"|"21572062"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333562"|"21572063"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333563"|"21572064"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333564"|"21572065"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21333565"|"21572066"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333566"|"21572067"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333567"|"21572068"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333568"|"21572069"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Keiser component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"21333569"|"21572070"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Galata soil is a minor component."|"21333570"|"21572071"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21333571"|"21572072"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rapelje soil is a minor component."|"21333572"|"21572073"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kyle component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21333573"|"21572074"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Galata soil is a minor component."|"21333574"|"21572075"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333575"|"21572076"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21333576"|"21572077"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21333577"|"21572078"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kyle component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21333578"|"21572079"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vananda soil is a minor component."|"21333579"|"21572080"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333580"|"21572081"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21333581"|"21572082"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Galata soil is a minor component."|"21333582"|"21572083"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kyle component makes up 85 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 9 within 30 inches of the soil surface."|"21333583"|"21572084"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3c. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333584"|"21572085"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333585"|"21572086"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333586"|"21572087"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333587"|"21572088"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333588"|"21572089"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333589"|"21572090"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333590"|"21572091"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McRae component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333591"|"21572092"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333592"|"21572093"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333593"|"21572094"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333594"|"21572095"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21333595"|"21572096"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thurlow soil is a minor component."|"21333596"|"21572097"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333597"|"21572098"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 85 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333598"|"21572099"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 30 percent of the map unit. Slopes are 8 to 35 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333599"|"21572100"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333600"|"21572101"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333601"|"21572102"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 60 percent of the map unit. Slopes are 8 to 35 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333602"|"21572103"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21333603"|"21572104"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vona soil is a minor component."|"21333604"|"21572105"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Remmit soil is a minor component."|"21333605"|"21572106"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333606"|"21572107"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 60 percent of the map unit. Slopes are 15 to 35 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333607"|"21572108"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21333608"|"21572109"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333609"|"21572110"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21333610"|"21572111"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 40 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333611"|"21572112"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 55 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333612"|"21572113"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333613"|"21572114"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 30 percent of the map unit. Slopes are 35 to 75 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333614"|"21572115"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333615"|"21572116"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333616"|"21572117"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Midway component makes up 40 percent of the map unit. Slopes are 35 to 70 percent.  The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (swc)    Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333617"|"21572118"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21333618"|"21572119"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elso component makes up 35 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333619"|"21572120"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nihill component makes up 60 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AE001MT Silty (si) Rru 58a-e 10-14 P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333620"|"21572121"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333621"|"21572122"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333622"|"21572123"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333623"|"21572124"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vona soil is a minor component."|"21333624"|"21572125"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21333625"|"21572126"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Remmit soil is a minor component."|"21333626"|"21572127"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Midway soil is a minor component."|"21333627"|"21572128"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ocean lake component makes up 65 percent of the map unit. Slopes are 15 to 45 percent.  The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21333628"|"21572129"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rapelje component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21333629"|"21572130"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333630"|"21572131"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333631"|"21572132"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rapelje component makes up 90 percent of the map unit. Slopes are 2 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21333632"|"21572133"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333633"|"21572134"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333634"|"21572135"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333635"|"21572136"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"21333636"|"21572137"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333637"|"21572138"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333638"|"21572139"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333639"|"21572140"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 25 percent of the map unit. Slopes are 6 to 30 percent.  The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE397MT Very Shallow (vsw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333640"|"21572141"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 70 percent of the map unit. Slopes are 5 to 30 percent.  The parent material consists of loamy colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333641"|"21572142"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Somewhat poorly drained soils soil is a minor component."|"21333642"|"21572143"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 35 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333643"|"21572144"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333644"|"21572145"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333645"|"21572146"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ringling soil is a minor component."|"21333646"|"21572147"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 55 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333647"|"21572148"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relan soil is a minor component."|"21333648"|"21572149"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333649"|"21572150"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333650"|"21572151"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Remmit component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333651"|"21572152"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vona soil is a minor component."|"21333652"|"21572153"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333653"|"21572154"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333654"|"21572155"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Remmit component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333655"|"21572156"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vona soil is a minor component."|"21333656"|"21572157"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333657"|"21572158"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McRae soil is a minor component."|"21333658"|"21572159"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Remmit component makes up 60 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of loamy colluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333659"|"21572160"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333660"|"21572161"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elso soil is a minor component."|"21333661"|"21572162"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ocean lake component makes up 30 percent of the map unit. Slopes are 8 to 25 percent.  The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE019MT Shallow (sw)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21333662"|"21572163"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333663"|"21572164"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Campspass soil is a minor component."|"21333664"|"21572165"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barvon soil is a minor component."|"21333665"|"21572166"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"21333666"|"21572167"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 90 percent of the map unit. Slopes are 20 to 50 percent.  The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE397MT Very Shallow (vsw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333667"|"21572168"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Campspass soil is a minor component."|"21333668"|"21572169"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Barvon soil is a minor component."|"21333669"|"21572170"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 45 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE392MT Shallow (sw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"21333670"|"21572171"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 45 percent of the map unit. Slopes are 15 to 50 percent.  The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE397MT Very Shallow (vsw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333671"|"21572172"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus soil is a minor component."|"21333672"|"21572173"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farland soil is a minor component."|"21333673"|"21572174"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ringling component makes up 50 percent of the map unit. Slopes are 6 to 25 percent.  The parent material consists of residuum weathered from porcellanite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE397MT Very Shallow (vsw)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21333674"|"21572175"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relan component makes up 45 percent of the map unit. Slopes are 6 to 25 percent.  The parent material consists of loamy colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE394MT Silty (si)   Rru 58a-e  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333675"|"21572176"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21333676"|"21572177"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poorly drained soils soil is a minor component."|"21333677"|"21572178"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"21333927"|"21572428"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"21333928"|"21572429"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ralore soil is a minor component."|"21333929"|"21572430"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ismay soil is a minor component."|"21333930"|"21572431"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333931"|"21572432"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21333932"|"21572433"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21333933"|"21572434"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"21333934"|"21572435"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terrace escarpments component makes up 100 percent of the map unit. Slopes are 8 to 35 percent.  The parent material consists of loamy colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE004MT Silty-steep (sistp)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333678"|"21572179"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333679"|"21572180"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333680"|"21572181"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333681"|"21572182"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 90 percent of the map unit. Slopes are 0 to 2 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333682"|"21572183"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333683"|"21572184"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333684"|"21572185"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333685"|"21572186"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333686"|"21572187"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333687"|"21572188"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21333688"|"21572189"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Heldt soil is a minor component."|"21333689"|"21572190"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 90 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333690"|"21572191"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hesper soil is a minor component."|"21333691"|"21572192"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fort Collins soil is a minor component."|"21333692"|"21572193"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21333693"|"21572194"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Thurlow component makes up 90 percent of the map unit. Slopes are 8 to 15 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AE002MT Clayey (cy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333694"|"21572195"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vananda component makes up 95 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE014MT Dense Clay (dc)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"21333695"|"21572196"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bew soil is a minor component."|"21333696"|"21572197"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kyle soil is a minor component."|"21333697"|"21572198"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vona component makes up 90 percent of the map unit. Slopes are 2 to 4 percent.  The parent material consists of loamy alluvium and/or sandy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333698"|"21572199"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Remmit soil is a minor component."|"21333699"|"21572200"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333700"|"21572201"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Remmit component makes up 35 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333701"|"21572202"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vona component makes up 60 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium and/or sandy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AE003MT Sandy (sy)   Rru 58a-e  10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333702"|"21572203"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ocean lake soil is a minor component."|"21333703"|"21572204"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cushman soil is a minor component."|"21333704"|"21572205"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333705"|"21572206"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arwite component makes up 85 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, alluvial fans, uplands. The parent material consists of alluvium and/or eolian deposits derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (Sy) 15-17 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21333706"|"21572207"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vonalf soil is a minor component."|"21333707"|"21572208"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ashollow soil is a minor component."|"21333708"|"21572209"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moskee soil is a minor component."|"21333709"|"21572210"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vonalf soil is a minor component."|"21333710"|"21572211"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Xema soil is a minor component."|"21333711"|"21572212"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333712"|"21572213"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oldwolf soil is a minor component."|"21333713"|"21572214"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arwite component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium and/or eolian deposits derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (sy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21333714"|"21572215"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elwop component makes up 30 percent of the map unit. Slopes are 0 to 6 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium and/or eolian deposits over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (sy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333715"|"21572216"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333716"|"21572217"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Arwite component makes up 45 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans, hills, ridges, uplands. The parent material consists of alluvium and/or eolian deposits derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (Sy) 15-17 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21333717"|"21572218"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moskee soil is a minor component."|"21333718"|"21572219"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vonalf component makes up 35 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans, hills, ridges, uplands. The parent material consists of alluvium and/or eolian deposits derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (Sy) 15-17 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent.  "|"21333719"|"21572220"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Xema soil is a minor component."|"21333720"|"21572221"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elwop soil is a minor component."|"21333721"|"21572222"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Deekay component makes up 80 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, alluvial fans, uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (Ly) 15-17  PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333722"|"21572223"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oshoto soil is a minor component."|"21333723"|"21572224"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Recluse soil is a minor component."|"21333724"|"21572225"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ziggy soil is a minor component."|"21333725"|"21572226"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jaywest soil is a minor component."|"21333726"|"21572227"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oshoto soil is a minor component."|"21333727"|"21572228"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Recluse soil is a minor component."|"21333728"|"21572229"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Deekay component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, alluvial fans, uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (Ly) 15-17  PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333729"|"21572230"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jaywest soil is a minor component."|"21333730"|"21572231"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moorhead component makes up 35 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, alluvial fans, uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (Ly) 15-17  PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333731"|"21572232"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Recluse soil is a minor component."|"21333732"|"21572233"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ziggy soil is a minor component."|"21333733"|"21572234"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arwite soil is a minor component."|"21333734"|"21572235"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ucross soil is a minor component."|"21333735"|"21572236"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Deekay component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on ridges on sedimentary plains, hills on sedimentary plains. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333736"|"21572237"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oldwolf component makes up 30 percent of the map unit. Slopes are 0 to 6 percent. This component is on ridges on sedimentary plains, hills on sedimentary plains. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333737"|"21572238"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leiter soil is a minor component."|"21333738"|"21572239"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ucross soil is a minor component."|"21333739"|"21572240"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Echeta component makes up 45 percent of the map unit. Slopes are 6 to 15 percent. This component is on ridges, hills, uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (Cy) 15-17 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333740"|"21572241"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Samsil soil is a minor component."|"21333741"|"21572242"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moorhead soil is a minor component."|"21333742"|"21572243"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cromack component makes up 35 percent of the map unit. Slopes are 6 to 15 percent. This component is on ridges, hills, uplands. The parent material consists of alluvium over residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (Cy) 15-17 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333743"|"21572244"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hiland soil is a minor component."|"21333899"|"21572400"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cushman component makes up 30 percent of the map unit. Slopes are 0 to 6 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY122WY Loamy (Ly) 10-14 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333900"|"21572401"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Theedle soil is a minor component."|"21333901"|"21572402"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbac soil is a minor component."|"21333902"|"21572403"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zigweid soil is a minor component."|"21333903"|"21572404"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Forkwood component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY122WY Loamy (Ly) 10-14 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333904"|"21572405"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oshoto soil is a minor component."|"21333744"|"21572245"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333745"|"21572246"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Platmak soil is a minor component."|"21333746"|"21572247"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jaywest component makes up 80 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, alluvial fans, uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (Ly) 15-17  PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333747"|"21572248"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moorhead soil is a minor component."|"21333748"|"21572249"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333749"|"21572250"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Platmak soil is a minor component."|"21333750"|"21572251"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spottedhorse soil is a minor component."|"21333751"|"21572252"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leiter soil is a minor component."|"21333752"|"21572253"
02/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jaywest component makes up 45 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants on sedimentary plains, alluvial fans on sedimentary plains. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333753"|"21572254"
02/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moorhead component makes up 35 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants on sedimentary plains, alluvial fans on sedimentary plains. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333754"|"21572255"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Echeta soil is a minor component."|"21333755"|"21572256"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nuncho soil is a minor component."|"21333756"|"21572257"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Felix, ponded soil is a minor component."|"21333757"|"21572258"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333758"|"21572259"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moorhead component makes up 80 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants, alluvial fans, uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (Cy) 15-17 PZ ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333759"|"21572260"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambria soil is a minor component."|"21333919"|"21572420"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shingle component makes up 20 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 4 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY162WY Shallow Loamy (SwLy) 10-14 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333920"|"21572421"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Theedle component makes up 40 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY122WY Loamy (Ly) 10-14 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333921"|"21572422"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilight soil is a minor component."|"21333922"|"21572423"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Taluce soil is a minor component."|"21333923"|"21572424"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland soil is a minor component."|"21333924"|"21572425"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kishona component makes up 20 percent of the map unit. Slopes are 3 to 20 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY122WY Loamy (Ly) 10-14 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333925"|"21572426"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turnercrest soil is a minor component."|"21333926"|"21572427"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cromack soil is a minor component."|"21333955"|"21572456"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ucross component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333956"|"21572457"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ziggy soil is a minor component."|"21333957"|"21572458"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Iwait component makes up 30 percent of the map unit. Slopes are 0 to 6 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333958"|"21572459"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oldwolf soil is a minor component."|"21333959"|"21572460"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairburn component makes up 20 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21333905"|"21572406"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Deekay soil is a minor component."|"21333906"|"21572407"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elwop soil is a minor component."|"21333907"|"21572408"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ucross component makes up 35 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"21333908"|"21572409"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pitchdraw soil is a minor component."|"21333909"|"21572410"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cromack soil is a minor component."|"21333910"|"21572411"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Iwait component makes up 25 percent of the map unit. Slopes are 3 to 20 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333911"|"21572412"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333833"|"21572334"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21333834"|"21572335"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toby soil is a minor component."|"21333835"|"21572336"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri, DEEP component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 50 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (sy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333836"|"21572337"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21333837"|"21572338"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 30 percent of the map unit. Slopes are 0 to 6 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (sy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333838"|"21572339"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri, DEEP soil is a minor component."|"21333803"|"21572304"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Toby soil is a minor component."|"21333804"|"21572305"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21333805"|"21572306"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 40 percent of the map unit. Slopes are 3 to 20 percent. This component is on hills, ridges, uplands. The parent material consists of alluvium over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333806"|"21572307"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 30 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, ridges, uplands. The parent material consists of alluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent.  "|"21333807"|"21572308"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 15 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, ridges, uplands. The parent material consists of alluvium over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent.  "|"21333808"|"21572309"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 6 to 45 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333785"|"21572286"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 30 percent of the map unit. Slopes are 6 to 45 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium over residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY258WY Shallow Clayey (swcy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333786"|"21572287"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333787"|"21572288"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21333788"|"21572289"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333789"|"21572290"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21333790"|"21572291"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"21333791"|"21572292"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Haverdad soil is a minor component."|"21333829"|"21572330"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clarkelen component makes up 45 percent of the map unit. Slopes are 0 to 6 percent. This component is on stream terraces on uplands, flood plains on uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY128WY Lowland (ll)  10-14"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333830"|"21572331"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boruff component makes up 15 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains, valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during April, May. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY174WY Subirrigated (sb) 10-17"" Pz ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 5 within 30 inches of the soil surface."|"21333831"|"21572332"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Draknab component makes up 35 percent of the map unit. Slopes are 0 to 6 percent. This component is on stream terraces on uplands, flood plains on uplands. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY128WY Lowland (ll)  10-14"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333832"|"21572333"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cromack component makes up 45 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium over residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333815"|"21572316"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ucross soil is a minor component."|"21333816"|"21572317"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Samsil component makes up 35 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY258WY Shallow Clayey (swcy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333817"|"21572318"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairburn soil is a minor component."|"21333818"|"21572319"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland soil is a minor component."|"21333819"|"21572320"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leiter soil is a minor component."|"21333820"|"21572321"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21333885"|"21572386"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333886"|"21572387"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21333887"|"21572388"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 45 percent of the map unit. Slopes are 6 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333888"|"21572389"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21333889"|"21572390"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 6 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333890"|"21572391"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333877"|"21572378"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 35 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333878"|"21572379"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 25 percent of the map unit. Slopes are 3 to 15 percent. This component is on fan remnants on uplands, hills on uplands, ridges on uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333879"|"21572380"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 20 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333880"|"21572381"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21333881"|"21572382"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21333882"|"21572383"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21333883"|"21572384"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333884"|"21572385"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"21333792"|"21572293"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, WOODED component makes up 20 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333793"|"21572294"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall, WOODED component makes up 25 percent of the map unit. Slopes are 3 to 20 percent. This component is on fan remnants on uplands, hills on uplands, ridges on uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333794"|"21572295"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21333795"|"21572296"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333796"|"21572297"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, WOODED component makes up 35 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333797"|"21572298"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333798"|"21572299"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ziggy soil is a minor component."|"21333760"|"21572261"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cromack soil is a minor component."|"21333761"|"21572262"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Echeta component makes up 45 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants on uplands, alluvial fans on uplands. The parent material consists of loamy alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333762"|"21572263"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jaywest soil is a minor component."|"21333763"|"21572264"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Moorhead component makes up 40 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants on uplands, alluvial fans on uplands. The parent material consists of loamy alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333764"|"21572265"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Samsil component makes up 30 percent of the map unit. Slopes are 10 to 45 percent. This component is on hills, sedimentary plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY258WY Shallow Clayey (swcy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333941"|"21572442"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oldwolf soil is a minor component."|"21333942"|"21572443"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cromack soil is a minor component."|"21333943"|"21572444"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairburn component makes up 35 percent of the map unit. Slopes are 10 to 45 percent. This component is on hills, sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333944"|"21572445"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"21333945"|"21572446"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ucross soil is a minor component."|"21333946"|"21572447"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pitchdraw soil is a minor component."|"21333947"|"21572448"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri, DEEP soil is a minor component."|"21333839"|"21572340"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foreleft component makes up 80 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants on uplands, alluvial fans on uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333840"|"21572341"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanstel soil is a minor component."|"21333841"|"21572342"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pinehill soil is a minor component."|"21333842"|"21572343"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333843"|"21572344"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Foreleft component makes up 50 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333844"|"21572345"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 30 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium over residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333845"|"21572346"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21333846"|"21572347"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333847"|"21572348"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"21333848"|"21572349"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pinehill soil is a minor component."|"21333849"|"21572350"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri, DEEP soil is a minor component."|"21333850"|"21572351"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gateson, wooded component makes up 40 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium and/or eolian deposits over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21333809"|"21572310"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Xema, wooded component makes up 25 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium and/or eolian deposits over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21333810"|"21572311"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mittenbutte, wooded component makes up 20 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria.   "|"21333811"|"21572312"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vonalf, wooded soil is a minor component."|"21333812"|"21572313"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Spottedhorse, wooded soil is a minor component."|"21333813"|"21572314"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arwite, wooded soil is a minor component."|"21333814"|"21572315"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clarkelen soil is a minor component."|"21333799"|"21572300"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boruff soil is a minor component."|"21333800"|"21572301"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haverdad component makes up 85 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 36 inches during April, May. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY128WY Lowland (ll)  10-14"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333801"|"21572302"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kishona soil is a minor component."|"21333802"|"21572303"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigsandy component makes up 35 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during April, May. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333891"|"21572392"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 50 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333892"|"21572393"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333893"|"21572394"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanstel soil is a minor component."|"21333894"|"21572395"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333895"|"21572396"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland soil is a minor component."|"21333912"|"21572413"
03/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ironbutte, wooded component makes up 35 percent of the map unit. Slopes are 3 to 60 percent. This component is on hills, hills. The parent material consists of colluvium derived from porcellanite over fractured and displaced porcellanite. Depth to a root restrictive layer, strongly contrasting textural stratification, is 7 to 20 inches (depth from the mineral surface is 7 to 19 inches). The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s. Irrigated land capability classification is 8s. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21333913"|"21572414"
03/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairburn, wooded component makes up 30 percent of the map unit. Slopes are 3 to 60 percent. This component is on hills, hills. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches (depth from the mineral surface is 10 to 19 inches). The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 8e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"21333914"|"21572415"
03/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mittenbutte, wooded component makes up 15 percent of the map unit. Slopes are 3 to 60 percent. This component is on hills, hills. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches (depth from the mineral surface is 10 to 19 inches). The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 8e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333915"|"21572416"
03/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Xema, wooded soil is a minor component."|"21333916"|"21572417"
03/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ucross, wooded soil is a minor component."|"21333917"|"21572418"
03/24/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elwop, wooded soil is a minor component."|"21333918"|"21572419"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kirby, WOODED component makes up 40 percent of the map unit. Slopes are 6 to 45 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium and/or colluvium derived from porcellanite. Depth to a root restrictive layer, strongly contrasting textural stratification, is 10 to 20 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333778"|"21572279"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, WOODED component makes up 25 percent of the map unit. Slopes are 6 to 45 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333779"|"21572280"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep, WOODED component makes up 15 percent of the map unit. Slopes are 6 to 45 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 85 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent.  "|"21333780"|"21572281"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333781"|"21572282"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"21333782"|"21572283"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"21333783"|"21572284"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333784"|"21572285"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333863"|"21572364"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pylon soil is a minor component."|"21333864"|"21572365"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Echeta soil is a minor component."|"21333865"|"21572366"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinehill component makes up 85 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans on uplands, fan remnants on uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333866"|"21572367"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21333867"|"21572368"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333868"|"21572369"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333869"|"21572370"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21333870"|"21572371"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinehill component makes up 50 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333871"|"21572372"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pylon component makes up 35 percent of the map unit. Slopes are 3 to 15 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333872"|"21572373"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333851"|"21572352"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanstel soil is a minor component."|"21333852"|"21572353"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pylon soil is a minor component."|"21333853"|"21572354"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinehill, LOAM component makes up 45 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans on uplands, fan remnants on uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333854"|"21572355"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinehill, CLAY LOAM component makes up 40 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans on uplands, fan remnants on uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"21333855"|"21572356"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinehill component makes up 45 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333856"|"21572357"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pylon component makes up 35 percent of the map unit. Slopes are 3 to 15 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333857"|"21572358"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333858"|"21572359"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"21333859"|"21572360"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pylon soil is a minor component."|"21333860"|"21572361"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"21333861"|"21572362"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"21333862"|"21572363"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockypoint, occasionally flooded component makes up 50 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood-plain steps, sedimentary plains. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333960"|"21572461"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boruff, occasionally flooded component makes up 40 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood-plain steps, sedimentary plains. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer, ,  inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during April, May. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 1 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333961"|"21572462"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sodawells soil is a minor component."|"21333962"|"21572463"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Iwait soil is a minor component."|"21333963"|"21572464"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boruff soil is a minor component."|"21333825"|"21572326"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rockypoint component makes up 50 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains on valleys, stream terraces on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333826"|"21572327"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sodawells component makes up 40 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333827"|"21572328"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pathfinder soil is a minor component."|"21333828"|"21572329"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pathfinder component makes up 30 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333821"|"21572322"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rockypoint soil is a minor component."|"21333822"|"21572323"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sodawells component makes up 45 percent of the map unit. Slopes are 0 to 3 percent. This component is on stream terraces on valleys, flood plains on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333823"|"21572324"
03/23/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boruff component makes up 15 percent of the map unit. Slopes are 0 to 3 percent. This component is on flood plains on valleys. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during April, May. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY228WY Lowland (ll)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"21333824"|"21572325"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klinedraw soil is a minor component."|"21333935"|"21572436"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Oldwolf soil is a minor component."|"21333936"|"21572437"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ucross component makes up 45 percent of the map unit. Slopes are 3 to 15 percent. This component is on hills, sedimentary plains. The parent material consists of slope alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333937"|"21572438"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Xema soil is a minor component."|"21333938"|"21572439"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mittenbutte soil is a minor component."|"21333939"|"21572440"
06/04/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairburn component makes up 35 percent of the map unit. Slopes are 3 to 15 percent. This component is on hills, sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333940"|"21572441"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland soil is a minor component."|"21333765"|"21572266"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pitchdraw soil is a minor component."|"21333766"|"21572267"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cromack soil is a minor component."|"21333767"|"21572268"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Samsil soil is a minor component."|"21333768"|"21572269"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ucross component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills on uplands, ridges on uplands. The parent material consists of alluvium over residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333769"|"21572270"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairburn component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on ridges on uplands, hills on uplands. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY262WY Shallow Loamy (swly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 7e. Irrigated land capability classification is 7e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333770"|"21572271"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vanstel component makes up 50 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans on uplands, fan remnants on uplands. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY222WY Loamy (ly)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333873"|"21572374"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pinehill component makes up 35 percent of the map unit. Slopes are 0 to 6 percent. This component is on fan remnants on uplands, alluvial fans on uplands. The parent material consists of alluvium derived from calcareous shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY204WY Clayey (cy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"21333874"|"21572375"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foreleft soil is a minor component."|"21333875"|"21572376"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"21333876"|"21572377"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Taluce component makes up 15 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY166WY Shallow Sandy (SwSy) 10-14 PZ ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333948"|"21572449"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hiland soil is a minor component."|"21333949"|"21572450"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vonalee component makes up 40 percent of the map unit. Slopes are 3 to 15 percent. This component is on hills, sedimentary plains. The parent material consists of eolian deposits and/or slope alluvium derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY150WY Sandy (Sy) 10-14 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333950"|"21572451"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbac soil is a minor component."|"21333951"|"21572452"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Julesburg soil is a minor component."|"21333952"|"21572453"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turnercrest soil is a minor component."|"21333953"|"21572454"
03/02/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Terro component makes up 25 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills, sedimentary plains. The parent material consists of eolian deposits and/or slope alluvium over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY150WY Sandy (Sy) 10-14 PZ ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"21333954"|"21572455"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arwite soil is a minor component."|"21333771"|"21572272"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elwop soil is a minor component."|"21333772"|"21572273"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairburn soil is a minor component."|"21333773"|"21572274"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Julesburg soil is a minor component."|"21333774"|"21572275"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mittenbutte component makes up 15 percent of the map unit. Slopes are 3 to 30 percent. This component is on ridges on sedimentary plains, hills on sedimentary plains. The parent material consists of alluvium and/or colluvium over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY266WY Shallow Sandy (swsy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333775"|"21572276"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vonalf component makes up 40 percent of the map unit. Slopes are 3 to 15 percent. This component is on ridges on sedimentary plains, hills on sedimentary plains. The parent material consists of alluvium and/or eolian deposits derived from calcareous sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (sy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 2 percent.  "|"21333776"|"21572277"
08/20/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Xema component makes up 25 percent of the map unit. Slopes are 3 to 30 percent. This component is on hills on sedimentary plains, ridges on sedimentary plains. The parent material consists of alluvium and/or eolian deposits over residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058BY250WY Sandy (sy)  15-17"" Northern Plains Precipi ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21333777"|"21572278"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21333897"|"21572398"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21333898"|"21572399"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Miscellaneous water is a miscellaneous area."|"21333896"|"21572397"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits is a miscellaneous area."|"21333358"|"21571859"
