05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346767"|"21586006"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346768"|"21586007"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman, extremely bouldery component makes up 60 percent of the map unit. Slopes are 45 to 80 percent. This component is on mountains, glacial-valley walls. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346769"|"21586008"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hargran soil is a minor component."|"21346770"|"21586009"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346771"|"21586010"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 30 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346335"|"21585574"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kadygulch soil is a minor component."|"21346336"|"21585575"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346337"|"21585576"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346338"|"21585577"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346339"|"21585578"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 45 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346340"|"21585579"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 40 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346341"|"21585580"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346342"|"21585581"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 50 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346343"|"21585582"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346344"|"21585583"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346345"|"21585584"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 35 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346346"|"21585585"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Helmville soil is a minor component."|"21346347"|"21585586"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mohaggin soil is a minor component."|"21346348"|"21585587"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346349"|"21585588"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346350"|"21585589"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 55 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346351"|"21585590"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 30 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346352"|"21585591"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346353"|"21585592"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346354"|"21585593"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 65 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346355"|"21585594"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 25 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346356"|"21585595"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346357"|"21585596"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 70 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346358"|"21585597"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 15 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346359"|"21585598"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346360"|"21585599"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346361"|"21585600"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346362"|"21585601"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346363"|"21585602"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 45 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346364"|"21585603"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 40 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 33 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346365"|"21585604"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346366"|"21585605"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 33 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346286"|"21585525"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346285"|"21585524"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346284"|"21585523"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, very stony component makes up 15 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346283"|"21585522"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346282"|"21585521"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346281"|"21585520"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from andesite and/or colluvium derived from rhyolite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346280"|"21585519"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346279"|"21585518"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346278"|"21585517"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes, mountains. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346277"|"21585516"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch, dry soil is a minor component."|"21346276"|"21585515"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346275"|"21585514"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, very stony component makes up 15 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346274"|"21585513"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346273"|"21585512"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346272"|"21585511"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 60 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346271"|"21585510"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346270"|"21585509"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kadygulch soil is a minor component."|"21346269"|"21585508"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 35 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346268"|"21585507"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346267"|"21585506"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346266"|"21585505"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Macmeal soil is a minor component."|"21346265"|"21585504"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kellygulch component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346264"|"21585503"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346263"|"21585502"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kadygulch soil is a minor component."|"21346262"|"21585501"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Curlew soil is a minor component."|"21346261"|"21585500"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346260"|"21585499"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 15 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346259"|"21585498"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haugan component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346258"|"21585497"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kellygulch component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346257"|"21585496"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346256"|"21585495"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346255"|"21585494"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Curlew soil is a minor component."|"21346254"|"21585493"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346253"|"21585492"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346252"|"21585491"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from andesite and/or rhyolite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346251"|"21585490"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346250"|"21585489"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde component makes up 40 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 39 to 72 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346249"|"21585488"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 50 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346248"|"21585487"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"21346247"|"21585486"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott, extremely stony soil is a minor component."|"21346246"|"21585485"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch soil is a minor component."|"21346245"|"21585484"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wilde soil is a minor component."|"21346244"|"21585483"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 80 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21346243"|"21585482"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346242"|"21585481"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346241"|"21585480"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crow soil is a minor component."|"21346240"|"21585479"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 70 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346239"|"21585478"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346238"|"21585477"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 15 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346237"|"21585476"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Macmeal soil is a minor component."|"21346236"|"21585475"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346235"|"21585474"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346234"|"21585473"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 45 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346233"|"21585472"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346232"|"21585471"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 30 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346231"|"21585470"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346230"|"21585469"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch, extremely stony, greater slopes soil is a minor component."|"21346229"|"21585468"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, extremely stony component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346228"|"21585467"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, extremely stony soil is a minor component."|"21346227"|"21585466"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346226"|"21585465"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346225"|"21585464"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Perma soil is a minor component."|"21346224"|"21585463"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346223"|"21585462"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 20 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM138MT Shallow Droughty (swdr)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346222"|"21585461"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 65 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from mixed. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346221"|"21585460"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346220"|"21585459"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 40 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from mixed. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346219"|"21585458"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346218"|"21585457"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kamack soil is a minor component."|"21346217"|"21585456"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kamack component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from mixed. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346216"|"21585455"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346215"|"21585454"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kadygulch soil is a minor component."|"21346214"|"21585453"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, very stony, lesser slopes soil is a minor component."|"21346213"|"21585452"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott, extremely stony component makes up 25 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346212"|"21585451"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 30 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346211"|"21585450"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, very stony component makes up 35 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from igneous and metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346210"|"21585449"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346209"|"21585448"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 30 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346208"|"21585447"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Venapass component makes up 15 percent of the map unit. Slopes are 1 to 3 percent. This component is on marshes on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346057"|"21585296"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah component makes up 20 percent of the map unit. Slopes are 1 to 5 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346056"|"21585295"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru, bouldery component makes up 30 percent of the map unit. Slopes are 1 to 15 percent. This component is on stream terraces, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21346055"|"21585294"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beehive component makes up 40 percent of the map unit. Slopes are 1 to 8 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"21346054"|"21585293"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"21346053"|"21585292"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21346052"|"21585291"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346051"|"21585290"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 15 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346334"|"21585573"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346333"|"21585572"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 40 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from rhyolite and/or andesite and/or granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346332"|"21585571"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346331"|"21585570"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346330"|"21585569"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346329"|"21585568"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Growden component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346328"|"21585567"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346327"|"21585566"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346326"|"21585565"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346325"|"21585564"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346324"|"21585563"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346323"|"21585562"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Growden soil is a minor component."|"21346322"|"21585561"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346321"|"21585560"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346320"|"21585559"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346319"|"21585558"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346318"|"21585557"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346317"|"21585556"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346316"|"21585555"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346315"|"21585554"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346314"|"21585553"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346313"|"21585552"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346312"|"21585551"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wilde soil is a minor component."|"21346311"|"21585550"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346310"|"21585549"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346309"|"21585548"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21346308"|"21585547"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346307"|"21585546"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346306"|"21585545"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346305"|"21585544"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346304"|"21585543"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346303"|"21585542"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346302"|"21585541"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346301"|"21585540"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346300"|"21585539"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346299"|"21585538"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346298"|"21585537"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kadygulch soil is a minor component."|"21346297"|"21585536"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346296"|"21585535"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, extremely stony component makes up 20 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346295"|"21585534"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 65 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346294"|"21585533"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346293"|"21585532"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kadygulch soil is a minor component."|"21346292"|"21585531"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman, very stony component makes up 25 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP904MT Shallow Warm Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346291"|"21585530"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 70 percent of the map unit. Slopes are 30 to 60 percent. This component is on dissected mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from dolomite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346290"|"21585529"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346289"|"21585528"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 30 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346288"|"21585527"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346287"|"21585526"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 55 percent of the map unit. Slopes are 15 to 40 percent. This component is on erosion remnants. The parent material consists of colluvium derived from tertiary deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346076"|"21585315"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crow soil is a minor component."|"21346075"|"21585314"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346074"|"21585313"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Priestlake soil is a minor component."|"21346073"|"21585312"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346072"|"21585311"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 80 percent of the map unit. Slopes are 2 to 15 percent. This component is on alluvial fans. The parent material consists of slope alluvium and/or alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346071"|"21585310"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jurvannah soil is a minor component."|"21346070"|"21585309"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21346069"|"21585308"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jurvannah soil is a minor component."|"21346068"|"21585307"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Beehive soil is a minor component."|"21346067"|"21585306"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"21346066"|"21585305"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 15 percent of the map unit. Slopes are 2 to 20 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium over slope alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346065"|"21585304"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, stony component makes up 75 percent of the map unit. Slopes are 2 to 20 percent. This component is on stream terraces. The parent material consists of stony alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346064"|"21585303"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chillybu component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on marshes on flood plains, mountains. The parent material consists of organic material over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during March, April, May, June. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346063"|"21585302"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346062"|"21585301"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beehive component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"21346061"|"21585300"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21346060"|"21585299"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"21346059"|"21585298"
11/08/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346058"|"21585297"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Roman soil is a minor component."|"21346128"|"21585367"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346127"|"21585366"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346126"|"21585365"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346125"|"21585364"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346124"|"21585363"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346123"|"21585362"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde component makes up 50 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346122"|"21585361"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 35 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346121"|"21585360"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346120"|"21585359"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346119"|"21585358"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 35 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346118"|"21585357"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 30 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from volcanic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346117"|"21585356"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Perma soil is a minor component."|"21346116"|"21585355"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 20 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346115"|"21585354"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346114"|"21585353"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wilde soil is a minor component."|"21346113"|"21585352"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 60 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21346112"|"21585351"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346111"|"21585350"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346110"|"21585349"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346088"|"21585327"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilde soil is a minor component."|"21346087"|"21585326"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leighcan soil is a minor component."|"21346086"|"21585325"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 40 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346085"|"21585324"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346084"|"21585323"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mariel, occasionally ponded component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on proglacial lakes (relict). The parent material consists of organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 88 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346083"|"21585322"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake, occasionally ponded component makes up 65 percent of the map unit. Slopes are 0 to 2 percent. This component is on kettles, drainageways. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346082"|"21585321"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jurvannah soil is a minor component."|"21346081"|"21585320"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew component makes up 15 percent of the map unit. Slopes are 1 to 8 percent. This component is on drainageways. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346080"|"21585319"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haugan component makes up 30 percent of the map unit. Slopes are 15 to 40 percent. This component is on erosion remnants. The parent material consists of tertiary age colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346079"|"21585318"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 55 percent of the map unit. Slopes are 15 to 40 percent. This component is on erosion remnants. The parent material consists of tertiary age colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346078"|"21585317"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haugan component makes up 35 percent of the map unit. Slopes are 15 to 40 percent. This component is on erosion remnants. The parent material consists of tertiary age colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346077"|"21585316"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346149"|"21585388"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch, dry soil is a minor component."|"21346148"|"21585387"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 80 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346147"|"21585386"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346146"|"21585385"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346145"|"21585384"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346144"|"21585383"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, very stony component makes up 80 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346143"|"21585382"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346142"|"21585381"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346141"|"21585380"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346140"|"21585379"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roman soil is a minor component."|"21346139"|"21585378"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346138"|"21585377"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leighcan, lesser slopes soil is a minor component."|"21346137"|"21585376"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolby soil is a minor component."|"21346136"|"21585375"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 80 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346135"|"21585374"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Roman soil is a minor component."|"21346134"|"21585373"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346133"|"21585372"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346132"|"21585371"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 20 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346131"|"21585370"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 70 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346130"|"21585369"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 75 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346129"|"21585368"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 25 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"21346109"|"21585348"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346108"|"21585347"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 40 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346107"|"21585346"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346106"|"21585345"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Macmeal soil is a minor component."|"21346105"|"21585344"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346104"|"21585343"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346103"|"21585342"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346102"|"21585341"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilde, lesser slopes soil is a minor component."|"21346101"|"21585340"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilde, extremely cobbly surface soil is a minor component."|"21346100"|"21585339"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde component makes up 80 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346099"|"21585338"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch soil is a minor component."|"21346098"|"21585337"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott, extremely stony soil is a minor component."|"21346097"|"21585336"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346096"|"21585335"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wilde soil is a minor component."|"21346095"|"21585334"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde, very stony component makes up 80 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 40 to 72 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346094"|"21585333"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346093"|"21585332"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346092"|"21585331"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346091"|"21585330"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346090"|"21585329"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kadygulch, lesser slopes soil is a minor component."|"21346089"|"21585328"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 60 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346170"|"21585409"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346169"|"21585408"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346168"|"21585407"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346167"|"21585406"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346166"|"21585405"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 35 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346165"|"21585404"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346164"|"21585403"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346163"|"21585402"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 40 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346162"|"21585401"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346161"|"21585400"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346160"|"21585399"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346159"|"21585398"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346158"|"21585397"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346157"|"21585396"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346156"|"21585395"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346155"|"21585394"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 35 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346154"|"21585393"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 50 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346153"|"21585392"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346152"|"21585391"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville soil is a minor component."|"21346151"|"21585390"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hun soil is a minor component."|"21346150"|"21585389"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, very stony component makes up 70 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346188"|"21585427"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346187"|"21585426"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346186"|"21585425"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346185"|"21585424"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolby, lesser slopes soil is a minor component."|"21346184"|"21585423"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346183"|"21585422"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolby soil is a minor component."|"21346182"|"21585421"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 85 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346181"|"21585420"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346180"|"21585419"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346179"|"21585418"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 25 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346178"|"21585417"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 65 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346177"|"21585416"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346176"|"21585415"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 40 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346175"|"21585414"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 45 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346174"|"21585413"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346173"|"21585412"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346172"|"21585411"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 25 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346171"|"21585410"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346207"|"21585446"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kamack soil is a minor component."|"21346206"|"21585445"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kamack component makes up 55 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346205"|"21585444"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346204"|"21585443"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346203"|"21585442"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346202"|"21585441"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 30 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346201"|"21585440"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 55 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346200"|"21585439"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346199"|"21585438"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346198"|"21585437"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346197"|"21585436"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mohaggin soil is a minor component."|"21346196"|"21585435"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 35 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346195"|"21585434"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 50 percent of the map unit. Slopes are 40 to 60 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346194"|"21585433"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch soil is a minor component."|"21346193"|"21585432"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346192"|"21585431"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346191"|"21585430"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 80 percent of the map unit. Slopes are 40 to 60 percent. This component is on steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346190"|"21585429"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346189"|"21585428"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 50 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346367"|"21585606"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 25 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346368"|"21585607"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346369"|"21585608"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount component makes up 15 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountains, moderately steep mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346370"|"21585609"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346371"|"21585610"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346372"|"21585611"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 50 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346373"|"21585612"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346374"|"21585613"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346375"|"21585614"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 35 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346376"|"21585615"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mohaggin soil is a minor component."|"21346377"|"21585616"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346378"|"21585617"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346379"|"21585618"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 55 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346380"|"21585619"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 20 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346381"|"21585620"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346382"|"21585621"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 60 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346383"|"21585622"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 25 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346384"|"21585623"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mohaggin soil is a minor component."|"21346385"|"21585624"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346386"|"21585625"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, very stony component makes up 15 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346387"|"21585626"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 40 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346388"|"21585627"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 35 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346389"|"21585628"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346390"|"21585629"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346391"|"21585630"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mohaggin soil is a minor component."|"21346392"|"21585631"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, extremely stony soil is a minor component."|"21346393"|"21585632"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 45 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346394"|"21585633"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 40 percent of the map unit. Slopes are 20 to 40 percent. This component is on moderately steep mountain slopes. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346395"|"21585634"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346396"|"21585635"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346397"|"21585636"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 60 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346398"|"21585637"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 25 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346399"|"21585638"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346400"|"21585639"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346401"|"21585640"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kamack component makes up 70 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346402"|"21585641"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kamack soil is a minor component."|"21346403"|"21585642"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin component makes up 20 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346404"|"21585643"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346405"|"21585644"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 70 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from volcanic rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM138MT Shallow Droughty (swdr)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346406"|"21585645"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Borky component makes up 20 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from rhyolite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346407"|"21585646"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346408"|"21585647"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346409"|"21585648"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 50 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from mixed. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346410"|"21585649"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 35 percent of the map unit. Slopes are 20 to 40 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM138MT Shallow Droughty (swdr)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346411"|"21585650"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346412"|"21585651"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Perma soil is a minor component."|"21346413"|"21585652"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346414"|"21585653"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haugan component makes up 40 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346415"|"21585654"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Perma soil is a minor component."|"21346416"|"21585655"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 15 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346417"|"21585656"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346418"|"21585657"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch component makes up 35 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346419"|"21585658"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346420"|"21585659"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott, extremely stony soil is a minor component."|"21346421"|"21585660"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde component makes up 55 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 39 to 72 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346422"|"21585661"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 30 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21346423"|"21585662"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilde, greater slopes soil is a minor component."|"21346424"|"21585663"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346425"|"21585664"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 45 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346426"|"21585665"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 30 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346427"|"21585666"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lolopeak soil is a minor component."|"21346428"|"21585667"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346429"|"21585668"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346430"|"21585669"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, very stony component makes up 15 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP902MT Shallow Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346431"|"21585670"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, stony component makes up 75 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 25 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346432"|"21585671"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hun soil is a minor component."|"21346433"|"21585672"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346434"|"21585673"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 55 percent of the map unit. Slopes are 2 to 25 percent. This component is on ridges. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 25 to 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346435"|"21585674"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mohaggin soil is a minor component."|"21346436"|"21585675"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 2 to 25 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346437"|"21585676"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 20 percent of the map unit. Slopes are 2 to 25 percent. This component is on ridges. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346438"|"21585677"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346439"|"21585678"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346440"|"21585679"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346441"|"21585680"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Growden component makes up 75 percent of the map unit. Slopes are 2 to 20 percent. This component is on ridges. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346442"|"21585681"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 2 to 30 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346443"|"21585682"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346444"|"21585683"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 40 percent of the map unit. Slopes are 5 to 35 percent. This component is on ridges. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346445"|"21585684"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 30 percent of the map unit. Slopes are 5 to 35 percent. This component is on ridges. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 25 to 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346446"|"21585685"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346447"|"21585686"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 5 to 35 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346448"|"21585687"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346449"|"21585688"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Growden component makes up 30 percent of the map unit. Slopes are 5 to 35 percent. This component is on ridges. The parent material consists of volcanic ash over colluvium derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346450"|"21585689"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 5 to 35 percent. This component is on ridges. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346451"|"21585690"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346452"|"21585691"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 45 percent of the map unit. Slopes are 5 to 35 percent. This component is on ridges. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 25 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346453"|"21585692"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346454"|"21585693"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 55 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountainsides. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346455"|"21585694"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346456"|"21585695"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mohaggin soil is a minor component."|"21346457"|"21585696"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346458"|"21585697"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346459"|"21585698"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Agneston component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 33 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346460"|"21585699"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346461"|"21585700"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346462"|"21585701"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346463"|"21585702"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346464"|"21585703"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 55 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346465"|"21585704"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 60 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346466"|"21585705"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 15 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346467"|"21585706"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 15 percent of the map unit. Slopes are 10 to 25 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 50 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346468"|"21585707"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346469"|"21585708"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346470"|"21585709"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346471"|"21585710"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346472"|"21585711"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346473"|"21585712"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin component makes up 50 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346474"|"21585713"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 25 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountainsides. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346475"|"21585714"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346476"|"21585715"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 15 percent of the map unit. Slopes are 10 to 25 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 50 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346477"|"21585716"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346478"|"21585717"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346479"|"21585718"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346480"|"21585719"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun, moist component makes up 15 percent of the map unit. Slopes are 10 to 25 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 50 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346481"|"21585720"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 70 percent of the map unit. Slopes are 15 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346482"|"21585721"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346483"|"21585722"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346484"|"21585723"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Growden component makes up 40 percent of the map unit. Slopes are 8 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over colluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346485"|"21585724"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 25 percent of the map unit. Slopes are 0 to 8 percent. This component is on drainageways on mountain slopes. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 3 inches during May, June, July. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346486"|"21585725"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolopeak component makes up 25 percent of the map unit. Slopes are 8 to 50 percent. This component is on mountainsides. The parent material consists of volcanic ash over sandy and gravelly colluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346487"|"21585726"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346488"|"21585727"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubycreek soil is a minor component."|"21346489"|"21585728"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 20 percent of the map unit. Slopes are 10 to 40 percent. This component is on upland slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346490"|"21585729"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake component makes up 50 percent of the map unit. Slopes are 10 to 50 percent. This component is on upland slopes. The parent material consists of colluvium and/or till derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346491"|"21585730"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 20 percent of the map unit. Slopes are 2 to 10 percent. This component is on drainageways on upland slopes. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346492"|"21585731"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346493"|"21585732"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346494"|"21585733"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hun component makes up 20 percent of the map unit. Slopes are 40 to 60 percent. This component is on cirque headwalls. The parent material consists of volcanic ash over colluvium and/or till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 50 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346495"|"21585734"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346496"|"21585735"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346497"|"21585736"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake component makes up 45 percent of the map unit. Slopes are 40 to 75 percent. This component is on cirque headwalls. The parent material consists of colluvium and/or till derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346498"|"21585737"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346499"|"21585738"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346500"|"21585739"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hun soil is a minor component."|"21346501"|"21585740"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount soil is a minor component."|"21346502"|"21585741"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman, extremely bouldery component makes up 20 percent of the map unit. Slopes are 25 to 80 percent. This component is on cirque headwalls. The parent material consists of volcanic ash over colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346503"|"21585742"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346504"|"21585743"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346505"|"21585744"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346506"|"21585745"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 20 percent of the map unit. Slopes are 25 to 80 percent. This component is on cirque headwalls. The parent material consists of volcanic ash over colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346507"|"21585746"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346508"|"21585747"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346509"|"21585748"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Teewinot component makes up 20 percent of the map unit. Slopes are 45 to 90 percent. This component is on cirque headwalls. The parent material consists of colluvium and/or till over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346510"|"21585749"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346511"|"21585750"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 35 percent of the map unit. Slopes are 25 to 75 percent. This component is on cirque headwalls. The parent material consists of volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346512"|"21585751"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346513"|"21585752"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346514"|"21585753"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Roman soil is a minor component."|"21346515"|"21585754"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on peaks. The parent material consists of till over residuum weathered from granite and/or mixed. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346516"|"21585755"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake component makes up 55 percent of the map unit. Slopes are 15 to 50 percent. This component is on peaks. The parent material consists of colluvium and/or till derived from granite and/or mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346517"|"21585756"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346518"|"21585757"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346519"|"21585758"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on moraines on cirque floors. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346520"|"21585759"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Vitricryands component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on moraines on cirque floors. The parent material consists of volcanic ash over till derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346521"|"21585760"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 15 percent of the map unit. Slopes are 0 to 8 percent. This component is on cirque floors. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346522"|"21585761"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346523"|"21585762"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346524"|"21585763"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on moraines on cirque floors. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346525"|"21585764"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hoxie component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on cirque floors. The parent material consists of fine-silty till derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is very high.  Shrink-swell potential is moderate. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346526"|"21585765"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346527"|"21585766"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346528"|"21585767"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on cirque floors. The parent material consists of till over residuum weathered from granite and/or mixed. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346529"|"21585768"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on cirque floors. The parent material consists of volcanic ash over till derived from granite and gneiss and/or mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346530"|"21585769"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346531"|"21585770"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346532"|"21585771"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubycreek soil is a minor component."|"21346533"|"21585772"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346534"|"21585773"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 40 percent of the map unit. Slopes are 5 to 45 percent. This component is on mountain slopes. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346535"|"21585774"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake component makes up 30 percent of the map unit. Slopes are 5 to 45 percent. This component is on mountain slopes. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346536"|"21585775"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repkie, extremely bouldery component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines, mountains. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346537"|"21585776"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Repkie soil is a minor component."|"21346538"|"21585777"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346539"|"21585778"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Curlew soil is a minor component."|"21346540"|"21585779"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely bouldery component makes up 40 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines. The parent material consists of till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346541"|"21585780"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake, extremely bouldery component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346542"|"21585781"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Priestlake soil is a minor component."|"21346543"|"21585782"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman, extremely bouldery component makes up 50 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346544"|"21585783"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 15 percent of the map unit. Slopes are 0 to 8 percent. This component is on depressions on moraines. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 0 inches during May, June, July. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346545"|"21585784"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346546"|"21585785"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru, extremely bouldery component makes up 65 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346547"|"21585786"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346548"|"21585787"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 15 percent of the map unit. Slopes are 0 to 8 percent. This component is on depressions on moraines. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346549"|"21585788"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek, extremely bouldery component makes up 15 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346550"|"21585789"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Priestlake soil is a minor component."|"21346551"|"21585790"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Roman component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346552"|"21585791"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Rubycreek component makes up 30 percent of the map unit. Slopes are 8 to 45 percent. This component is on moraines. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346553"|"21585792"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346554"|"21585793"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lilylake component makes up 15 percent of the map unit. Slopes are 0 to 8 percent. This component is on depressions on moraines. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346555"|"21585794"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346556"|"21585795"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repkie, extremely bouldery component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, moraines on glacial-valley floors. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346557"|"21585796"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346558"|"21585797"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew, very bouldery component makes up 10 percent of the map unit. Slopes are 0 to 8 percent. This component is on glacial-valley floors. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BS327MT Wet Meadow (wm) 20""+ P.z. ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346559"|"21585798"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely bouldery component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines, stream terraces. The parent material consists of till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346560"|"21585799"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346561"|"21585800"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake, extremely bouldery component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors, mountains. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346562"|"21585801"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman, extremely bouldery component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors, mountains. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346563"|"21585802"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, extremely bouldery soil is a minor component."|"21346564"|"21585803"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah, very bouldery component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on glacial-valley floors, mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches (depth from the mineral surface is 6 inches) during May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R043BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346565"|"21585804"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346566"|"21585805"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346567"|"21585806"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jeru soil is a minor component."|"21346568"|"21585807"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346569"|"21585808"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346570"|"21585809"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines. The parent material consists of till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346571"|"21585810"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on glacial-valley floors. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346572"|"21585811"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek, bouldery component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, moraines on glacial-valley floors. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346573"|"21585812"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beehive component makes up 20 percent of the map unit. Slopes are 2 to 10 percent. This component is on flood plains on glacial-valley floors. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"21346574"|"21585813"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mariel soil is a minor component."|"21346575"|"21585814"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 30 percent of the map unit. Slopes are 0 to 8 percent. This component is on drainageways on glacial-valley floors. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 0 inches during May, June, July. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346576"|"21585815"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346577"|"21585816"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346578"|"21585817"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jeru soil is a minor component."|"21346579"|"21585818"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346580"|"21585819"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346581"|"21585820"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines. The parent material consists of till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346582"|"21585821"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on glacial-valley floors. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346583"|"21585822"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lilylake soil is a minor component."|"21346584"|"21585823"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Priestlake soil is a minor component."|"21346585"|"21585824"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346586"|"21585825"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346587"|"21585826"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346588"|"21585827"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on glacial-valley floors. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346589"|"21585828"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346590"|"21585829"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346591"|"21585830"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poin, rubbly component makes up 25 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346592"|"21585831"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jeru, extremely bouldery soil is a minor component."|"21346593"|"21585832"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346594"|"21585833"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Poin soil is a minor component."|"21346595"|"21585834"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Priestlake soil is a minor component."|"21346596"|"21585835"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346597"|"21585836"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 30 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls. The parent material consists of colluvium and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346598"|"21585837"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346599"|"21585838"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346600"|"21585839"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, extremely stony component makes up 30 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346601"|"21585840"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roman, extremely bouldery soil is a minor component."|"21346602"|"21585841"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru, extremely bouldery component makes up 45 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium and/or till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346603"|"21585842"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346604"|"21585843"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346605"|"21585844"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubycreek, extremely bouldery soil is a minor component."|"21346606"|"21585845"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hargran, extremely bouldery soil is a minor component."|"21346607"|"21585846"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru, extremely bouldery component makes up 50 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, moraines, mountains. The parent material consists of colluvium and/or till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346608"|"21585847"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jeru, extremely bouldery, dry soil is a minor component."|"21346609"|"21585848"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, extremely bouldery soil is a minor component."|"21346610"|"21585849"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346611"|"21585850"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346612"|"21585851"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hargran, extremely bouldery soil is a minor component."|"21346613"|"21585852"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, extremely bouldery soil is a minor component."|"21346614"|"21585853"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake, extremely bouldery component makes up 45 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium and/or till derived from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 39 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346615"|"21585854"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek, extremely bouldery component makes up 35 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls, mountains. The parent material consists of volcanic ash over colluvium and/or till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346616"|"21585855"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346617"|"21585856"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346618"|"21585857"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hargran soil is a minor component."|"21346619"|"21585858"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346620"|"21585859"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 45 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls. The parent material consists of volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346621"|"21585860"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 40 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, moraines. The parent material consists of till and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346622"|"21585861"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346623"|"21585862"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346624"|"21585863"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubycreek soil is a minor component."|"21346625"|"21585864"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346626"|"21585865"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Vitricryands component makes up 45 percent of the map unit. Slopes are 45 to 80 percent. This component is on moraines on glacial-valley walls. The parent material consists of volcanic ash over till derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 50 inches during April, May, June, July. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346627"|"21585866"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquandic Cryaquepts component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, moraines. The parent material consists of volcanic ash over colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil meets hydric criteria.   "|"21346628"|"21585867"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346629"|"21585868"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubycreek soil is a minor component."|"21346630"|"21585869"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346631"|"21585870"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346632"|"21585871"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek component makes up 40 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls. The parent material consists of volcanic ash over till and/or colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346633"|"21585872"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 25 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, moraines. The parent material consists of till and/or colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346634"|"21585873"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346635"|"21585874"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346636"|"21585875"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Roman soil is a minor component."|"21346637"|"21585876"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346638"|"21585877"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jeru component makes up 40 percent of the map unit. Slopes are 45 to 80 percent. This component is on glacial-valley walls, moraines. The parent material consists of till and/or colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346639"|"21585878"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hargran component makes up 25 percent of the map unit. Slopes are 45 to 80 percent. This component is on avalanche chutes on glacial-valley walls. The parent material consists of colluvium and/or till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July. Organic matter content in the surface horizon is about 50 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346640"|"21585879"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346641"|"21585880"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346642"|"21585881"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hargran soil is a minor component."|"21346643"|"21585882"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake component makes up 25 percent of the map unit. Slopes are 45 to 90 percent. This component is on glacial-valley walls. The parent material consists of colluvium and/or till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346644"|"21585883"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346645"|"21585884"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 65 percent of the map unit. Slopes are 15 to 50 percent. This component is on landslides. The parent material consists of mass movement deposits derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346646"|"21585885"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on drainageways on landslides. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent. This component is in the F043BP906MT Subirrigated Cold Woodland ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346647"|"21585886"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolby, very stony soil is a minor component."|"21346648"|"21585887"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346649"|"21585888"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346650"|"21585889"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346651"|"21585890"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott, extremely stony soil is a minor component."|"21346652"|"21585891"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde, extremely stony component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 39 to 72 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346653"|"21585892"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Totelake soil is a minor component."|"21346654"|"21585893"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346655"|"21585894"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346656"|"21585895"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott, extremely stony component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346657"|"21585896"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 39 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346658"|"21585897"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kadygulch, very bouldery component makes up 35 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346659"|"21585898"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kadygulch, lesser slopes soil is a minor component."|"21346660"|"21585899"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346661"|"21585900"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346662"|"21585901"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch, moist soil is a minor component."|"21346663"|"21585902"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, extremely stony component makes up 15 percent of the map unit. Slopes are 60 to 75 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346664"|"21585903"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 75 percent of the map unit. Slopes are 60 to 75 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346665"|"21585904"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346666"|"21585905"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346667"|"21585906"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346668"|"21585907"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 35 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346669"|"21585908"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21346670"|"21585909"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346671"|"21585910"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346672"|"21585911"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346673"|"21585912"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346674"|"21585913"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346675"|"21585914"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346676"|"21585915"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, extremely stony component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346677"|"21585916"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346678"|"21585917"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 45 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346679"|"21585918"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby, very stony component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346680"|"21585919"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leighcan, lesser slopes soil is a minor component."|"21346681"|"21585920"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, extremely stony component makes up 15 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346682"|"21585921"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346683"|"21585922"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346684"|"21585923"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346685"|"21585924"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 80 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346686"|"21585925"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346687"|"21585926"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346688"|"21585927"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346689"|"21585928"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346690"|"21585929"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 50 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346691"|"21585930"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klootch, lesser slopes soil is a minor component."|"21346692"|"21585931"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount, very stony soil is a minor component."|"21346693"|"21585932"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 35 percent of the map unit. Slopes are 60 to 70 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"21346694"|"21585933"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346695"|"21585934"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346696"|"21585935"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346697"|"21585936"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Shermount soil is a minor component."|"21346698"|"21585937"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, extremely stony component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346699"|"21585938"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346700"|"21585939"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346701"|"21585940"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346702"|"21585941"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346703"|"21585942"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346704"|"21585943"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 30 to 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346705"|"21585944"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346706"|"21585945"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346707"|"21585946"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346708"|"21585947"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Tolby soil is a minor component."|"21346709"|"21585948"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346710"|"21585949"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 50 percent of the map unit. Slopes are 50 to 90 percent. This component is on landslides on mountain slopes. The parent material consists of mass movement deposits derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346711"|"21585950"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 25 percent of the map unit. Slopes are 50 to 90 percent. This component is on landslides on mountain slopes. The parent material consists of sandy and gravelly mass movement deposits derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 30 to 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346712"|"21585951"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346713"|"21585952"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346714"|"21585953"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Klootch soil is a minor component."|"21346715"|"21585954"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 75 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346716"|"21585955"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 15 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346717"|"21585956"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346718"|"21585957"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346719"|"21585958"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Totelake soil is a minor component."|"21346720"|"21585959"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott, extremely stony soil is a minor component."|"21346721"|"21585960"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Specie, extremely stony component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 39 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346722"|"21585961"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346723"|"21585962"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Specie, extremely stony, lesser slopes soil is a minor component."|"21346724"|"21585963"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346725"|"21585964"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Specie, extremely stony component makes up 40 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346726"|"21585965"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott, extremely stony component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346727"|"21585966"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346728"|"21585967"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346729"|"21585968"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 50 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346730"|"21585969"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott, extremely stony component makes up 15 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346731"|"21585970"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Specie, very stony component makes up 25 percent of the map unit. Slopes are 60 to 80 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 39 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346732"|"21585971"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Specie, very stony, lesser slopes soil is a minor component."|"21346733"|"21585972"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346734"|"21585973"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346735"|"21585974"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, very stony component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346736"|"21585975"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, extremely stony component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346737"|"21585976"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Perma soil is a minor component."|"21346738"|"21585977"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346739"|"21585978"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346740"|"21585979"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346741"|"21585980"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman, very stony component makes up 45 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM138MT Shallow Droughty (swdr)   Lru 43b-m ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346742"|"21585981"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 25 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346743"|"21585982"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Perma soil is a minor component."|"21346744"|"21585983"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346745"|"21585984"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346746"|"21585985"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346747"|"21585986"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Holter soil is a minor component."|"21346748"|"21585987"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 45 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346749"|"21585988"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sharrott component makes up 25 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite and gneiss. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346750"|"21585989"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346751"|"21585990"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346752"|"21585991"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Leighcan soil is a minor component."|"21346753"|"21585992"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Lolopeak soil is a minor component."|"21346754"|"21585993"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolby component makes up 50 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of sandy and gravelly colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346755"|"21585994"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 25 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346756"|"21585995"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346757"|"21585996"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346758"|"21585997"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Helmville soil is a minor component."|"21346759"|"21585998"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 50 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346760"|"21585999"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 25 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346761"|"21586000"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Mariel soil is a minor component."|"21346763"|"21586002"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Roman soil is a minor component."|"21346764"|"21586003"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 50 percent of the map unit. Slopes are 0 to 8 percent. This component is on drainageways on glacial-valley floors. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346765"|"21586004"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Oxyaquic Dystrocryepts component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on glacial-valley floors, stream terraces on glacial-valley floors. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 36 inches during April, May, June, July. Organic matter content in the surface horizon is about 50 percent.  Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.   "|"21346766"|"21586005"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346778"|"21586017"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"21346779"|"21586018"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubycreek, extremely bouldery soil is a minor component."|"21346780"|"21586019"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, extremely stony component makes up 25 percent of the map unit. Slopes are 45 to 90 percent. This component is on cirque headwalls. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP902MT Shallow Cold Woodland, Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346781"|"21586020"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346787"|"21586026"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346788"|"21586027"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lilylake soil is a minor component."|"21346789"|"21586028"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubycreek soil is a minor component."|"21346790"|"21586029"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shermount, extremely bouldery component makes up 30 percent of the map unit. Slopes are 10 to 45 percent. This component is on weakly glaciated ridges. The parent material consists of till over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346791"|"21586030"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman, extremely bouldery component makes up 55 percent of the map unit. Slopes are 10 to 45 percent. This component is on weakly glaciated mountain slopes. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346792"|"21586031"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346772"|"21586011"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346773"|"21586012"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch, very stony component makes up 20 percent of the map unit. Slopes are 10 to 45 percent. This component is on weakly glaciated mountain slopes. The parent material consists of colluvium derived from quartzite and/or till derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346774"|"21586013"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shermount soil is a minor component."|"21346775"|"21586014"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rubycreek, extremely bouldery component makes up 50 percent of the map unit. Slopes are 10 to 45 percent. This component is on weakly glaciated mountain slopes. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346776"|"21586015"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lilylake component makes up 20 percent of the map unit. Slopes are 0 to 12 percent. This component is on weakly glaciated mountain slopes. The parent material consists of organic material over alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during May, June, July, August. Organic matter content in the surface horizon is about 40 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346777"|"21586016"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repkie, extremely bouldery component makes up 30 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, moraines. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346793"|"21586032"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sharrott soil is a minor component."|"21346794"|"21586033"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka, extremely bouldery component makes up 50 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountains, moraines. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346795"|"21586034"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew component makes up 10 percent of the map unit. Slopes are 0 to 8 percent. This component is on depressions on moraines. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BY181MT Wet Meadow (wm)   Lru 43b-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346796"|"21586035"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Losthorse soil is a minor component."|"21346797"|"21586036"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346798"|"21586037"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346799"|"21586038"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Repp soil is a minor component."|"21346800"|"21586039"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holter component makes up 50 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346801"|"21586040"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolman component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium over residuum weathered from quartzite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346802"|"21586041"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wilde component makes up 15 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountain slopes. The parent material consists of colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346803"|"21586042"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346035"|"21585274"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hun soil is a minor component."|"21346036"|"21585275"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata, very stony component makes up 25 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines. The parent material consists of volcanic ash over drift derived from sandstone and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 8 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346037"|"21585276"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21346038"|"21585277"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando component makes up 30 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines. The parent material consists of volcanic ash over colluvium and/or till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346039"|"21585278"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21346040"|"21585279"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21346762"|"21586001"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jeru soil is a minor component."|"21346804"|"21586043"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Priestlake soil is a minor component."|"21346805"|"21586044"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346806"|"21586045"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Littlesalmon component makes up 20 percent of the map unit. Slopes are 30 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of volcanic ash over colluvium and/or till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346807"|"21586046"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, extremely stony component makes up 31 percent of the map unit. Slopes are 30 to 80 percent. This component is on cirque headwalls, mountains. The parent material consists of residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP902MT Whitebark Pine, Whitebark Pine-subalpine Fir ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"21346808"|"21586047"
03/19/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346809"|"21586048"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Jeru soil is a minor component."|"21346810"|"21586049"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Littlesalmon soil is a minor component."|"21346811"|"21586050"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Matcher soil is a minor component."|"21346812"|"21586051"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Priestlake component makes up 35 percent of the map unit. Slopes are 0 to 20 percent. This component is on mountains, ridges. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346813"|"21586052"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood component makes up 25 percent of the map unit. Slopes are 0 to 20 percent. This component is on ridges, mountains. The parent material consists of residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346814"|"21586053"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346815"|"21586054"
02/01/2012 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346816"|"21586055"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"21346028"|"21585267"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bata, very stony component makes up 15 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines. The parent material consists of volcanic ash over drift derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 8 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346029"|"21585268"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"21346030"|"21585269"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Caseypeak soil is a minor component."|"21346031"|"21585270"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cryohemists soil is a minor component."|"21346032"|"21585271"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando, extremely bouldery component makes up 30 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines. The parent material consists of drift derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346033"|"21585272"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Littlesalmon component makes up 20 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines. The parent material consists of volcanic ash over drift derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346034"|"21585273"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 45 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346956"|"21586195"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346046"|"21585285"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jeru soil is a minor component."|"21346047"|"21585286"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 40 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of volcanic ash over colluvium derived from quartzite and/or dolomite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346048"|"21585287"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21346049"|"21585288"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sig component makes up 15 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of colluvium derived from sandstone and siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346050"|"21585289"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346041"|"21585280"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Waldbillig soil is a minor component."|"21346042"|"21585281"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"21346043"|"21585282"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Klootch component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on cirque headwalls, cirque walls, patterned ground. The parent material consists of volcanic ash over colluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346044"|"21585283"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sig component makes up 25 percent of the map unit. Slopes are 45 to 70 percent. This component is on cirque headwalls. The parent material consists of colluvium derived from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346045"|"21585284"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on drainageways on stream terraces, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY182MT Bottomland 44a Lru P, Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346826"|"21586065"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"21346827"|"21586066"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Shallow To Gravel (swgr)   Lru 44a-b, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346828"|"21586067"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 40 inches during May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AY150MT Bottomland 44a Lru P, Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7e. This soil does not meet hydric criteria.   "|"21346829"|"21586068"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sheafman soil is a minor component."|"21346857"|"21586096"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Victor soil is a minor component."|"21346858"|"21586097"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Victor soil is a minor component."|"21346859"|"21586098"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F044AP905MT Upland Warm Woodland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346860"|"21586099"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sheafman component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Shallow To Gravel (swgr)   Lru 44a-b, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346861"|"21586100"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 50 percent of the map unit. Slopes are 4 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346960"|"21586199"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely stony component makes up 45 percent of the map unit. Slopes are 4 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of stony and bouldery outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21346961"|"21586200"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Nirling soil is a minor component."|"21346962"|"21586201"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Groff soil is a minor component."|"21346833"|"21586072"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew component makes up 65 percent of the map unit. Slopes are 0 to 2 percent. This component is on abandoned channels on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 3 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY080MT Bottomland 44a Lru P, Riparian Meadow (rm)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346834"|"21586073"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 40 inches during May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AY150MT Bottomland 44a Lru P, Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21346835"|"21586074"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fredburr soil is a minor component."|"21346836"|"21586075"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 65 percent of the map unit. Slopes are 8 to 45 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP808MT Shallow To Gravel (swgr)   Lru 44a-b, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346823"|"21586062"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"21346824"|"21586063"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew component makes up 25 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY080MT Bottomland 44a Lru P, Riparian Meadow (rm)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346825"|"21586064"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolo component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on inset fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Loamy (lo)   Lru 44a-a, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"21346939"|"21586178"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"21346940"|"21586179"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dominic component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB134MT Shallow To Gravel (swgr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346980"|"21586219"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losttrail component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA032MT Loamy (lo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346981"|"21586220"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Overwhich soil is a minor component."|"21346982"|"21586221"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Riverrun soil is a minor component."|"21346983"|"21586222"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Grayhorse component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, drainageways on inset fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 28 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"21346830"|"21586069"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Capiron soil is a minor component."|"21346831"|"21586070"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Fairway soil is a minor component."|"21346832"|"21586071"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete, very stony component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on intermontane basins, outwash fans. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21346837"|"21586076"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Sheafman soil is a minor component."|"21346838"|"21586077"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sheafman component makes up 80 percent of the map unit. Slopes are 4 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Shallow To Gravel (swgr)   Lru 44a-b, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346839"|"21586078"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chereete soil is a minor component."|"21346840"|"21586079"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Victor soil is a minor component."|"21346841"|"21586080"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346842"|"21586081"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Burnt Fork soil is a minor component."|"21346843"|"21586082"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Brid soil is a minor component."|"21346844"|"21586083"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hartbench component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Loamy (lo)   Lru 44a-a, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21346847"|"21586086"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clasoil soil is a minor component."|"21346848"|"21586087"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely stony component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments on outwash fans, intermontane basins. The parent material consists of colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F044AP905MT Upland Warm Woodland 44a Lru P ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346849"|"21586088"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chereete, stony soil is a minor component."|"21346850"|"21586089"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Repkie, bouldery soil is a minor component."|"21346851"|"21586090"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Overwhich soil is a minor component."|"21346852"|"21586091"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Groff component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on intermontane basins, drainageways on outwash fans. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria.   "|"21346853"|"21586092"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew, rarely flooded component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY182MT Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346854"|"21586093"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Fredburr soil is a minor component."|"21346913"|"21586152"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew, rarely flooded component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, abandoned channels on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY080MT Riparian Meadow (rm)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346912"|"21586151"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun, rarely flooded component makes up 70 percent of the map unit. Slopes are 0 to 2 percent. This component is on intermontane basins, flood-plain steps. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 40 inches during May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21346911"|"21586150"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"21346910"|"21586149"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"21346909"|"21586148"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"21346908"|"21586147"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 40 inches during May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AY150MT Bottomland 44a Lru P, Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21346907"|"21586146"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Wemple soil is a minor component."|"21346906"|"21586145"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Durston component makes up 40 percent of the map unit. Slopes are 5 to 15 percent. This component is on intermontane basins, hillslopes. The parent material consists of loess over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BM032MT Loamy (lo)   Lru 43b-m ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346905"|"21586144"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"||"The Wickes component makes up 55 percent of the map unit. Slopes are 5 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"21346904"|"21586143"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chereete, very stony soil is a minor component."|"21346938"|"21586177"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repkie, bouldery component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP911MT Upland Warm Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346937"|"21586176"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, bouldery component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP911MT Upland Warm Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346936"|"21586175"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Nirling soil is a minor component."|"21346926"|"21586165"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete, stony component makes up 25 percent of the map unit. Slopes are 15 to 25 percent. This component is on escarpments on outwash fans, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346925"|"21586164"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely stony component makes up 70 percent of the map unit. Slopes are 15 to 25 percent. This component is on intermontane basins, escarpments on outwash fans. The parent material consists of stony and bouldery colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346924"|"21586163"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on intermontane basins, outwash fans. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346856"|"21586095"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clasoil soil is a minor component."|"21346846"|"21586085"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hartbench component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AP808MT Loamy (lo)   Lru 44a-a, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21346845"|"21586084"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sheafman soil is a minor component."|"21346918"|"21586157"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F044AP905MT Upland Warm Woodland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346917"|"21586156"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sheafman soil is a minor component."|"21346920"|"21586159"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F044AP905MT Upland Warm Woodland 44a Lru P ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346919"|"21586158"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverrun component makes up 15 percent of the map unit. Slopes are 2 to 6 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 40 inches during May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AY150MT Bottomland 44a Lru P, Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"21346916"|"21586155"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poverty component makes up 15 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 17 inches) during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y, Subirrigated Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 4w. This soil meets hydric criteria.   "|"21346915"|"21586154"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, rubbly component makes up 70 percent of the map unit. Slopes are 4 to 35 percent. This component is on escarpments, intermontane basins. The parent material consists of colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Shallow To Gravel (swgr)   Lru 44a-b, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346914"|"21586153"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on flood plains on glacial-valley floors. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 9 inches during May, June, July. Organic matter content in the surface horizon is about 50 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"21346951"|"21586190"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Crawfish soil is a minor component."|"21346950"|"21586189"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on moraines on glacial-valley floors. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 33 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346949"|"21586188"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346948"|"21586187"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346947"|"21586186"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346955"|"21586194"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hargran soil is a minor component."|"21346954"|"21586193"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346953"|"21586192"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346952"|"21586191"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 25 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines, mountains. The parent material consists of volcanic ash over till derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346995"|"21586234"
01/14/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sig component makes up 30 percent of the map unit. Slopes are 10 to 35 percent. This component is on ground moraines, mountains. The parent material consists of drift over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346994"|"21586233"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Jeru soil is a minor component."|"21346993"|"21586232"
09/02/2015 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bata soil is a minor component."|"21346992"|"21586231"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Finn soil is a minor component."|"21346991"|"21586230"
08/22/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346990"|"21586229"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains. The parent material consists of alluvium derived from mixed. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"21346946"|"21586185"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beehive component makes up 45 percent of the map unit. Slopes are 1 to 8 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches during April, May, June. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346945"|"21586184"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Water soil is a minor component."|"21346944"|"21586183"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bandy soil is a minor component."|"21346822"|"21586061"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Totelake soil is a minor component."|"21346821"|"21586060"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Totelake component makes up 45 percent of the map unit. Slopes are 20 to 50 percent. This component is on landslides. The parent material consists of sandy and gravelly mass movement deposits derived from granite. Depth to a root restrictive layer, bedrock, paralithic, is 40 to 72 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346820"|"21586059"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Kellygulch soil is a minor component."|"21346819"|"21586058"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346818"|"21586057"
02/25/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Macmeal component makes up 30 percent of the map unit. Slopes are 20 to 50 percent. This component is on landslides. The parent material consists of colluvium and/or mass movement deposits derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 40 to 72 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346817"|"21586056"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crawfish component makes up 50 percent of the map unit. Slopes are 45 to 70 percent. This component is on cirque headwalls. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346786"|"21586025"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roman component makes up 20 percent of the map unit. Slopes are 15 to 50 percent. This component is on cirque headwalls. The parent material consists of volcanic ash over till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 60 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346785"|"21586024"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hun soil is a minor component."|"21346784"|"21586023"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rubble land soil is a minor component."|"21346783"|"21586022"
08/09/2010 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346782"|"21586021"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poverty soil is a minor component."|"21346875"|"21586114"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nirling component makes up 15 percent of the map unit. Slopes are 2 to 8 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y, Subirrigated Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria.   "|"21346874"|"21586113"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 75 percent of the map unit. Slopes are 8 to 35 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F044AP905MT Upland Warm Woodland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346873"|"21586112"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Poverty soil is a minor component."|"21346855"|"21586094"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Victor soil is a minor component."|"21346862"|"21586101"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments on outwash fans, intermontane basins. The parent material consists of colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F044AP905MT Upland Warm Woodland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346863"|"21586102"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sheafman component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on escarpments on outwash fans, intermontane basins. The parent material consists of colluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Shallow To Gravel (swgr)   Lru 44a-b, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346864"|"21586103"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely stony component makes up 70 percent of the map unit. Slopes are 8 to 15 percent. This component is on intermontane basins, outwash fans. The parent material consists of stony and bouldery outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346957"|"21586196"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete, stony component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346958"|"21586197"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Nirling soil is a minor component."|"21346959"|"21586198"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346921"|"21586160"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poverty component makes up 40 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, outwash fans. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 4w. This soil meets hydric criteria.   "|"21346922"|"21586161"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Bandy soil is a minor component."|"21346923"|"21586162"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sheafman component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AB134MT Shallow To Gravel (swgr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346865"|"21586104"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Victor soil is a minor component."|"21346866"|"21586105"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blossberg component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria.   "|"21346867"|"21586106"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Overwhich component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash fans, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346868"|"21586107"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Victor soil is a minor component."|"21346869"|"21586108"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poverty component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 4w. This soil meets hydric criteria.   "|"21346930"|"21586169"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Chereete soil is a minor component."|"21346931"|"21586170"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Nirling soil is a minor component."|"21346932"|"21586171"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Losthorse, extremely stony component makes up 65 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of stony and bouldery outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"21346927"|"21586166"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Nirling soil is a minor component."|"21346928"|"21586167"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poverty component makes up 25 percent of the map unit. Slopes are 1 to 4 percent. This component is on intermontane basins, drainageways on outwash fans. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 4w. This soil meets hydric criteria.   "|"21346929"|"21586168"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Overwhich component makes up 70 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AY150MT Subirrigated (sb)   Lru 44a-y ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346870"|"21586109"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Nirling soil is a minor component."|"21346871"|"21586110"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Curlew, rarely flooded component makes up 20 percent of the map unit. Slopes are 2 to 4 percent. This component is on drainageways on outwash fans, intermontane basins. The parent material consists of alluvium derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY182MT Wet Meadow Organic (wmo)   Lru 44a-y ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"21346872"|"21586111"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Gregson soil is a minor component."|"21346933"|"21586172"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Chereete component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"21346934"|"21586173"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hartbench component makes up 45 percent of the map unit. Slopes are 1 to 4 percent. This component is on outwash fans, intermontane basins. The parent material consists of outwash derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044AA032MT Loamy (lo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21346935"|"21586174"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blossberg component makes up 30 percent of the map unit. Slopes are 0 to 8 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AY082MT Meadow (m)   Lru 44a-y ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"21346963"|"21586202"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lick, bouldery component makes up 60 percent of the map unit. Slopes are 8 to 35 percent. This component is on intermontane basins, moraines. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R044AB162MT Thin Loamy (tlo)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346964"|"21586203"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hartbench soil is a minor component."|"21346965"|"21586204"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lick component makes up 80 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346966"|"21586205"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Clasoil soil is a minor component."|"21346967"|"21586206"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hartbench soil is a minor component."|"21346968"|"21586207"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lick component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on intermontane basins, hillslopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21346984"|"21586223"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lumpgulch component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium derived from granite over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21346985"|"21586224"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on intermontane basins, hillslopes. The parent material consists of slope alluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21346986"|"21586225"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lick component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346987"|"21586226"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lumpgulch component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, mountain slopes, intermontane basins. The parent material consists of colluvium derived from granite over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346988"|"21586227"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 8 to 35 percent. This component is on hillslopes, intermontane basins, mountain slopes. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346989"|"21586228"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hartbench soil is a minor component."|"21346969"|"21586208"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lick, bouldery component makes up 80 percent of the map unit. Slopes are 8 to 15 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the R044AB110MT Sandy (sy)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346970"|"21586209"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Clasoil soil is a minor component."|"21346971"|"21586210"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Hartbench soil is a minor component."|"21346972"|"21586211"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lick, bouldery component makes up 70 percent of the map unit. Slopes are 8 to 35 percent. This component is on moraines, intermontane basins. The parent material consists of till derived from granite and gneiss. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346973"|"21586212"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Clasoil soil is a minor component."|"21346974"|"21586213"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Repkie soil is a minor component."|"21346975"|"21586214"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"||"The Sawicki, stony component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on hillslopes, intermontane basins. The parent material consists of slope alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AB036MT Droughty (dr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"21346876"|"21586115"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, rubbly component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on intermontane basins, hills. The parent material consists of slope alluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AA136MT Shallow Loamy (swlo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"21346877"|"21586116"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Durston soil is a minor component."|"21346878"|"21586117"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farnuf component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AA032MT Loamy (lo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346879"|"21586118"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, rubbly component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, intermontane basins. The parent material consists of slope alluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AB038MT Droughty Steep (drstp)   Lru 44a-b ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346880"|"21586119"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Durston soil is a minor component."|"21346881"|"21586120"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"21346882"|"21586121"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"||"The Sawicki, extremely stony component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on intermontane basins, hillslopes. The parent material consists of slope alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044AB036MT Droughty (dr)   Lru 44a-b ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"21346883"|"21586122"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quast, stony component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of eolian deposits over alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AA032MT Loamy (lo)   Lru 44a-a ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21346884"|"21586123"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346885"|"21586124"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, rubbly component makes up 45 percent of the map unit. Slopes are 15 to 50 percent. This component is on hillslopes, mountains. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044AP805MT Shallow Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346886"|"21586125"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quast, stony component makes up 20 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, mountains. The parent material consists of eolian deposits over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"21346887"|"21586126"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wickes, stony soil is a minor component."|"21346888"|"21586127"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"21346889"|"21586128"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"||"The Pianohill component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on swales on hillslopes, intermontane basins. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM040MT Loamy Steep (lostp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"21346890"|"21586129"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blaincreek soil is a minor component."|"21346891"|"21586130"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wheelbarrow component makes up 40 percent of the map unit. Slopes are 15 to 50 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer, bedrock, lithic, is 26 to 39 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BA134MT Shallow To Gravel (swgr)   Lru 43b-a ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346892"|"21586131"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346893"|"21586132"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"||"The Sawicki component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, hillslopes. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BM038MT Droughty Steep (drstp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346894"|"21586133"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash, stony component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, intermontane basins. The parent material consists of colluvium over residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BM138MT Shallow Droughty (swdr)   Lru 43b-m ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346895"|"21586134"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Blaincreek soil is a minor component."|"21346896"|"21586135"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"||"The Roegulch, rubbly component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on intermontane basins, escarpments, hillslopes. The parent material consists of colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"21346897"|"21586136"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Repkie component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on hillslopes, escarpments, intermontane basins. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"21346898"|"21586137"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolo component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on drainageways, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BC032MT Loamy (lo)   Lru 43b-c ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"21346899"|"21586138"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Quast soil is a minor component."|"21346900"|"21586139"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farnuf component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM040MT Loamy Steep (lostp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 17 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346901"|"21586140"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quast component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of eolian deposits over colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BM040MT Loamy Steep (lostp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346902"|"21586141"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wemple component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of eolian deposits and/or colluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BM040MT Loamy Steep (lostp)   Lru 43b-m ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a slightly sodic horizon within 30 inches of the soil surface."|"21346903"|"21586142"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"21346976"|"21586215"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wemple component makes up 45 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of eolian deposits and/or slope alluvium over residuum weathered from granite. Depth to a root restrictive layer, bedrock, lithic, is 40 to 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BM032MT Loamy (lo)   Lru 43b-m ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a slightly sodic horizon within 30 inches of the soil surface."|"21346977"|"21586216"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Farnuf component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BM032MT Loamy (lo)   Lru 43b-m ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 17 percent. There are no saline horizons within 30 inches of the soil surface. "|"21346978"|"21586217"
05/06/2013 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Haccke component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hillslopes, intermontane basins. The parent material consists of sodium affected eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA006MT Claypan (cp)   Lru 44b-a ecological site. Nonirrigated land capability classification is 4s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"21346979"|"21586218"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Droughty Steep (drstp)   Lru 44a-a, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346941"|"21586180"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Riverside component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on eroded fan remnants, intermontane basins. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044AP808MT Gravelly (gr)   Lru 44a-a, Upland Grassland 44a Lru P ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"21346942"|"21586181"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloron soil is a minor component."|"21346943"|"21586182"
