09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum over hard sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121198"|"22456509"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121199"|"22456510"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of clayey residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22121200"|"22456511"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Assinniboine component makes up 90 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121201"|"22456980"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121202"|"22456981"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121203"|"22456982"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121204"|"22456983"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121009"|"22456394"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Megonot component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on swales on plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z., Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121010"|"22456395"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobase component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on swales on plains. The parent material consists of clayey alluvium derived from shale and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z., Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"22121011"|"22456396"
07/15/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Richey soil is a minor component."|"22121150"|"22456397"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121151"|"22456398"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Korchea component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood-plain steps, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121152"|"22456399"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121153"|"22456400"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairway component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC044MT Subirrigated (Sb)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121154"|"22456401"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"22121155"|"22456402"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larry soil is a minor component."|"22121156"|"22456403"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Linwell soil is a minor component."|"22121085"|"22456526"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 87 percent of the map unit. Slopes are 4 to 8 percent. This component is on swales on fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121022"|"22456774"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121023"|"22456775"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evanston soil is a minor component."|"22121024"|"22456776"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Creed soil is a minor component."|"22121025"|"22456777"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121012"|"22457007"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"22121013"|"22457008"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121014"|"22457009"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments, plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121015"|"22457010"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments, plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121016"|"22457011"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121017"|"22457012"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Macar soil is a minor component."|"22121004"|"22456540"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soapcreek soil is a minor component."|"22121005"|"22456541"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Swampcreek soil is a minor component."|"22121006"|"22456542"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22120996"|"22456543"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Reedpoint component makes up 85 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments, plains. The parent material consists of loamy residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC058MT Very Shallow (VSw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22120997"|"22456544"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22120998"|"22456545"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22120999"|"22456546"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121000"|"22456547"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121003"|"22456539"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairway component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC044MT Bottomland, Subirrigated (sb)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121002"|"22456538"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"22121001"|"22456537"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22121643"|"22456659"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121642"|"22456658"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121641"|"22456657"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121640"|"22456656"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC049MT Silty-steep (sistp)   Rru 58a-c  11-14"" P.z. (combined R058ac046mt, R058ac0 ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121639"|"22456655"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 48 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121638"|"22456654"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121637"|"22456653"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klayent soil is a minor component."|"22120932"|"22456536"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ledger soil is a minor component."|"22120931"|"22456535"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22120930"|"22456534"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22120929"|"22456533"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121059"|"22457006"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22121058"|"22457005"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 70 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments, foothills. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121057"|"22457004"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121056"|"22457003"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"22121055"|"22457002"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121054"|"22457001"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121065"|"22456532"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"22121064"|"22456531"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of silty and clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC516MT Draft Silty-steep (sistp)   Rru 46-c  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121063"|"22456530"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amherst soil is a minor component."|"22121062"|"22456529"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121061"|"22456528"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121060"|"22456527"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121053"|"22456773"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Creed component makes up 40 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer, natric, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (Cp)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 17 within 30 inches of the soil surface."|"22121052"|"22456772"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gerdrum component makes up 50 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces, plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer, natric, is 2 to 4 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC054MT Claypan (Cp)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"22121051"|"22456771"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"22121050"|"22456770"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121049"|"22456769"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22121048"|"22456768"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22121072"|"22457000"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22120937"|"22456790"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22120938"|"22456791"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22120939"|"22456792"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boxwell soil is a minor component."|"22120940"|"22456793"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22120941"|"22456794"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22120942"|"22456795"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nesda component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22120933"|"22457019"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McIlwaine component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy  over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22120934"|"22457020"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Meadowcreek soil is a minor component."|"22120935"|"22457021"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Albicalis soil is a minor component."|"22120936"|"22457022"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121071"|"22456999"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121070"|"22456998"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hinterland component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22121069"|"22456997"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Timberlin component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of loamy colluvium and, or residuum weathered from tuff breccia. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 7e.     "|"22121146"|"22456799"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Warwood component makes up 40 percent of the map unit. Slopes are 35 to 45 percent. This component is on mountains. The parent material consists of loamy alluvium or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121147"|"22456800"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pintlar soil is a minor component."|"22121148"|"22456801"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"22121149"|"22456802"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121068"|"22456996"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121067"|"22456995"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22121066"|"22456994"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121084"|"22456525"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"22121083"|"22456524"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amor component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121082"|"22456523"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121081"|"22456522"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"22121080"|"22456521"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"22121079"|"22456520"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vershal soil is a minor component."|"22121078"|"22456519"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"22121077"|"22456767"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Albicalis component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC043MT Wet Meadow (WM)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"22121076"|"22456766"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121075"|"22456765"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Korchea component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood-plain steps, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121074"|"22456764"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fairway component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 4 percent. This component is in the R058AC044MT Subirrigated (Sb)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121073"|"22456763"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121047"|"22456993"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Birney component makes up 30 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of gravelly colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121046"|"22456992"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121045"|"22456991"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121044"|"22456990"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121043"|"22456989"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121042"|"22456988"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121029"|"22456762"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121028"|"22456761"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cambeth component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of silty residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121027"|"22456760"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121026"|"22456759"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121099"|"22457029"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121100"|"22457030"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vershal soil is a minor component."|"22121101"|"22457031"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ticell soil is a minor component."|"22121102"|"22457032"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wayden component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from shale and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XS619MT Draft Shallow Clay (swc)   Rru 46-s  13-16"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121103"|"22457033"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22121104"|"22457034"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"22121105"|"22457035"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sagedale soil is a minor component."|"22121106"|"22457036"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"22121086"|"22456809"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shambo component makes up 85 percent of the map unit. Slopes are 4 to 8 percent.  The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent.  The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121087"|"22456810"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"22121088"|"22456811"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fairfield soil is a minor component."|"22121089"|"22456812"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121090"|"22456813"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Linwell soil is a minor component."|"22121091"|"22456814"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22120990"|"22457037"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Reedpoint component makes up 85 percent of the map unit. Slopes are 2 to 15 percent. This component is on plains. The parent material consists of loamy residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC058MT Very Shallow (VSw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22120991"|"22457038"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hinterland soil is a minor component."|"22120992"|"22457039"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22120993"|"22457040"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22120994"|"22457041"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22120995"|"22457042"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121132"|"22456815"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 33 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121133"|"22456816"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121134"|"22456817"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedwest soil is a minor component."|"22121135"|"22456818"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121136"|"22456819"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z., Shallow Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121008"|"22456393"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121007"|"22456392"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ledger soil is a minor component."|"22121041"|"22456391"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thibadeau soil is a minor component."|"22121040"|"22456390"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"22121039"|"22456389"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gerdrum soil is a minor component."|"22121038"|"22456388"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absher component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces. The parent material consists of silty and clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC053MT Dense Clay (DC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"22121037"|"22456387"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Creed soil is a minor component."|"22121036"|"22456386"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22121679"|"22457099"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121678"|"22457098"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121677"|"22457097"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121676"|"22457096"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 15 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121675"|"22457095"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist component makes up 60 percent of the map unit. Slopes are 15 to 65 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121674"|"22457094"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121673"|"22457093"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, moist component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121686"|"22456912"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, moist component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121685"|"22456911"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"22121668"|"22456901"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121669"|"22456902"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121670"|"22456903"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on pediments on sedimentary plains. The parent material consists of interbedded residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121671"|"22456904"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on pediments on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121672"|"22456905"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121693"|"22456660"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121694"|"22456661"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121695"|"22456662"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121696"|"22456663"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121697"|"22456664"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eapa component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121157"|"22457050"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"22121158"|"22457051"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121159"|"22457052"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"22121160"|"22457053"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121684"|"22456910"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121683"|"22456909"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121682"|"22456908"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22121681"|"22456907"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121680"|"22456906"
09/21/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121035"|"22456518"
09/21/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Reedpoint component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 4 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC058MT Shallow Grassland, Very Shallow (vsw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"22121034"|"22456517"
09/21/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"22121033"|"22456516"
09/21/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hinterland soil is a minor component."|"22121032"|"22456515"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121525"|"22457054"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121526"|"22457055"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121527"|"22457056"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"22121528"|"22457057"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beenom, calcareous component makes up 70 percent of the map unit. Slopes are 1 to 8 percent. This component is on structural benches on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121529"|"22457058"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121530"|"22457059"
09/21/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls on plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z., Upland Grassland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121031"|"22456514"
09/21/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimmick soil is a minor component."|"22121030"|"22456513"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Klayent soil is a minor component."|"22120928"|"22456987"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ledger component makes up 85 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during January, February, March, April, May, December. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"22120927"|"22456986"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22120926"|"22456985"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thibadeau soil is a minor component."|"22120925"|"22456984"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The GRAVEL PITS is a miscellaneous area."|"22121443"|"22456512"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"22121435"|"22456758"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121434"|"22456757"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121433"|"22456756"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 85 percent of the map unit. Slopes are 2 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121432"|"22456755"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121431"|"22456754"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 35 percent of the map unit. Slopes are 25 to 50 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121430"|"22456979"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121644"|"22456647"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121645"|"22456648"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121646"|"22456649"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121647"|"22456650"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, calcareous component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 14 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121648"|"22456651"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121649"|"22456652"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121698"|"22456673"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"22121699"|"22456674"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121700"|"22456675"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"22121701"|"22456676"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 12 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AE199MT Shallow Clay (SwC)    RRU 58A-E  10-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121702"|"22456677"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121703"|"22456678"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"22121704"|"22456679"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121705"|"22456680"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121706"|"22456681"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 30 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121707"|"22456682"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121708"|"22456683"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Orinoco soil is a minor component."|"22121709"|"22456684"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullhook soil is a minor component."|"22121710"|"22456685"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121711"|"22456686"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambeth component makes up 35 percent of the map unit. Slopes are 25 to 50 percent. This component is on hills on sedimentary plains. The parent material consists of alluvium derived from siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121429"|"22456978"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121428"|"22456977"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121427"|"22456976"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121426"|"22456975"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121425"|"22456974"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121601"|"22456883"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121712"|"22457106"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121713"|"22457107"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"22121714"|"22457108"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121715"|"22457109"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint, calcareous component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121716"|"22457110"
07/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121717"|"22457111"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121506"|"22457060"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121507"|"22457061"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom, calcareous soil is a minor component."|"22121508"|"22457062"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 80 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills on plains, structural benches on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121509"|"22457063"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121510"|"22457064"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121511"|"22457065"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121631"|"22456641"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121632"|"22456642"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"22121633"|"22456643"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121634"|"22456644"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121635"|"22456645"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 14 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121636"|"22456646"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Megonot component makes up 40 percent of the map unit. Slopes are 1 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121512"|"22456840"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobase component makes up 45 percent of the map unit. Slopes are 1 to 8 percent. This component is on fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"22121513"|"22456841"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatoville soil is a minor component."|"22121514"|"22456842"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121515"|"22456843"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Orinoco soil is a minor component."|"22121516"|"22456844"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121517"|"22456845"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121687"|"22457100"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom, calcareous soil is a minor component."|"22121688"|"22457101"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121689"|"22457102"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121690"|"22457103"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121691"|"22457104"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121692"|"22457105"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121540"|"22456846"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bonfri soil is a minor component."|"22121541"|"22456847"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121600"|"22456882"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"22121599"|"22456881"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on stream terraces on sedimentary plains. The parent material consists of alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121598"|"22456880"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 95 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121424"|"22456505"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Birney soil is a minor component."|"22121423"|"22456504"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Linwell soil is a minor component."|"22121095"|"22456381"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121094"|"22456380"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"22121093"|"22456379"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"22121092"|"22456378"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22121021"|"22456957"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121020"|"22456956"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22121019"|"22456955"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121018"|"22456954"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shane component makes up 50 percent of the map unit. Slopes are 4 to 10 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121357"|"22456734"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121356"|"22456733"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"22121355"|"22456953"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shane component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121354"|"22456952"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121353"|"22456951"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"22121352"|"22456732"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shane component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121351"|"22456731"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121350"|"22456730"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121349"|"22456482"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cheadle component makes up 30 percent of the map unit. Slopes are 25 to 70 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 5 to 10 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 4 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121348"|"22456481"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"22121347"|"22456480"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on moraines, hills. The parent material consists of alluvium and/or colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC516MT Draft Silty-steep (sistp)   Rru 46-c  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121346"|"22456479"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121345"|"22456478"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, bouldery loam soil is a minor component."|"22121344"|"22456477"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Garlet soil is a minor component."|"22121343"|"22456357"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"22121342"|"22456356"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 85 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines, hills. The parent material consists of alluvium and/or colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC516MT Draft Silty-steep (sistp)   Rru 46-c  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121341"|"22456355"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, bouldery loam soil is a minor component."|"22121340"|"22456354"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"22121339"|"22456729"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 85 percent of the map unit. Slopes are 4 to 25 percent. This component is on moraines, hills. The parent material consists of alluvium and/or colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XC516MT Draft Silty-steep (sistp)   Rru 46-c  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22121338"|"22456728"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121337"|"22456727"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud, bouldery loam soil is a minor component."|"22121336"|"22456726"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121335"|"22456353"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121334"|"22456352"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121333"|"22456351"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121332"|"22456350"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121331"|"22456349"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"22121330"|"22456348"
06/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 35 percent of the map unit. Slopes are 45 to 75 percent. This component is on mountainsides. The parent material consists of colluvium and/or residuum weathered from igneous rock and/or sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F046XP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121329"|"22456347"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"22121328"|"22456346"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121327"|"22456950"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 35 percent of the map unit. Slopes are 25 to 50 percent. This component is on hills. The parent material consists of residuum over hard sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121326"|"22456949"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"22121325"|"22456948"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sebud soil is a minor component."|"22121324"|"22456947"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121323"|"22456345"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 85 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121322"|"22456344"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac, channery loam soil is a minor component."|"22121321"|"22456343"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121320"|"22456342"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121319"|"22456341"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121318"|"22456340"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenzie component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on basin floors. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during March, April, May, June. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil meets hydric criteria.  The soil has a moderately saline horizon within 30 inches of the soil surface. "|"22121317"|"22456339"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lardell soil is a minor component."|"22121316"|"22456338"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"22121315"|"22456337"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121314"|"22456946"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"22121313"|"22456945"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121312"|"22456944"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, alluvial fans. The parent material consists of alluvium derived from siltstone and/or shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"22121311"|"22456943"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121310"|"22456942"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lonna component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans. The parent material consists of silty alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 15 within 30 inches of the soil surface."|"22121098"|"22456725"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121097"|"22456724"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22121096"|"22456723"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nesda component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans, stream terraces. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS108MT Draft Subirrigated (sb)   Rru 46-s  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121309"|"22456941"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121308"|"22456940"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lolo, stony soil is a minor component."|"22121307"|"22456939"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolo component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces, alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 24 inches during April, May, June, July, August. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS108MT Draft Subirrigated (sb)   Rru 46-s  15-19"" P.z. ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121306"|"22456938"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"22121305"|"22456937"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larry soil is a minor component."|"22121304"|"22456936"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121303"|"22456471"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolo, very gravelly loam component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"22121302"|"22456470"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lolo component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"22121301"|"22456469"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lolo, stony soil is a minor component."|"22121300"|"22456468"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121299"|"22456467"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"22121298"|"22456466"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larry soil is a minor component."|"22121297"|"22456465"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"22121296"|"22456722"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohler component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121295"|"22456721"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121294"|"22456720"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121293"|"22456719"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havrelon soil is a minor component."|"22121292"|"22456935"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lohler component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121291"|"22456934"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121290"|"22456933"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"22121289"|"22456464"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lardell component makes up 95 percent of the map unit. Slopes are 0 to 2 percent. This component is on basin floors, alluvial fans. The parent material consists of clayey alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 27 inches during May, June, July, August. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC051MT Saline Lowland (sl)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 47 within 30 inches of the soil surface."|"22121288"|"22456463"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McKenzie soil is a minor component."|"22121287"|"22456462"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lolo soil is a minor component."|"22121241"|"22456321"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Grail component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121240"|"22456320"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"22121239"|"22456319"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121238"|"22456707"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121237"|"22456706"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem soil is a minor component."|"22121236"|"22456705"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"22121235"|"22456704"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121166"|"22456917"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121165"|"22456916"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121234"|"22456449"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121233"|"22456448"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121232"|"22456447"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121231"|"22456703"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cheadle soil is a minor component."|"22121230"|"22456702"
06/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 55 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountainsides. The parent material consists of colluvium and/or residuum weathered from igneous rock and/or sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F046XP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121229"|"22456701"
06/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sebud component makes up 35 percent of the map unit. Slopes are 25 to 60 percent. This component is on moraines, hills. The parent material consists of alluvium and/or colluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the F046XP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121228"|"22456700"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"22121662"|"22456672"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambeth component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 41 to 49 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121661"|"22456671"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121660"|"22456670"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on pediments on sedimentary plains. The parent material consists of interbedded residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121659"|"22456669"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambeth component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of silty residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 41 to 49 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121658"|"22456668"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"22121657"|"22456667"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121656"|"22456666"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on pediments on sedimentary plains. The parent material consists of interbedded residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121655"|"22456665"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121227"|"22456699"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121226"|"22456698"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Birney component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121225"|"22456697"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121224"|"22456696"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121223"|"22456695"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambeth soil is a minor component."|"22121222"|"22456694"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverell component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121221"|"22456915"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"22121220"|"22456914"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121219"|"22456913"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverell component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC194MT Shallow To Gravel (swgr)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121218"|"22456446"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 75 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121217"|"22456445"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"22121216"|"22456444"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"22121215"|"22456693"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 15 inches during May, June, July, August. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC044MT Subirrigated (sb)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 5w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121214"|"22456692"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larry soil is a minor component."|"22121213"|"22456691"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"22121212"|"22456443"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Attewan component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121211"|"22456442"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121210"|"22456441"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Assinniboine component makes up 60 percent of the map unit. Slopes are 6 to 12 percent. This component is on low hills. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121209"|"22456440"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121208"|"22456439"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 30 percent of the map unit. Slopes are 6 to 12 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121207"|"22456438"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121206"|"22456437"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121205"|"22456436"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121164"|"22456690"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sinnigam soil is a minor component."|"22121163"|"22456689"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121162"|"22456688"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121161"|"22456687"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22120969"|"22456411"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hinterland component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22120982"|"22456784"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22120981"|"22456783"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22120980"|"22456782"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22120979"|"22456781"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22120978"|"22456780"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22120977"|"22456779"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22120976"|"22456778"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on swales on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z., Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22120989"|"22456410"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22120988"|"22456409"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22120987"|"22456408"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22120986"|"22456407"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22120985"|"22456406"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22120984"|"22456405"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hinterland component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on knolls on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z., Shallow Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22120983"|"22456404"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on swales on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22120970"|"22456412"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22120971"|"22456413"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22120972"|"22456414"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22120973"|"22456415"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22120974"|"22456416"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boxwell soil is a minor component."|"22120975"|"22456417"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"22120962"|"22456418"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22120963"|"22456419"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22120964"|"22456420"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22120965"|"22456421"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22120966"|"22456422"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22120967"|"22456423"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boxwell soil is a minor component."|"22120968"|"22456424"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22120957"|"22456785"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 70 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments, plains. The parent material consists of loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22120958"|"22456786"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22120959"|"22456787"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22120960"|"22456788"
09/03/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22120961"|"22456789"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22120949"|"22456425"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22120950"|"22456426"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 20 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22120951"|"22456427"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22120952"|"22456428"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22120953"|"22456429"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 30 percent of the map unit. Slopes are 2 to 15 percent. This component is on knolls on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22120954"|"22456430"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22120955"|"22456431"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hinterland soil is a minor component."|"22120956"|"22456432"
09/03/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22120943"|"22457013"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22120944"|"22457014"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on swales on plains. The parent material consists of loamy residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z., Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22120945"|"22457015"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22120946"|"22457016"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22120947"|"22457017"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on knolls on plains. The parent material consists of loamy residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z., Shallow Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22120948"|"22457018"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121143"|"22456796"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from gabbro. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121144"|"22456797"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arrowpeak soil is a minor component."|"22121145"|"22456798"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121126"|"22456548"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent.  "|"22121127"|"22456549"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wayden component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of clayey residuum weathered from shale and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XS619MT Draft Shallow Clay (swc)   Rru 46-s  13-16"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121128"|"22456550"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121129"|"22456551"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shambo soil is a minor component."|"22121130"|"22456552"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Farnuf soil is a minor component."|"22121131"|"22456553"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121120"|"22457023"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS619MT Draft Shallow Clay (swc)   Rru 46-s  13-16"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22121121"|"22457024"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"22121122"|"22457025"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 51 percent of the map unit. Slopes are 8 to 15 percent. This component is on swales on plains. The parent material consists of silty and clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121123"|"22457026"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121124"|"22457027"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"22121125"|"22457028"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS619MT Draft Shallow Clay (swc)   Rru 46-s  13-16"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22121114"|"22456803"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"22121115"|"22456804"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121116"|"22456805"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on swales on plains. The parent material consists of silty and clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121117"|"22456806"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121118"|"22456807"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winifred soil is a minor component."|"22121119"|"22456808"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121107"|"22456554"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 50 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121108"|"22456555"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vershal soil is a minor component."|"22121109"|"22456556"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wayden component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on escarpments. The parent material consists of clayey residuum weathered from shale and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XS619MT Draft Shallow Clay (swc)   Rru 46-s  13-16"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121110"|"22456557"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121111"|"22456558"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mowbray soil is a minor component."|"22121112"|"22456559"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121113"|"22456560"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Miscellaneous Water is a miscellaneous area."|"22121567"|"22457043"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"22121454"|"22456820"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thibadeau soil is a minor component."|"22121455"|"22456821"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"22121456"|"22456822"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlake component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC045MT Overflow (ov)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"22121457"|"22456823"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 50 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XP801MT Plains Cottonwood/western Snowberry C.t. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121458"|"22456824"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121459"|"22456825"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, channeled soil is a minor component."|"22121460"|"22456826"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121531"|"22456433"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"22121532"|"22456434"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Eapa, calcareous component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121533"|"22456435"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marmarth component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (Sy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121534"|"22457044"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121535"|"22457045"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121536"|"22457046"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121537"|"22457047"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beenom component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on structural benches on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"22121538"|"22457048"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121539"|"22457049"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121484"|"22456827"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"22121485"|"22456828"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"22121486"|"22456829"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Warhorse soil is a minor component."|"22121487"|"22456830"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 80 percent of the map unit. Slopes are 1 to 6 percent. This component is on low hills on plains. The parent material consists of alluvium derived from sandstone and shale and/or residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121488"|"22456831"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22121489"|"22456832"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"22121490"|"22456589"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121491"|"22456590"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marmarth component makes up 90 percent of the map unit. Slopes are 1 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (Sy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121492"|"22456591"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121493"|"22456833"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Megonot component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (Cy)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121494"|"22456834"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (SwC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121495"|"22456835"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121496"|"22456836"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Abor soil is a minor component."|"22121497"|"22456837"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121498"|"22456838"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"22121499"|"22456839"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 45 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121500"|"22456592"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121501"|"22456593"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121197"|"22456508"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121196"|"22456507"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121195"|"22456506"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills on plains. The parent material consists of colluvium derived from sandstone and/or residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121502"|"22456594"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121503"|"22456595"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121504"|"22456596"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121505"|"22456597"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 15 to 60 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121572"|"22457082"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 20 percent of the map unit. Slopes are 15 to 60 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121573"|"22457083"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121574"|"22457084"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121575"|"22457085"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121576"|"22457086"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121577"|"22457087"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absher component makes up 85 percent of the map unit. Slopes are 0 to 6 percent. This component is on alluvial fans, stream terraces. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC053MT Dense Clay (dc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"22121194"|"22456753"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121193"|"22456752"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 95 percent of the map unit. Slopes are 2 to 4 percent. This component is on sedimentary plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121422"|"22456503"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Birney soil is a minor component."|"22121421"|"22456502"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Attewan soil is a minor component."|"22121420"|"22456751"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamac component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on sedimentary plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121419"|"22456750"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"22121418"|"22456749"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121417"|"22456385"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amherst soil is a minor component."|"22121416"|"22456384"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"22121415"|"22456383"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Work component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, hills. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS104MT Draft Silty (si)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121414"|"22456382"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121413"|"22456748"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"22121412"|"22456747"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reeder soil is a minor component."|"22121411"|"22456746"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 45 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountainsides. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121410"|"22456745"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hilger component makes up 25 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from sandstone and shale and/or granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121409"|"22456744"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wayden component makes up 50 percent of the map unit. Slopes are 15 to 50 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R046XS619MT Draft Shallow Clay (swc)   Rru 46-s  13-16"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121408"|"22456377"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121407"|"22456376"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 30 percent of the map unit. Slopes are 15 to 50 percent. This component is on hills. The parent material consists of residuum over hard sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121406"|"22456375"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121405"|"22456374"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121404"|"22456373"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nesda soil is a minor component."|"22121403"|"22456372"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustochrepts component makes up 40 percent of the map unit. Slopes are 2 to 4 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"22121402"|"22456371"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustifluvents component makes up 45 percent of the map unit. Slopes are 0 to 2 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"22121401"|"22456370"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121400"|"22456369"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villsprings soil is a minor component."|"22121399"|"22456368"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kiwanis soil is a minor component."|"22121398"|"22456973"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nesda soil is a minor component."|"22121397"|"22456972"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"22121396"|"22456971"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquents component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains.  Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil meets hydric criteria.   "|"22121395"|"22456970"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ustifluvents component makes up 45 percent of the map unit. Slopes are 0 to 2 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"22121394"|"22456969"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie soil is a minor component."|"22121393"|"22456968"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121392"|"22456967"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"22121391"|"22456367"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Turner component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on stream terraces, outwash terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121390"|"22456366"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121389"|"22456365"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Amherst component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on hills. The parent material consists of clayey residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22121192"|"22456364"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121191"|"22456363"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 20 percent of the map unit. Slopes are 4 to 8 percent. This component is on hills. The parent material consists of residuum over hard sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121190"|"22456362"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121189"|"22456361"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shane soil is a minor component."|"22121188"|"22456360"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121187"|"22456359"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121186"|"22456358"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"22121388"|"22456966"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Turner component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, outwash terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121387"|"22456965"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121386"|"22456964"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverton soil is a minor component."|"22121385"|"22456501"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Turner component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces, outwash terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121384"|"22456500"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner, seeped soil is a minor component."|"22121383"|"22456499"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121382"|"22456498"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Camborthids component makes up 35 percent of the map unit. Slopes are 2 to 4 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"22121381"|"22456743"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Torrifluvents component makes up 45 percent of the map unit. Slopes are 0 to 2 percent.   Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil does not meet hydric criteria.   "|"22121380"|"22456742"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121379"|"22456741"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villsprings soil is a minor component."|"22121378"|"22456740"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121377"|"22456963"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac, channery loam component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121376"|"22456962"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121375"|"22456961"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121374"|"22456960"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 55 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121373"|"22456959"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lambeth soil is a minor component."|"22121372"|"22456958"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beenom component makes up 20 percent of the map unit. Slopes are 4 to 8 percent. This component is on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"22121371"|"22456497"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121370"|"22456496"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22121369"|"22456495"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 70 percent of the map unit. Slopes are 4 to 8 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121368"|"22456494"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beenom soil is a minor component."|"22121367"|"22456739"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121366"|"22456738"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121365"|"22456737"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawa component makes up 85 percent of the map unit. Slopes are 0 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"22121364"|"22456493"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121363"|"22456492"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121362"|"22456491"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work, gravelly clay loam soil is a minor component."|"22121361"|"22456490"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work, stony clay loam soil is a minor component."|"22121360"|"22456489"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"22121359"|"22456736"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabba component makes up 30 percent of the map unit. Slopes are 4 to 10 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22121358"|"22456735"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121185"|"22456488"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sinnigam component makes up 35 percent of the map unit. Slopes are 15 to 50 percent. This component is on hills on sedimentary plains. The parent material consists of hard sandstone residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22121184"|"22456487"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 45 percent of the map unit. Slopes are 15 to 50 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121183"|"22456486"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121182"|"22456485"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121181"|"22456484"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hilger soil is a minor component."|"22121180"|"22456483"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121179"|"22456476"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sinnigam component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on sedimentary plains. The parent material consists of hard sandstone residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22121178"|"22456475"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 55 percent of the map unit. Slopes are 8 to 15 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121177"|"22456474"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shane soil is a minor component."|"22121176"|"22456473"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121175"|"22456472"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121286"|"22456718"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on knolls on plains. The parent material consists of clayey residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22121285"|"22456717"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121284"|"22456716"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambeth component makes up 65 percent of the map unit. Slopes are 4 to 15 percent. This component is on sedimentary plains. The parent material consists of alluvium derived from siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121283"|"22456715"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121282"|"22456932"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wayden soil is a minor component."|"22121281"|"22456931"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121280"|"22456930"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambeth component makes up 65 percent of the map unit. Slopes are 4 to 15 percent. This component is on sedimentary plains. The parent material consists of alluvium derived from siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121279"|"22456929"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121278"|"22456461"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rentsac soil is a minor component."|"22121277"|"22456460"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121276"|"22456459"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonna soil is a minor component."|"22121275"|"22456458"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lambeth component makes up 90 percent of the map unit. Slopes are 2 to 15 percent. This component is on sedimentary plains. The parent material consists of alluvium derived from siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121274"|"22456457"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121273"|"22456714"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobar component makes up 95 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"22121272"|"22456713"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121174"|"22456456"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sinnigam component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on sedimentary plains. The parent material consists of hard sandstone residuum. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22121173"|"22456455"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 65 percent of the map unit. Slopes are 2 to 8 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121172"|"22456454"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shane soil is a minor component."|"22121171"|"22456453"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121170"|"22456452"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamac soil is a minor component."|"22121271"|"22456451"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobar component makes up 95 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium derived from shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"22121270"|"22456450"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121269"|"22456712"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 30 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills. The parent material consists of residuum over hard sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R046XS114MT Draft Shallow (sw)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121268"|"22456711"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sinnigam soil is a minor component."|"22121267"|"22456710"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absarokee soil is a minor component."|"22121266"|"22456709"
07/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hilger component makes up 45 percent of the map unit. Slopes are 25 to 60 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from sandstone and shale and/or granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R046XS106MT Sandy (Sy)   RRU 46-S  15-19"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121265"|"22456708"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121264"|"22456336"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 2w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121263"|"22456335"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem soil is a minor component."|"22121262"|"22456334"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"22121261"|"22456333"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121260"|"22456332"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 90 percent of the map unit. Slopes are 2 to 4 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121259"|"22456331"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem soil is a minor component."|"22121258"|"22456330"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"22121257"|"22456928"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121256"|"22456927"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121255"|"22456926"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlem soil is a minor component."|"22121254"|"22456925"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"22121253"|"22456329"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121252"|"22456328"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121251"|"22456327"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Villard soil is a minor component."|"22121250"|"22456326"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ryell soil is a minor component."|"22121249"|"22456325"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121248"|"22456324"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Harlem component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121247"|"22456323"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lolo soil is a minor component."|"22121246"|"22456924"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Grail component makes up 90 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 13 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121245"|"22456923"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Work soil is a minor component."|"22121244"|"22456922"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lohler soil is a minor component."|"22121243"|"22456921"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turner soil is a minor component."|"22121242"|"22456322"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121169"|"22456920"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sinnigam soil is a minor component."|"22121168"|"22456919"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absarokee component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on divides, hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R046XS105MT Draft Clayey (cy)   Rru 46-s  13-19"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121167"|"22456918"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121542"|"22456848"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121543"|"22456849"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on plains, swales on plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121544"|"22456850"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121545"|"22456851"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121436"|"22456605"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121437"|"22456606"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121438"|"22456607"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121439"|"22456608"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Twilight component makes up 28 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills on plains. The parent material consists of colluvium derived from sandstone and/or residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121440"|"22456609"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 22 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans on plains, swales on plains. The parent material consists of alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121441"|"22456610"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 35 percent of the map unit. Slopes are 8 to 25 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121442"|"22456611"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121618"|"22456890"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep, dry component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121619"|"22456891"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart, dry component makes up 30 percent of the map unit. Slopes are 8 to 60 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121620"|"22456892"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121621"|"22456893"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121622"|"22456894"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121623"|"22456895"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22121137"|"22456852"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 40 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on plains. The parent material consists of clayey residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121138"|"22456853"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121139"|"22456854"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Reedpoint soil is a minor component."|"22121140"|"22456855"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121141"|"22456856"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hinterland soil is a minor component."|"22121142"|"22456857"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121552"|"22456612"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on plains, structural benches on plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22121553"|"22456613"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121554"|"22456614"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121555"|"22456615"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 4 to 35 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121556"|"22456616"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121557"|"22456617"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullhook soil is a minor component."|"22121558"|"22456858"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 30 percent of the map unit. Slopes are 8 to 60 percent. This component is on hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121559"|"22456859"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121560"|"22456860"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 20 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121561"|"22456861"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121562"|"22456862"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121563"|"22456863"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121564"|"22456864"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans on plains, hills on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121565"|"22456865"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre, occasionally flooded soil is a minor component."|"22121566"|"22456866"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"22121450"|"22456867"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121451"|"22456868"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glendive soil is a minor component."|"22121452"|"22456869"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121453"|"22456870"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"22121461"|"22456572"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Glendive component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22121462"|"22456573"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havre, calcareous component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121463"|"22456574"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bullhook soil is a minor component."|"22121464"|"22456575"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121465"|"22456576"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121466"|"22456577"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Absher component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer, natric, is 1 to 3 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC053MT Dense Clay (DC)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 44 within 30 inches of the soil surface."|"22121467"|"22457066"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nobe component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on fan remnants on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during March, April, May, June. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC619MT Saline Subirrigated (SSb)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a strongly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 43 within 30 inches of the soil surface."|"22121468"|"22457067"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vanda soil is a minor component."|"22121469"|"22457068"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"22121470"|"22457069"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121471"|"22457070"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"22121472"|"22457071"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Busby component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of loamy alluvium derived from sandstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC042MT Sandy (sy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121608"|"22456624"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"22121609"|"22456625"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121610"|"22456626"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121611"|"22456627"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121473"|"22456578"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills on plains. The parent material consists of colluvium derived from sedimentary rock and/or residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121474"|"22456579"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 20 percent of the map unit. Slopes are 4 to 8 percent. This component is on fans on plains, low hills on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121475"|"22456580"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121476"|"22456581"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"22121477"|"22456582"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121478"|"22456583"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces on sedimentary plains. The parent material consists of alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121595"|"22456877"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121596"|"22456878"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121597"|"22456879"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121578"|"22456561"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121579"|"22456562"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121580"|"22456563"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"22121581"|"22456564"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121582"|"22456565"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121583"|"22456871"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rominell soil is a minor component."|"22121584"|"22456872"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121585"|"22456873"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121586"|"22456874"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121587"|"22456875"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yamacall component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans on sedimentary plains. The parent material consists of alluvium derived from interbedded sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121588"|"22456876"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatoville soil is a minor component."|"22121602"|"22456884"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobase component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on plains on sedimentary plains. The parent material consists of clayey alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121603"|"22456885"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121604"|"22456886"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"22121605"|"22456887"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121606"|"22456888"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"22121607"|"22456889"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"22121479"|"22456584"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatoville soil is a minor component."|"22121480"|"22456585"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Verson soil is a minor component."|"22121481"|"22456586"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121482"|"22456587"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ethridge component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on alluvial fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121483"|"22456588"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121518"|"22456598"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Warhorse soil is a minor component."|"22121519"|"22456599"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121520"|"22456600"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"22121521"|"22456601"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Megonot soil is a minor component."|"22121522"|"22456602"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on plains. The parent material consists of alluvium derived from sandstone and shale and/or residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is very low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22121523"|"22456603"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kobase soil is a minor component."|"22121524"|"22456604"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Neldore soil is a minor component."|"22121624"|"22456634"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121625"|"22456635"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yawdim component makes up 55 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of residuum weathered from clayey shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC059MT Shallow Clay (swc)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121626"|"22456636"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Orinoco soil is a minor component."|"22121627"|"22456637"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatoville soil is a minor component."|"22121628"|"22456638"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"22121629"|"22456639"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Abor component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on hills on sedimentary plains. The parent material consists of clayey residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22121630"|"22456640"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thibadeau soil is a minor component."|"22121444"|"22457072"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bigsandy soil is a minor component."|"22121445"|"22457073"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bullhook component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"22121446"|"22457074"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lostriver component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is high. This soil is rarely flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC050MT Saline Upland (su)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 22 within 30 inches of the soil surface."|"22121447"|"22457075"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Havre soil is a minor component."|"22121448"|"22457076"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121449"|"22457077"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yamacall soil is a minor component."|"22121589"|"22456566"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Delpoint component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (Si)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121590"|"22456567"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 45 percent of the map unit. Slopes are 2 to 15 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (Sw)   RRU 58A-C  11-14"" p.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121591"|"22456568"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121592"|"22456569"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121593"|"22456570"
06/30/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22121594"|"22456571"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marvan soil is a minor component."|"22121546"|"22456618"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Harlake soil is a minor component."|"22121547"|"22456619"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lostriver soil is a minor component."|"22121548"|"22456620"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zatoville soil is a minor component."|"22121549"|"22456621"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kobase component makes up 65 percent of the map unit. Slopes are 2 to 8 percent. This component is on fans on plains, stream terraces on plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC041MT Clayey (cy)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 11 within 30 inches of the soil surface."|"22121550"|"22456622"
09/08/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gullied land is a miscellaneous area."|"22121551"|"22456623"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121612"|"22456628"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121613"|"22456629"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blacksheep component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on hills on sedimentary plains. The parent material consists of sandy residuum weathered from calcareous sandstone over semiconsolidated residuum weathered from calcareous sandstone. Depth to a root restrictive layer, bedrock, paralithic, is 6 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121614"|"22456630"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22121615"|"22456631"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22121616"|"22456632"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22121617"|"22456633"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22121568"|"22457078"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rentsac component makes up 50 percent of the map unit. Slopes are 1 to 4 percent. This component is on low hills on sedimentary plains, structural benches on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121569"|"22457079"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22121570"|"22457080"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beenom component makes up 30 percent of the map unit. Slopes are 1 to 4 percent. This component is on structural benches on sedimentary plains. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"22121571"|"22457081"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 40 percent of the map unit. Slopes are 2 to 4 percent. This component is on pediments on sedimentary plains. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121663"|"22457088"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121664"|"22457089"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Twilight soil is a minor component."|"22121665"|"22457090"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Eapa soil is a minor component."|"22121666"|"22457091"
05/21/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on pediments on sedimentary plains. The parent material consists of interbedded residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121667"|"22457092"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blacksheep soil is a minor component."|"22121650"|"22456896"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bonfri component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from sandstone and shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC040MT Silty (si)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"22121651"|"22456897"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cabbart component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on low hills on sedimentary plains. The parent material consists of residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R058AC057MT Shallow (sw)   Rru 58a-c  11-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22121652"|"22456898"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"22121653"|"22456899"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22121654"|"22456900"
