"1"|"Absarokee clay loam, 2 to 8 percent slopes"||5|5.2|89|||"None"|"None"|"0"|4.02|7.69|13.34|13.54|"Well drained"|"Well drained"|"C"||97|"3"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.096|"Moderate"|"0"|0.325|"348138"
"10"|"Assinniboine-Rentsac complex, 6 to 12 percent slopes"||9|8.9|46|||"None"|"None"|"0"|3.64|6.89|11.41|13.81|"Well drained"|"Well drained"|"B"||97|"4"|63|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.104|"Severe"|"0"|0.407|"348139"
"11"|"Attewan loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|4.33|7.92|11.82|13.61|"Well drained"|"Well drained"|"B"|"3"|90|"3"|95|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.127|"Slight"|"0"|0.95|"348140"
"12"|"Attewan loam, seeped, 0 to 4 percent slopes"||2|2.1||38|38|"None"|"None"|"5"|4.36|7.96|11.89|13.74|"Somewhat poorly drained"|"Somewhat poorly drained"|"B/D"||95|"5"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.825|"Slight"|"5"|1|"348141"
"13"|"Attewan-Beaverell gravelly loams, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.59|6.9|10.36|12.08|"Well drained"|"Well drained"|"B"|"3"|80|"3"|80|"Somewhat limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.111|"Slight"|"0"|0.95|"348142"
"14"|"Beaverell very gravelly loam, 0 to 8 percent slopes"||4|4||||"None"|"None"|"0"|2.62|4.05|6.23|8.18|"Well drained"|"Well drained"|"B"||85|"6"|85|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.074|"Slight"|"0"|0.92|"348143"
"15"|"Birney-Yawdim-Rock outcrop association, steep"||25|24.8|36|||"None"|"None"|"0"|3.79|6.42|9.81|12.66|"Well drained"|"Well drained"|"B"||73|"6"|72|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.934|"Severe"|"0"|0.97|"348144"
"16"|"Bonfri-Lambeth complex, 2 to 8 percent slopes"||5|5.1|91|||"None"|"None"|"0"|4.34|8.43|15.09|16.04|"Well drained"|"Well drained"|"C"|"3"|85|"3"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.27|"Moderate"|"0"|1|"348145"
"17"|"Bonfri-Lambeth complex, 8 to 15  percent slopes"||12|11.9|91|||"None"|"None"|"0"|4.26|8.39|15.15|15.86|"Well drained"|"Well drained"|"C"||100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.492|"Severe"|"0"|1|"348146"
"18"|"Garlet-Sebud association, very steep"||43|44||||"None"|"None"|"0"|2.46|4.23|7.65|10.99|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348147"
"19"|"Glendive fine sandy loam, 0 to 4 percent slopes"||2|2||||"Rare"|"Rare"|"0"|3.99|8.21|16.67|25.07|"Well drained"|"Well drained"|"A"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.128|"Slight"|"0"|0.405|"348148"
"2"|"Absarokee clay loam, 8 to 15 percent slopes"||12|12.8|89|||"None"|"None"|"0"|3.96|7.54|13.01|13.1|"Well drained"|"Well drained"|"C"||100|"4"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.132|"Moderate"|"0"|0.663|"348149"
"20"|"Glendive fine sandy loam, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|3.97|8.16|16.54|24.91|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.151|"Slight"|"5"|0.66|"348150"
"21"|"Grail clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.64|8.54|16.81|25.26|"Well drained"|"Well drained"|"C"|"2"|93|"3"|96|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.072|"Slight"|"0"|0.997|"348151"
"22"|"Grail clay loam, 4 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|4.66|8.58|17.03|25.64|"Well drained"|"Well drained"|"C"|"3"|94|"3"|97|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.072|"Moderate"|"0"|0.969|"348152"
"23"|"Harlem clay loam, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|3.98|7.99|15.74|23.42|"Well drained"|"Well drained"|"C"|"3"|90|"3"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.242|"Slight"|"0"|0.95|"348153"
"24"|"Harlem clay loam, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.04|8.07|16.01|23.83|"Well drained"|"Well drained"|"C"|"3"|93|"3"|97|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.268|"Slight"|"3"|1|"348154"
"25"|"Havre loam, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.25|8.26|16.13|23.95|"Well drained"|"Well drained"|"B"|"2"|90|"3"|94|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.07|"Slight"|"0"|0.084|"348155"
"26"|"Havre loam, 2 to 4 percent slopes"||3|2.9||||"Rare"|"Rare"|"0"|4.27|8.28|16.3|24.33|"Well drained"|"Well drained"|"B"|"2"|90|"3"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.075|"Moderate"|"0"|0.073|"348156"
"27"|"Havre loam, occasionally flooded"||1|1||||"Occasional"|"Occasional"|"0"|4.27|8.27|16.26|24.25|"Well drained"|"Well drained"|"B"|"2"|90|"3"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.086|"Slight"|"3"|0.64|"348157"
"28"|"Hilger-Castner-Rock outcrop complex, 25 to 60 percent slopes"||43|41.8|46|||"None"|"None"|"0"|2.69|4.38|6.06|7.65|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348158"
"29"|"Kobar clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.02|8.02|16.02|23.98|"Well drained"|"Well drained"|"C"|"3"|95|"3"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.31|"Slight"|"0"|0.95|"348159"
"3"|"Absarokee-Sinnigam clay loams, 2 to 8 percent slopes"||5|5.1|46|||"None"|"None"|"0"|3.78|6.92|10.99|11.12|"Well drained"|"Well drained"|"C"||96|"3"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.098|"Moderate"|"0"|0.524|"348160"
"30"|"Kobar clay loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.02|8.02|16.02|23.98|"Well drained"|"Well drained"|"C"|"3"|100|"3"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.31|"Moderate"|"0"|0.95|"348161"
"31"|"Lambeth silt loam, 2 to 15 percent slopes"||9|9||||"None"|"None"|"0"|4.9|9.54|18.74|27.89|"Well drained"|"Well drained"|"C"||94|"4"|93|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Very limited"|0.949|"Severe"|"0"|0.321|"348162"
"32"|"Lambeth-Rentsac complex, 4 to 15 percent slopes"||10|9.6|46|||"None"|"None"|"0"|4.61|8.48|15.29|22.04|"Well drained"|"Well drained"|"C"||92|"4"|65|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.901|"Severe"|"0"|0.462|"348163"
"33"|"Lambeth-Yawdim complex, 4 to 15 percent slopes"||10|10.5|36|||"None"|"None"|"0"|4.73|8.53|14.95|21.34|"Well drained"|"Well drained"|"C"||67|"4"|65|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.757|"Severe"|"0"|0.512|"348164"
"34"|"Lardell clay loam, 0 to 2 percent slopes"||1|1.1||69|69|"Rare"|"Rare"|"2"|2.02|4|7.97|11.94|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"7"|98|"7"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.248|"Slight"|"2"|1|"348165"
"35"|"Lohler clay loam, 0 to 2 percent slopes"||1|1.1||||"Rare"|"Rare"|"0"|4.66|8.68|16.52|24.27|"Well drained"|"Well drained"|"C"|"3"|95|"3"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.122|"Slight"|"0"|0.95|"348166"
"36"|"Lohler clay loam, 2 to 4 percent slopes"||3|2.9||||"Rare"|"Rare"|"0"|3.8|7.6|14.97|22.3|"Moderately well drained"|"Moderately well drained"|"C"|"2"|94|"3"|97|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.104|"Moderate"|"0"|0.846|"348167"
"37"|"Lolo complex, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"7"|3.26|6.39|10.17|13.29|"Well drained"|"Well drained"|"A"|"4"|72|"6"|72|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.163|"Slight"|"7"|0.773|"348168"
"74"|"Gravel pits"||30|30||||||"0"|||||"Excessively drained"|"Excessively drained"|||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"361410"
"102B"|"Ledger family, clay loam, 1 to 4 percent slopes"||3|3||84|84|"Rare"|"Rare"|"0"|3.95|6.95|12.68|17.92|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"6"|85|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.333|"Moderate"|"0"|0.989|"361411"
"153C"|"Ethridge-Reedpoint complex, 2 to 8 percent slopes"||5|4.9|13|||"None"|"None"|"3"|3.03|5.52|10.14|14.64|"Well drained"|"Well drained"|"C"|"3"|55|"3"|53|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.314|"Moderate"|"3"|0.97|"361412"
"155E"|"Cabbart-Delpoint loams, moist, 15 to 35 percent slopes"||25|25.1|41|||"None"|"None"|"0"|3.71|6.55|7.14|7.37|"Well drained"|"Well drained"|"D"||100|"7"|99|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.978|"Severe"|"0"|0.989|"361413"
"157F"|"Cabbart, moist-Delpoint-Rock outcrop complex, 15 to 60 percent slopes"||35|33|41|||"None"|"None"|"0"|3.68|6.23|6.69|6.95|"Well drained"|"Well drained"|"D"||100|"7"|84|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"361414"
"163C"|"Absher clay loam, 0 to 8 percent slopes"||4|3.9||||"None"|"None"|"0"|3.01|4.83|8.09|10.97|"Well drained"|"Well drained"|"D"|"7"|85|"7"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.503|"Moderate"|"3"|0.996|"361415"
"138D"|"Cabbart-Megonot-Kobase clay loams, 2 to 15 percent slopes"||9|9.2|43|||"None"|"None"|"0"|4.12|7.43|10.16|11.76|"Well drained"|"Well drained"|"D"|"4"|55|"4"|55|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.309|"Severe"|"0"|0.982|"361416"
"148E"|"Cabbart-Cambeth complex, 4 to 35 percent slopes"||20|15.9|43|||"None"|"None"|"0"|4.63|8.29|11.14|11.14|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.716|"Severe"|"0"|0.665|"361417"
"439B"|"Fairway-Korchea loams, channeled, 0 to 4 percent slopes"||2|2||84|84|"Rare"|"Rare"|"0"|4.72|9.08|17.6|24.47|"Well drained"|"Somewhat poorly drained"|"B"|"3"|96|"3"|96|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.183|"Slight"|"1"|0.48|"361418"
"167F"|"Yawdim-Birney-Rock outcrop complex, 15 to 60 percent slopes"||38|37|30|||"None"|"None"|"0"|3.93|5.56|6.99|8.41|"Well drained"|"Well drained"|"D"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.975|"Severe"|"0"|0.986|"361419"
"213A"|"Korchea-Fairway-Albicalis loams, channeled, 0 to 4 percent slopes"||2|2.2||46|46|"Rare"|"Rare"|"0"|4.68|9.06|17.7|24.78|"Somewhat poorly drained"|"Poorly drained"|"C"|"3"|80|"3"|80|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.328|"Slight"|"15"|0.65|"361420"
"220C"|"Amor-Work complex, 2 to 8 percent slopes"||5|5|86|||"None"|"None"|"0"|4.56|8.51|14.72|17.47|"Well drained"|"Well drained"|"C"|"4"|94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.122|"Moderate"|"0"|0.376|"361421"
"206D"|"Hinterland-Rentsac-Cabbart complex, 2 to 15 percent slopes"||9|8.8|33|||"None"|"None"|"0"|3.51|5.2|5.44|5.44|"Well drained"|"Well drained"|"D"||96|"6"|60|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.219|"Moderate"|"0"|0.976|"361422"
"170C"|"Gerdrum-Creed complex, 0 to 8 percent slopes"||4|4||||"None"|"None"|"0"|3.46|6.33|11.04|15.66|"Well drained"|"Well drained"|"D"|"7"|52|"7"|52|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.422|"Moderate"|"0"|1|"361423"
"202E"|"Castner-Absarokee complex, 15 to 35 percent slopes"||25|24.9|41|||"None"|"None"|"0"|3.36|5.79|7.31|7.64|"Well drained"|"Well drained"|"D"||100|"7"|52|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.996|"Severe"|"0"|1|"361424"
"201F"|"Yawdim-Rock outcrop complex, 15 to 60 percent slopes"||38|37.4|30|||"None"|"None"|"0"|4.06|5.03|5.07|5.07|"Well drained"|"Well drained"|"D"||100|"7"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.984|"Severe"|"0"|1|"361425"
"146C"|"Ethridge clay loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.31|8.5|16.21|23.69|"Well drained"|"Well drained"|"C"|"3"|98|"3"|92|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.336|"Moderate"|"0"|0.95|"361426"
"103A"|"Havre loam, 0 to 2 percent slopes"||1|1.2||||"Rare"|"Rare"|"0"|4.36|8.36|16.34|24.25|"Well drained"|"Well drained"|"B"|"3"|96|"3"|96|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.361|"Slight"|"0"|0.11|"361427"
"140F"|"Yawdim-Rentsac complex, 15 to 60 percent slopes"||38|37.6|30|||"None"|"None"|"0"|3.48|4.67|4.73|4.73|"Well drained"|"Well drained"|"D"||100|"7"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.987|"Severe"|"0"|1|"361428"
"139E"|"Cabbart-Delpoint loams, 15 to 65 percent slopes"||25|24.8|41|||"None"|"None"|"0"|3.67|6.48|7.05|7.25|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.978|"Severe"|"0"|0.989|"361429"
"135A"|"Fairway loam, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.89|9.32|17.55|22.44|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|96|"4"|96|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.184|"Slight"|"4"|0.98|"361430"
"131F"|"Reedpoint very channery loam, 15 to 60 percent slopes"||38|37.7|13|||"None"|"None"|"0"|1.26|1.48|1.54|1.54|"Well drained"|"Well drained"|"D"||100|"7"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Slight"|"0"|1|"361432"
"130D"|"Tanna-Hinterland clay loams, 8 to 15 percent slopes"||12|11.9|33|||"None"|"None"|"0"|3.98|6.68|8.22|8.22|"Well drained"|"Well drained"|"D"|"4"|54|"4"|54|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.32|"Severe"|"0"|0.985|"361433"
"130C"|"Tanna-Hinterland clay loams, 2 to 8 percent slopes"||5|5|33|||"None"|"None"|"0"|3.94|6.61|8.15|8.15|"Well drained"|"Well drained"|"D"|"3"|54|"4"|50|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.319|"Moderate"|"0"|0.971|"361434"
"129D"|"Tanna-Cabbart complex, 8 to 15 percent slopes"||12|11.9|43|||"None"|"None"|"0"|4.28|7.87|9.58|9.66|"Well drained"|"Well drained"|"D"|"4"|58|"4"|58|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.307|"Severe"|"0"|0.965|"361435"
"129C"|"Tanna-Cabbart complex, 2 to 8 percent slopes"||5|5|43|||"None"|"None"|"0"|4.28|7.91|9.7|9.86|"Well drained"|"Well drained"|"D"|"3"|59|"4"|50|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.304|"Moderate"|"0"|0.95|"361436"
"116F"|"Cabbart-Rock outcrop complex, 15 to 60 percent slopes"||38|36.5|43|||"None"|"None"|"0"|4.48|7.6|7.96|8.26|"Well drained"|"Well drained"|"D"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.975|"Severe"|"0"|0.986|"361437"
"115D"|"Yawdim-Rentsac-Cabbart complex, 2 to 15 percent slopes"||9|8.9|36|||"None"|"None"|"0"|3.66|5.62|5.74|5.74|"Well drained"|"Well drained"|"D"|"6"|62|"6"|62|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.238|"Severe"|"0"|0.993|"361438"
"112D"|"Cabbart-Delpoint, calcareous loams, 8 to 15 percent slopes"||12|12|43|||"None"|"None"|"0"|4.4|7.84|9.54|9.87|"Well drained"|"Well drained"|"D"|"6"|52|"6"|52|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.268|"Severe"|"0"|0.985|"361439"
"112C"|"Cabbart-Delpoint, calcareous loams, 2 to 8 percent slopes"||5|5|43|||"None"|"None"|"0"|4.4|7.86|9.6|9.92|"Well drained"|"Well drained"|"D"|"6"|52|"6"|52|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.269|"Moderate"|"0"|0.96|"361440"
"1107A"|"Nesda-McIlwaine loams, 0 to 2 percent slopes"||1|1||84|84|"Occasional"|"Occasional"|"0"|4.23|6.96|10.11|12.46|"Well drained"|"Somewhat poorly drained"|"B"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.058|"Slight"|"5"|1|"361442"
"408F"|"Warwood-Timerlin-Cowood complex, 35 to 60 percent slopes"||40|43.4|41|||"None"|"None"|"0"|3.86|6.57|11.35|15.03|"Well drained"|"Well drained"|"B"||100|"7"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.98|"Severe"|"0"|1|"361443"
"73"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"348210"
"9"|"Assinniboine fine sandy loam, 2 to 15 percent slopes"||9|8.9||||"None"|"None"|"0"|3.87|7.77|14.28|20.78|"Well drained"|"Well drained"|"B"||100|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.093|"Severe"|"0"|0.11|"348209"
"8"|"Amherst-Absarokee-Castner complex, 8 to 15 percent slopes"||12|13|46|||"None"|"None"|"0"|3.78|6.57|7.27|7.44|"Well drained"|"Well drained"|"D"||97|"6"|35|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.364|"Severe"|"0"|0.97|"348208"
"72"|"Cabbart loam, 2 to 15 percent slopes"||9|9|43|||"None"|"None"|"0"|4.37|7.35|7.41|7.41|"Well drained"|"Well drained"|"D"||100|"6"|90|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.094|"Severe"|"0"|0.997|"348207"
"71"|"Yawdim-Lambeth-Rock outcrop association, steep"||38|35.9|36|||"None"|"None"|"0"|4.6|7.88|12.37|16.65|"Well drained"|"Well drained"|"D"||100|"7"|73|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.957|"Severe"|"0"|1|"348206"
"70"|"Yamacall loam, 8 to 15 percent slopes"||10|10||||"None"|"None"|"0"|4.15|7.63|13.98|20.24|"Well drained"|"Well drained"|"B"|"2"|90|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.206|"Severe"|"0"|0.203|"348205"
"7"|"Absher clay loam, 0 to 6 percent slopes"||3|3.3|77|||"None"|"None"|"0"|2.73|4.68|8.09|10.64|"Moderately well drained"|"Moderately well drained"|"D"|"7"|85|"7"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.271|"Moderate"|"0"|1|"348204"
"69"|"Yamac loam, 4 to 8 percent slopes"||6|7||||"None"|"None"|"0"|4.34|8.26|16.01|22.96|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.242|"Moderate"|"0"|0.05|"348203"
"68"|"Yamac loam, 2 to 4 percent slopes"||3|4.1||||"None"|"None"|"0"|4.34|8.26|16.01|22.96|"Well drained"|"Well drained"|"B"|"2"|95|"3"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.242|"Moderate"|"0"|0.05|"348202"
"67"|"Yamac loam, 0 to 2 percent slopes"||1|1.3||||"None"|"None"|"0"|4.41|8.4|16.16|23.03|"Well drained"|"Well drained"|"B"|"2"|90|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.194|"Slight"|"0"|0.066|"348201"
"66"|"Work loam, 8 to 15 percent slopes"||12|11.9||||"None"|"None"|"0"|4.35|8.28|14.45|19.37|"Well drained"|"Well drained"|"C"|"4"|85|"4"|90|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.091|"Severe"|"0"|0.652|"348200"
"65"|"Work loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.33|8.24|15.42|21.92|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.131|"Moderate"|"0"|0.537|"348199"
"64"|"Winkler-Hilger-Rock outcrop association, steep"||43|41.3||||"None"|"None"|"0"|2.63|5.03|9.25|13.28|"Somewhat excessively drained"|"Well drained"|"A"||95|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348198"
"63"|"Wayden-Castner association, steep"||33|33.9|36|||"None"|"None"|"0"|3.4|4.98|5.21|5.43|"Well drained"|"Well drained"|"D"||100|"7"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348197"
"62"|"Ustifluvents-ustochrepts association, gently sloping"||1|2.1||||||"0"|4|7.78|12.38|14.42|||||95||85|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.188|"Not rated"|"5"|1|"348196"
"61"|"Ustifluvents-fluvaquents association, flooded"||1|1.1||||||"0"|3.98|7.06|10.76|13.96|||||91||85|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.248|"Not rated"|"43"|1|"348195"
"60"|"Turner stony clay loam, 4 to 15 percent slopes"||10|9.6||||"None"|"None"|"0"|3.59|7.21|9.81|11.75|"Well drained"|"Well drained"|"B"||92|"6"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.093|"Moderate"|"0"|0.944|"348194"
"6"|"Absarokee-Amherst-Castner complex, 4 to 8 percent slopes"||6|7.6|46|||"None"|"None"|"0"|3.83|6.84|8.08|8.43|"Well drained"|"Well drained"|"D"||92|"3"|44|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.126|"Moderate"|"0"|0.931|"348193"
"59"|"Turner clay loam, 4 to 8 percent slopes"||6|5.7||||"None"|"None"|"0"|3.9|7.72|10.33|12.18|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.092|"Moderate"|"0"|0.944|"348192"
"58"|"Turner clay loam, 2 to 4 percent slopes"||3|2.9||||"None"|"None"|"0"|3.95|7.81|10.35|12.07|"Well drained"|"Well drained"|"B"|"3"|90|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.085|"Moderate"|"0"|0.965|"348191"
"57"|"Torrifluvents-Camborthids association, gently sloping"||1|1.9||||||"0"|4.25|8.63|14.51|16.58|||||90||80|"Not rated"|"Not rated"|"Not limited"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.261|"Not rated"|"10"|1|"348190"
"56"|"Tanna-Rentsac complex, 4 to 15 percent slopes"||10|9.9|46|||"None"|"None"|"0"|3.88|6.98|10.53|10.91|"Well drained"|"Well drained"|"D"|"4"|55|"4"|59|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.437|"Severe"|"0"|0.972|"348189"
"55"|"Tanna-Beenom complex, 4 to 8 percent slopes"||6|6.1|46|||"None"|"None"|"0"|4.03|7.63|11.66|11.66|"Well drained"|"Well drained"|"D"|"3"|70|"3"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.216|"Moderate"|"0"|1|"348188"
"54"|"Tanna clay loam, 8 to 15 percent slopes"||12|11.7|77|||"None"|"None"|"0"|3.97|7.74|12.93|12.93|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.241|"Severe"|"0"|1|"348187"
"53"|"Tanna clay loam, 2 to 8 percent slopes"||5|5.1|69|||"None"|"None"|"0"|4.07|8.03|11.16|11.8|"Well drained"|"Well drained"|"D"|"3"|97|"3"|97|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.329|"Moderate"|"0"|0.966|"348186"
"52"|"Shawa silty clay loam, 0 to 8 percent slopes"||4|4.8||||"None"|"None"|"0"|3.99|7.76|14.99|22.12|"Well drained"|"Well drained"|"B"|"4"|85|"3"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.12|"Moderate"|"0"|0.094|"348185"
"51"|"Shane-Cabba clay loams, 4 to 10 percent slopes"||7|10.4|38|||"None"|"None"|"0"|3.81|6.97|9.93|10.23|"Well drained"|"Well drained"|"D"|"4"|50|"4"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.199|"Moderate"|"0"|0.93|"348184"
"50"|"Shane clay loam, 8 to 15 percent slopes"||12|14.2|76|||"None"|"None"|"0"|3.87|7.68|11.89|12.1|"Well drained"|"Well drained"|"D"|"4"|85|"4"|93|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.185|"Severe"|"0"|0.971|"348183"
"5"|"Absarokee-Sinnigam complex, 15 to 50 percent slopes"||33|32.2|46|||"None"|"None"|"0"|3.35|6.12|7.18|7.42|"Well drained"|"Well drained"|"C"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.952|"Severe"|"0"|1|"348182"
"49"|"Shane clay loam, 4 to 8 percent slopes"||6|8.5|76|||"None"|"None"|"0"|3.87|7.68|11.89|12.1|"Well drained"|"Well drained"|"D"|"4"|85|"4"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.185|"Moderate"|"0"|0.944|"348181"
"48"|"Sebud-Cheadle association, very steep"||38|42|23|||"None"|"None"|"0"|2.42|3.52|5.7|7.89|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348180"
"47"|"Sebud stony loam, 25 to 50 percent slopes"||38|38.8||||"None"|"None"|"0"|2.46|4.06|7.24|10.4|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"348179"
"46"|"Sebud stony loam, 4 to 25 percent slopes"||15|17.5||||"None"|"None"|"0"|2.39|3.95|7.08|10.2|"Well drained"|"Well drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Not limited"|0.15|"Moderate"|"0"|1|"348178"
"45"|"Rock outcrop-Yawdim association, steep"|||23.2|36||||"None"|"0"|4.3|6.81|8.85|9.85|"Well drained"|"Well drained"|||58||50|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Not rated"|"Poor"|"Not rated"|"Not rated"|0.888|"Severe"|"0"|0.949|"348177"
"44"|"Rock outcrop-Garlet association, very steep"|||55.7|||||"None"|"0"|3.19|5.01|8.23|11.34|"Well drained"|"Well drained"|||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348176"
"43"|"Rock outcrop-Castner association, steep"|||39.6|46||||"None"|"0"|3.1|4.34|4.76|5.18|"Well drained"|"Well drained"|||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"348175"
"42"|"Rentsac loam, 15 to 30 percent slopes"||23|23.3|46|||"None"|"None"|"0"|3.8|5.63|6.03|6.23|"Well drained"|"Well drained"|"D"||100|"7"|91|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.985|"Severe"|"0"|1|"348174"
"41"|"McKenzie clay, saline"||1|1.1||0|0|"None"|"None"|"90"|2.03|4|7.95|11.9|"Poorly drained"|"Poorly drained"|"D"||90|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.925|"Slight"|"90"|1|"348173"
"40"|"Lonna silt loam, 8 to 15 percent slopes"||12|11.7||||"None"|"None"|"0"|4.43|8.36|15.45|22.12|"Well drained"|"Well drained"|"B"||93|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Very limited"|0.947|"Severe"|"0"|0.659|"348172"
"4"|"Absarokee-Sinnigam clay loams, 8 to 15 percent slopes"||12|11.9|46|||"None"|"None"|"0"|3.74|6.77|10.48|10.71|"Well drained"|"Well drained"|"C"||93|"4"|62|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.099|"Moderate"|"0"|0.777|"348171"
"39"|"Lonna silt loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|4.47|8.55|16.06|23.21|"Well drained"|"Well drained"|"B"|"4"|85|"4"|85|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.399|"Moderate"|"0"|0.35|"348170"
"38"|"Lolo and Nesda soils, flooded"||1|1.3||61|61|"Occasional"|"Occasional"|"8"|3.66|6.36|9.52|12.53|"Well drained"|"Well drained"|"B"|"6"|35|"6"|74|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.177|"Slight"|"8"|0.978|"348169"
"331F"|"Wayden-Castner complex, 15 to 60 percent slopes"||38|36.7|41|||"None"|"None"|"0"|3.43|5.6|6.04|6.48|"Well drained"|"Well drained"|"D"||100|"7"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.955|"Severe"|"0"|0.981|"361444"
"330D"|"Absarokee-Amherst complex, 8 to 15 percent slopes"||12|11.9|46|||"None"|"None"|"0"|3.88|7.21|8.62|8.62|"Well drained"|"Well drained"|"C"|"4"|53|"4"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.147|"Severe"|"0"|0.893|"361445"
"330C"|"Absarokee-Amherst complex, 2 to 8 percent slopes"||5|5|46|||"None"|"None"|"0"|3.87|7.17|8.53|8.53|"Well drained"|"Well drained"|"D"|"4"|52|"4"|52|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.146|"Moderate"|"0"|0.898|"361446"
"283F"|"Castner-Wayden complex, moist, 15 to 60 percent slopes"||38|37.3|41|||"None"|"None"|"0"|3.18|5.07|5.29|5.49|"Well drained"|"Well drained"|"D"||100|"7"|96|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.982|"Severe"|"0"|1|"361447"
"262D"|"Wayden-Castner-Cabba complex, 2 to 15 percent slopes"||9|8.8|38|||"None"|"None"|"0"|3.56|5.85|6.21|6.45|"Well drained"|"Well drained"|"D"|"6"|61|"6"|61|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.448|"Severe"|"0"|0.984|"361448"
"224C"|"Shambo loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.65|9.02|17.74|26.44|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.119|"Moderate"|"0"|0.065|"361449"
"131D"|"Reedpoint very channery loam, 2 to 15 percent slopes"||9|9|13|||"None"|"None"|"0"|1.37|1.61|1.69|1.69|"Well drained"|"Well drained"|"D"||100|"7"|86|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.241|"Slight"|"0"|1|"600116"
"333F"|"Shawmut-Castner-Rock outcrop complex, 15 to 60 percent slopes"||38|38|41|||"None"|"None"|"0"|2.91|4.58|6.33|7.83|"Well drained"|"Well drained"|"B"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"600120"
"M-W"|"Miscellaneous water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"997402"
"12A"|"Havre-Harlake complex, 0 to 2 percent slopes, occasionally flooded, channeled"||1|1||||"Occasional"|"Occasional"|"0"|4.01|7.94|15.69|23.43|"Well drained"|"Well drained"|"B"|"2"|50|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.286|"Slight"|"3"|0.743|"1712460"
"152B"|"Eapa loam, calcareous, 0 to 8 percent slopes"||4|4||||"None"|"None"|"0"|4.22|8.61|17.53|26.7|"Well drained"|"Well drained"|"B"||90|"4"|85|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.217|"Moderate"|"0"|0.05|"1712538"
"154B"|"Marmarth-Beenom complex, 2 to 8 percent slopes"||5|5|46|||"None"|"None"|"0"|3.97|7.48|9.96|9.96|"Well drained"|"Well drained"|"C"||95|"4"|52|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.101|"Moderate"|"0"|0.74|"1712540"
"154C"|"Bonfri-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.95|"1712541"
"154D"|"Cabbart-Bonfri loams, 4 to 15 percent slopes"||10|7.8|41|||"None"|"None"|"0"|3.93|7.07|9.7|9.7|"Well drained"|"Well drained"|"D"||55|"6"|55|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Severe"|"0"|0.807|"1712542"
"52B"|"Eapa loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.46|8.88|17.83|26.82|"Well drained"|"Well drained"|"B"||90|"3"|98|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.219|"Moderate"|"0"|0.029|"1712548"
"53A"|"Tanna loam, 1 to 6 percent slopes"||4|4.3|64|||"None"|"None"|"0"|4.05|7.06|8.93|9.17|"Well drained"|"Well drained"|"D"|"3"|83|"3"|83|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.271|"Moderate"|"0"|1|"1712549"
"54A"|"Marmarth fine sandy loam, 1 to 8 percent slopes"||5|5.3|79|||"None"|"None"|"0"|3.96|7.92|12.55|13.03|"Well drained"|"Well drained"|"C"||100|"4"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.054|"Moderate"|"0"|0.5|"1712550"
"55B"|"Beenom loam, 1 to 8 percent slopes"||5|5.5|50|||"None"|"None"|"0"|4.25|7.99|8.61|8.61|"Well drained"|"Well drained"|"C"||95|"6"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.191|"Moderate"|"0"|0.94|"1712551"
"68C"|"Megonot-Yawdim silty clay loams, 4 to 15 percent slopes"||10|9.7|41|||"None"|"None"|"0"|4.25|7.28|10.03|10.52|"Well drained"|"Well drained"|"D"||94|"4"|51|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.581|"Severe"|"0"|1|"1712552"
"80E"|"Blacksheep-Rock outcrop-Twilight complex, 8 to 45 percent slopes"||27|22.9|46|||"None"|"None"|"0"|3.86|6.7|7.28|7.47|"Well drained"|"Well drained"|"D"||98|"7"|58|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.783|"Severe"|"0"|0.961|"1712553"
"82E"|"Cabbart-Delpoint, calcareous-Rock outcrop complex, 8 to 45 percent slopes"||27|24|41|||"None"|"None"|"0"|3.74|6.52|6.99|7.18|"Well drained"|"Well drained"|"D"||100|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.768|"Severe"|"0"|0.976|"1712555"
"84C"|"Cabbart-Yawdim-Delpoint complex, 4 to 15 percent slopes"||10|9.6|38|||"None"|"None"|"0"|3.55|6.07|7.04|7.42|"Well drained"|"Well drained"|"D"||92|"6"|85|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.367|"Severe"|"0"|0.95|"1712556"
"84D"|"Cabbart-Yawdim-Badland complex, 4 to 35 percent slopes"||20|17.4|41|||"None"|"None"|"0"|3.6|6.26|7.13|7.81|"Well drained"|"Well drained"|"D"||91|"7"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.686|"Severe"|"0"|1|"1712557"
"84F"|"Cabbart-Rock outcrop-Yawdim complex, 15 to 60 percent slopes"||25|25.3|28|||"None"|"None"|"0"|3.89|5.91|6.16|6.37|"Well drained"|"Well drained"|"D"||98|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.979|"Severe"|"0"|0.99|"1712558"
"87B"|"Delpoint, calcareous-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|3.01|5.28|6.09|6.23|"Well drained"|"Well drained"|"C"|"4"|55|"6"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.282|"Moderate"|"0"|0.98|"1712559"
"89C"|"Rentsac fine sandy loam, 2 to 8 percent slopes"||5|5.3|30|||"None"|"None"|"0"|2.49|3.34|3.51|3.51|"Well drained"|"Well drained"|"D"||97|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.033|"Slight"|"0"|0.984|"1712560"
"132B"|"Twilight-Blacksheep sandy loams, 2 to 8 percent slopes"||8|7.5|46|||"None"|"None"|"0"|3.42|6.38|9.16|9.61|"Well drained"|"Well drained"|"B"|"4"|54|"4"|52|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.962|"1712562"
"140B"|"Kobase-Megonot silty clay loams, 1 to 8 percent slopes"||5|4.9|89|||"None"|"None"|"0"|4.24|7.8|13.51|17.45|"Well drained"|"Well drained"|"D"||53|"3"|45|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.332|"Moderate"|"0"|1|"1712563"
"189C"|"Rentsac-Cabbart complex, 2 to 15 percent slopes"||9|9.4|41|||"None"|"None"|"0"|2.84|4.58|4.73|4.73|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.109|"Slight"|"0"|1|"1712564"
"235C"|"Busby-Twilight fine sandy loams, 2 to 8 percent slopes"||5|5|64|||"None"|"None"|"0"|3.69|7.3|12.37|16.46|"Well drained"|"Well drained"|"A"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Moderate"|"0"|0.595|"1712566"
"283E"|"Blacksheep-Twilight-Busby complex, 8 to 25 percent slopes"||17|13.2|46|||"None"|"None"|"0"|3.69|7.13|9.92|12.11|"Well drained"|"Well drained"|"D"||70|"4"|60|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.055|"Severe"|"0"|0.846|"1712567"
"285F"|"Blacksheep, dry-Cabbart, dry-Rock outcrop, complex, 8 to 60 percent slopes"||21|24.5|30|||"None"|"None"|"0"|3.59|5.6|6.33|6.94|"Well drained"|"Well drained"|"D"||93|"7"|68|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.713|"Severe"|"0"|0.944|"1712568"
"369D"|"Rentsac-Tanna complex, 2 to 15 percent slopes"||9|9|41|||"None"|"None"|"0"|3.01|5.42|6.56|6.64|"Well drained"|"Well drained"|"D"|"7"|52|"7"|52|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.184|"Slight"|"0"|1|"1712569"
"586E"|"Cabbart-Rentsac-Rock outcrop, complex, 4 to 35 percent slopes"||20|14.6|30|||"None"|"None"|"0"|3.54|4.71|4.89|4.89|"Well drained"|"Well drained"|"D"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.258|"Severe"|"0"|0.991|"1712570"
"780F"|"Cabbart-Yamacall-Havre, rarely flooded, loams, 2 to 60 percent slopes"||34|13.5|30|||"None"|"Rare"|"0"|4.2|7.09|11.89|16.64|"Well drained"|"Well drained"|"B"||45|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.464|"Severe"|"0"|0.483|"1712572"
"9A"|"Havre loam, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.15|8.1|15.93|23.76|"Well drained"|"Well drained"|"B"|"2"|85|"3"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.226|"Slight"|"3"|0.112|"1712575"
"14A"|"Havre, calcareous-Glendive complex, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|4.03|7.84|15.12|22.4|"Well drained"|"Well drained"|"B"|"4"|83|"4"|83|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.189|"Slight"|"7"|0.335|"1712576"
"22B"|"Nobe-Absher complex, 0 to 4 percent"||2|2||84|84|"None"|"None"|"0"|2.24|4.01|7.41|10.82|"Somewhat poorly drained"|"Somewhat poorly drained"|"D"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.423|"Slight"|"0"|1|"1712577"
"30C"|"Busby fine sandy loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.36|6.76|13.62|19.94|"Well drained"|"Well drained"|"A"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.034|"Moderate"|"0"|0.432|"1712578"
"31C"|"Delpoint-Cabbart-Yamacall loams, 4 to 15 percent slopes"||10|9.2|41|||"None"|"None"|"0"|4.23|7.74|10.42|12.23|"Well drained"|"Well drained"|"D"||77|"4"|50|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.21|"Severe"|"0"|0.763|"1712579"
"33A"|"Yamacall loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.09|7.54|14.19|20.71|"Well drained"|"Well drained"|"B"|"2"|85|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.197|"Slight"|"0"|0.15|"1712580"
"33B"|"Yamacall loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.06|8.02|15.7|23.13|"Well drained"|"Well drained"|"B"|"3"|93|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.198|"Moderate"|"0"|0.132|"1712581"
"36B"|"Yamacall-Delpoint loams, 2 to 8 percent slopes"||5|5.2|71|||"None"|"None"|"0"|3.76|7.34|12.36|16|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.204|"Moderate"|"0"|0.359|"1712582"
"40B"|"Kobase silty clay loam, 2 to 8 percent slopes"||5|4.8||||"None"|"None"|"0"|4.3|8.25|16.06|23.88|"Well drained"|"Well drained"|"C"|"3"|82|"3"|82|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.321|"Moderate"|"0"|0.93|"1712583"
"51A"|"Ethridge clay loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.38|8.47|16.25|24.01|"Well drained"|"Well drained"|"C"|"3"|92|"3"|97|"Very limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.304|"Slight"|"0"|0.95|"1712584"
"253C"|"Tanna-Cabbart loams, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4.18|7.15|8.32|8.48|"Well drained"|"Well drained"|"D"|"3"|58|"3"|58|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.247|"Moderate"|"0"|0.998|"1712588"
"460E"|"Yawdim-Abor complex, 8 to 35 percent slopes"||21|18.1|46|||"None"|"None"|"0"|4.16|7.53|9.32|9.68|"Well drained"|"Well drained"|"D"||95|"7"|64|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.821|"Severe"|"0"|1|"1712856"
"107A"|"Lostriver-Bullhook complex, 0 to 2 percent slopes, rarely flooded"||1|1||||"Rare"|"Rare"|"0"|3.85|7.43|14.56|21.69|"Well drained"|"Well drained"|"C"||85|"6"|82|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.343|"Slight"|"5"|0.92|"1717961"
"182D"|"Cabbart-Delpoint loams, 4 to 15 percent slopes"||10|8.1|41|||"None"|"None"|"0"|3.84|6.95|8.79|9.21|"Well drained"|"Well drained"|"D"||55|"6"|50|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.23|"Severe"|"0"|0.799|"1717962"
"640B"|"Kobase-Gullied land complex, 2 to 8 percent slopes"||5|4.6||||"None"|"None"|"0"|4.21|8.11|15.67|23.22|"Well drained"|"Well drained"|"C"|"3"|65|"3"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.356|"Moderate"|"0"|1|"1717963"
"83D"|"Cabbart-Rock outcrop-Blacksheep complex, 8 to 45 percent slopes"||27|25.2|41|||"None"|"None"|"0"|3.46|5.74|6.22|6.51|"Well drained"|"Well drained"|"D"||97|"7"|63|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.904|"Severe"|"0"|0.968|"1914294"
"189B"|"Rentsac-Beenom complex, 1 to 4 percent slopes"||3|3.4|30|||"None"|"None"|"0"|3.24|5.12|5.59|5.59|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.155|"Moderate"|"0"|0.95|"1914300"
"354B"|"Bonfri-Cabbart loams, 0 to 4 percent slopes"||2|2.9|41|||"None"|"None"|"0"|4.02|7.38|11.13|11.51|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.95|"1914301"
"453C"|"Cabbart-Bonfri loams, 2 to 8 percent slopes"||5|5.5|41|||"None"|"None"|"0"|3.87|6.98|9.88|9.88|"Well drained"|"Well drained"|"D"|"6"|50|"6"|52|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.21|"Moderate"|"0"|1|"1914302"
