05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glaciers is a miscellaneous area."|"22109261"|"22444497"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109273"|"22444509"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109274"|"22444510"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109275"|"22444511"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109262"|"22444498"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kaina component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AX952MT 43a Lower Subalpine Cool Moist Conferous ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109263"|"22444499"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Goathaunt, bouldery soil is a minor component."|"22109282"|"22444518"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet, extremely stony component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the R043AX968MT 43a Montane Stable Colluvial Slope ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109283"|"22444519"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very stony, moist component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, mountains. The parent material consists of mixed volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AX952MT 43a Lower Subalpine Cool Moist Conferous ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109284"|"22444520"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109270"|"22444506"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nataga, extremely stony component makes up 75 percent of the map unit. Slopes are 35 to 60 percent. This component is on avalanche chutes, mountains. The parent material consists of colluvium and/or mass movement deposits derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R043AX962MT 43a Alpine Unstable Talus ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109271"|"22444507"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ledgefork soil is a minor component."|"22109272"|"22444508"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waterpeak component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on avalanche chutes, mountains. The parent material consists of colluvium and/or mass movement deposits derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AX961MT 43a Subalpine Avalanche ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109291"|"22444527"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boatman, very stony component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on avalanche chutes, mountains. The parent material consists of colluvium and/or mass movement deposits derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AX961MT 43a Subalpine Avalanche ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109292"|"22444528"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109293"|"22444529"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109294"|"22444530"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109285"|"22444521"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Glaciers is a miscellaneous area."|"22109286"|"22444522"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109287"|"22444523"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cuberant component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, rises on cirque floors. The parent material consists of colluvium and/or till over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109288"|"22444524"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"22109289"|"22444525"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bridgefore component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on cirque floors, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109290"|"22444526"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kintla soil is a minor component."|"22109318"|"22444554"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder, occasionally flooded soil is a minor component."|"22109319"|"22444555"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109276"|"22444512"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109277"|"22444513"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kaina, extremely stony component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines on cirque platforms, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22109278"|"22444514"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder, occasionally flooded soil is a minor component."|"22109279"|"22444515"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nooney, very stony soil is a minor component."|"22109280"|"22444516"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109281"|"22444517"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109300"|"22444536"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Piegan soil is a minor component."|"22109301"|"22444537"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, very bouldery component makes up 40 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109302"|"22444538"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scalplock soil is a minor component."|"22109303"|"22444539"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109304"|"22444540"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Scalplock soil is a minor component."|"22109305"|"22444541"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood soil is a minor component."|"22109306"|"22444542"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cuberant, very stony component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109307"|"22444543"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very bouldery component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109308"|"22444544"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109336"|"22444572"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109337"|"22444573"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet, extremely stony component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the R043AX968MT 43a Montane Stable Colluvial Slope ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109449"|"22444685"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kaina, very stony component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, mountains. The parent material consists of colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AX952MT 43a Lower Subalpine Cool Moist Conferous ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109448"|"22444684"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, bouldery component makes up 15 percent of the map unit. Slopes are 35 to 60 percent. This component is on glacial-valley walls, mountains. The parent material consists of volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043AX956MT 43a Subalpine Coniferous Cool Moderately Dry ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109447"|"22444683"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109446"|"22444682"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Backroad soil is a minor component."|"22109445"|"22444681"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cosely component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, glacial-valley walls. The parent material consists of volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109385"|"22444621"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkridge component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, glacial-valley walls. The parent material consists of volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109384"|"22444620"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pasturecreek, bouldery component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, glacial-valley walls. The parent material consists of volcanic ash over colluvium and/or till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109383"|"22444619"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"22109382"|"22444618"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"22109381"|"22444617"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, calcareous soil is a minor component."|"22109338"|"22444574"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, bouldery component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109339"|"22444575"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, extremely stony component makes up 45 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109340"|"22444576"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, calcareous soil is a minor component."|"22109450"|"22444686"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109451"|"22444687"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, bouldery component makes up 35 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109452"|"22444688"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, extremely stony component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109453"|"22444689"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109320"|"22444556"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109321"|"22444557"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, extremely stony component makes up 35 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109322"|"22444558"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109454"|"22444690"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109455"|"22444691"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, very bouldery soil is a minor component."|"22109456"|"22444692"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, extremely stony component makes up 25 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109457"|"22444693"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109323"|"22444559"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109324"|"22444560"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, extremely stony component makes up 20 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109325"|"22444561"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109295"|"22444531"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109296"|"22444532"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, very bouldery soil is a minor component."|"22109297"|"22444533"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nooney, extremely stony component makes up 15 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109298"|"22444534"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Cryaquents, occasionally flooded component makes up 15 percent of the map unit. Slopes are 0 to 2 percent. This component is on valleys, flood plains. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"22109299"|"22444535"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah, frequently flooded component makes up 70 percent of the map unit. Slopes are 0 to 2 percent. This component is on valleys, flood plains. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"22109327"|"22444563"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"22109328"|"22444564"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"22109329"|"22444565"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Parkcity component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, stream terraces. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109330"|"22444566"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Typic Cryaquents, stony, occasionally flooded soil is a minor component."|"22109331"|"22444567"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah, frequently flooded component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, flood plains. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"22109332"|"22444568"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Broad Canyon, stony component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on valleys, stream terraces. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109333"|"22444569"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Parkcity component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, valleys. The parent material consists of outwash derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AX966MT 43a Montane Loamy Outwash Terrace ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109326"|"22444562"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Risingwolf, dry soil is a minor component."|"22109345"|"22444581"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock, stony component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, valleys. The parent material consists of outwash derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AX959MT 43a Montane Warm Dry Coniferous ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109346"|"22444582"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Broad Canyon, stony component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces, valleys. The parent material consists of outwash derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043AA036MT Droughty (dr)   Lru 43a-a ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109347"|"22444583"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cosely component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on mountains, outwash terraces. The parent material consists of volcanic ash over outwash derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109458"|"22444694"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Hapludands component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on mountains, outwash terraces. The parent material consists of volcanic ash over outwash derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109459"|"22444695"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sunroad component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on mountains, outwash terraces. The parent material consists of volcanic ash over outwash derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109460"|"22444696"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109341"|"22444577"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"22109342"|"22444578"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, very bouldery component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109343"|"22444579"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nooney soil is a minor component."|"22109344"|"22444580"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Watsondraw, dry component makes up 65 percent of the map unit. Slopes are 15 to 35 percent. This component is on lateral moraines, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109427"|"22444663"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hollandlake component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109428"|"22444664"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mohaggin, dry soil is a minor component."|"22109429"|"22444665"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mikesell component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109485"|"22444721"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poia, occasionally ponded soil is a minor component."|"22109486"|"22444722"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, dry component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109487"|"22444723"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings, stony component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109488"|"22444724"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leighcan soil is a minor component."|"22109430"|"22444666"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Odark soil is a minor component."|"22109431"|"22444667"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock, stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109432"|"22444668"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poia, occasionally ponded soil is a minor component."|"22109442"|"22444678"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vulture component makes up 35 percent of the map unit. Slopes are 10 to 35 percent. This component is on lateral moraines, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109443"|"22444679"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ipasha, occasionally flooded component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, drainageways. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"22109444"|"22444680"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Apikuni component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on lateral moraines, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109489"|"22444725"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on lateral moraines, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109490"|"22444726"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vulture component makes up 45 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109491"|"22444727"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sinopah, frequently ponded component makes up 100 percent of the map unit. Slopes are 0 to 2 percent. This component is on fens on glacial-valley floors, valleys. The parent material consists of volcanic ash layered organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during March, April, May, June. Organic matter content in the surface horizon is about 70 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"22109334"|"22444570"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poia, occasionally ponded component makes up 30 percent of the map unit. Slopes are 0 to 4 percent. This component is on depressions on glacial-valley floors, mountains. The parent material consists of outwash and/or till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"22109335"|"22444571"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pippin, stony component makes up 20 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash terraces on glacial-valley floors, mountains. The parent material consists of outwash derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109353"|"22444589"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Cryaquents, occasionally flooded component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on drainageways on glacial-valley floors, mountains. The parent material consists of alluvium over outwash and/or till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"22109354"|"22444590"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Broad Canyon soil is a minor component."|"22109355"|"22444591"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Foolhen, frequently ponded soil is a minor component."|"22109356"|"22444592"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very stony, dry component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109461"|"22444697"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kintla soil is a minor component."|"22109462"|"22444698"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sherlock component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109463"|"22444699"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109348"|"22444584"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kintla soil is a minor component."|"22109349"|"22444585"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very stony, dry component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109350"|"22444586"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sherlock component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109351"|"22444587"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109464"|"22444700"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bordengulch component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, rises on cirque platforms. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109465"|"22444701"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Katkitos soil is a minor component."|"22109466"|"22444702"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Piegan soil is a minor component."|"22109467"|"22444703"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Coerock, bouldery component makes up 40 percent of the map unit. Slopes are 8 to 35 percent. This component is on depressions on cirque platforms, mountains. The parent material consists of volcanic ash over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109468"|"22444704"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Risingwolf, moist soil is a minor component."|"22109469"|"22444705"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109352"|"22444588"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wolftail, occasionally flooded component makes up 20 percent of the map unit. Slopes are 0 to 15 percent. This component is on drainageways on cirque platforms, mountains. The parent material consists of volcanic ash mixed with alluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"22109369"|"22444605"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vaywood component makes up 30 percent of the map unit. Slopes are 0 to 15 percent. This component is on mountains, rises on cirque platforms. The parent material consists of mixed volcanic ash over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109370"|"22444606"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Katkitos component makes up 35 percent of the map unit. Slopes are 0 to 15 percent. This component is on mountains, depressions on cirque platforms. The parent material consists of mixed volcanic ash over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"22109371"|"22444607"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coerock soil is a minor component."|"22109372"|"22444608"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"22109470"|"22444706"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkpeak component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, solifluction sheets on ridges. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109471"|"22444707"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Piegan component makes up 25 percent of the map unit. Slopes are 8 to 35 percent. This component is on nivation hollows on ridges, mountains. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109472"|"22444708"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Scalplock, stony component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109473"|"22444709"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very stony, dry component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on ground moraines, valleys. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AX951MT 43a Lower Subalpine Cool Dry Coniferous ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22109357"|"22444593"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on ground moraines, valleys. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AX959MT 43a Montane Warm Dry Coniferous ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109358"|"22444594"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on ground moraines, valleys. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AX959MT 43a Montane Warm Dry Coniferous ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109359"|"22444595"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Typic Cryaquents, occasionally flooded soil is a minor component."|"22109360"|"22444596"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very stony, dry component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on valleys, ground moraines. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22109474"|"22444710"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vulture component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on valleys, ground moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109475"|"22444711"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock, stony component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on valleys, ground moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109476"|"22444712"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crownmountain, frequently ponded soil is a minor component."|"22109477"|"22444713"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, stony, dry component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, landslides. The parent material consists of mixed volcanic ash over mass movement deposits derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109373"|"22444609"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crownmountain, frequently ponded component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, landslides. The parent material consists of mass movement deposits derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6w.  This soil meets hydric criteria.   "|"22109374"|"22444610"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sherlock component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, landslides. The parent material consists of mixed volcanic ash over mass movement deposits derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109375"|"22444611"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pasturecreek component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109365"|"22444601"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkridge component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109366"|"22444602"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Hapludands component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109367"|"22444603"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkridge component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109368"|"22444604"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pasturecreek component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on mountains, lateral moraines. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109395"|"22444631"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cosely soil is a minor component."|"22109396"|"22444632"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Backroad soil is a minor component."|"22109397"|"22444633"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Leighcan soil is a minor component."|"22109386"|"22444622"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines on glacial-valley walls, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AX959MT 43a Montane Warm Dry Coniferous ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109387"|"22444623"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings, stony component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines on glacial-valley walls, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AX951MT 43a Lower Subalpine Cool Dry Coniferous ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109388"|"22444624"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin, stony, dry component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines on glacial-valley walls, mountains. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AX951MT 43a Lower Subalpine Cool Dry Coniferous ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109389"|"22444625"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sherlock soil is a minor component."|"22109390"|"22444626"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109391"|"22444627"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cuberant component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, colluvial aprons. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109392"|"22444628"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nataga, extremely stony component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, colluvial aprons. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109393"|"22444629"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Altyn soil is a minor component."|"22109394"|"22444630"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Odark, stony soil is a minor component."|"22109376"|"22444612"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mikesell component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, mountains. The parent material consists of till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BX953MT 43b Montane Deciduous Clayey Outwash Terrace ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109403"|"22444639"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Apikuni component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, mountains. The parent material consists of till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109404"|"22444640"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, mountains. The parent material consists of till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043AX951MT 43a Lower Subalpine Cool Dry Coniferous ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109405"|"22444641"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mikesell component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, mountains. The parent material consists of till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109409"|"22444645"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poia, occasionally ponded soil is a minor component."|"22109410"|"22444646"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Odark, stony component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, mountains. The parent material consists of till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109425"|"22444661"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ericson component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, mountains. The parent material consists of till derived from metamorphic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109426"|"22444662"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109438"|"22444674"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kegsprings component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109439"|"22444675"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Muddycreek component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains, mountain slopes. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109440"|"22444676"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Watsondraw, moist soil is a minor component."|"22109441"|"22444677"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22109433"|"22444669"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Watsondraw, dry soil is a minor component."|"22109434"|"22444670"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crawfish soil is a minor component."|"22109435"|"22444671"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, dry component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of mixed volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AX951MT 43a Lower Subalpine Cool Dry Coniferous ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109436"|"22444672"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet, extremely stony component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the R043AX968MT 43a Montane Stable Colluvial Slope ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109437"|"22444673"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kaina, extremely stony soil is a minor component."|"22109398"|"22444634"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cuberant component makes up 40 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains, cirque headwalls. The parent material consists of colluvium over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109399"|"22444635"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Risingwolf soil is a minor component."|"22109400"|"22444636"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder, occasionally flooded soil is a minor component."|"22109401"|"22444637"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nooney soil is a minor component."|"22109402"|"22444638"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, non-calcareous soil is a minor component."|"22109419"|"22444655"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet, very stony component makes up 30 percent of the map unit. Slopes are 60 to 80 percent. This component is on cirque headwalls, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"22109420"|"22444656"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Piegan soil is a minor component."|"22109421"|"22444657"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkridge component makes up 20 percent of the map unit. Slopes are 4 to 15 percent. This component is on glacial-valley floors, mountains. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"22109422"|"22444658"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rollins component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on glacial-valley floors, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22109423"|"22444659"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pasturecreek, bouldery component makes up 55 percent of the map unit. Slopes are 2 to 15 percent. This component is on depressions on glacial-valley floors, mountains. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"22109424"|"22444660"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, very stony, dry component makes up 45 percent of the map unit. Slopes are 8 to 35 percent. This component is on valleys, ground moraines. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109478"|"22444714"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kegsprings soil is a minor component."|"22109479"|"22444715"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 30 percent of the map unit. Slopes are 8 to 35 percent. This component is on valleys, ground moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109480"|"22444716"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Broad Canyon component makes up 20 percent of the map unit. Slopes are 8 to 35 percent. This component is on valleys, ground moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109481"|"22444717"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet, extremely stony component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, colluvial aprons. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22109418"|"22444654"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nataga, very stony component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, colluvial aprons. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109417"|"22444653"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Risingwolf, stony, dry soil is a minor component."|"22109416"|"22444652"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, colluvial aprons. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109415"|"22444651"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sunroad soil is a minor component."|"22109414"|"22444650"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cosely soil is a minor component."|"22109413"|"22444649"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pasturecreek component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, alluvial fans. The parent material consists of volcanic ash over alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"22109412"|"22444648"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pippin component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, alluvial fans. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109411"|"22444647"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ericson, very stony component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on valleys, marginal ground moraines. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"22109406"|"22444642"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ipasha, occasionally flooded component makes up 15 percent of the map unit. Slopes are 0 to 15 percent. This component is on drainageways on marginal ground moraines, valleys. The parent material consists of alluvium over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 4 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent.  Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"22109407"|"22444643"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Leighcan component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on marginal ground moraines, valleys. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109408"|"22444644"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poia soil is a minor component."|"22109482"|"22444718"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jurvannah, frequently flooded component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on valleys, drainageways. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 0 inches during April, May, June, July. Organic matter content in the surface horizon is about 2 percent.  Nonirrigated land capability classification is 7w. Irrigated land capability classification is 7w. This soil meets hydric criteria.   "|"22109483"|"22444719"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Broad Canyon, very stony component makes up 40 percent of the map unit. Slopes are 4 to 15 percent. This component is on valleys, stream terraces. The parent material consists of alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria.   "|"22109484"|"22444720"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Goathaunt soil is a minor component."|"22109361"|"22444597"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Pippin component makes up 15 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on glacial-valley floors, mountains. The parent material consists of till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109362"|"22444598"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mohaggin, moist component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, glacial-valley floors. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109363"|"22444599"
05/16/2017 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Risingwolf, stony, moist component makes up 30 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains, depressions on glacial-valley floors. The parent material consists of mixed volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109364"|"22444600"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"22109309"|"22444545"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"22109255"|"22444491"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lingshire component makes up 35 percent of the map unit. Slopes are 4 to 35 percent. This component is on swales, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109256"|"22444492"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wander, stony component makes up 25 percent of the map unit. Slopes are 4 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109257"|"22444493"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hourglass component makes up 15 percent of the map unit. Slopes are 4 to 25 percent. This component is on swales, mountain slopes, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109258"|"22444494"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, very stony soil is a minor component."|"22109259"|"22444495"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Potlatch soil is a minor component."|"22109260"|"22444496"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, sandstone, shale soil is a minor component."|"22109310"|"22444546"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lingshire component makes up 15 percent of the map unit. Slopes are 8 to 25 percent. This component is on swales, mountains. The parent material consists of slope alluvium and/or colluvium derived from sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent.  Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109311"|"22444547"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wander, stony component makes up 35 percent of the map unit. Slopes are 8 to 45 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109312"|"22444548"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood, very stony component makes up 25 percent of the map unit. Slopes are 8 to 45 percent. This component is on ridges, mountains. The parent material consists of colluvium over residuum weathered from sedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109313"|"22444549"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Potlatch soil is a minor component."|"22109314"|"22444550"
05/07/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adel soil is a minor component."|"22109315"|"22444551"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22109316"|"22444552"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mariaspass, stony component makes up 25 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109317"|"22444553"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jefflake component makes up 15 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 22 inches (depth from the mineral surface is 20 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the F043BP906MT Subirrigated Cold Woodland ecological site. Nonirrigated land capability classification is 7w.  This soil does not meet hydric criteria.   "|"22109377"|"22444613"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Potlatch soil is a minor component."|"22109378"|"22444614"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, very stony soil is a minor component."|"22109379"|"22444615"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig component makes up 35 percent of the map unit. Slopes are 35 to 70 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109380"|"22444616"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22109264"|"22444500"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mariaspass, stony component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium over residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent.  Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22109265"|"22444501"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Jefflake component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 22 inches (depth from the mineral surface is 20 inches) during April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the F043BP906MT Subirrigated Cold Woodland ecological site. Nonirrigated land capability classification is 6w.  This soil does not meet hydric criteria.   "|"22109266"|"22444502"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Potlatch soil is a minor component."|"22109267"|"22444503"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, very stony soil is a minor component."|"22109268"|"22444504"
05/20/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig, very stony component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"22109269"|"22444505"
