07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"22325128"|"22708459"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farland soil is a minor component."|"22325129"|"22708460"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wyola soil is a minor component."|"22325130"|"22708461"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325131"|"22708462"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Adger component makes up 85 percent of the map unit. Slopes are 1 to 8 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE073MT Dense Clay (dc) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"22325132"|"22708463"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325133"|"22708464"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"22325180"|"22708511"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahl soil is a minor component."|"22325181"|"22708512"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farland soil is a minor component."|"22325182"|"22708513"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cambert component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of silty residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325183"|"22708514"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cabba component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22325184"|"22708515"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cherry component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325185"|"22708516"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tinsley soil is a minor component."|"22325186"|"22708517"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325187"|"22708518"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"22325188"|"22708519"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"22325189"|"22708520"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cambert component makes up 30 percent of the map unit. Slopes are 15 to 25 percent. This component is on hills. The parent material consists of silty residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325190"|"22708521"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cabba component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22325191"|"22708522"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325192"|"22708523"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325193"|"22708524"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farland soil is a minor component."|"22325194"|"22708525"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cabba soil is a minor component."|"22325195"|"22708526"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cambert soil is a minor component."|"22325196"|"22708527"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cherry component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325197"|"22708528"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dimmick component makes up 85 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions on till plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is very high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R053AY711MT Recharge Closed Depression (cdr) ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.  There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325117"|"22708448"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325118"|"22708449"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McKenzie soil is a minor component."|"22325119"|"22708450"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"22325120"|"22708451"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adger soil is a minor component."|"22325121"|"22708452"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"22325198"|"22708529"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325199"|"22708530"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325200"|"22708531"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Dooley component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on moraines. The parent material consists of sandy eolian deposits over dense till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325201"|"22708532"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Telstad soil is a minor component."|"22325202"|"22708533"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Evanston component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XC217MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325203"|"22708534"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Hillon soil is a minor component."|"22325204"|"22708535"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"22325205"|"22708536"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325206"|"22708537"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325207"|"22708538"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farland component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325208"|"22708539"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cambert soil is a minor component."|"22325209"|"22708540"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cabba soil is a minor component."|"22325210"|"22708541"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325211"|"22708542"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farland component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325212"|"22708543"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cherry component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of silty alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325213"|"22708544"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"22325214"|"22708545"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"22325215"|"22708546"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farland soil is a minor component."|"22325216"|"22708547"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farnuf component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325217"|"22708548"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havre soil is a minor component."|"22325218"|"22708549"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Fluvaquents component makes up 95 percent of the map unit. Slopes are 0 to 1 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.     This soil meets hydric criteria.   "|"22325219"|"22708550"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"22325134"|"22708465"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wyola soil is a minor component."|"22325135"|"22708466"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farland soil is a minor component."|"22325136"|"22708467"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Farnuf component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325137"|"22708468"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Adger component makes up 50 percent of the map unit. Slopes are 1 to 8 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE073MT Dense Clay (dc) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"22325138"|"22708469"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325139"|"22708470"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"22325220"|"22708551"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Harlem soil is a minor component."|"22325221"|"22708552"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Fluvaquents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R053AE068MT Wet Meadow (wm) 10-14"" P.z. ecological site.   This soil meets hydric criteria.   "|"22325222"|"22708553"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Glendive component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC212MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325223"|"22708554"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Banks soil is a minor component."|"22325224"|"22708555"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havre soil is a minor component."|"22325225"|"22708556"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"22325226"|"22708557"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325227"|"22708558"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wyola soil is a minor component."|"22325228"|"22708559"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"22325229"|"22708560"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Grail component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on till plains. The parent material consists of clayey local alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325230"|"22708561"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325231"|"22708562"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havre soil is a minor component."|"22325232"|"22708563"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Harlem component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC205MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325233"|"22708564"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Glendive soil is a minor component."|"22325234"|"22708565"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Harlem soil is a minor component."|"22325235"|"22708566"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havre component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC217MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"22325236"|"22708567"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Somewhat poorly drained soils soil is a minor component."|"22325237"|"22708568"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Glendive component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC212MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325238"|"22708569"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Harlem soil is a minor component."|"22325239"|"22708570"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havre component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC217MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"22325240"|"22708571"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lallie, occasionally flooded soil is a minor component."|"22325729"|"22709060"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trembles, occasionally flooded soil is a minor component."|"22325730"|"22709061"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fluvaquents, channeled, frequently flooded soil is a minor component."|"22325731"|"22709062"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Havrelon, occasionally flooded component makes up 80 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood-plain steps on river valleys. The parent material consists of fine-loamy alluvium derived from sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R054XY041ND Loamy Terrace ecological site. Nonirrigated land capability classification is 2e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"22325732"|"22709063"
08/23/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ridgelawn, occasionally flooded soil is a minor component."|"22325733"|"22709064"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Trembles soil is a minor component."|"22325241"|"22708572"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havrelon component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"22325242"|"22708573"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"22325243"|"22708574"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Banks soil is a minor component."|"22325244"|"22708575"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325245"|"22708576"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"22325246"|"22708577"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Trembles component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325247"|"22708578"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havrelon component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"22325248"|"22708579"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Trembles component makes up 30 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325249"|"22708580"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"22325250"|"22708581"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Havrelon component makes up 60 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"22325251"|"22708582"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Banks soil is a minor component."|"22325252"|"22708583"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farland soil is a minor component."|"22325140"|"22708471"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325141"|"22708472"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Nobe component makes up 40 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE071MT Saline Upland (su) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a strongly sodic horizon within 30 inches of the soil surface."|"22325142"|"22708473"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Adger component makes up 50 percent of the map unit. Slopes are 1 to 4 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE073MT Dense Clay (dc) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"22325143"|"22708474"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325144"|"22708475"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Telstad soil is a minor component."|"22325642"|"22708973"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ferd soil is a minor component."|"22325643"|"22708974"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elloam soil is a minor component."|"22325644"|"22708975"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Hillon component makes up 45 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY710MT Limy (ly) Dry Grassland, Limy (ly) Dry Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"22325645"|"22708976"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"22325646"|"22708977"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22325647"|"22708978"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chinook soil is a minor component."|"22325648"|"22708979"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325649"|"22708980"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Joplin component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY712MT Loamy (lo) Dry Grassland, Loamy (lo) Dry Shrubland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325650"|"22708981"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Joplin soil is a minor component."|"22325635"|"22708966"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Hillon component makes up 80 percent of the map unit. Slopes are 15 to 60 percent. This component is on hillslopes on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY711MT Limy-steep (lystp) Dry Grassland, Limy-steep (lystp) Dry Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"22325636"|"22708967"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"22325637"|"22708968"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Busby soil is a minor component."|"22325638"|"22708969"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kremlin soil is a minor component."|"22325639"|"22708970"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yawdim soil is a minor component."|"22325640"|"22708971"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"22325641"|"22708972"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325253"|"22708584"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tinsley soil is a minor component."|"22325254"|"22708585"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Evanston soil is a minor component."|"22325255"|"22708586"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC617MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22325256"|"22708587"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Hillon component makes up 75 percent of the map unit. Slopes are 8 to 15 percent. This component is on till plains. The parent material consists of loamy glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC217MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325257"|"22708588"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325258"|"22708589"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC617MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22325259"|"22708590"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Hillon component makes up 75 percent of the map unit. Slopes are 15 to 45 percent. This component is on till plains. The parent material consists of loamy glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC223MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325260"|"22708591"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"22325261"|"22708592"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"22325262"|"22708593"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lallie component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on oxbows. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 5 percent. This component is in the R053AE068MT Wet Meadow (wm) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325263"|"22708594"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325264"|"22708595"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325265"|"22708596"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lihen component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on till plains. The parent material consists of sandy alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"22325266"|"22708597"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325267"|"22708598"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"22325268"|"22708599"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lohler component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325269"|"22708600"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lohler component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"22325270"|"22708601"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowdoin soil is a minor component."|"22325271"|"22708602"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325272"|"22708603"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"22325273"|"22708604"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325274"|"22708605"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Martinsdale component makes up 90 percent of the map unit. Slopes are 1 to 8 percent. This component is on terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"22325275"|"22708606"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"22325276"|"22708607"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McKenzie component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions on till plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is very high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY703MT Discharge Closed Depression (cdd) ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 8 within 30 inches of the soil surface."|"22325122"|"22708453"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimmick soil is a minor component."|"22325123"|"22708454"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"22325124"|"22708455"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adger soil is a minor component."|"22325125"|"22708456"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nobe soil is a minor component."|"22325145"|"22708476"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cambert soil is a minor component."|"22325146"|"22708477"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cabba soil is a minor component."|"22325147"|"22708478"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325148"|"22708479"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Adger soil is a minor component."|"22325149"|"22708480"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Badland is a miscellaneous area."|"22325150"|"22708481"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dimmick soil is a minor component."|"22325113"|"22708444"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Adger soil is a minor component."|"22325114"|"22708445"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Nishon component makes up 90 percent of the map unit. Slopes are 0 to 1 percent. This component is on closed depressions on till plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is very high. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 0 inches during April, May, June. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY711MT Recharge Closed Depression (cdr) ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325115"|"22708446"
05/13/2020 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Grail soil is a minor component."|"22325116"|"22708447"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Adger soil is a minor component."|"22325277"|"22708608"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325278"|"22708609"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325279"|"22708610"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Nobe component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 60 inches during January, February, March, April, May, June, December. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE072MT Saline Overflow (sov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a strongly sodic horizon within 30 inches of the soil surface."|"22325280"|"22708611"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325281"|"22708612"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325282"|"22708613"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"22325283"|"22708614"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"22325284"|"22708615"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Parshall component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on swales. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325285"|"22708616"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325286"|"22708617"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Dooley soil is a minor component."|"22325287"|"22708618"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325288"|"22708619"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Bowbells soil is a minor component."|"22325289"|"22708620"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Parshall component makes up 90 percent of the map unit. Slopes are 0 to 4 percent. This component is on swales. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 51 inches during April, May, June, July, August, September. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE070MT Subirrigated (sb) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"22325290"|"22708621"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Weingart soil is a minor component."|"22325720"|"22709051"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Absher soil is a minor component."|"22325721"|"22709052"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Kevin soil is a minor component."|"22325722"|"22709053"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ethridge soil is a minor component."|"22325723"|"22709054"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Thoeny soil is a minor component."|"22325724"|"22709055"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Phillips component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of clayey till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY712MT Loamy (lo) Dry Grassland, Loamy (lo) Dry Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325725"|"22709056"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"22325726"|"22709057"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325727"|"22709058"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elloam component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of clayey till. Depth to a root restrictive layer, natric, is 2 to 4 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY731MT Thin Claypan (tcp) Dry Grassland, Thin Claypan (tcp) Dry Shrubland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 12 within 30 inches of the soil surface."|"22325728"|"22709059"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Trembles soil is a minor component."|"22325291"|"22708622"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Banks soil is a minor component."|"22325292"|"22708623"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Riverwash is a miscellaneous area."|"22325293"|"22708624"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Adger soil is a minor component."|"22325294"|"22708625"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Grail soil is a minor component."|"22325295"|"22708626"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325296"|"22708627"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nishon soil is a minor component."|"22325297"|"22708628"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"22325298"|"22708629"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Wyola component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE061MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325299"|"22708630"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325300"|"22708631"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325301"|"22708632"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Martinsdale soil is a minor component."|"22325302"|"22708633"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tally component makes up 90 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills. The parent material consists of coarse-loamy alluvium and/or sandy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325303"|"22708634"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"22325304"|"22708635"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325305"|"22708636"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325306"|"22708637"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tally component makes up 90 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of coarse-loamy alluvium and/or sandy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325307"|"22708638"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"22325308"|"22708639"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325309"|"22708640"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325310"|"22708641"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lihen component makes up 30 percent of the map unit. Slopes are 1 to 8 percent. This component is on till plains. The parent material consists of sandy alluvium and/or eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 6 percent.  "|"22325311"|"22708642"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tally component makes up 60 percent of the map unit. Slopes are 1 to 8 percent. This component is on hills. The parent material consists of coarse-loamy alluvium and/or sandy eolian deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325312"|"22708643"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"22325313"|"22708644"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Glendive soil is a minor component."|"22325151"|"22708482"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Trembles soil is a minor component."|"22325152"|"22708483"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"22325153"|"22708484"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Somewhat poorly drained soils soil is a minor component."|"22325154"|"22708485"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havre soil is a minor component."|"22325155"|"22708486"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Banks component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3w.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325156"|"22708487"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Telstad component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on recessionial moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY712MT Loamy (lo) Dry Grassland, Loamy (lo) Dry Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325712"|"22709043"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Joplin component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on recessionial moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY712MT Loamy (lo) Dry Grassland, Loamy (lo) Dry Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325713"|"22709044"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"22325714"|"22709045"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Fortbenton soil is a minor component."|"22325715"|"22709046"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ferd soil is a minor component."|"22325716"|"22709047"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325717"|"22709048"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Marmarth soil is a minor component."|"22325718"|"22709049"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elloam soil is a minor component."|"22325719"|"22709050"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Joplin component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY712MT Loamy (lo) Dry Grassland, Loamy (lo) Dry Shrubland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325651"|"22708982"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"The Hillon component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY710MT Limy (ly) Dry Grassland, Limy (ly) Dry Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 7 within 30 inches of the soil surface."|"22325652"|"22708983"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evanston soil is a minor component."|"22325653"|"22708984"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Hillon soil is a minor component."|"22325654"|"22708985"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Fortbenton soil is a minor component."|"22325655"|"22708986"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Delpoint soil is a minor component."|"22325656"|"22708987"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325657"|"22708988"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Richey soil is a minor component."|"22325605"|"22708936"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"22325606"|"22708937"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bascovy component makes up 35 percent of the map unit. Slopes are 8 to 25 percent. This component is on hillslopes on till plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is very high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY702MT Clayey (cy) Dry Grassland, Clayey (cy) Dry Shrubland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"22325607"|"22708938"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Neldore component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on hillslopes on till plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R052XY724MT Shallow Clay (swc) Dry Grassland, Shallow Clay (swc) Dry Shrubland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 10 within 30 inches of the soil surface."|"22325608"|"22708939"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arsite soil is a minor component."|"22325609"|"22708940"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vaeda soil is a minor component."|"22325610"|"22708941"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Volborg soil is a minor component."|"22325611"|"22708942"
08/27/2018 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sunburst, gravelly surface soil is a minor component."|"22325612"|"22708943"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cabba soil is a minor component."|"22325314"|"22708645"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325315"|"22708646"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"22325316"|"22708647"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 85 percent of the map unit. Slopes are 15 to 45 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22325317"|"22708648"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Hillon soil is a minor component."|"22325318"|"22708649"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Banks soil is a minor component."|"22325319"|"22708650"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Somewhat poorly drained soils soil is a minor component."|"22325320"|"22708651"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"22325321"|"22708652"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Trembles component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325322"|"22708653"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Trembles component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of coarse-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325323"|"22708654"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Banks soil is a minor component."|"22325324"|"22708655"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"22325325"|"22708656"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325326"|"22708657"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325327"|"22708658"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Martinsdale soil is a minor component."|"22325328"|"22708659"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Beaverton soil is a minor component."|"22325329"|"22708660"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325330"|"22708661"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325331"|"22708662"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325332"|"22708663"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325333"|"22708664"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Martinsdale soil is a minor component."|"22325334"|"22708665"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325335"|"22708666"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Beaverton soil is a minor component."|"22325336"|"22708667"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325337"|"22708668"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325338"|"22708669"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325339"|"22708670"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tinsley soil is a minor component."|"22325340"|"22708671"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325341"|"22708672"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325342"|"22708673"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325343"|"22708674"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Martinsdale soil is a minor component."|"22325344"|"22708675"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Beaverton component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on outwash terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE079MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"22325345"|"22708676"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325346"|"22708677"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tinsley soil is a minor component."|"22325347"|"22708678"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325348"|"22708679"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325349"|"22708680"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325350"|"22708681"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Beaverton component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on outwash terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE079MT Shallow To Gravel (swgr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  "|"22325351"|"22708682"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Turner component makes up 50 percent of the map unit. Slopes are 8 to 12 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R053AE062MT Sandy (sy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 12 percent.  "|"22325352"|"22708683"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lihen soil is a minor component."|"22325157"|"22708488"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325158"|"22708489"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325159"|"22708490"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Blanchard component makes up 90 percent of the map unit. Slopes are 4 to 25 percent. This component is on dunes. The parent material consists of eolian sands. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE076MT Sands (sa) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"22325160"|"22708491"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"22325353"|"22708684"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havre soil is a minor component."|"22325354"|"22708685"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Typic Fluvaquents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R053AE068MT Wet Meadow (wm) 10-14"" P.z. ecological site.   This soil meets hydric criteria.   "|"22325355"|"22708686"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"22325356"|"22708687"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Typic Ustifluvents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site.   This soil does not meet hydric criteria.   "|"22325357"|"22708688"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325358"|"22708689"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"22325359"|"22708690"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Ustic Torrifluvents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R052XC207MT Overflow (ov) 10-14"" P.z. ecological site.   This soil does not meet hydric criteria.   "|"22325360"|"22708691"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lallie soil is a minor component."|"22325361"|"22708692"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Riverwash soil is a minor component."|"22325362"|"22708693"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Ustifluvents component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches.  This component is in the R053AE072MT Saline Overflow (sov) 10-14"" P.z. ecological site.   This soil does not meet hydric criteria.   "|"22325363"|"22708694"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Thebo soil is a minor component."|"22325364"|"22708695"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lisam soil is a minor component."|"22325365"|"22708696"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Vanda component makes up 90 percent of the map unit. Slopes are 4 to 10 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC205MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"22325366"|"22708697"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"22325367"|"22708698"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Lisam component makes up 15 percent of the map unit. Slopes are 10 to 15 percent. This component is on plains. The parent material consists of residuum weathered from calcareous shale. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches is very low. Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC215MT Shallow Clay (swc) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"22325368"|"22708699"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Thebo component makes up 30 percent of the map unit. Slopes are 6 to 15 percent. This component is on plains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC205MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325369"|"22708700"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Hillon soil is a minor component."|"22325370"|"22708701"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Vanda component makes up 45 percent of the map unit. Slopes are 4 to 10 percent. This component is on alluvial fans. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R052XC205MT Clayey (cy) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"22325371"|"22708702"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325372"|"22708703"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cambert soil is a minor component."|"22325373"|"22708704"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Beaverton soil is a minor component."|"22325374"|"22708705"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22325375"|"22708706"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cabba component makes up 25 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22325376"|"22708707"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Wabek component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on terraces. The parent material consists of gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325377"|"22708708"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325378"|"22708709"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Beaverton soil is a minor component."|"22325379"|"22708710"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22325380"|"22708711"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Wabek component makes up 50 percent of the map unit. Slopes are 8 to 12 percent. This component is on terraces. The parent material consists of gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325381"|"22708712"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Turner soil is a minor component."|"22325382"|"22708713"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"22325569"|"22708900"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"22325570"|"22708901"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"22325571"|"22708902"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"22325572"|"22708903"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"22325573"|"22708904"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on ground moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325574"|"22708905"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325575"|"22708906"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"22325576"|"22708907"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"22325577"|"22708908"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"22325578"|"22708909"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Amor soil is a minor component."|"22325579"|"22708910"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahill soil is a minor component."|"22325580"|"22708911"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Williams, low precipitation component makes up 45 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325581"|"22708912"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325582"|"22708913"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325583"|"22708914"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Grail soil is a minor component."|"22325161"|"22708492"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325162"|"22708493"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Parshall soil is a minor component."|"22325163"|"22708494"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Nishon soil is a minor component."|"22325164"|"22708495"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Williams soil is a minor component."|"22325165"|"22708496"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Bowbells component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on swales. The parent material consists of local loamy alluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"22325166"|"22708497"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Bowbells component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on swales. The parent material consists of local loamy alluvium and/or till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE067MT Overflow (ov) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 3e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 7 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325167"|"22708498"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 40 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325590"|"22708921"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 35 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY032MT Loamy (lo)   Lru 53a-y ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325591"|"22708922"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"22325592"|"22708923"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wyola soil is a minor component."|"22325593"|"22708924"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dooley soil is a minor component."|"22325594"|"22708925"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cambert soil is a minor component."|"22325595"|"22708926"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325596"|"22708927"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"22325597"|"22708928"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 60 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325598"|"22708929"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vida component makes up 25 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325599"|"22708930"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Williams soil is a minor component."|"22325600"|"22708931"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22325601"|"22708932"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"22325602"|"22708933"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nishon soil is a minor component."|"22325603"|"22708934"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bowbells soil is a minor component."|"22325604"|"22708935"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Zahill component makes up 75 percent of the map unit. Slopes are 15 to 60 percent. This component is on hillslopes on till plains. The parent material consists of fine-loamy till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AY040MT Loamy Steep (lostp)   Lru 53a-y ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"22325584"|"22708915"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabba soil is a minor component."|"22325585"|"22708916"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vida soil is a minor component."|"22325586"|"22708917"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wabek soil is a minor component."|"22325587"|"22708918"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zahl soil is a minor component."|"22325588"|"22708919"
08/22/2016 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Arnegard soil is a minor component."|"22325589"|"22708920"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahl soil is a minor component."|"22325383"|"22708714"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325384"|"22708715"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cambert component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of silty residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325385"|"22708716"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cabba component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22325386"|"22708717"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, knolls. The parent material consists of loamy glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325387"|"22708718"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325388"|"22708719"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahl soil is a minor component."|"22325389"|"22708720"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325390"|"22708721"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cabba component makes up 30 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22325391"|"22708722"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Rock outcrop soil is a minor component."|"22325392"|"22708723"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 30 percent of the map unit. Slopes are 15 to 30 percent. This component is on hills, knolls. The parent material consists of loamy glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325393"|"22708724"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cambert component makes up 30 percent of the map unit. Slopes are 15 to 20 percent. This component is on hills. The parent material consists of silty residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325394"|"22708725"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325395"|"22708726"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325396"|"22708727"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahl soil is a minor component."|"22325397"|"22708728"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Farnuf soil is a minor component."|"22325398"|"22708729"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"22325399"|"22708730"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 75 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills, knolls. The parent material consists of loamy glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE060MT Silty (si) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325400"|"22708731"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cabba soil is a minor component."|"22325401"|"22708732"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahl soil is a minor component."|"22325402"|"22708733"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325403"|"22708734"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tally soil is a minor component."|"22325404"|"22708735"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Tinsley component makes up 15 percent of the map unit. Slopes are 15 to 45 percent. This component is on terraces. The parent material consists of sandy and gravelly outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE621MT Gravel (gr) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"22325405"|"22708736"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Zahill component makes up 75 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills, knolls. The parent material consists of loamy glacial till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"22325406"|"22708737"
05/26/2006 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"22325127"|"22708458"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Lohler soil is a minor component."|"22325168"|"22708499"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havrelon soil is a minor component."|"22325169"|"22708500"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Havre soil is a minor component."|"22325170"|"22708501"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Harlem soil is a minor component."|"22325171"|"22708502"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Bowdoin component makes up 90 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is moderately well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches is moderate.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R053AE073MT Dense Clay (dc) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a moderately saline horizon within 30 inches of the soil surface. The soil has a moderately sodic horizon within 30 inches of the soil surface."|"22325172"|"22708503"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The McKenzie soil is a minor component."|"22325173"|"22708504"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Wabek soil is a minor component."|"22325174"|"22708505"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Tinsley soil is a minor component."|"22325175"|"22708506"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Zahill soil is a minor component."|"22325176"|"22708507"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cambert component makes up 25 percent of the map unit. Slopes are 15 to 25 percent. This component is on hills. The parent material consists of silty residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE064MT Silty-steep (sistp) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  The soil has a slightly sodic horizon within 30 inches of the soil surface."|"22325177"|"22708508"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"The Cabba component makes up 60 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of loamy residuum weathered from interbedded sedimentary rock. Depth to a root restrictive layer, bedrock, paralithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches is very low. Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R053AE077MT Shallow (sw) 10-14"" P.z. ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"22325178"|"22708509"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major components.  The Cherry soil is a minor component."|"22325179"|"22708510"
08/19/2019 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"22325126"|"22708457"
07/14/2010 00:00:00|"Nontechnical description"|"GENSOIL"||"Generated brief soil descriptions are created for major soil components.  The Land fill is a miscellaneous area."|"22325407"|"22708738"
