"100F"|"Rubble land"|||43||||||"0"|2.25|4.38|5.88|7.38|||||100|"8"|95|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"344133"
"115B"|"Thoeny-Elloam-Absher complex, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|4.13|7.87|15.18|22.54|"Well drained"|"Well drained"|"D"|"6"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.26|"Slight"|"1"|0.995|"344134"
"12C"|"Beaverton gravelly loams, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.04|4.77|6.89|8.91|"Well drained"|"Well drained"|"B"|"4"|95|"6"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.062|"Moderate"|"0"|0.973|"344135"
"14C"|"Brockway silt loam, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|4.6|8.6|16.61|24.63|"Well drained"|"Well drained"|"C"||98|"4"|98|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.328|"Moderate"|"0"|0.293|"344137"
"15E"|"Lambeth silt loam, 8 to 25 percent slopes"||17|17.5||||"None"|"None"|"0"|4.84|9.59|19.08|28.57|"Well drained"|"Well drained"|"C"||99|"6"|96|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.985|"Severe"|"0"|0.993|"344138"
"15F"|"Lambeth silt loam, 25 to 70 percent slopes"||48|47.6||||"None"|"None"|"0"|4.83|9.56|19.03|28.49|"Well drained"|"Well drained"|"C"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344139"
"16B"|"Degrand fine sandy loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.73|7.45|13.71|15.76|"Well drained"|"Well drained"|"B"|"4"|95|"4"|96|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.083|"Slight"|"0"|0.99|"344140"
"171C"|"Delpoint-Cabbart loams, 2 to 8 percent slopes"||5|5.2|30|||"None"|"None"|"0"|4.33|6.97|8.48|8.78|"Well drained"|"Well drained"|"C"|"4"|52|"4"|52|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.225|"Moderate"|"0"|0.892|"344142"
"18E"|"Yawdim silty clay, 8 to 25 percent slopes"||17|17.1|30|||"None"|"None"|"0"|4.24|5.24|5.42|5.55|"Well drained"|"Well drained"|"D"||99|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.502|"Severe"|"0"|0.997|"344144"
"190B"|"Hedstrom fine sandy loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|3.61|7.32|10.57|13.02|"Well drained"|"Well drained"|"B"|"4"|97|"4"|97|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.037|"Slight"|"0"|0.98|"344145"
"200F"|"Badland"|||31.1||||||"0"|4.36|7.41|11.02|13.89|||||97|"8"|85|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|0.813|"Not rated"|"0"|0.859|"344147"
"201D"|"Cabba-Wayden complex, 4 to 15 percent slopes"||10|10.2|30|||"None"|"None"|"0"|4.07|5.1|5.27|5.4|"Well drained"|"Well drained"|"D"||97|"6"|91|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.297|"Severe"|"0"|0.983|"344148"
"201F"|"Cabba-Wayden-Rock outcrop complex, 15 to 60 percent slopes"||38|37.5|30|||"None"|"None"|"0"|4.1|4.98|4.98|4.98|"Well drained"|"Well drained"|"D"||100|"7"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344150"
"211E"|"Cabbart-Yawdim complex, 8 to 25 percent slopes"||17|17.1|30|||"None"|"None"|"0"|4.37|5.31|5.49|5.64|"Well drained"|"Well drained"|"D"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.351|"Severe"|"0"|0.998|"344151"
"211F"|"Cabbart-Yawdim-Rock outcrop complex, 25 to 70 percent"||48|46.5|30|||"None"|"None"|"0"|4.36|5.36|5.68|5.97|"Well drained"|"Well drained"|"D"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.981|"Severe"|"0"|1|"344152"
"21E"|"Cabbart-Delpoint loams, 8 to 25 percent slopes"||17|15.5|30|||"None"|"None"|"0"|4.37|6.67|8.1|8.67|"Well drained"|"Well drained"|"D"||97|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.255|"Severe"|"0"|0.932|"344153"
"221E"|"Hillon-Kevin clay loams, 8 to 25 percent slopes"||17|16||||"None"|"None"|"0"|4.29|8.49|16.4|23.82|"Well drained"|"Well drained"|"C"||96|"6"|87|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.245|"Severe"|"0"|0.96|"344154"
"224B"|"Joplin-Hillon loams, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|4.18|8.37|16.3|23.37|"Well drained"|"Well drained"|"C"|"3"|58|"3"|58|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.228|"Slight"|"1"|0.525|"344155"
"224E"|"Hillon-Joplin loams, 8 to 25 percent slopes"||17|15.8||||"None"|"None"|"0"|4.1|8.16|15.76|22.73|"Well drained"|"Well drained"|"C"||96|"6"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.215|"Severe"|"0"|0.939|"344156"
"225F"|"Hillon-Cabbart loams, 15 to 60 percent slopes"||38|33.8|38|||"None"|"None"|"0"|3.82|6.69|10.58|14.15|"Well drained"|"Well drained"|"C"||96|"7"|81|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.879|"Severe"|"0"|0.936|"344157"
"22F"|"Hillon loam, 15 to 60 percent slopes"||38|33.6||||"None"|"None"|"0"|4.01|7.89|14.98|21.74|"Well drained"|"Well drained"|"C"||98|"7"|83|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.864|"Severe"|"0"|0.94|"344158"
"23B"|"Acel silty clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"2"|4.25|8.24|16.22|24.2|"Well drained"|"Well drained"|"C"||98|"3"|96|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.344|"Slight"|"2"|1|"344159"
"24B"|"Farnuf loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"2"|4.31|8.32|15.89|22.98|"Well drained"|"Well drained"|"B"|"3"|95|"3"|98|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.142|"Slight"|"2"|0.047|"344160"
"261C"|"Auchard-Williams complex, 2 to 8 percent slopes"||5|5.3|56|||"None"|"None"|"0"|4.43|8.15|12.69|16.85|"Well drained"|"Well drained"|"D"|"4"|45|"6"|50|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.11|"Moderate"|"0"|0.95|"344162"
"271D"|"Beaverell-Tinsley complex, 4 to 15 percent slopes"||10|9.7||||"None"|"None"|"0"|2.2|3.17|4.55|5.92|"Well drained"|"Well drained"|"B"||94|"6"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.049|"Moderate"|"0"|1|"344163"
"272C"|"Attewan-Tinsley complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|2.97|5.28|6.97|8.34|"Well drained"|"Well drained"|"B"|"3"|52|"3"|52|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.086|"Moderate"|"0"|1|"344164"
"27B"|"Attewan loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.25|7.92|9.98|11.63|"Well drained"|"Well drained"|"B"|"3"|98|"3"|98|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.14|"Slight"|"0"|1|"344165"
"28A"|"Nishon clay loam, 0 to 1 percent slopes"||0|0.1||0|0|"None"|"None"|"93"|4.67|9.15|17.79|25.82|"Poorly drained"|"Poorly drained"|"C/D"|"3"|95|"3"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.947|"Slight"|"93"|0.975|"344168"
"301C"|"Marvan-Vanda complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"1"|3.14|6.01|11.23|16.26|"Well drained"|"Well drained"|"D"|"4"|67|"4"|69|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.505|"Moderate"|"1"|1|"344169"
"302B"|"Marvan clay, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|3.41|6.43|11.77|16.84|"Well drained"|"Well drained"|"D"|"4"|99|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.505|"Slight"|"1"|1|"344170"
"304B"|"Marvan-Joplin, complex, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|3.76|7.14|13.2|19.09|"Well drained"|"Well drained"|"D"||53|"6"|55|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.376|"Slight"|"0"|1|"344171"
"306D"|"Marvan-Yawdim-Cabbart complex, 4 to 15 percent slopes"||6|8.2|30|||"None"|"None"|"0"|3.88|5.92|8.76|11.46|"Well drained"|"Well drained"|"D"||98|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.455|"Severe"|"0"|1|"344172"
"30B"|"Marvan silty clay, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|3.41|6.43|11.77|16.83|"Well drained"|"Well drained"|"D"|"4"|99|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.505|"Slight"|"1"|1|"344173"
"30C"|"Marvan silty clay, 4 to 8 percent slopes"||6|6||||"None"|"None"|"1"|3.42|6.44|11.76|16.8|"Well drained"|"Well drained"|"D"|"4"|97|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.505|"Moderate"|"1"|1|"344174"
"311B"|"Ferd-Creed-Gerdrum complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"2"|3.85|7.07|13.08|19.05|"Well drained"|"Well drained"|"C"|"3"|40|"3"|41|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.328|"Slight"|"2"|1|"344175"
"321B"|"Kobase silty clay loam, calcareous, 0 to 4 percent"||2|2||||"None"|"None"|"1"|3.99|7.98|15.94|23.91|"Well drained"|"Well drained"|"C"|"4"|99|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.337|"Slight"|"1"|1|"344176"
"321C"|"Kobase silty clay loam, calcareous, 4 to 8 percent"||6|5.9||||"None"|"None"|"1"|4|8|15.98|23.97|"Well drained"|"Well drained"|"C"|"4"|98|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.342|"Moderate"|"1"|1|"344177"
"323B"|"Sagedale silty clay, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|4.24|8.28|15.73|22.99|"Well drained"|"Well drained"|"C"||97|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Slight"|"0"|1|"344179"
"323C"|"Sagedale silty clay, 4 to 8 percent slopes"||6|6.3||||"None"|"None"|"0"|4.24|8.28|15.75|23.01|"Well drained"|"Well drained"|"C"||97|"4"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.51|"Moderate"|"0"|1|"344180"
"32B"|"Kobase silty clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|4|7.99|15.96|23.94|"Well drained"|"Well drained"|"C"|"4"|98|"4"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.338|"Slight"|"1"|1|"344181"
"32C"|"Kobase silty clay loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"1"|4|7.99|15.98|23.96|"Well drained"|"Well drained"|"C"|"4"|99|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.342|"Moderate"|"1"|1|"344182"
"331B"|"Phillips-Elloam complex, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"1"|4.24|8.33|16.2|23.6|"Well drained"|"Well drained"|"C"|"3"|60|"3"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.256|"Slight"|"1"|0.985|"344183"
"34A"|"Linnet clay, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"2"|3.9|7.65|15.15|22.33|"Well drained"|"Well drained"|"C"|"4"|97|"4"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.508|"Slight"|"2"|1|"344185"
"351B"|"Kenilworth-Fortbenton fine sandy loams, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|3.93|8.04|16.33|24.29|"Well drained"|"Well drained"|"C"|"4"|94|"4"|94|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.115|"Slight"|"1"|0.513|"344186"
"35B"|"Assinniboine fine sandy loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.11|8.45|14.96|21.43|"Well drained"|"Well drained"|"C"|"4"|95|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.089|"Slight"|"0"|0.511|"344187"
"363B"|"Cozberg-Chinook fine sandy loams, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"0"|3.64|7.14|12.57|16.66|"Well drained"|"Well drained"|"A"|"4"|94|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Not rated"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.022|"Slight"|"0"|0.764|"344188"
"368C"|"Fortbenton-Hillon complex, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.83|7.54|15.43|22.94|"Well drained"|"Well drained"|"C"|"4"|89|"4"|91|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.129|"Moderate"|"0"|0.503|"344190"
"36C"|"Chinook fine sandy loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.65|7.16|13.72|20.19|"Well drained"|"Well drained"|"A"|"4"|90|"4"|95|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.07|"Moderate"|"0"|0.475|"344192"
"37B"|"Evanston loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|4.3|8.3|16.46|24.94|"Well drained"|"Well drained"|"B"|"2"|95|"3"|99|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.147|"Slight"|"1"|0.03|"344193"
"37C"|"Evanston loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"1"|4.3|8.3|16.45|24.94|"Well drained"|"Well drained"|"B"|"3"|96|"3"|98|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.147|"Moderate"|"1"|0.026|"344194"
"385B"|"Ethridge-Kobase complex, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"3"|4.21|8.23|16.18|24.12|"Well drained"|"Well drained"|"C"|"3"|55|"3"|58|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.356|"Slight"|"3"|1|"344195"
"38B"|"Ethridge silty clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|4.37|8.44|16.42|24.41|"Well drained"|"Well drained"|"C"|"3"|95|"3"|96|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.337|"Slight"|"1"|1|"344196"
"39C"|"Lisk sandy loam, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"0"|3.36|6.43|11.92|15.83|"Well drained"|"Well drained"|"A"|"4"|94|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.019|"Moderate"|"0"|0.483|"344199"
"39E"|"Lisk sandy loam, 8 to 25 percent slopes"||17|16.8||||"None"|"None"|"0"|3.35|6.43|11.87|15.69|"Well drained"|"Well drained"|"A"||96|"6"|94|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.098|"Severe"|"0"|0.989|"344200"
"401C"|"Gerdrum-Yamacall loams, 2 to 8 percent slopes"||3|4.1||||"None"|"None"|"0"|3.72|6.89|12.99|19.09|"Well drained"|"Well drained"|"D"|"6"|48|"6"|48|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.25|"Moderate"|"0"|0.577|"344201"
"41C"|"Reeder loam, 2 to 8 percent slopes"||5|5.2|58|||"None"|"None"|"0"|4.55|8.45|10.04|10.23|"Well drained"|"Well drained"|"C"|"3"|90|"3"|94|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.134|"Moderate"|"0"|0.9|"344203"
"421C"|"Joplin-Hillon loams, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"1"|4.18|8.35|16.28|23.33|"Well drained"|"Well drained"|"C"|"3"|55|"3"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.225|"Moderate"|"1"|0.497|"344204"
"43B"|"Marmarth loam, 0 to 4 percent slopes"||2|2.4|56|||"None"|"None"|"0"|4.53|8.42|9.95|10.34|"Well drained"|"Well drained"|"C"||91|"3"|91|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.129|"Slight"|"0"|0.934|"344205"
"441C"|"Kevin-Hillon clay loams, 2 to 8 percent slopes"||4|4.8||||"None"|"None"|"1"|4.35|8.57|16.72|24.35|"Well drained"|"Well drained"|"C"|"3"|59|"3"|62|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.254|"Moderate"|"1"|0.97|"344206"
"442C"|"Kevin-Elloam complex, 2 to 8 percent slopes"||5|4.3||||"None"|"None"|"1"|4.33|8.48|16.52|24.04|"Well drained"|"Well drained"|"C"|"3"|58|"3"|58|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.261|"Moderate"|"1"|1|"344208"
"445E"|"Kevin-Hillon-Nishon complex, 0 to 25 percent slopes"||10|12.5||0|0|"None"|"None"|"20"|4.18|8.38|16.62|24.79|"Well drained"|"Poorly drained"|"C"||55|"4"|65|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.508|"Severe"|"20"|1|"344210"
"471B"|"Marias-Kobase complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"3"|3.91|7.63|15.05|22.47|"Well drained"|"Well drained"|"D"|"4"|97|"4"|97|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.441|"Slight"|"3"|1|"344211"
"47B"|"Marias silty clay, 0 to 4 percent slopes"||2|2||||"None"|"None"|"2"|3.86|7.37|14.39|21.4|"Well drained"|"Well drained"|"D"|"4"|98|"4"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.51|"Slight"|"2"|1|"344212"
"491B"|"Enbar-Nesda loams, 0 to 4 percent slopes"||2|2||114|114|"Occasional"|"Occasional"|"0"|3.64|6.58|11.69|16.98|"Somewhat poorly drained"|"Somewhat poorly drained"|"B"||100|"3"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.029|"Slight"|"0"|0.778|"344214"
"493B"|"Enbar-Bigsandy-Korchea loams, 0 to 4 percent slopes"||2|1.7||46|46|"Occasional"|"Occasional"|"0"|4.27|8.38|15.82|23.04|"Somewhat poorly drained"|"Poorly drained"|"B"||80|"3"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.18|"Slight"|"32"|0.621|"344215"
"503B"|"Telstad-Joplin loams, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|4.28|8.64|17.16|24.46|"Well drained"|"Well drained"|"C"|"3"|88|"3"|88|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.229|"Slight"|"1"|0.545|"344217"
"503C"|"Telstad-Joplin loams, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"2"|4.3|8.68|17.13|24.34|"Well drained"|"Well drained"|"C"|"3"|90|"3"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.241|"Moderate"|"2"|0.548|"344218"
"512F"|"Elve-Rubble land complex, 25 to 60 percent slopes"||43|43||||"None"|"None"|"0"|2.24|4.35|5.89|7.42|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344219"
"51F"|"Elve very cobbly loam, 25 to 60 percent slopes"||43|42.9||||"None"|"None"|"0"|2.25|4.37|5.87|7.37|"Somewhat excessively drained"|"Somewhat excessively drained"|"A"||100|"7"|93|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344220"
"521C"|"Elloam-Absher complex, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|4.05|7.65|14.87|22.23|"Well drained"|"Well drained"|"D"|"6"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.265|"Slight"|"1"|0.995|"344221"
"531C"|"Turner-Beaverton complex, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|3.63|6.45|9.07|11.07|"Well drained"|"Well drained"|"B"|"3"|55|"3"|55|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.073|"Moderate"|"0"|0.981|"344224"
"54B"|"Lawther clay, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.15|8.11|15.14|22.17|"Well drained"|"Well drained"|"C"||100|"4"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.51|"Slight"|"2"|1|"344225"
"54C"|"Lawther clay, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"3"|4.15|8.11|15.16|22.2|"Well drained"|"Well drained"|"C"||100|"4"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.525|"Moderate"|"3"|1|"344226"
"561B"|"Scobey-Kevin clay loams, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"2"|4.37|8.55|16.72|24.36|"Well drained"|"Well drained"|"C"|"2"|87|"3"|89|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.271|"Slight"|"2"|1|"344227"
"561C"|"Scobey-Kevin clay loams, 2 to 8 percent slopes"||5|5.2||||"None"|"None"|"2"|4.38|8.67|17.02|24.61|"Well drained"|"Well drained"|"C"|"3"|89|"3"|89|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.269|"Moderate"|"2"|1|"344228"
"58B"|"Lonna silty clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|4.49|8.59|16.58|24.02|"Well drained"|"Well drained"|"B"|"4"|96|"4"|97|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.336|"Slight"|"1"|0.091|"344229"
"58C"|"Lonna silty clay loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.5|8.6|16.6|24.04|"Well drained"|"Well drained"|"B"|"4"|99|"4"|99|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Somewhat limited"|"Not rated"|"Not rated"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.329|"Moderate"|"0"|0.081|"344230"
"5A"|"McKenzie clay, 0 to 1 percent slopes"||0|0.1||0|0|"None"|"None"|"93"|4.44|8.67|16.39|23.9|"Poorly drained"|"Poorly drained"|"C/D"|"5"|88|"5"|88|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.947|"Slight"|"93"|0.975|"344231"
"601A"|"Havre-Glendive, complex, 0 to 2 percent slopes"||1|1.1||||"Occasional"|"Occasional"|"0"|3.97|8.08|15.81|22.88|"Well drained"|"Well drained"|"B"|"3"|50|"3"|54|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.042|"Slight"|"0"|0.606|"344232"
"603B"|"Thibadeau loam, 0 to 4 percent slopes"||2|1.9||84|84|"Occasional"|"Occasional"|"0"|4.44|8.61|16.52|24.42|"Moderately well drained"|"Moderately well drained"|"D"|"4"|94|"6"|94|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.069|"Slight"|"3"|1|"344233"
"605C"|"Yamacall-Havre loams, 0 to 8 percent slopes"||4|2.9||||"None"|"Occasional"|"0"|4.17|8.12|15.87|23.58|"Well drained"|"Well drained"|"B"|"3"|50|"3"|50|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.142|"Moderate"|"2"|0.322|"344234"
"60A"|"Havre clay loam, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|4.01|7.99|15.95|23.86|"Well drained"|"Well drained"|"C"|"2"|93|"3"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.088|"Slight"|"3"|0.328|"344235"
"631B"|"Nunemaker silty clay loam, calcareous, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|3.8|7.31|14.33|21.34|"Well drained"|"Well drained"|"C"|"4"|98|"4"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.339|"Slight"|"1"|1|"344236"
"631C"|"Nunemaker silty clay loam, calcareous, 4 to 8 percent slopes"||6|6||||"None"|"None"|"1"|3.8|7.3|14.27|21.22|"Well drained"|"Well drained"|"C"|"4"|97|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.344|"Moderate"|"1"|1|"344237"
"63B"|"Nunemaker silty clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|3.95|7.45|14.47|21.48|"Well drained"|"Well drained"|"C"|"4"|98|"4"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.337|"Slight"|"1"|1|"344238"
"63C"|"Nunemaker silty clay loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"1"|3.95|7.45|14.47|21.48|"Well drained"|"Well drained"|"C"|"4"|99|"4"|99|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.344|"Moderate"|"1"|1|"344239"
"64D"|"Barkof clay, 4 to 15 percent slopes"||10|10.2|66|||"None"|"None"|"0"|4|7.6|9.96|10.04|"Well drained"|"Well drained"|"D"|"4"|87|"4"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"344240"
"661C"|"Twilight-Blacksheep fine sandy loams, 2 to 8 percent slopes"||5|5.2|46|||"None"|"None"|"0"|3.72|7.07|10.74|11.04|"Well drained"|"Well drained"|"B"|"4"|64|"4"|64|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.053|"Moderate"|"0"|0.496|"344241"
"671C"|"Bearpaw-Vida-Nishon clay loams, 0 to 8 percent slopes"||5|4.5||0|0|"None"|"None"|"15"|4.12|8.24|15.79|23.3|"Well drained"|"Poorly drained"|"C"|"3"|80|"3"|81|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.215|"Moderate"|"15"|1|"344242"
"673B"|"Bearpaw-Noonan complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|4.46|8.68|16.81|24.46|"Well drained"|"Well drained"|"C"|"3"|59|"3"|59|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.155|"Slight"|"1"|1|"344243"
"67B"|"Bearpaw clay loam, 0 to 4 percent slopes"||2|2||||"None"|"None"|"1"|4.61|9.07|17.55|25.25|"Well drained"|"Well drained"|"C"|"3"|94|"3"|94|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.159|"Slight"|"1"|1|"344244"
"691D"|"Vida-Williams, Zahill-high precipitation loams, 4 to 15 percent slopes"||10|9.8||||"None"|"None"|"2"|4.36|8.69|16.76|23.82|"Well drained"|"Well drained"|"C"||94|"4"|89|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.141|"Severe"|"2"|0.553|"344246"
"692D"|"Vida-Bearpaw-Zahill clay loams, 4 to 15 percent slopes"||10|9.7||||"None"|"None"|"2"|4.48|8.85|17.08|24.56|"Well drained"|"Well drained"|"C"||92|"4"|87|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.168|"Moderate"|"2"|1|"344247"
"693D"|"Vida-Bearpaw-Nishon clay loams, 0 to 15 percent slopes"||10|6.3||0|0|"None"|"None"|"25"|4.09|8.16|15.78|23.36|"Well drained"|"Poorly drained"|"C"||70|"4"|64|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.317|"Severe"|"25"|1|"344248"
"695C"|"Vida-Zahill clay loams, 2 to 8 percent slopes"||5|5||||"None"|"None"|"1"|4.01|8.01|16.02|24.02|"Well drained"|"Well drained"|"C"|"3"|66|"3"|68|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.086|"Moderate"|"1"|0.999|"344249"
"695E"|"Zahill-Vida clay loams, 8 to 25 percent slopes"||17|15.7||||"None"|"None"|"0"|4.39|8.66|16.64|24.04|"Well drained"|"Well drained"|"C"||93|"6"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.133|"Severe"|"0"|1|"344250"
"69C"|"Bearpaw-Vida clay loams, 2 to 8 percent slopes"||5|5||||"None"|"None"|"1"|4.56|8.99|17.42|25.05|"Well drained"|"Well drained"|"C"|"3"|89|"3"|89|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.155|"Moderate"|"1"|1|"344251"
"702F"|"Winspect-Winspect, cool-Rock outcrop complex, 25 to 60 percent slopes"||43|42.6||||"None"|"None"|"0"|3.18|5.65|10.5|15.29|"Well drained"|"Well drained"|"C"||100|"7"|74|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"344252"
"712E"|"Roy-Barkof complex, 8 to 25 percent slopes"||17|17|66|||"None"|"None"|"0"|3.53|6.45|9.58|11.02|"Well drained"|"Well drained"|"C"||100|"6"|91|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.282|"Severe"|"0"|0.98|"344253"
"712F"|"Roy-Barkof-Rock outcrop complex, 25 to 60 percent slopes"||43|38.6|66|||"None"|"None"|"0"|3.51|6.38|9.57|11.08|"Well drained"|"Well drained"|"C"||100|"7"|82|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.968|"Severe"|"0"|0.991|"344254"
"71D"|"Roy complex, 8 to 15 percent slopes"||12|12.2||||"None"|"None"|"0"|2.95|5.22|9.04|11.66|"Well drained"|"Well drained"|"C"||100|"4"|64|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.098|"Moderate"|"0"|0.65|"344255"
"71F"|"Roy gravelly clay loam, 15 to 45 percent slopes"||30|28.9||||"None"|"None"|"0"|3.16|5.45|9.27|11.85|"Well drained"|"Well drained"|"C"||100|"6"|94|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.927|"Severe"|"0"|0.978|"344256"
"723F"|"Zahill-Cabba complex, 15 to 45 percent slopes"||30|29.7|30|||"None"|"None"|"0"|4.08|6.81|11.65|16.48|"Well drained"|"Well drained"|"C"||100|"6"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.973|"Severe"|"0"|1|"344257"
"72F"|"Zahill-Zahl clay loams, 15 to 60 percent slopes"||38|32.1||||"None"|"None"|"0"|4.37|8.56|16.06|23.19|"Well drained"|"Well drained"|"C"||100|"7"|79|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.817|"Severe"|"0"|1|"344258"
"75C"|"Benz clay loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|2.98|5.72|11.2|16.68|"Well drained"|"Well drained"|"C"||100|"6"|96|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.25|"Moderate"|"0"|1|"344261"
"77D"|"Tinsley gravelly sandy loam, 4 to 15 percent slopes"||10|10||||"None"|"None"|"0"|1.34|1.86|2.88|3.89|"Excessively drained"|"Excessively drained"|"A"||100|"7"|97|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Not limited"|0.004|"Moderate"|"0"|1|"344262"
"77F"|"Tinsley gravelly sandy loam, 15 to 70 percent slopes"||43|40||||"None"|"None"|"0"|1.37|1.91|2.93|3.96|"Excessively drained"|"Excessively drained"|"A"||100|"7"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|0.902|"Severe"|"0"|1|"344263"
"781C"|"Creed-Weingart complex, 2 to 8 percent slopes"||5|5.2|64|||"None"|"None"|"0"|3.48|5.91|9.25|12.02|"Well drained"|"Well drained"|"C"|"4"|55|"4"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.287|"Moderate"|"0"|0.989|"344264"
"791B"|"Yamacall loam, calcareous, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|4.25|8.37|16.42|24.46|"Well drained"|"Well drained"|"B"|"4"|90|"4"|97|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.203|"Slight"|"0"|0.009|"344265"
"79B"|"Yamacall loam, 0 to 4 percent slopes"||2|2.3||||"None"|"None"|"0"|4.21|8.26|16.17|24.07|"Well drained"|"Well drained"|"B"|"2"|90|"3"|93|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.2|"Slight"|"0"|0.02|"344266"
"801B"|"Williams-Vida loams, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"1"|4.46|8.89|17.3|24.59|"Well drained"|"Well drained"|"C"|"3"|93|"3"|93|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.135|"Slight"|"1"|0.519|"344267"
"801C"|"Williams-Vida loams, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"1"|4.45|8.88|17.22|24.41|"Well drained"|"Well drained"|"C"|"3"|92|"3"|91|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.134|"Moderate"|"1"|0.518|"344268"
"812A"|"Glendive-Havre, complex, 0 to 2 percent slopes"||1|1||||"Rare"|"Rare"|"0"|3.81|7.88|15.53|22.36|"Well drained"|"Well drained"|"A"|"4"|55|"4"|58|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.057|"Slight"|"0"|0.296|"344269"
"82B"|"Wyola silty clay loam, 0 to 4 percent slopes"||2|2.2||||"None"|"None"|"3"|4.16|8.07|15.57|23.07|"Well drained"|"Well drained"|"C"|"3"|92|"3"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.159|"Slight"|"3"|0.986|"344270"
"86C"|"Work clay loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.09|8.08|14.78|21.18|"Well drained"|"Well drained"|"C"|"3"|93|"3"|98|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.098|"Moderate"|"0"|0.303|"344272"
"87C"|"Tamaneen complex, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|3.76|7.48|12.31|14.89|"Well drained"|"Well drained"|"C"||66|"3"|96|"Somewhat limited"|"Not limited"|"Not limited"|"Not rated"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.113|"Moderate"|"0"|0.368|"344273"
"882F"|"Perma-Whitlash gravelly loams, 25 to 70 percent slopes"||48|47.3|41|||"None"|"None"|"0"|3.22|5.23|8|9.31|"Somewhat excessively drained"|"Well drained"|"B"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.98|"Severe"|"0"|1|"344274"
"88C"|"Perma gravelly loam, 2 to 8 percent slopes"||5|5.4||||"None"|"None"|"0"|3.27|5.66|9.83|11.9|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"|"4"|92|"4"|94|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.065|"Moderate"|"0"|0.362|"344275"
"88E"|"Perma gravelly loam, 8 to 25 percent slopes"||17|17.3||||"None"|"None"|"0"|3.27|5.66|9.83|11.9|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"||98|"6"|92|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.099|"Severe"|"0"|0.98|"344276"
"892F"|"Whitlash-Rock outcrop complex, 25 to 70 percent slopes"||48|46.9|41|||"None"|"None"|"0"|3.13|4.45|4.58|4.64|"Well drained"|"Well drained"|"D"||100|"7"|66|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.972|"Severe"|"0"|1|"344277"
"90A"|"Harlake silty clay, 0 to 1 percent slopes"||1|1||||"Rare"|"Rare"|"0"|3.97|7.92|15.7|22.15|"Well drained"|"Well drained"|"C"|"4"|92|"4"|92|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.487|"Slight"|"3"|1|"344278"
"92D"|"Sunburst-Kevin clay loams, 4 to 15 percent slopes"||10|9.8||||"None"|"None"|"1"|4.33|8.59|16.64|24.1|"Well drained"|"Well drained"|"C"||88|"4"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.264|"Moderate"|"1"|1|"344279"
"92F"|"Sunburst clay loam, 15 to 60 percent slopes"||38|33.2||||"None"|"None"|"0"|4.22|8.22|15.59|22.67|"Well drained"|"Well drained"|"C"||98|"7"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.868|"Severe"|"0"|0.96|"344280"
"94C"|"Busby fine sandy loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.49|6.96|12.65|17.16|"Well drained"|"Well drained"|"A"|"4"|96|"4"|98|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.005|"Moderate"|"0"|0.985|"344284"
"94E"|"Busby fine sandy loam, 8 to 25 percent slopes"||17|17.3||||"None"|"None"|"0"|3.49|6.97|12.61|17.03|"Well drained"|"Well drained"|"A"||100|"6"|96|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.099|"Severe"|"0"|0.995|"344285"
"952F"|"Dast-Rock outcrop complex, 15 to 45 percent slopes"||30|28.1|66|||"None"|"None"|"0"|3.37|6.57|8.72|8.95|"Well drained"|"Well drained"|"B"||100|"6"|68|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.903|"Severe"|"0"|0.994|"344286"
"98C"|"Kremlin loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.46|8.9|17.61|25.58|"Well drained"|"Well drained"|"B"|"3"|92|"3"|92|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.203|"Moderate"|"0"|0.021|"344289"
"DAM"|"Dam"||10|10||||"None"|"None"|"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344291"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"344292"
