"102A"|"Fairberg silt loam, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.9|9.4|18.4|22.24|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.058|"Slight"|"5"|1|"147977"
"1154B"|"Binvar cobbly loam, 0 to 4 percent slopes"||2|2||46|46|"Rare"|"Rare"|"0"|3.85|7.85|11.88|13.38|"Poorly drained"|"Poorly drained"|"B/D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.436|"Slight"|"100"|1|"147978"
"11A"|"Newtman mucky peat, 0 to 3 percent slopes"||2|1.9||15|15|"Rare"|"Rare"|"0"|10.26|18.33|25.5|31.31|"Very poorly drained"|"Very poorly drained"|"C/D"|"5"|85|"5"|85|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.891|"Slight"|"93"|0.965|"147979"
"124E"|"Crago-Musselshell complex, cool, 8 to 35 percent slopes"||22|22||||"None"|"None"|"0"|3.07|5.99|10.94|14.97|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.82|"Moderate"|"0"|1|"147980"
"127A"|"Musselshell-Crago complex, 0 to 2 percent slopes"||2|2||||"None"|"None"|"0"|3.28|6.41|11.51|15.52|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.249|"Slight"|"0"|0.553|"147981"
"127C"|"Musselshell cobbly loam, cool, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.29|6.49|11.65|15.59|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.117|"Moderate"|"0"|0.464|"147982"
"129B"|"Amesha-Musselshell complex, cool, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.94|8.06|15.92|22.7|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.109|"Slight"|"0"|0|"147983"
"130B"|"Danvers gravelly clay loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.13|8.24|16.04|21.18|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.043|"Slight"|"0"|1|"147984"
"145C"|"Reedwest loam, 2 to 8 percent slopes"||5|5|91|||"None"|"None"|"0"|4.71|8.68|15.15|15.6|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.044|"Moderate"|"0"|0.9|"147985"
"152B"|"Beaverton-Turner complex, 1 to 3 percent slopes, foothills"||2|2||||"None"|"None"|"0"|3.24|6.13|8.41|10.19|"Well drained"|"Well drained"|"B"|"6"|55|"6"|55|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.12|"Slight"|"0"|1|"147986"
"154B"|"Martinsdale gravelly loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.01|8.16|16.06|23.67|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.053|"Slight"|"0"|0.5|"147987"
"158C"|"Bacbuster-Reedwest-Tolbert complex, 2 to 8 percent slopes"||5|5|41|||"None"|"None"|"0"|4.38|7.82|13.32|13.32|"Well drained"|"Well drained"|"D"|"4"|75|"4"|75|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Moderate"|"0"|1|"147988"
"158D"|"Bacbuster-Reedwest-Castner complex, 4 to 15 percent slopes"||10|10.4|41|||"None"|"None"|"0"|4.43|7.89|13.61|13.61|"Well drained"|"Well drained"|"D"||100|"4"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.076|"Moderate"|"0"|1|"147989"
"161C"|"Vershal-Azaar complex, 2 to 8 percent slopes"||5|4.2|20|||"None"|"None"|"0"|3.22|5.22|7.5|7.5|"Well drained"|"Well drained"|"D"|"7"|60|"7"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.094|"Moderate"|"0"|1|"147990"
"174C"|"Frenchcreek very gravelly loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|2.46|4.18|6.63|9.73|"Well drained"|"Well drained"|"A"|"4"|100|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.078|"Moderate"|"0"|0.902|"147992"
"186C"|"Delpoint-Cabbart complex, cool, 2 to 8 percent slopes"||5|5|46|||"None"|"None"|"0"|4.07|7.84|10.36|10.36|"Well drained"|"Well drained"|"C"|"4"|80|"4"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.134|"Moderate"|"0"|1|"147994"
"186E"|"Delpoint-Cabbart complex, cool, 8 to 35 percent slopes"||22|22|46|||"None"|"None"|"0"|4.06|7.71|9.76|9.76|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"147995"
"197C"|"Monaberg gravelly silt loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.72|7.67|15.88|23.27|"Well drained"|"Well drained"|"B"|"6"|100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0|"Moderate"|"0"|0.032|"147996"
"201B"|"Bigsandy loam, 0 to 4 percent slopes"||2|2||46|46|"Occasional"|"Occasional"|"90"|3.88|7.33|14.76|20.94|"Poorly drained"|"Poorly drained"|"B/D"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.397|"Slight"|"90"|1|"147998"
"202A"|"Fairberg-Villmeagher complex, 0 to 2 percent slopes"||1|1||46|46|"Rare"|"Rare"|"0"|4.89|9.39|18.39|23.71|"Somewhat poorly drained"|"Poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.177|"Slight"|"35"|1|"147999"
"21C"|"Rhame-Blacksheep complex, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|3.83|6.07|8.95|8.95|"Well drained"|"Well drained"|"B"|"4"|55|"4"|55|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.035|"Moderate"|"0"|1|"148000"
"230B"|"Danvers-Kiev complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.38|8.33|16.07|21.86|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Very limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.039|"Moderate"|"0"|0.75|"148001"
"245C"|"Reedwest gravelly loam, 2 to 8 percent slopes"||5|5.1|91|||"None"|"None"|"0"|4.01|8.03|14.73|15.5|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.026|"Moderate"|"0"|0.95|"148003"
"246C"|"Farnuf loam, 2 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|4.7|9.06|17.12|23.42|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.029|"Moderate"|"0"|0.1|"148004"
"24B"|"Crago-Musselshell complex, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.13|6.03|10.97|14.35|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.266|"Slight"|"0"|0.7|"148005"
"250B"|"Lepner gravelly loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.67|7.31|14.01|20.31|"Well drained"|"Well drained"|"C"|"6"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.041|"Slight"|"0"|0.9|"148006"
"254B"|"Meagher gravelly loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.87|7.68|13.61|18.42|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.027|"Slight"|"0"|0.05|"148007"
"254C"|"Meagher gravelly loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.87|7.68|13.61|18.42|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.027|"Moderate"|"0"|0.296|"148008"
"258C"|"Bacbuster-Auchard-Reedwest complex, 2 to 8 percent slopes"||5|5|84|||"None"|"None"|"0"|4.64|8.56|15.12|15.12|"Well drained"|"Well drained"|"D"|"4"|70|"4"|70|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.039|"Moderate"|"0"|1|"148009"
"25E"|"Shambo-Cabba complex, 8 to 35 percent slopes, foothills"||17|19|30|||"None"|"None"|"0"|4.4|7.35|12.63|16.94|"Well drained"|"Well drained"|"B"||100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.376|"Severe"|"0"|1|"148010"
"266C"|"Kiev gravelly loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.93|7.52|14.17|19.57|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.026|"Moderate"|"0"|0.1|"148012"
"274C"|"Perma gravelly loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.77|6.01|9.44|11.74|"Somewhat excessively drained"|"Somewhat excessively drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.015|"Moderate"|"0"|0.9|"148013"
"28B"|"Creed-Gerdrum complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4|7.69|14.42|19.95|"Well drained"|"Well drained"|"C"|"6"|60|"6"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.195|"Slight"|"0"|1|"148014"
"29B"|"Amesha silt loam, cool, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.27|8.14|15.79|22.8|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.121|"Moderate"|"0"|0.1|"148015"
"2A"|"Fairway silt loam, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.94|9.4|17.91|21.28|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.161|"Slight"|"5"|1|"148016"
"302A"|"Fairbirch silt loam, 0 to 2 percent slopes"||1|1||46|46|"Rare"|"Rare"|"0"|4.9|9.39|16.48|20.18|"Poorly drained"|"Poorly drained"|"B/D"|"4"|100|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.393|"Slight"|"0"|1|"148017"
"30B"|"Danvers clay loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.55|8.67|16.67|22.58|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.04|"Moderate"|"0"|0.95|"148018"
"327B"|"Musselshell loam, cool, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|3.59|6.79|11.92|15.78|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.117|"Slight"|"0"|0.1|"148020"
"343A"|"Turner gravelly loam, 0 to 2 percent slopes"||1|1.1||||"None"|"None"|"0"|3.82|7.83|10.76|12.76|"Well drained"|"Well drained"|"B"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.028|"Slight"|"0"|1|"148021"
"346C"|"Farnuf-Work cobbly loams, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.15|8.29|16.09|23.09|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.03|"Moderate"|"0"|0.265|"148022"
"354B"|"Meagher loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.32|8.13|14.06|18.87|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.027|"Moderate"|"0"|0.296|"148023"
"958C"|"Bacbuster-Reedwest complex, 2 to 8 percent slopes"||5|5|91|||"None"|"None"|"0"|4.77|8.77|16.04|16.04|"Well drained"|"Well drained"|"D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Moderate"|"0"|1|"148024"
"3A"|"Soapcreek-Fairway complex, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|5.14|9.86|18.52|24.47|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.174|"Slight"|"0"|1|"148025"
"402A"|"Fairsmith silt loam, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.97|9.47|18.08|22.78|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.078|"Slight"|"10"|1|"148026"
"409A"|"Meadowcreek loam, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.72|9.4|15.49|17.1|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.061|"Slight"|"5"|1|"148027"
"427B"|"Musselshell-Crago complex, cool, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.25|6.12|10.55|13.88|"Well drained"|"Well drained"|"B"|"4"|100|"4"|70|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.12|"Moderate"|"0"|0.3|"148028"
"430B"|"Danvers cobbly clay loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.28|8.5|16.5|22.41|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.033|"Slight"|"0"|0.95|"148029"
"430C"|"Danvers cobbly clay loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.28|8.62|17.07|23.1|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.032|"Moderate"|"0"|0.95|"148030"
"443B"|"Turner-Beaverton complex, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|3.84|7|10.54|12.54|"Well drained"|"Well drained"|"B"|"4"|100|"4"|70|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.026|"Slight"|"0"|1|"148031"
"445B"|"Fairfield gravelly loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.69|7.26|14.36|21.43|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.029|"Slight"|"0"|0.5|"148032"
"44C"|"Tolbert channery loam, 2 to 8 percent slopes"||5|4.9|41|||"None"|"None"|"0"|3.36|5.37|5.95|5.95|"Well drained"|"Well drained"|"D"|"7"|90|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.028|"Moderate"|"0"|1|"148033"
"44E"|"Tolbert channery loam, 8 to 35 percent slopes"||20|19.3|41|||"None"|"None"|"0"|3.33|5.3|5.78|5.78|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.461|"Severe"|"0"|1|"148034"
"454C"|"Martinsdale stony loam, 1 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.95|7.92|15.42|22.71|"Well drained"|"Well drained"|"C"|"6"|90|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.017|"Moderate"|"0"|0.511|"148035"
"458C"|"Reedwest-Bacbuster complex, 2 to 8 percent slopes"||5|5|91|||"None"|"None"|"0"|4.69|8.37|14.72|15.07|"Well drained"|"Well drained"|"C"|"4"|90|"4"|90|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.032|"Moderate"|"0"|0.951|"148036"
"463A"|"Utica-Binna complex, cool, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.46|5.76|8.06|9.71|"Excessively drained"|"Well drained"|"B"|"6"|70|"6"|70|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.048|"Slight"|"0"|0.715|"148038"
"46C"|"Farnuf-Work complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.69|9.01|17.25|24.7|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.031|"Moderate"|"0"|0.45|"148039"
"501B"|"Mannixlee-Clunton, frequently flooded-Meadowcreek complex, 0 to 4 percent slopes"||2|2.1||15|15|"Rare"|"Frequent"|"0"|6.33|11.34|18.87|22.85|"Poorly drained"|"Very poorly drained"|"C/D"|"4"|65|"4"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.529|"Slight"|"65"|0.988|"148040"
"502A"|"Fairsmith-Nesda complex, 0 to 2 percent slopes"||1|1||84|84|"Rare"|"Rare"|"0"|4.74|8.75|15.92|19.99|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.052|"Slight"|"5"|1|"148041"
"52B"|"Beaverton-Turner complex, 1 to 3 percent slopes"||2|2||||"None"|"None"|"0"|3.49|5.86|8.52|10.52|"Well drained"|"Well drained"|"B"|"4"|100|"6"|70|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.022|"Slight"|"0"|1|"148042"
"543B"|"Tamaneen cobbly clay loam, 0 to 4 percent slopes"||2|2.1||||"None"|"None"|"0"|3.92|7.4|10.66|13.51|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.031|"Slight"|"0"|0.45|"148043"
"545C"|"Varney-Rothiemay complex, cool, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|4.15|7.8|15.07|21.77|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.133|"Moderate"|"0"|0|"148044"
"548D"|"Shawmut gravelly loam, 8 to 15 percent slopes"||12|12||||"None"|"None"|"0"|3.7|6.58|10.43|13.13|"Well drained"|"Well drained"|"B"||100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.028|"Moderate"|"0"|0.67|"148046"
"54B"|"Martinsdale loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.49|8.7|16.55|24.03|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.018|"Moderate"|"0"|0.45|"148047"
"554B"|"Martinsdale-Meagher complex, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.93|7.99|15.18|21.75|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.02|"Slight"|"0"|0.311|"148048"
"558E"|"Bacbuster-Vershal complex, 8 to 35 percent slopes"||10|11.5|20|||"None"|"None"|"0"|4|7.33|10.92|11.32|"Well drained"|"Well drained"|"D"||95|"6"|65|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.059|"Severe"|"0"|0.974|"148049"
"561D"|"Blaincreek-Castner complex, 2 to 15 percent slopes"||9|9|41|||"None"|"None"|"0"|3.08|5.2|5.97|5.97|"Well drained"|"Well drained"|"C"||100|"6"|70|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.027|"Moderate"|"0"|1|"148050"
"563A"|"Binna-Utica complex, cool, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|4.06|6.98|10.47|12.34|"Well drained"|"Well drained"|"B"|"4"|75|"4"|75|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.093|"Slight"|"0"|0.288|"148051"
"566C"|"Kiev-Martinsdale complex, 4 to 8 percent slopes, foothills"||6|6||||"None"|"None"|"0"|4.12|7.9|15.27|21.94|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.022|"Moderate"|"0"|0.2|"148052"
"58C"|"Bacbuster clay loam, 2 to 8 percent slopes"||5|5.1|76|||"None"|"None"|"0"|4.69|9.19|14.05|14.45|"Well drained"|"Well drained"|"D"|"4"|95|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Moderate"|"0"|1|"148053"
"59D"|"Gurney-Tolbert complex, 2 to 15 percent slopes"||9|9|41|||"None"|"None"|"0"|3.99|7.4|9.68|9.68|"Well drained"|"Well drained"|"C"||100|"4"|60|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.033|"Severe"|"0"|1|"148054"
"604A"|"Villmeagher-Villsprings complex, 0 to 2 percent slopes"||1|1||46|46|"Rare"|"Rare"|"0"|5.96|10.45|18.14|23.51|"Poorly drained"|"Poorly drained"|"B/D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.436|"Slight"|"100"|1|"148055"
"60B"|"Work clay loam, 2 to 4 percent slopes, foothills"||3|3||||"None"|"None"|"0"|4.41|8.42|15.72|22.14|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Slight"|"0"|1|"148056"
"60C"|"Work clay loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|4.39|8.37|15.43|21.73|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.033|"Moderate"|"0"|0.9|"148057"
"61E"|"Holter-Castner complex, 8 to 35 percent slopes"||22|22|41|||"None"|"None"|"0"|3.31|5.39|8.64|11.06|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"148058"
"63C"|"Windham gravelly loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.22|5.06|8.21|11.36|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.028|"Moderate"|"0"|0.519|"148059"
"643A"|"Tamaneen loam, 0 to 3 percent slopes"||2|2||||"None"|"None"|"0"|4.34|7.86|11.09|13.34|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.037|"Slight"|"0"|0.55|"148060"
"648A"|"Shawmut very gravelly loam, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|2.87|5.07|8.69|12.04|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.029|"Slight"|"0"|0.413|"148061"
"654B"|"Coyoteflats-Crago complex, cool, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.61|6.98|12.25|16.41|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.136|"Slight"|"0"|0.3|"148062"
"658E"|"Reedwest-Bacbuster-Cabba complex, 8 to 35 percent slopes"||22|22|30|||"None"|"None"|"0"|4.6|7.8|13.17|13.17|"Well drained"|"Well drained"|"D"||100|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"148064"
"6A"|"Nesda-Meadowcreek complex, 0 to 2 percent slopes, rarely flooded"||1|1||84|84|"Rare"|"Rare"|"0"|4.29|7.39|10.27|11.45|"Well drained"|"Somewhat poorly drained"|"B"|"4"|100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.097|"Slight"|"5"|1|"148066"
"704A"|"Villsprings silt loam, 0 to 2 percent slopes"||1|1||46|46|"Rare"|"Rare"|"0"|5.85|10.31|16.72|18.58|"Poorly drained"|"Poorly drained"|"C/D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.396|"Slight"|"90"|1|"148067"
"743B"|"Tamaneen gravelly clay loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.74|7.14|10.07|12.62|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.037|"Slight"|"0"|0.465|"148068"
"743C"|"Tamaneen gravelly clay loam, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|3.74|7.14|10.07|12.62|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.037|"Moderate"|"0"|0.465|"148069"
"754B"|"Coyoteflats cobbly loam, cool, 0 to 2 percent slopes"||1|1||||"None"|"None"|"0"|3.83|7.33|12.69|17.19|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.132|"Slight"|"0"|0.074|"148071"
"754C"|"Coyoteflats cobbly loam, cool, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.83|7.33|12.69|17.19|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.132|"Moderate"|"0"|0.074|"148072"
"758B"|"Gerbana silty clay loam, 2 to 8 percent slopes"||5|4.8|89|||"None"|"None"|"0"|4.73|8.86|15.04|15.62|"Well drained"|"Well drained"|"D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.043|"Moderate"|"0"|1|"148073"
"763E"|"Windham-Holter-Lap complex, 8 to 35 percent slopes"||22|22|48|||"None"|"None"|"0"|3.24|5.37|8.47|11.12|"Well drained"|"Well drained"|"B"||100|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"148074"
"76D"|"Bridger silt loam, 4 to 15 percent slopes"||10|9.7||||"None"|"None"|"0"|4.71|8.59|15.33|20.66|"Well drained"|"Well drained"|"C"||90|"6"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0.01|"Severe"|"2"|0.286|"148076"
"843D"|"Tamaneen loam, 4 to 15 percent slopes, stony"||10|9.3||||"None"|"None"|"0"|4.33|8.06|11.69|14.87|"Well drained"|"Well drained"|"C"||85|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.031|"Severe"|"0"|0.525|"148077"
"845C"|"Roundor-Cabba complex, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|4.47|7.9|10.96|10.96|"Well drained"|"Well drained"|"C"|"4"|75|"4"|75|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.032|"Moderate"|"0"|1|"148078"
"854B"|"Varney-Coyoteflats complex, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.98|8|15.11|21.68|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.208|"Slight"|"0"|0.08|"148079"
"854C"|"Varney-Coyoteflats complex, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.98|8|15.11|21.68|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.208|"Moderate"|"0"|0.08|"148080"
"858C"|"Bacbuster gravelly clay loam, 2 to 8 percent slopes"||5|5|99|||"None"|"None"|"0"|4.63|8.32|15.38|15.38|"Well drained"|"Well drained"|"D"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.042|"Moderate"|"0"|1|"148081"
"86C"|"Delpoint-Marmarth-Cabbart complex, 2 to 8 percent slopes"||5|5|46|||"None"|"None"|"0"|4.15|7.99|11.59|11.59|"Well drained"|"Well drained"|"C"|"4"|55|"4"|55|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.284|"Moderate"|"0"|1|"148082"
"945C"|"Reedwest-Roundor-Cabba complex, 2 to 8 percent slopes, foothills"||5|5|30|||"None"|"None"|"0"|4.61|8.26|12.84|12.84|"Well drained"|"Well drained"|"C"|"4"|85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.029|"Moderate"|"0"|1|"148083"
"945E"|"Reedwest-Roundor-Cabba complex, 8 to 35 percent slopes, foothills"||22|22|30|||"None"|"None"|"0"|4.59|8.05|12.43|12.43|"Well drained"|"Well drained"|"C"||100|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"148084"
"954C"|"Meagher cobbly loam, 2 to 8 percent slopes, stony"||5|5||||"None"|"None"|"0"|3.72|6.89|12.55|18.14|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.028|"Moderate"|"0"|0.062|"148085"
"958E"|"Reedwest-Bacbuster-Martinsdale, stony complex, 8 to 35 percent slopes"||22|22|91|||"None"|"None"|"0"|4.12|8.23|15.52|17.27|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"148086"
"968C"|"Bacbuster-Work complex, 2 to 8 percent slopes"||6|5.6|94|||"None"|"None"|"0"|4.5|8.78|16|17.5|"Well drained"|"Well drained"|"D"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.038|"Moderate"|"0"|0.9|"148087"
"96A"|"Korell silt loam, 0 to 3 percent slopes"||2|2||||"None"|"None"|"0"|5|9.4|17.92|26.18|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.034|"Slight"|"0"|0.694|"148088"
"96C"|"Korell silt loam, 3 to 8 percent slopes"||6|5.8||||"None"|"None"|"0"|5|9.4|17.92|26.18|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.034|"Moderate"|"0"|0.694|"148089"
"65F"|"Jeffcity, extremely stony-Connieo, rubbly-Rock outcrop complex, 20 to 60 percent slopes"||30|30.6|46|||"None"|"None"|"0"|4.12|7.31|9.56|10.18|"Well drained"|"Well drained"|"C"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"581771"
"65E"|"Connieo, rubbly-Burtoner, very stony-Rock outcrop complex, 15 to 30 percent slopes"||20|19|46|||"None"|"None"|"0"|3.86|7.35|9.17|9.44|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.884|"Moderate"|"0"|0.974|"581772"
"65D"|"Connieo, extremely stony-Jeffcity, very stony complex, 2 to 15 percent slopes"||8|7.5|46|||"None"|"None"|"0"|3.9|7.09|7.77|7.77|"Well drained"|"Well drained"|"D"|"6"|95|"6"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.937|"Slight"|"0"|1|"581773"
"64D"|"Windham-Lap complex, 4 to 15 percent slopes"||8|8.9|48|||"None"|"None"|"0"|3.09|5.06|7.69|10.33|"Well drained"|"Well drained"|"D"|"4"|50|"4"|50|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.03|"Moderate"|"0"|0.474|"581784"
"64E"|"Lap-Windham-Rock outcrop complex, 15 to 35 percent slopes"||25|23.6|48|||"None"|"None"|"0"|3.18|5.2|6.59|7.98|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.861|"Severe"|"0"|1|"603505"
"70C"|"Ipano-Reedwest complex, 2 to 8 percent slopes"||6|5.6|62|||"None"|"None"|"0"|4.13|7.44|9.14|9.14|"Well drained"|"Well drained"|"C"|"4"|80|"4"|80|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.041|"Moderate"|"0"|1|"603546"
"71D"|"Vershal-Absarokee-Whitlash complex, 4 to 15 percent slopes"||10|8.6|20|||"None"|"None"|"0"|2.99|4.65|5.77|5.77|"Well drained"|"Well drained"|"D"||65|"7"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.043|"Moderate"|"0"|1|"603547"
"66D"|"Kiev-Work complex, 4 to 15 percent slopes"||10|9.1||||"None"|"None"|"0"|4.65|8.86|16.14|23.39|"Well drained"|"Well drained"|"B"||70|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Severe"|"0"|0.214|"603548"
"106F"|"Wilsall-Reedwest-Cabba complex, 15 to 45 percent slopes"||25|23.5|33|||"None"|"None"|"0"|4.11|6.18|8.15|8.15|"Well drained"|"Well drained"|"D"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.85|"Severe"|"0"|1|"603549"
"9A"|"Mannixlee-Villard complex, 0 to 4 percent slopes"||2|2||46|46|"Occasional"|"Occasional"|"0"|6.01|10.99|18.51|22.07|"Poorly drained"|"Poorly drained"|"B/D"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.436|"Slight"|"95"|1|"603550"
"70F"|"Vershal-Castner-Rock outcrop complex, 25 to 60 percent slopes"||35|34.1|20|||"None"|"None"|"0"|2.49|3.32|3.67|3.68|"Well drained"|"Well drained"|"D"||99|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.989|"Severe"|"0"|1|"603551"
"70D"|"Tolbert-Vershal-Absarook complex, 4 to 15 percent slopes"||8|8.4|20|||"None"|"None"|"0"|2.8|4.28|5.2|5.2|"Well drained"|"Well drained"|"D"|"6"|45|"6"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.038|"Moderate"|"0"|1|"603552"
"71C"|"Ticell-Vershal-Absarook complex, 2 to 8 percent slopes"||4|4.1|20|||"None"|"None"|"0"|3.56|6.04|7.33|7.33|"Well drained"|"Well drained"|"D"|"6"|50|"6"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.042|"Moderate"|"0"|1|"603553"
"103F"|"Maiden-Lap-complex, 15 to 60 percent slopes"||25|33.6|48|||"None"|"None"|"0"|3.14|4.92|5.68|5.68|"Well drained"|"Well drained"|"D"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"603911"
"543C"|"Tamaneen cobbly loam, 3 to 8 percent slopes"||5|5.1||||"None"|"None"|"0"|3.88|7.88|13.03|17.53|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.037|"Moderate"|"0"|0.825|"604733"
"170E"|"Cheadle-Copenhaver-Sebud complex, 15 to 35 percent slopes"||30|23.9|33|||"None"|"None"|"0"|3.2|4.8|5.73|6.66|"Well drained"|"Well drained"|"D"||100|"7"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.62|"Severe"|"0"|1|"618806"
"372E"|"Timberlin, extremely bouldery-Bairsping, very bouldery-Libeg, bouldery complex, 15 to 45 percent slopes"||30|29.5|59|||"None"|"None"|"0"|3.34|5.68|7.61|8.36|"Well drained"|"Well drained"|"C"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"618937"
"272E"|"Bairspring-Lymanson-Rock outcrop complex, 15 to 45 percent slopes"||35|29|64|||"None"|"None"|"0"|3.99|6.96|8.69|8.69|"Well drained"|"Well drained"|"B"||100|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.801|"Severe"|"0"|1|"618942"
"10A"|"Tamaneen-Lepner complex, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.35|8.22|14.58|20.27|"Well drained"|"Well drained"|"C"|"4"|60|"4"|60|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.079|"Slight"|"10"|0.888|"636948"
"12D"|"Bowery-Lolo complex, 2 to 12 percent slopes"||4|5.2||130|130|"None"|"None"|"0"|4.82|9.22|16.25|22.57|"Moderately well drained"|"Moderately well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.132|"Moderate"|"10"|0.1|"637022"
"140D"|"Shanley-Blaincreek, stony complex, 4 to 15 percent slopes"||10|9.9|76|||"None"|"None"|"0"|3.77|6.78|12.47|17.42|"Well drained"|"Well drained"|"C"||80|"4"|65|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.128|"Moderate"|"0"|0.725|"637148"
"140E"|"Sawicki, extremely stony-Blaincreek, very bouldery complex, 15 to 35 percent slopes"||25|24.5|76|||"None"|"None"|"0"|3.1|6.21|10.55|13.78|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.95|"Moderate"|"0"|1|"637158"
"364F"|"Farlin, stony-Levengood-Skaggs complex, 15 to 45 percent slopes"||35|29.3|80|||"None"|"None"|"0"|4.37|6.72|9.91|12.66|"Well drained"|"Well drained"|"B"||100|"7"|53|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.831|"Severe"|"0"|1|"637167"
"150D"|"Tibson, stony-Millerlake, very bouldery-Marcel, bouldery complex, 4 to 15 percent slopes"||8|7.6||84|84|"None"|"None"|"0"|4.14|7.39|13.46|18.71|"Well drained"|"Somewhat poorly drained"|"B"|"6"|100|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0.022|"Slight"|"0"|0.485|"637234"
"158E"|"Bacbuster-Castner complex, 15 to 45 percent slopes"||25|27.4|39|||"None"|"None"|"0"|3.86|7|7.48|7.48|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"637237"
"160B"|"Hereimcreek-Work complex, 0 to 4 percent slopes"||2|2||45|45|"None"|"None"|"0"|4.72|8.98|17.68|25.93|"Poorly drained"|"Poorly drained"|"C/D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.312|"Slight"|"60"|0.8|"637246"
"164D"|"Hardhart-Farlin, stony-Checkerboard complex, 4 to 15 percent slopes"||8|7.6|47|||"None"|"None"|"0"|3.41|5.44|7.9|9.47|"Well drained"|"Well drained"|"C"|"6"|80|"6"|80|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.001|"Moderate"|"0"|0.65|"637252"
"164E"|"Skaggs-Farlin, stony-Levengood complex, 8 to 25 percent slopes"||16|15|80|||"None"|"None"|"0"|4.05|6.45|9.64|11.96|"Well drained"|"Well drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.015|"Severe"|"0"|0.924|"637258"
"165D"|"Woodhall, very bouldery-Nieman, extremely stony complex, 4 to 15 percent slopes"||12|12|41|||"None"|"None"|"0"|3.53|5.52|6.93|6.93|"Well drained"|"Well drained"|"C"||100|"6"|100|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.965|"Moderate"|"0"|1|"637260"
"165E"|"Nieman, very bouldery-Woodhall, very bouldery-Sebud complex, 15 to 45 percent slopes"||30|26.6|41|||"None"|"None"|"0"|3.77|5.9|7.11|8.06|"Well drained"|"Well drained"|"D"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.895|"Severe"|"0"|1|"637271"
"16C"|"Lolo gravelly loam, 2 to 8 percent slopes"||5|4.7||||"None"|"None"|"0"|4.46|8.13|13.94|19.47|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.025|"Moderate"|"0"|0.118|"637497"
"170D"|"Catlinsprings-Dalys complex, 4 to 15 percent slopes"||8|8|20|||"None"|"None"|"0"|2.74|3.26|3.84|3.84|"Well drained"|"Well drained"|"D"|"7"|85|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.002|"Moderate"|"0"|1|"637499"
"170F"|"Catlinsprings-Rock outcrop complex, 15 to 45 percent slopes"||30|28|28|||"None"|"None"|"0"|2.8|3.86|5.28|5.6|"Well drained"|"Well drained"|"D"||95|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.971|"Severe"|"5"|1|"637519"
"240E"|"Redchief, very stony-Sebud-Duckcreek complex, 15 to 35 percent slopes"||25|23.5|92|||"None"|"None"|"0"|4.17|7.36|12.64|16.49|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.85|"Severe"|"0"|1|"637520"
"264E"|"Maciver, stony-Skaggs complex, 15 to 45 percent slopes"||20|24.6|80|||"None"|"None"|"0"|4.54|7|10.27|12.76|"Well drained"|"Well drained"|"C"||100|"6"|67|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.655|"Severe"|"0"|1|"637530"
"265E"|"Sawicki, extremely bouldery-Tolbert, extremely bouldery-Rock outcrop complex, 15 to 35 percent slopes"||20|19.5|38|||"None"|"None"|"0"|3.22|5.4|8.91|12.24|"Well drained"|"Well drained"|"C"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Moderate"|"0"|1|"637534"
"303F"|"Bairspring, very stony-Sigbird complex, 35 to 60 percent slopes"||45|47|36|||"None"|"None"|"0"|3.46|5.42|8.06|8.06|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Slight"|"0"|1|"637784"
"23D"|"Medicinelodge-Adel-Mooseflat complex, 4 to 15 percent slopes"||10|9.4||15|15|"Occasional"|"Occasional"|"0"|5.68|10.79|18.61|24.38|"Poorly drained"|"Very poorly drained"|"C/D"||85|"6"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.45|"Severe"|"75"|0.791|"637785"
"340E"|"Duckcreek-Houlihan-Nieman, stony complex, 15 to 45 percent slopes"||25|22.9|41|||"None"|"None"|"0"|4.55|8.77|15.36|18.65|"Well drained"|"Well drained"|"D"||100|"6"|77|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.808|"Severe"|"2"|1|"637790"
"350E"|"Whitlash, rubbly-Blaincreek, very bouldery-Rock outcrop, complex, 15 to 35 percent slopes"||25|22.4|46||||"None"|"0"|3.52|5.74|6.86|6.86|"Well drained"|"Well drained"|"D"||100|"7"|40|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.73|"Moderate"|"0"|1|"637794"
"365F"|"Libeg, very bouldery-Houlihan, bouldery-Rock outcrop complex, 15 to 60 percent slopes"||35|35||||"None"|"None"|"0"|3.63|7.13|13.56|19.39|"Well drained"|"Well drained"|"C"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"638586"
"40D"|"Bacbuster-Chivington complex, 4 to 15 percent slopes"||12|9.6|94|||"None"|"None"|"0"|4.77|9.18|17.35|20.68|"Well drained"|"Well drained"|"D"||60|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.038|"Severe"|"0"|0.906|"638953"
"40E"|"Bacbuster, very bouldery-Cabba, extremely stony-Castner complex, 15 to 45 percent slopes"||25|28.4|33|||"None"|"None"|"0"|3.41|5.79|9.12|9.12|"Well drained"|"Well drained"|"D"||100|"7"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"639050"
"464E"|"Maiden-Lap-Rock outcrop complex, 15 to 45 percent slopes"||25|23.1|48|||"None"|"None"|"0"|3.54|5.83|7.02|7.33|"Well drained"|"Well drained"|"C"||100|"7"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.813|"Severe"|"0"|1|"639195"
"464F"|"Maiden-Warneke-Rock outcrop complex, 25 to 60 percent slopes"||35|35|48|||"None"|"None"|"0"|2.88|4.55|4.99|5.27|"Well drained"|"Well drained"|"C"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"639197"
"50D"|"Whitlash-Rock outcrop complex, 4 to 15 percent slopes"||12|11.5|46|||"None"|"None"|"0"|3.48|5.01|5.01|5.01|"Well drained"|"Well drained"|"D"||90|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.031|"Moderate"|"0"|1|"639199"
"50E"|"Winspect, very bouldery-Blaincreek, very stony-Tolbert, very stony complex, 8 to 35 percent slopes"||20|23.4|46|||"None"|"None"|"0"|2.85|5.29|8.53|10.89|"Well drained"|"Well drained"|"B"||100|"6"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.876|"Moderate"|"0"|1|"639209"
"564D"|"Windham-Kiev-Roundor complex, 4 to 15 percent slopes"||8|8|90|||"None"|"None"|"0"|3.58|6.86|12.67|17.27|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.026|"Moderate"|"0"|0.2|"639214"
"63D"|"Windham-Kiev complex, 8 to 15 percent slopes"||12|11.5||||"None"|"None"|"0"|3.52|6.45|11.96|17.46|"Well drained"|"Well drained"|"B"||100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.032|"Moderate"|"0"|0.516|"639267"
"65C"|"Pianohill-Clasoil complex, 2 to 8 percent slopes"||4|4.1|76|||"None"|"None"|"0"|4.54|8.87|13.35|14.32|"Well drained"|"Well drained"|"C"|"4"|93|"4"|93|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.028|"Moderate"|"0"|0.85|"639268"
"664D"|"Farlin, stony-Raynesford complex, 8 to 15 percent slopes"||12|11.2||||"None"|"None"|"0"|3.97|6.99|12.83|18.6|"Well drained"|"Well drained"|"B"||100|"6"|95|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Not rated"|"Somewhat limited"|"Not rated"|"Not rated"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.012|"Moderate"|"0"|0.435|"639275"
"664E"|"Farlin, stony-Hardhart-Checkerboard, stony complex, 15 to 35 percent slopes"||25|24.8|47|||"None"|"None"|"0"|3.29|5.46|8.65|11.25|"Well drained"|"Well drained"|"B"||100|"6"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.975|"Moderate"|"0"|1|"639556"
"70E"|"Castner-Vershal complex, 15 to 35 percent slopes"||25|24.6|20|||"None"|"None"|"0"|2.67|3.59|4.06|4.06|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.959|"Severe"|"0"|1|"639637"
"72C"|"Newlancreek-Sixteenmile-Absarook complex, 2 to 8 percent slopes"||5|5|10|||"None"|"None"|"0"|3.12|5.51|6.67|6.67|"Well drained"|"Well drained"|"D"|"6"|50|"6"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.314|"Moderate"|"0"|1|"639639"
"72D"|"Whitlash-Sixteenmile complex, 4 to 15 percent slopes"||10|9.8|10|||"None"|"None"|"0"|2.54|3.87|4.3|4.3|"Well drained"|"Well drained"|"D"||90|"6"|50|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.419|"Moderate"|"0"|1|"639685"
"72E"|"Castner-Sixteenmile-Oraid complex, 15 to 35 percent slopes"||25|24.2|10|||"None"|"None"|"0"|1.29|2.13|2.24|2.24|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.917|"Severe"|"0"|1|"639710"
"72F"|"Castner-Sixteenmile-Rock outcrop complex, 35 to 60 percent slope"||40|39.4|10|||"None"|"None"|"0"|1.47|2.5|2.58|2.58|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"639809"
"764F"|"Farlin-Hardhart, stony-Checkerboard, extremely stony complex, 15 to 60 percent slopes"||25|29.4|48|||"None"|"None"|"0"|3.25|5.04|7.25|8.81|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"639900"
"858E"|"Cabba-Bacbuster-Fairfield complex, 8 to 35 percent slopes"||25|19.5|33|||"None"|"None"|"0"|3.69|6.02|7.37|8.5|"Well drained"|"Well drained"|"D"||100|"7"|60|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.617|"Severe"|"0"|0.925|"639902"
"864E"|"Whitecow, stony-Abac complex, 8 to 35 percent slopes"||15|16.8|30|||"None"|"None"|"0"|3.56|5.55|8.4|11.24|"Well drained"|"Well drained"|"B"||100|"6"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.2|"Moderate"|"0"|1|"639904"
"968E"|"Bacbuster-Reedwest complex, 8 to 25 percent slopes"||15|15|91|||"None"|"None"|"0"|4.23|8.48|15.66|15.66|"Well drained"|"Well drained"|"D"||100|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.048|"Moderate"|"0"|1|"640012"
"GP"|"Gravel Pit"|||||||||"0"|||||||||100|"8"|100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"657187"
"M-W"|"Sewage Lagoon"|||||||||"0"||||||||"8"|100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"657188"
"W"|"Water"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"657189"
"64F"|"Windham-Rock outcrop complex, 30 to 70 percent slopes"||50|48.6||||"None"|"None"|"0"|2.68|5.05|9.46|13.87|"Well drained"|"Well drained"|"B"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"657190"
"843E"|"Tamaneen very cobbly loam, 8 to 35 percent slopes, extremely stony"||22|20.3||||"None"|"None"|"0"|3.63|7.56|12.91|18|"Well drained"|"Well drained"|"C"||90|"6"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.903|"Severe"|"0"|1|"657193"
"470B"|"Absarokee-Sinnigam complex, 0 to 4 percent slopes"||2|2|48|||"None"|"None"|"0"|4.5|7.85|9.61|9.61|"Well drained"|"Well drained"|"C"|"4"|55|"4"|55|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.04|"Slight"|"0"|1|"780799"
"14C"|"Shambo-Tally complex, 2 to 8 percent slopes"||4|4||||"None"|"None"|"0"|4.34|8.57|16.65|24.17|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.021|"Moderate"|"0"|0.1|"780828"
"366C"|"Duckcreek clay loam, 2 to 8 percent slopes"||4|4.2|92|||"None"|"None"|"0"|4.83|9.11|15.57|15.57|"Well drained"|"Well drained"|"D"|"6"|90|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.001|"Moderate"|"0"|1|"780831"
"150E"|"Duckcreek-Melville complex, 15 to 35 percent slopes"||25|22.8|92|||"None"|"None"|"0"|4.75|9.23|15.39|17.54|"Well drained"|"Well drained"|"D"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.775|"Severe"|"0"|1|"780836"
"440D"|"Bacbuster-Work complex, 4 to 15 percent slopes, extremely bouldery"||8|8|94|||"None"|"None"|"0"|3.99|8.24|16.01|18.64|"Well drained"|"Well drained"|"D"|"7"|65|"7"|65|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|1|"Slight"|"0"|1|"780847"
"166D"|"Bacbuster-Meagher-Castner complex, 4 to 15 percent slopes"||8|7.6|39|||"None"|"None"|"0"|3.95|7.79|14.08|14.98|"Well drained"|"Well drained"|"D"|"7"|80|"7"|80|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.047|"Moderate"|"0"|0.859|"780853"
"564E"|"Windham-Lap, stony complex, 15 to 35 percent slopes"||25|23.7|48|||"None"|"None"|"0"|3.16|5.49|9.17|12.86|"Well drained"|"Well drained"|"B"||100|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.868|"Severe"|"0"|1|"780859"
"358C"|"Owenspring-Hardhart-Philipsburg complex, 2 to 8 percent slopes"||6|6|78|||"None"|"None"|"0"|4.19|7.69|12.58|13.68|"Well drained"|"Well drained"|"C"|"6"|80|"6"|80|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.022|"Moderate"|"0"|0.8|"780864"
"458E"|"Farlin, stony-Roxal-Levengood complex, 8 to 35 percent slopes"||15|16.7|25|||"None"|"None"|"0"|4|6.12|9.5|12.88|"Well drained"|"Well drained"|"B"||100|"6"|75|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.272|"Moderate"|"0"|0.873|"780870"
"358D"|"Farlin, stony-Findon, very stony complex, 4 to 15 percent slopes"||10|10.7|90|||"None"|"None"|"0"|3.55|6.15|10.96|13.89|"Well drained"|"Well drained"|"B"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.038|"Moderate"|"0"|0.509|"780874"
"166C"|"Kiev-Fairfield complex, 2 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.87|7.37|14.33|20.63|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.027|"Moderate"|"0"|0.15|"780882"
"472C"|"Fairway-Turrah complex, 2 to 8 percent slopes"||4|4||46|46|"None"|"None"|"0"|5.33|9.78|18.21|24.71|"Somewhat poorly drained"|"Poorly drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.151|"Moderate"|"30"|0.698|"813817"
"872C"|"Absarokee-Reedwest complex, 2 to 8 percent slopes"||5|5|84|||"None"|"None"|"0"|4.65|8.73|15.37|16.34|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.024|"Moderate"|"0"|0.925|"813819"
"167D"|"Newlancreek-Absarook complex, 4 to 15 percent slopes, stony"||10|10|34|||"None"|"None"|"0"|3.75|5.66|6.89|6.89|"Well drained"|"Well drained"|"D"||100|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.018|"Moderate"|"0"|1|"813822"
"128A"|"Lepner-Tetonview complex, 0 to 2 percent slopes, foothills"||1|1||30|30|"None"|"None"|"90"|3.99|7.87|14.96|21.09|"Well drained"|"Poorly drained"|"C"|"6"|75|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.902|"Slight"|"20"|1|"813952"
"240D"|"Meagher, extremely stony-Absarook, very stony-complex, 4 to 15 percent slopes"||10|10|84|||"None"|"None"|"0"|4.07|7.2|12.21|14.71|"Well drained"|"Well drained"|"B"||100|"6"|60|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.756|"Moderate"|"0"|1|"814055"
"270E"|"Mollet-Adel complex, 8 to 35 percent slopes"||25|19.8||||"None"|"None"|"0"|4.94|9.1|16.52|23.62|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.7|"Severe"|"10"|0.89|"814093"
"272F"|"Quaint-Veatch-Rock outcrop, 35 to 70 percent slopes"||55|55|33|||"None"|"None"|"0"|2.14|2.99|3.47|3.47|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"814109"
"264F"|"Farlin-Hardhart, stony-Rock outcrop complex, 25 to 60 percent slopes"||35|39.1|78|||"None"|"None"|"0"|3.96|6.17|8.32|9.68|"Well drained"|"Well drained"|"B"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"815425"
"450D"|"Absarook, stony-Meagher, extremely bouldery-Bacbuster, very bouldery complex, 4 to 15 percent slopes"||10|10|64|||"None"|"None"|"0"|4.11|7.19|10.98|12.48|"Well drained"|"Well drained"|"C"||100|"6"|100|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.409|"Moderate"|"0"|1|"815478"
"450E"|"Tolbert, extremely bouldery-Hoppers-Rock outcrop complex, 8 to 35 percent slopes"||22|22|46|||"None"|"None"|"0"|3.77|6.53|6.88|6.88|"Well drained"|"Well drained"|"D"||100|"7"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.926|"Severe"|"0"|1|"815482"
"565D"|"Jeffcity, very bouldery-Tolbert, very bouldery-Rock outcrop complex, 4 to 15 percent slopes"||9|8.1|38|||"None"|"None"|"0"|3.64|5.86|6.9|7.48|"Well drained"|"Well drained"|"D"||60|"6"|45|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.228|"Moderate"|"0"|0.887|"815856"
"665D"|"Belain-Hedoes-complex, 2 to 8 percent slopes"||5|5.5|98|||"None"|"None"|"0"|3.73|7.06|12.45|14.05|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.013|"Moderate"|"0"|1|"816524"
"458D"|"Roundor-Maiden complex, 4 to 15 percent slopes, very bouldery"||9|9|55|||"None"|"None"|"0"|3.51|6.31|11.02|11.02|"Well drained"|"Well drained"|"C"||100|"6"|60|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.099|"Severe"|"0"|1|"816582"
"565E"|"Baxton, very stony-Riverside, extremely stony-Catgulch, extremely stony complex, 8 to 35 percent slopes"||22|19.9|43|||"None"|"None"|"0"|3.05|5.27|6.72|7.12|"Well drained"|"Well drained"|"B"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.929|"Severe"|"0"|1|"816843"
"540E"|"Darret, very bouldery-Abac, extremely bouldery-Holter, very bouldery complex, 8 to 35 percent slopes"||20|18.2|30|||"None"|"None"|"0"|3.72|6.78|11.66|13.52|"Well drained"|"Well drained"|"C"||100|"6"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.583|"Moderate"|"0"|1|"816892"
"550D"|"Philipsburg-Nieman-Woodhall complex, 4 to 15 percent slopes, very stony"||10|10|41|||"None"|"None"|"0"|3.96|7.13|11|13.6|"Well drained"|"Well drained"|"C"||100|"6"|95|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.124|"Moderate"|"0"|0.667|"817698"
"672D"|"Absarook. stony-Castner, very stony complex, 4 to 15 percent slopes"||9|9|39|||"None"|"None"|"0"|4.03|7.24|11.04|11.54|"Well drained"|"Well drained"|"C"||100|"4"|55|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.043|"Severe"|"0"|0.919|"817721"
"858F"|"Cabba-Amor complex, 15 to 45 percent slopes"||30|28.7|30|||"None"|"None"|"0"|4.29|6.18|7.78|8.11|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"817727"
"672E"|"Quincreek, very bouldery-Castner, very stony complex, 15 to 35 percent slopes"||25|25|31|||"None"|"None"|"0"|3.19|5.04|7.67|7.97|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"817729"
"465F"|"Worock-Targhee complex, 35 to 60 percent slopes, rubbly"||45|45|60|||"None"|"None"|"0"|3.54|5.47|8.11|9.85|"Well drained"|"Well drained"|"B"||100|"7"|88|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"894118"
"465E"|"Libeg, bouldery-Bangtail-Redchief, very stony complex, 4 to 35 percent slopes"||25|21|94|||"None"|"None"|"0"|4.12|7.55|13.1|15.92|"Well drained"|"Well drained"|"C"||95|"6"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|0.725|"Moderate"|"5"|1|"894120"
"167E"|"Newlancreek, very bouldery-Absarook, stony complex, 15 to 35 percent slopes"||25|23.9|34|||"None"|"None"|"0"|3.76|5.54|6.52|6.52|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.895|"Severe"|"0"|1|"894127"
"864D"|"Wickes-Fairfield complex, 4 to 15 percent slopes, stony"||11|10|78|||"None"|"None"|"0"|3.9|6.77|10.76|13.01|"Well drained"|"Well drained"|"C"||70|"4"|90|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.026|"Severe"|"0"|0.789|"1382198"
"38D"|"Woodhall-Woodhurst, very stony-Bavdark complex, 8 to 15 percent slopes"||12|11.7|62|||"None"|"None"|"0"|3.87|6.1|8.44|9.22|"Well drained"|"Well drained"|"C"||100|"6"|85|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Not limited"|0.002|"Moderate"|"0"|0.889|"1383032"
"38E"|"Woodhall-Woodhurst complex, 15 to 35 percent slopes, stony"||25|23.7|72|||"None"|"None"|"0"|4|6.12|8.17|8.17|"Well drained"|"Well drained"|"C"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.868|"Severe"|"0"|1|"1383038"
"138E"|"Bairspring-Poin complex, 10 to 35 percent slopes, stony"||25|22.3|45|||"None"|"None"|"0"|3.62|5.94|7.5|7.5|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.725|"Moderate"|"0"|1|"1383039"
"371C"|"Sixteenmile-Blaincreek-Brickner complex, 2 to 8 percent slopes"||5|5.2|18|||"None"|"None"|"0"|2.65|3.33|3.56|3.56|"Well drained"|"Well drained"|"D"|"7"|75|"7"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.012|"Slight"|"0"|1|"1383367"
"371D"|"Sixteenmile-Krakon-Breeton complex, 4 to 15 percent slopes"||10|9.5|20|||"None"|"None"|"0"|2.13|2.94|4.37|5.38|"Well drained"|"Well drained"|"D"||75|"7"|75|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.002|"Moderate"|"0"|1|"1383368"
"670D"|"Crampton-Castner-Vigilante complex, 4 to 15 percent slopes"||10|9.2|39|||"None"|"None"|"0"|3.51|5.59|7.47|7.65|"Well drained"|"Well drained"|"C"||60|"6"|60|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.024|"Slight"|"0"|1|"1383369"
"670E"|"Crampton-Castner complex, 15 to 35 percent slopes"||25|25|39|||"None"|"None"|"0"|3.5|5.47|7.05|7.17|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Slight"|"0"|1|"1383370"
"670F"|"Castner-Crampton complex, 25 to 60 percent slopes"||40|39.2|39|||"None"|"None"|"0"|3.39|5.03|6.03|6.12|"Well drained"|"Well drained"|"D"||100|"7"|92|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1383371"
"270C"|"Bowery-Meadowcreek-Whitlash complex, 2 to 8 percent slopes"||2|2.4|27|84|84|"Rare"|"Rare"|"0"|4.66|8.3|13.55|18.1|"Moderately well drained"|"Somewhat poorly drained"|"B"|"4"|70|"4"|70|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.123|"Slight"|"10"|0.55|"1383372"
"171F"|"Bairspring-Woodhall-Poin complex, 20 to 60 percent slopes"||30|35.8|41|||"None"|"None"|"0"|3.46|5.61|6.18|6.18|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1383373"
"466C"|"Reedwest, very stony-Martinsdale complex, 2 to 8 percent slopes"||5|5.6|65|||"None"|"None"|"0"|4.37|8.3|12.57|14.45|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.024|"Moderate"|"0"|0.85|"1383374"
"138F"|"Ratiopeak-Tiban complex, 25 to 60 percent slopes"||50|50||||"None"|"None"|"0"|4.77|7.71|12.14|17.04|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"1383375"
"238E"|"Catgulch-Labre complex, 15 to 45 percent slopes"||38|33.2|43|||"None"|"None"|"0"|2.82|4.62|5.76|6.81|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.979|"Severe"|"0"|1|"1383376"
"238D"|"Placerton, stony-Martinsdale-Tolbert, stony complex, 4 to 15 percent slopes"||9|9|36|||"None"|"None"|"0"|3.64|7.16|11.29|13.35|"Well drained"|"Well drained"|"C"||100|"4"|80|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.018|"Moderate"|"0"|0.767|"1383377"
"80D"|"Reedwest-Cabba-Watne complex, 4 to 15 percent slopes"||11|10.4|33|||"None"|"None"|"0"|3.95|7.21|12.05|14.15|"Well drained"|"Well drained"|"C"||100|"4"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.041|"Moderate"|"0"|0.81|"1383382"
"90D"|"Quincreek, very stony-Gnojek, extremely stony-Pachel, stony complex, 8 to 15 percent slopes"||12|12|37|||"None"|"None"|"0"|2.95|4.9|6.29|7.39|"Well drained"|"Well drained"|"C"||100|"7"|80|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.709|"Moderate"|"0"|0.942|"1383383"
"90C"|"Absarook, stony-Gnojek, very stony complex, 2 to 8 percent slopes"||6|6|42|||"None"|"None"|"0"|3.92|7.1|9.88|10.62|"Well drained"|"Well drained"|"C"|"4"|70|"4"|70|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.037|"Moderate"|"0"|0.926|"1383384"
"90F"|"Gnojek, very stony-Veatch, extremely stony-Rock outcrop complex, 25 to 60 percent slopes"||40|35.1|37|||"None"|"None"|"0"|2.83|4.37|5.59|6.58|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.886|"Severe"|"0"|0.935|"1383386"
"338E"|"Crackerville-Veatch complex, 15 to 45 percent slopes"||30|30|58|||"None"|"None"|"0"|3.17|5.32|6.6|6.6|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1383861"
"171E"|"Bairspring-Poin-Libeg complex, 15 to 45 percent slopes"||25|25|37|||"None"|"None"|"0"|3.65|5.76|7.53|7.91|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1385435"
"172E"|"Lymanson, rubbly-Libeg, extremely bouldery complex, 15 to 35 percent slopes"||25|25|97|||"None"|"None"|"0"|4.21|7.39|11.16|12.28|"Well drained"|"Well drained"|"C"||100|"7"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1386114"
"271F"|"Kimpton-Owenspring complex, 35 to 60 percent slopes"||40|38.5|61|||"None"|"None"|"0"|4.7|7.08|9.39|9.39|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1386144"
"290F"|"Libeg, extremely bouldery-Bangtail, rubbly-Demast very stony complex, 15 to 60 percent slopes"||25|28.5|99|||"None"|"None"|"0"|4.17|7.97|14.93|17.78|"Well drained"|"Well drained"|"C"||100|"6"|55|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.891|"Severe"|"0"|1|"1386187"
"390F"|"Sawicki, extremely stony-Wickes, very stony-Tolbert, very stony complex, 25 to 60 percent slopes"||40|40|40|||"None"|"None"|"0"|3.43|5.85|8.97|11.1|"Well drained"|"Well drained"|"C"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1387647"
"370C"|"Hoppers-Voldseth complex, 2 to 8 percent slopes"||6|6|55|84|84|"None"|"Rare"|"0"|4.38|8.45|10.85|12.35|"Well drained"|"Somewhat poorly drained"|"C"|"4"|90|"6"|70|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.015|"Moderate"|"0"|0.903|"1387711"
"490E"|"Redchief, very bouldery-Sicklesteets, very stony-Nieman, rubbly complex, 8 to 35 percent slopes"||12|17.4|41|||||"0"|4.06|6.9|11.65|16.39|"Well drained"|"Well drained"|"C"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Moderate"|"0"|1|"1389155"
"538E"|"Philipsburg-Woodhall, stony-Bangtail complex, 15 to 35 percent slopes"||25|26.5|76|||"None"|"None"|"0"|4.03|7.59|12.65|14.85|"Well drained"|"Well drained"|"C"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"1389503"
"638E"|"Castner-Gnojek, very stony-Quincreek, very stony complex, 15 to 45 percent slopes"||30|30|27|||"None"|"None"|"0"|2.35|3.15|3.34|3.34|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1389681"
"466E"|"Sawicki-Martinsdale, extremely stony complex, 8 to 25 percent slopes"||16|16||||"None"|"None"|"0"|3.87|7.74|14.44|20.21|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.472|"Severe"|"0"|1|"1396991"
"69D"|"Libeg, extremely bouldery-Demast, extremely bouldery-Melville, very stony complex, 4 to 15 percent slopes"||10|10|105|||"None"|"None"|"0"|3.78|6.9|12|14.61|"Well drained"|"Well drained"|"B"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Very limited"|0.85|"Moderate"|"0"|0.925|"1485119"
"766E"|"Varney, very bouldery-Beenom, very stony complex, cool, 15 to 45 percent slopes"||25|27|33|||"None"|"None"|"0"|4.05|7.03|10.63|13.03|"Well drained"|"Well drained"|"B"||100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1486983"
"855C"|"Coyoteflats-Fortlogan-Nebies, very stony, complex, cool, 2 to 8 percent slopes"||4|4|135|||"None"|"None"|"0"|3.91|6.93|12.55|17.23|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.122|"Slight"|"0"|0.577|"1487024"
"955D"|"Fortlogan cobbly sandy loam, cool, 4 to 15 percent slopes, very stony"||7|7|130|||"None"|"None"|"0"|3.52|6.67|12.49|14.75|"Well drained"|"Well drained"|"C"|"6"|85|"6"|85|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.032|"Moderate"|"0"|0.95|"1487090"
"80E"|"Sawicki, very stony-Wickes, extremely bouldery complex, 15 to 35 percent slopes"||25|25|78|||"None"|"None"|"0"|3.42|6.45|11.24|14.27|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Very limited"|1|"Moderate"|"0"|1|"1487636"
"180E"|"Whitecow, stony-Reedwest complex, 8 to 35 percent slopes"||20|20|91|||"None"|"None"|"0"|3.87|7.09|12.31|15.23|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Severe"|"0"|1|"1487639"
"955C"|"Varney, stony-Coyoteflats, very stony complex, cool, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.83|6.76|11.71|16.66|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.118|"Moderate"|"0"|0.205|"1487641"
"75E"|"Twinadams, stony-Rentsac complex, cool, 8 to 45 percent slopes"||25|25|36|||||"0"|2.65|4.16|5.43|5.78|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1487664"
"268E"|"Marmarth-Cabbart-Varney complex, cool, 8 to 35 percent slopes"||15|15|46|||"None"|"None"|"0"|4.14|7.91|12.9|14.62|"Well drained"|"Well drained"|"C"||100|"6"|75|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.139|"Severe"|"0"|1|"1487668"
"770D"|"Reedpoint-Twinadams complex, 4 to 15 percent slopes"||8|8|23|||||"0"|2.58|3.18|3.56|3.56|"Well drained"|"Well drained"|"D"|"7"|65|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.103|"Moderate"|"0"|1|"1487686"
"770E"|"Rentsac-Reedpoint complex, 8 to 35 percent slopes"||15|15|23|||||"0"|2.37|2.82|2.94|2.94|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.073|"Moderate"|"0"|1|"1487688"
"268C"|"Fortlogan-Coyoteflats-Cabbart complex, cool, 2 to 8 percent slopes"||4|4|46|||"None"|"None"|"0"|4.34|8.26|13.47|16.98|"Well drained"|"Well drained"|"C"|"4"|85|"4"|85|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.108|"Moderate"|"0"|0.85|"1529235"
"554C"|"Martinsdale-Meagher complex, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.98|8.04|15.23|21.8|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.052|"Moderate"|"0"|0.325|"1529492"
"177B"|"Rothiemay-Varney complex, cool, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.63|7.2|14.29|20.39|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.126|"Slight"|"0"|0|"1529885"
"234C"|"Rothiemay gravelly loam, cool, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.45|6.88|13.58|18.87|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.12|"Moderate"|"0"|0.1|"1530148"
"48B"|"Varney gravelly loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.29|8.04|15.54|23.04|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.298|"Slight"|"0"|0|"1530199"
"47B"|"Varney gravelly loam, cool, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.29|8.04|15.54|23.04|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.142|"Slight"|"0"|0|"1530200"
"541C"|"Fairfield-Kiev complex, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.95|7.45|14.43|21.03|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.028|"Moderate"|"0"|0.3|"1530244"
"137C"|"Musselshell cobbly loam, 2 to 8 percent slopes"||5|4.9||||"None"|"None"|"0"|3.3|6.5|11.66|15.58|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.244|"Moderate"|"0"|0.464|"1530333"
"139B"|"Amesha-Musselshell complex, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.94|8.06|15.92|22.7|"Well drained"|"Well drained"|"B"|"3"|100|"3"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.229|"Slight"|"0"|0|"1530347"
"136E"|"Delpoint-Cabbart complex. 8 to 35 percent slopes"||22|22|46|||"None"|"None"|"0"|4.05|7.7|9.69|9.69|"Well drained"|"Well drained"|"C"||100|"6"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.82|"Severe"|"0"|1|"1530370"
"84B"|"Crago-Musselshell complex, cool, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.13|6.03|10.73|13.76|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.128|"Slight"|"0"|0.7|"1530408"
"39B"|"Amesha silt loam, 1 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.21|8.01|15.52|22.25|"Well drained"|"Well drained"|"B"|"4"|100|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.25|"Moderate"|"0"|0.1|"1530858"
"337B"|"Musselshell loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.59|6.79|11.95|15.86|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.244|"Moderate"|"0"|0.1|"1530862"
"437B"|"Musselshell-Crago complex, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|3.47|6.57|11.66|15.39|"Well drained"|"Well drained"|"B"|"4"|70|"4"|70|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.251|"Moderate"|"0"|0.3|"1530863"
"36C"|"Delpoint-Marmarth-Cabbart complex, cool, 2 to 8 percent slopes"||5|5|46|||"None"|"None"|"0"|4.15|7.95|11.39|11.39|"Well drained"|"Well drained"|"C"|"4"|80|"4"|80|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.137|"Moderate"|"0"|1|"1530864"
"184E"|"Crago-Musselshell complex, 8 to 35 percent slopes"||22|22||||"None"|"None"|"0"|3.07|5.99|10.94|14.97|"Well drained"|"Well drained"|"B"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.82|"Moderate"|"0"|1|"1530871"
"49C"|"Assinniboine-Coyoteflats complex, cool, 2 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.62|7.33|13.14|17.5|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.067|"Moderate"|"0"|0.353|"1536810"
"155B"|"Varney-Coyoteflats complex, cool, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.84|7.47|14.09|20.39|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.136|"Slight"|"0"|0.026|"1537062"
"153B"|"Coyoteflats, very stony-Beaverell complex, cool, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|3.63|6.03|9.82|13.52|"Well drained"|"Well drained"|"C"|"4"|100|"4"|70|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.091|"Slight"|"10"|0.7|"1537460"
"748D"|"Shawmut stony loam, 8 to 15 percent slopes"||11|11||||"None"|"None"|"0"|3.69|6.54|10.3|13.45|"Well drained"|"Well drained"|"C"||100|"6"|90|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.029|"Moderate"|"0"|0.367|"1590378"
"280E"|"Hardhart, stony-Maciver-Nieman, very stony complex, 15 to 45 percent slopes"||30|30|41|||"None"|"None"|"0"|3.52|5.82|8.33|9.41|"Well drained"|"Well drained"|"C"||100|"7"|97|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1612397"
"364E"|"Hardhart-Checkerboard complex, 8 to 25 percent slopes, bouldery"||15|15|47|||"None"|"None"|"0"|2.83|4.67|5.76|5.76|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Not limited"|0|"Moderate"|"0"|1|"1612526"
"740F"|"Libeg, bouldery-Findon-Lake Creek, extremely stony complex, 25 to 60 percent slopes"||35|35|89|||"None"|"None"|"0"|3.75|6.69|10.99|12.89|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1612554"
"664F"|"Findon, stony-Checkerboard, very-stony, Hardhart,  stony-complex, 25 to 60 percent slopes"||30|36.1|47|||"None"|"None"|"0"|3.11|5.46|8.21|8.44|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1612675"
"240F"|"Leavitt, stony-Poin, very stony-Woodhurst, extremely bouldery complex, 25 to 60 percent slopes"||35|38.8|37|||"None"|"None"|"0"|4.39|7.46|12.17|16.11|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1612781"
"999F"|"Shanley, bouldery-Chivington-Meagher complex, 15 to 45 percent slopes"||30|23.3||||"None"|"None"|"0"|4.24|7.66|13.71|19.52|"Well drained"|"Well drained"|"C"||95|"6"|50|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.658|"Severe"|"5"|0.986|"1613224"
"840F"|"Jaegie-Helmville, stony-Yellowmule complex, 35 to 60 percent slopes"||45|44.2|79|||"None"|"None"|"0"|4.27|7.21|12.18|15.62|"Well drained"|"Well drained"|"B"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Severe"|"0"|1|"1613628"
"403F"|"Lonniebee-Stemple-Cowood, stony complex, 20 to 60 percent slopes"||40|37.9|44|||"None"|"None"|"0"|3.15|4.81|6.83|7.75|"Well drained"|"Well drained"|"C"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1650238"
"224C"|"Shambo loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.73|9.18|17.87|24.61|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.028|"Moderate"|"0"|0.115|"1858526"
"210D"|"Cabba loam, 2 to 15 percent slopes"||9|9|30|||"None"|"None"|"0"|4.02|5.06|5.22|5.22|"Well drained"|"Well drained"|"D"||100|"7"|90|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Very limited"|0.854|"Severe"|"0"|1|"1858528"
"215B"|"Macar loam, calcareous surface, 0 to 4 percent slopes"||2|2||||"None"|"None"|"0"|4.64|9.07|17.08|24.63|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.027|"Slight"|"0"|0.1|"1858530"
"679F"|"Bangtail-Copenhaver complex, 35 to 60 percent slopes"||48|48|38|||"None"|"None"|"0"|4.46|8.08|14.09|14.31|"Well drained"|"Well drained"|"C"||100|"7"|96|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1858533"
"212C"|"Burnel-Nythar complex, 2 to 8 percent slopes"||5|4.9||15|15|"None"|"Rare"|"0"|4.1|8.17|15.88|23.3|"Well drained"|"Very poorly drained"|"C"|"3"|85|"3"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.174|"Moderate"|"15"|0.609|"1858535"
"679E"|"Bangtail-Copenhaver complex, 8 to 25 percent slopes"||17|18.3|38|||"None"|"None"|"0"|4.34|7.75|13.31|13.6|"Well drained"|"Well drained"|"C"||100|"6"|68|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.127|"Severe"|"0"|1|"1858536"
"679D"|"Bangtail-Adel complex, 4 to 25 percent slopes"||15|15.2|94|||"None"|"None"|"0"|4.62|8.87|15.72|18.52|"Well drained"|"Well drained"|"C"||100|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.015|"Severe"|"0"|1|"1858538"
"523A"|"Enbar-Nythar complex, cool, 0 to 4 percent slopes"||2|1.9||15|15|"Rare"|"Rare"|"0"|4.54|9.04|17.11|23.16|"Somewhat poorly drained"|"Very poorly drained"|"C"|"4"|80|"4"|80|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.227|"Slight"|"22"|0.744|"1858539"
"263C"|"Whitecow, very bouldery-Yaple, extremely bouldery complex, 2 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.68|6.29|11.42|15.15|"Well drained"|"Well drained"|"B"|"6"|100|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.894|"Moderate"|"0"|0.894|"1858691"
"950F"|"Bundo, extremely bouldery-Woodhurst, very bouldery-Rock outcrop complex, 15 to 45 percent slopes"||40|38.3|73|||"None"|"None"|"0"|3.56|5.66|8.55|10.55|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"1858692"
"850D"|"Farnuf-Bacbuster complex, 4 to 15 percent slopes"||8|8|62|||"None"|"None"|"0"|4.77|9.54|15.74|20.72|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.024|"Moderate"|"0"|0.725|"1858694"
"20C"|"Voldseth-Groveland complex, 2 to 8 percent slopes, foothills"||2|2||84|84|"None"|"None"|"0"|4.71|9.22|16.91|23.31|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.076|"Slight"|"10"|0.709|"1858696"
"19C"|"Nesda-Meadowcreek complex, 2 to 8 percent slopes"||2|2||84|84|"Rare"|"Rare"|"0"|4.97|7.69|10.57|11.75|"Well drained"|"Somewhat poorly drained"|"B"|"4"|100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.041|"Slight"|"5"|1|"1858697"
"750D"|"Hoppers-Brickner complex, 4 to 15 percent slopes"||8|8|40|||"None"|"None"|"0"|3.87|6.88|7.31|7.31|"Well drained"|"Well drained"|"D"|"4"|50|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.079|"Moderate"|"0"|1|"1858699"
"131D"|"Reedpoint very channery loam, 2 to 15 percent slopes"||9|9|13|||"None"|"None"|"0"|1.37|1.61|1.69|1.69|"Well drained"|"Well drained"|"D"||100|"7"|86|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.241|"Slight"|"0"|1|"1860177"
"146C"|"Ethridge clay loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.64|8.97|17.66|26.29|"Well drained"|"Well drained"|"C"|"3"|100|"3"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.361|"Moderate"|"0"|0.965|"1860274"
"379E"|"Bridger cobbly loam, 15 to 35 percent slopes, stony"||25|26.2||||"None"|"None"|"0"|3.62|6.57|12.73|19.08|"Well drained"|"Well drained"|"C"||100|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"1901623"
"52C"|"Martinsdale loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.49|8.45|14.74|20.38|"Well drained"|"Well drained"|"C"|"3"|100|"3"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.078|"Moderate"|"0"|0.441|"2377552"
"92E"|"Martab loam, 15 to 45 percent slopes"||30|30||||"None"|"None"|"0"|4.94|9.01|16.37|23.35|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"2377553"
"366D"|"Windham cobbly loam, 8 to 15 percent slopes, stony"||12|12.7||||"None"|"None"|"0"|2.85|4.1|6.1|8.1|"Well drained"|"Well drained"|"B"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.127|"Moderate"|"0"|0.989|"2377555"
"379D"|"Bridger cobbly loam, 8 to 15 percent slopes, stony"||12|12.7||||"None"|"None"|"0"|3.62|6.57|12.73|19.08|"Well drained"|"Well drained"|"C"||100|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.091|"Moderate"|"0"|0.67|"2377556"
"452C"|"Quigley-Beanlake complex, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.19|7.87|14.83|21.7|"Well drained"|"Well drained"|"B"|"3"|95|"3"|95|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.055|"Moderate"|"0"|0.056|"2377559"
"452D"|"Quigley-Beanlake complex, 8 to 15 percent slopes"||12|11.9||||"None"|"None"|"0"|4.36|8.21|15.4|22.57|"Well drained"|"Well drained"|"B"||100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.051|"Severe"|"0"|0.627|"2377560"
"1466E"|"Windham cobbly loam, 15 to 45 percent slopes, stony"||30|31.1||||"None"|"None"|"0"|2.78|4.01|5.85|7.69|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377561"
"479F"|"Bangtail clay loam, 35 to 60 percent slopes"||48|48|94|||"None"|"None"|"0"|4.94|9.05|15.99|15.99|"Well drained"|"Well drained"|"C"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377562"
"481E"|"Hanson loam, 8 to 25 percent slopes"||17|17.9||||"None"|"None"|"0"|4.86|8.48|13.48|18.48|"Well drained"|"Well drained"|"B"||100|"6"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.147|"Severe"|"0"|1|"2377563"
"491E"|"Hanson-Whitore, stony complex, 15 to 45 percent slopes"||30|30||||"None"|"None"|"0"|4.4|7.67|12.53|17.35|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377564"
"512D"|"Enbar-Bowery-Nythar complex, 4 to 15 percent slopes"||6|6.4||15|15|"Rare"|"Rare"|"0"|4.74|9.44|17.59|24.2|"Somewhat poorly drained"|"Very poorly drained"|"C"|"3"|65|"3"|65|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.207|"Moderate"|"20"|0.605|"2377565"
"666E"|"Windham, stony-Lap, very stony complex, 15 to 45 percent slopes"||30|30.9|41|||"None"|"None"|"0"|2.7|3.96|5.6|7.08|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377567"
"786F"|"Whitecow, stony-Lap, very stony-Rock outcrop complex, 35 to 60 percent slopes"||48|48|41|||"None"|"None"|"0"|3.56|5.64|8.86|11.75|"Well drained"|"Well drained"|"B"||100|"7"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377570"
"790E"|"Accola-Whitore, stony complex, 15 to 45 percent slopes"||30|30.9||||"None"|"None"|"0"|4.27|7.81|12.72|17.08|"Well drained"|"Well drained"|"B"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377571"
"812E"|"Tolex very channery coarse sandy loam, 15 to 45 percent slopes"||30|30|38|||"None"|"None"|"0"|1.95|2.98|3.04|3.04|"Well drained"|"Well drained"|"D"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377572"
"966E"|"Windham, stony-Rock outcrop complex, 15 to 45 percent slopes"||30|30||||"None"|"None"|"0"|2.87|4.24|6.18|8.11|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377575"
"178E"|"Copenhaver-Rock outcrop complex, 8 to 35 percent slopes"||22|21.3|38|||"None"|"None"|"0"|3.27|4.67|5.48|5.48|"Well drained"|"Well drained"|"D"||100|"7"|70|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.736|"Moderate"|"0"|1|"2377795"
"500A"|"Soapcreek, moderately saline-Adger complex, 0 to 2 percent slopes, rarely flooded"||1|1||84|84|"Rare"|"Rare"|"0"|4.57|8.82|15.89|22.21|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|60|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.137|"Slight"|"10"|1|"2377804"
"501A"|"Soapcreek-Clunton complex, 0 to 4 percent slopes, occasionally flooded"||1|1.4||0|0|"Occasional"|"Occasional"|"0"|5.31|10.02|18.58|25.73|"Somewhat poorly drained"|"Very poorly drained"|"C"|"4"|70|"4"|70|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.369|"Slight"|"35"|0.984|"2377805"
"860F"|"Billman-Adel-Tolbert complex, 25 to 60 percent slopes"||35|35.8|41|||"None"|"None"|"0"|3.97|7.8|10.86|13.18|"Well drained"|"Well drained"|"D"||100|"7"|98|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2377808"
"869D"|"Absarokee-Tolbert complex, 4 to 15 percent slopes"||10|11|41|||"None"|"None"|"0"|3.58|6.47|7.77|7.77|"Well drained"|"Well drained"|"C"||100|"4"|60|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.129|"Moderate"|"0"|1|"2377809"
"946D"|"Bacbuster-Wilsall-Tolbert complex, 2 to 15 percent slopes"||4|6.6|30|||"None"|"None"|"0"|4.44|7.3|9.74|10.55|"Well drained"|"Well drained"|"D"|"4"|45|"7"|45|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.084|"Moderate"|"5"|1|"2377810"
"865D"|"Burtoner-Crackerville-Connieo complex, 4 to 15 percent slopes"||8|8|46|||||"0"|3.6|6.75|8.53|8.53|"Well drained"|"Well drained"|"C"|"6"|100|"6"|100|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.044|"Slight"|"0"|1|"2377890"
"748C"|"Shawmut stony loam, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.67|6.52|11.34|15.84|"Well drained"|"Well drained"|"B"|"6"|90|"6"|90|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.03|"Moderate"|"0"|0.008|"2379117"
"340D"|"Houlihan-Duckcreek complex, 4 to 15 percent slopes"||8|9.2|92|||"None"|"None"|"0"|4.74|9.3|16.89|21.14|"Well drained"|"Well drained"|"D"|"6"|50|"6"|90|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Not limited"|0.008|"Moderate"|"0"|0.5|"2383782"
"69E"|"Dailybasin, rubbly-Monaberg, extremely stony complex, 15 to 35 percent slopes"||25|25||||||"0"|4.21|7.68|13.42|18.07|"Well drained"|"Well drained"|"C"||100|"7"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Very limited"|1|"Moderate"|"10"|1|"2383923"
"988F"|"Redchief, very stony-Bangtail-Dailybasin, very bouldery complex, 8 to 45 percent slopes"||25|22.7|94|||"None"|"None"|"0"|4.37|7.69|13.18|16.29|"Well drained"|"Well drained"|"C"||95|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.75|"Severe"|"5"|1|"2383926"
"865E"|"Connieo-Burtoner-Crackerville complex, 8 to 35 percent slopes"||20|20|46|||||"0"|3.62|6.75|8.24|8.24|"Well drained"|"Well drained"|"C"||100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.5|"Moderate"|"0"|1|"2383946"
"865F"|"Whitlash, stony-Belain-Rock outcrop complex, 35 to 70 percent slopes"||50|50|46|||||"0"|3.58|6.12|8.91|9.39|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2383948"
"569F"|"Mountedith, stony-Worock, bouldery complex, 15 to 50 percent slopes"||35|30.3||||"None"|"None"|"0"|3.22|5.21|8.58|11.63|"Well drained"|"Well drained"|"B"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.789|"Severe"|"0"|1|"2383980"
"357E"|"Cabba-Vershal complex, 15 to 45 percent slopes"||30|29.2|20|||"None"|"None"|"0"|3.13|4.49|4.88|5.12|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.965|"Severe"|"0"|0.996|"2384109"
"435E"|"Bachus-Mayflower-Adel complex, 4 to 25 percent slopes"||15|15|64|||"None"|"None"|"0"|4.38|8.43|13|14.43|"Well drained"|"Well drained"|"D"||100|"6"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Not limited"|0|"Severe"|"0"|1|"2398250"
"335F"|"Booneville-Lingshire-Adel complex, 15 to 60 percent slopes"||40|38.3|92|||"None"|"None"|"0"|4.73|8.96|14.93|18.3|"Well drained"|"Well drained"|"C"||100|"7"|85|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"2398256"
"464G"|"Maiden, very stony-Rock outcrop-Warneke, extremely stony complex, 60 to 90 percent slopes"||75|75|48|||"None"|"None"|"0"|2.96|4.67|5.49|6.16|"Well drained"|"Well drained"|"C"||100|"8"|100|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2424400"
"156F"|"Skaggs, very stony-Levengood complex, 35 to 60 percent slopes"||47|48.1|58|||||"0"|3.88|6.3|8.58|10.61|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2424404"
"156G"|"Skaggs, very stony-Levengood, stony-Rock outcrop complex, 60 to 90 percent slopes"||75|73.2|58|||||"0"|3.77|6|7.84|9.37|"Well drained"|"Well drained"|"C"||100|"8"|100|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2424405"
"156E"|"Levengood-Skaggs, very stony-Raynesford complex, 15 to 35 percent slopes"||25|25|58|||||"0"|4.04|6.83|10.28|13.55|"Well drained"|"Well drained"|"B"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2425971"
"1264D"|"Daisypeak-Starley, stony-Trapper complex, 2 to 15 percent slopes"||8|8|42|||"None"|"None"|"0"|4.17|6.28|8.04|8.04|"Well drained"|"Well drained"|"C"|"6"|65|"6"|65|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Not limited"|0|"Moderate"|"0"|1|"2428667"
"1264E"|"Whitore-Checkerboard, very stony-Helmville families, complex, 8 to 35 percent slopes"||25|25|35|||"None"|"None"|"0"|4.27|6.54|9.78|12.24|"Well drained"|"Well drained"|"B"||100|"6"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2428668"
"680E"|"Shanley-Wickes, bouldery-Sinnigam, very bouldery complex, 15 to 35 percent slopes"||20|22.6|48|||"None"|"None"|"0"|3.95|6.84|10.78|13.81|"Well drained"|"Well drained"|"C"||100|"6"|73|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.754|"Severe"|"0"|1|"2479720"
"990F"|"Worock, extremely bouldery-Pricepeet, very bouldery-Jaegie, very stony complex, 8 to 45 percent slopes"||25|23.7||||"None"|"None"|"0"|4.34|7.14|12|16.22|"Well drained"|"Well drained"|"B"||90|"7"|60|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.944|"Severe"|"10"|1|"2479750"
"5654F"|"Vershal, extremely stony-Whitlash, stony-Rock outcrop complex, 15 to 60 percent slopes"||35|32.1|15|||"None"|"None"|"0"|1.6|2.18|2.18|2.18|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2485902"
"7703F"|"Worock-Lake Creek-Catlinsprings complex, 20 to 60 percent slopes, extremely stony"||45|41.1|36|||"None"|"None"|"0"|3.63|6.06|10.05|12.58|"Well drained"|"Well drained"|"C"||95|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.967|"Severe"|"5"|1|"2486031"
"5646E"|"Copenhaver-Dalys-Bridger complex, 8 to 45 percent slopes"||20|18.7|18|||"None"|"None"|"0"|3.18|4.95|7.42|9.42|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.37|"Severe"|"0"|1|"2486035"
"7601F"|"Copenhaver-Libeg complex, 15 to 60 percent slopes"||40|39.4|41|||"None"|"None"|"0"|3.13|5.14|7.07|8.84|"Well drained"|"Well drained"|"D"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2486036"
"413B"|"Nesda-Meadowcreek-Clunton complex, 0 to 4 percent slopes"||2|1.4||10|10|"Occasional"|"Occasional"|"20"|5.14|8.35|13.04|15.49|"Well drained"|"Very poorly drained"|"B"|"4"|40|"6"|40|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.308|"Slight"|"20"|1|"2487107"
"646E"|"Windham-Doney complex, moist, 15 to 45 percent slopes"||20|22.5|71|||"None"|"None"|"0"|3.8|6.71|9.46|10.71|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.725|"Severe"|"0"|1|"2487139"
"314C"|"Adel loam, 2 to 8 percent slopes"||5|5.6||||"None"|"None"|"0"|4.37|8.67|15.65|22.41|"Well drained"|"Well drained"|"B"|"6"|95|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.017|"Moderate"|"0"|0.076|"2493518"
"260D"|"Bacbuster-Wilsall complex, 4 to 15 percent slopes"||10|10|25|||"None"|"None"|"0"|4.65|7.68|12.24|12.24|"Well drained"|"Well drained"|"D"||100|"4"|65|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.058|"Severe"|"0"|0.99|"2493519"
"991F"|"Whitore-Rock outcrop complex, 35 to 70 percent slopes"||53|51.6||||"None"|"None"|"0"|3.42|5.93|10.41|14.63|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2493520"
"866E"|"Windham, stony-Hanson-Lap, stony complex, 8 to 35 percent slopes"||22|23.6|41|||"None"|"None"|"0"|3.95|6.36|9.81|13.25|"Well drained"|"Well drained"|"B"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.831|"Severe"|"0"|1|"2493521"
"879E"|"Bangtail-Copenhaver-Adel complex, 15 to 35 percent slopes"||25|24.6|38|||"None"|"None"|"0"|4.25|7.63|12.57|14.22|"Well drained"|"Well drained"|"C"||98|"6"|62|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.988|"Severe"|"2"|1|"2493522"
"9681E"|"Raynesford, stony-Hanson, very stony complex, 8 to 25 percent slopes"||17|17.9||||"None"|"None"|"0"|3.69|7.03|12.57|18.1|"Well drained"|"Well drained"|"C"||100|"6"|97|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.228|"Severe"|"0"|1|"2493523"
"614D"|"Adel loam, cool, 4 to 15 percent slopes"||10|10.2||||"None"|"None"|"0"|4.63|9.08|17.89|26.69|"Well drained"|"Well drained"|"B"||95|"6"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Not limited"|0.026|"Severe"|"5"|0.27|"2493525"
"439D"|"Tolbert-Blaincreek complex, 2 to 15 percent slopes"||9|9.1|41|||"None"|"None"|"0"|3.49|5.34|6.2|6.92|"Well drained"|"Well drained"|"D"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.042|"Moderate"|"0"|0.901|"2493526"
"5645F"|"Blaine-Tophat-Dalys complex, 15 to 60 percent slopes"||30|28.4|18|||"None"|"None"|"0"|3.29|6.08|9.6|12.34|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.842|"Severe"|"0"|1|"2493527"
"5405E"|"Adel-Dailybasin, very stony complex, 8 to 25 percent slopes"||15|14.3||||"None"|"None"|"0"|4.55|8.79|16.5|22.61|"Well drained"|"Well drained"|"B"||90|"6"|100|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Not limited"|0.123|"Moderate"|"10"|1|"2493528"
"5536E"|"Redchief, very stony-Stubbs-Dailybasin, extremely stony complex, 4 to 35 percent slopes"||15|16.4|81|||"None"|"None"|"0"|4|7.46|12.57|15.92|"Well drained"|"Well drained"|"C"||95|"6"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.383|"Moderate"|"5"|1|"2493529"
"5547E"|"Tophat-Adel-Bangtail complex, 4 to 25 percent slopes"||20|16.8|94|||"None"|"None"|"0"|4.68|8.93|16.43|22.08|"Well drained"|"Well drained"|"C"||95|"6"|95|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.347|"Severe"|"5"|0.89|"2493530"
"388D"|"Blaincreek, stony-Braziel-Tolbert, very stony complex, 4 to 15 percent slopes"||8|8|38|||"None"|"None"|"0"|3.4|6|8.98|10.27|"Well drained"|"Well drained"|"C"|"4"|75|"6"|50|"Somewhat limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.13|"Slight"|"0"|0.868|"2494742"
"388E"|"Blaincreek, stony-Braziel-Shanley complex, 15 to 35 percent slopes"||25|23.7|76|||"None"|"None"|"0"|3.65|6.5|10.3|12.51|"Well drained"|"Well drained"|"C"||100|"6"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.868|"Moderate"|"0"|1|"2494743"
"590D"|"Blackbear, very bouldery-Worock, bouldery-Pricepeet complex, 4 to 15 percent slopes"||12|10.4|76|||"None"|"None"|"0"|4.26|6.93|10.25|12.59|"Well drained"|"Well drained"|"C"||95|"6"|56|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.468|"Moderate"|"0"|1|"2494745"
"590F"|"Worock, rubbly-Blackbear, extremely bouldery-Pricepeet, very bouldery complex, 15 to 60 percent slopes"||25|34.7|76|||"None"|"None"|"0"|3.97|6.52|9.74|12.27|"Well drained"|"Well drained"|"B"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2494746"
"179E"|"Bridger loam, cool, 4 to 25 percent slopes"||15|15.1||||"None"|"None"|"0"|4.58|8.19|15.09|21.4|"Well drained"|"Well drained"|"C"||97|"6"|98|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.049|"Severe"|"3"|1|"2496271"
"ANS"|"Area not surveyed, access denied"|||||||||"0"|||||||||100||100|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"||"Not rated"|"0"||"2496274"
"460B"|"Work clay loam, 2 to 4 percent slopes"||3|3||||"None"|"None"|"0"|4.41|8.42|15.72|22.14|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Slight"|"0"|1|"2496368"
"258D"|"Bacbuster-Reedwest-Castner complex, 4 to 15 percent slopes, foothills"||10|10.4|41|||"None"|"None"|"0"|4.23|7.63|13.34|13.34|"Well drained"|"Well drained"|"D"||100|"4"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.077|"Severe"|"0"|1|"2496369"
"58D"|"Bacbuster-Reedwest-Castner complex, 4 to 15 percent slopes, mountains"||10|10.4|41|||"None"|"None"|"0"|4.46|7.92|13.64|13.64|"Well drained"|"Well drained"|"D"||100|"4"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.076|"Severe"|"0"|1|"2496370"
"258E"|"Bacbuster-Castner complex, 15 to 45 percent slopes, foothills"||25|27.4|39|||"None"|"None"|"0"|3.86|7|7.48|7.48|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2496371"
"58E"|"Bacbuster-Castner complex, 15 to 45 percent slopes, mountains"||25|27.4|39|||"None"|"None"|"0"|3.71|6.61|7.05|7.05|"Well drained"|"Well drained"|"D"||100|"6"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2496372"
"660B"|"Hereimcreek-Work complex, 0 to 4 percent slopes, foothills"||2|2||45|45|"None"|"None"|"0"|4.72|8.98|17.68|25.93|"Poorly drained"|"Poorly drained"|"C/D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.312|"Slight"|"60"|0.8|"2496373"
"401B"|"Fluvaquentic Haplaquolls-Typic Fluvaquents, 0 to 4 percent slopes, foothills"||2|2||46|46|"Frequent"|"Frequent"|"0"|2.51|5.03|10.05|15.08|"Poorly drained"|"Poorly drained"|"C/D"|"4"|55|"4"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.436|"Slight"|"100"|1|"2496374"
"843B"|"Tamaneen cobbly clay loam, 0 to 4 percent slopes, foothills"||2|2.1||||"None"|"None"|"0"|3.92|7.4|10.66|13.51|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Fair"|"Fair"|"Somewhat limited"|0.031|"Slight"|"0"|0.45|"2496375"
"445C"|"Reedwest-Roundor-Cabba complex, 2 to 8 percent slopes"||5|5|30|||"None"|"None"|"0"|4.61|8.26|12.84|12.84|"Well drained"|"Well drained"|"C"|"4"|85|"4"|85|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.029|"Moderate"|"0"|1|"2496377"
"120C"|"Voldseth-Groveland complex, 2 to 8 percent slopes"||2|2||84|84|"None"|"None"|"0"|4.71|9.23|16.92|23.32|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.076|"Slight"|"10"|0.709|"2496378"
"125E"|"Shambo-Cabba complex, 8 to 35 percent slopes"||17|19|30|||"None"|"None"|"0"|4.4|7.35|12.63|16.94|"Well drained"|"Well drained"|"B"||100|"6"|60|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.376|"Severe"|"0"|1|"2496380"
"154C"|"Meagher cobbly loam, 2 to 8 percent slopes, stony, foothills"||5|5||||"None"|"None"|"0"|3.72|6.89|12.55|18.14|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.028|"Moderate"|"0"|0.298|"2496381"
"758E"|"Reedwest-Bacbuster-Martinsdale, stony complex, 8 to 35 percent slopes, foothills"||22|22|91|||"None"|"None"|"0"|4.12|8.23|15.52|17.27|"Well drained"|"Well drained"|"C"||100|"6"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"2496382"
"1164G"|"Cowcoulee, stony-Ettienridge families, complex, 35 to 70 percent slopes"||55|55|74|||"None"|"None"|"0"|4.57|6.95|9.28|9.52|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2496546"
"1164E"|"Ettienridge-Checkerboard, very stony-Cowcoulee, stony families, complex, 15 to 35 percent slopes"||25|25|35|||"None"|"None"|"0"|4.46|6.46|8.2|8.2|"Well drained"|"Well drained"|"C"||100|"6"|78|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2496547"
"1251D"|"Lonniebee-Como, very stony-Cowood, extremely stony families, complex, 4 to 15 percent slopes"||10|10.1|44|||"None"|"None"|"0"|3.14|5.12|6.68|7.39|"Well drained"|"Well drained"|"C"||90|"6"|80|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.328|"Moderate"|"2"|1|"2496552"
"1174G"|"Ettienridge, very stony-Checkerboard, extremely stony families-Rock outcrop complex, 50 to 70 percent slopes"||60|60|35|||"None"|"None"|"0"|3.97|5.88|7.33|7.83|"Well drained"|"Well drained"|"D"||100|"7"|73|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2496565"
"2164F"|"Ettienridge, extremely stony-Checkerboard, rubbly families-Rock outcrop complex, 30 to 60 percent slopes"||40|40.9|35|||"None"|"None"|"0"|3.83|5.6|6.92|6.99|"Well drained"|"Well drained"|"C"||98|"7"|83|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.976|"Severe"|"0"|0.99|"2517331"
"681C"|"Doney-Cabba complex, 2 to 8 percent slopes"||4|4.9|30|||"None"|"None"|"0"|4.02|6.7|8.94|9.34|"Well drained"|"Well drained"|"C"|"4"|60|"4"|60|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.027|"Moderate"|"0"|0.95|"2517332"
"681D"|"Doney-Cabba complex, 8 to 15 percent slopes"||10|10.6|30|||"None"|"None"|"0"|4.03|6.56|8.64|9.04|"Well drained"|"Well drained"|"C"||90|"4"|55|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.415|"Severe"|"0"|0.95|"2517333"
"681E"|"Doney-Cabba complex, 15 to 35 percent slopes"||25|26.8|30|||"None"|"None"|"0"|4.03|6.56|8.64|9.04|"Well drained"|"Well drained"|"C"||100|"6"|55|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|0.951|"Severe"|"0"|1|"2517334"
"689C"|"Judith-Windham complex, 4 to 8 percent slopes"||6|5.9||||"None"|"None"|"0"|3.69|6.95|10.49|13.08|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.028|"Moderate"|"0"|0.405|"2517335"
"550C"|"Ratiopeak-Philipsburg complex, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|3.59|6.54|11.32|15.57|"Well drained"|"Well drained"|"C"|"6"|100|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.004|"Moderate"|"0"|0.38|"2517336"
"685E"|"Judith-Doney-Windham complex, 15 to 35 percent slopes"||25|25|71|||"None"|"None"|"0"|3.77|7.16|10.24|11.82|"Well drained"|"Well drained"|"C"||100|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2517337"
"532F"|"Waybe-Duckcreek-Sicklesteets complex, 15 to 60 percent slopes"||30|29.5|46|||"None"|"None"|"0"|4.55|8.32|12.11|13.98|"Well drained"|"Well drained"|"C"||100|"7"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Very limited"|1|"Severe"|"0"|1|"2517338"
"641C"|"Macar loam, calcareous surface, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.64|9.07|17.08|24.63|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.027|"Moderate"|"0"|0.1|"2517339"
"685D"|"Judith-Doney-Windham complex, 4 to 15 percent slopes"||10|10|71|||"None"|"None"|"0"|3.77|7.16|10.24|11.82|"Well drained"|"Well drained"|"C"||100|"4"|90|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.079|"Moderate"|"0"|0.62|"2517340"
"643B"|"Shambo loam, 2 to 4 percent slopes"||3|3.1||||"None"|"None"|"0"|4.84|9.3|17.78|24.5|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.028|"Slight"|"0"|0.067|"2517341"
"411A"|"Meadowcreek loam, 0 to 2 percent slopes, rarely flooded"||1|1||90|90|"Rare"|"Rare"|"0"|4.71|9.15|15.06|17.18|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|95|"4"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.277|"Slight"|"10"|1|"2517342"
"405A"|"Larry clay loam, 0 to 2 percent slopes, rarely flooded"||1|1||38|38|"Rare"|"Rare"|"0"|5.17|9.52|17.19|24.64|"Poorly drained"|"Poorly drained"|"C/D"|"3"|95|"3"|90|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.815|"Slight"|"90"|1|"2517343"
"437C"|"Delpoint-Cabbart complex, 2 to 8 percent slopes, fan"||4|5|41|||"None"|"None"|"0"|3.94|7.14|9.1|9.44|"Well drained"|"Well drained"|"C"|"3"|60|"4"|50|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.213|"Moderate"|"0"|0.95|"2517344"
"677C"|"Shawmut gravelly loam, 2 to 8 percent slopes"||5|5||||"None"|"None"|"0"|3.7|6.57|10.45|13.76|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.022|"Moderate"|"0"|0.281|"2517345"
"450C"|"Yamacall loam, calcareous surface, 4 to 8 percent slopes, fan"||6|6.1||||"None"|"None"|"0"|3.89|7.69|15.34|22.92|"Well drained"|"Well drained"|"B"|"4"|90|"4"|90|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.223|"Moderate"|"0"|0.1|"2517346"
"600B"|"Nesda, occasionally flooded-Meadowcreek, rarely flooded-McIlwaine, rarely flooded complex, 0 to 4 percent slopes"||2|2||90|90|"Rare"|"Occasional"|"5"|4.42|7.34|10.33|11.47|"Well drained"|"Somewhat poorly drained"|"C"|"4"|85|"4"|50|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Somewhat limited"|0.086|"Slight"|"5"|1|"2517347"
"615B"|"Fairway-Meadowcreek complex, 0 to 4 percent slopes"||2|2||90|90|"None"|"None"|"0"|4.86|9.08|16.33|19.42|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|90|"4"|90|"Not limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.125|"Slight"|"10"|0.965|"2517348"
"403A"|"Fairway loam, 0 to 2 percent slopes, rarely flooded"||1|1||90|90|"Rare"|"Rare"|"5"|4.53|8.57|16.4|19.55|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"3"|100|"3"|95|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.295|"Slight"|"5"|1|"2517349"
"443C"|"Ethridge-Rentsac complex, 2 to 8 percent slopes"||4|4.5|46|||"None"|"None"|"0"|4.34|7.98|14.38|20.38|"Well drained"|"Well drained"|"C"|"3"|70|"3"|70|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.288|"Moderate"|"0"|1|"2517350"
"558C"|"Bacbuster-Reedwest-Tolbert complex, 2 to 8 percent slopes, foothills"||5|5|41|||"None"|"None"|"0"|4.38|7.82|13.32|13.32|"Well drained"|"Well drained"|"D"|"4"|75|"4"|75|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Moderate"|"0"|1|"2517351"
"28A"|"Lepner-Tetonview complex, 0 to 2 percent slopes"||1|1||30|30|"None"|"None"|"90"|3.99|7.87|14.96|21.09|"Well drained"|"Poorly drained"|"C"|"6"|75|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.902|"Slight"|"20"|1|"2517352"
"662B"|"Meagher gravelly loam, 0 to 4 percent slopes, foothills"||2|2||||"None"|"None"|"0"|3.89|7.66|13.42|17.96|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.028|"Slight"|"0"|0.055|"2517353"
"66C"|"Kiev-Fairfield complex, 2 to 8 percent slopes, foothills"||6|6||||"None"|"None"|"0"|3.87|7.37|14.33|20.63|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.027|"Moderate"|"0"|0.15|"2517354"
"766C"|"Kiev-Martinsdale complex, 4 to 8 percent slopes"||6|6||||"None"|"None"|"0"|4.12|7.9|15.27|21.94|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.022|"Moderate"|"0"|0.2|"2517355"
"56C"|"Farnuf-Work complex, 2 to 8 percent slopes, foothills"||5|5||||"None"|"None"|"0"|4.69|9.01|17.25|24.7|"Well drained"|"Well drained"|"B"|"4"|100|"4"|100|"Somewhat limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.031|"Moderate"|"0"|0.45|"2517356"
"445E"|"Reedwest-Roundor-Cabba complex, 8 to 35 percent slopes"||22|22|30|||"None"|"None"|"0"|4.59|8.05|12.43|12.43|"Well drained"|"Well drained"|"C"||100|"6"|80|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.82|"Severe"|"0"|1|"2517357"
"654C"|"Martinsdale stony loam, 1 to 8 percent slopes, foothills"||5|5.1||||"None"|"None"|"0"|3.95|7.92|15.42|22.71|"Well drained"|"Well drained"|"C"|"6"|90|"6"|100|"Not limited"|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.017|"Moderate"|"0"|0.511|"2517359"
"54C"|"Martinsdale-Meagher complex, 4 to 8 percent slopes, foothills"||6|6||||"None"|"None"|"0"|3.93|7.99|15.18|21.75|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.052|"Moderate"|"0"|0.353|"2517360"
"266D"|"Kiev-Work complex, 4 to 15 percent slopes, foothills"||10|9.1||||"None"|"None"|"0"|4.6|8.8|16.09|23.34|"Well drained"|"Well drained"|"B"||70|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.034|"Severe"|"0"|0.203|"2523021"
"33A"|"Soapcreek-Fairway complex, 0 to 2 percent slopes, foothills"||1|1||84|84|"Rare"|"Rare"|"0"|5.14|9.86|18.52|24.47|"Somewhat poorly drained"|"Somewhat poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.174|"Slight"|"0"|1|"2523022"
"640D"|"Bacbuster-Chivington complex, 4 to 15 percent slopes, foothills"||12|9.6|94|||"None"|"None"|"0"|4.77|9.26|17.42|20.76|"Well drained"|"Well drained"|"D"||60|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.038|"Severe"|"0"|0.93|"2523023"
"653C"|"Work clay loam, 4 to 8 percent slopes, foothills"||6|6||||"None"|"None"|"0"|4.42|8.44|15.64|22.12|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Poor"|"Poor"|"Somewhat limited"|0.033|"Moderate"|"0"|0.316|"2523024"
"677D"|"Shawmut gravelly loam, 8 to 15 percent slopes, foothills"||12|12||||"None"|"None"|"0"|3.72|6.5|10.2|13.35|"Well drained"|"Well drained"|"C"||100|"4"|95|"Somewhat limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Somewhat limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.071|"Moderate"|"0"|0.651|"2523025"
"196A"|"Korell silt loam, 0 to 3 percent slopes, foothills"||2|2||||"None"|"None"|"0"|5|9.4|17.92|26.18|"Well drained"|"Well drained"|"C"|"4"|100|"4"|100|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Not limited"|"Not limited"|"Somewhat limited"|"Poor"|"Fair"|"Somewhat limited"|0.034|"Slight"|"0"|0.694|"2523026"
"4A"|"Villmeagher-Villsprings complex, 0 to 2 percent slopes, foothills"||1|1||46|46|"Rare"|"Rare"|"0"|5.96|10.45|18.14|23.51|"Poorly drained"|"Poorly drained"|"B/D"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Somewhat limited"|0.436|"Slight"|"100"|1|"2523027"
"102B"|"Bigsandy loam, 0 to 4 percent slopes, foothills"||2|2||46|46|"Occasional"|"Occasional"|"90"|3.88|7.33|14.76|20.94|"Poorly drained"|"Poorly drained"|"B/D"|"4"|90|"4"|90|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Fair"|"Somewhat limited"|0.397|"Slight"|"90"|1|"2523028"
"602A"|"Fairberg-Villmeagher complex, 0 to 2 percent slopes, foothills"||1|1||46|46|"Rare"|"Rare"|"0"|4.89|9.39|18.39|23.71|"Somewhat poorly drained"|"Poorly drained"|"C"|"4"|100|"4"|100|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Fair"|"Somewhat limited"|0.177|"Slight"|"35"|1|"2523029"
"560"|"Rubble land and Rock outcrop complex"|||43||||||"0"|2.65|3.77|3.77|3.77|||"D"||100|"8"|95|"Not rated"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Very limited"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|"Not rated"|1|"Not rated"|"0"|1|"2618240"
"2264F"|"Dryadine, extremely stony-Monumentpeak, rubbly-Helmville, stony families, complex, 25 to 60 percent slopes"||45|45|46|||"None"|"None"|"0"|3.32|5.08|6.79|7.68|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2979648"
"1117C"|"Dutchhollow, occasionally flooded-Crookedrun-Levengood families, complex, 1 to 8 percent slopes"||2|2.6||15|15|"Occasional"|"Occasional"|"0"|5.4|9.85|15.4|18.51|"Very poorly drained"|"Very poorly drained"|"C"|"6"|50|"6"|50|"Not limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.477|"Slight"|"45"|0.805|"2979650"
"1156E"|"Cowcoulee-Burnette family-Herakle family, stony, complex, 8 to 35 percent slopes"||20|20|43|||"None"|"None"|"0"|4.35|7.31|10.97|13.12|"Well drained"|"Well drained"|"C"||100|"6"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.5|"Severe"|"0"|1|"2979657"
"1064F"|"Maiden, stony-Lap, very stony families-Rock outcrop complex, 25 to 45 percent slopes"||35|35|48|||"None"|"None"|"0"|3.37|5.43|6.09|6.09|"Well drained"|"Well drained"|"D"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Slight"|"0"|1|"2979658"
"1064G"|"Maiden, stony-Lap, very stony families-Rock outcrop complex, 45 to 70 percent slopes"||55|55|48|||"None"|"None"|"0"|3.39|5.46|6.17|6.17|"Well drained"|"Well drained"|"D"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Slight"|"0"|1|"2979659"
"1064E"|"Maiden-Lap families-Rock outcrop, complex, 4 to 25 percent slopes"||8|8|48|||"None"|"None"|"0"|3.47|5.51|6.48|6.76|"Well drained"|"Well drained"|"C"||90|"6"|60|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.026|"Slight"|"0"|0.963|"2979660"
"1156F"|"Cowcoulee-Herakle, very stony-Skaggs, stony families, complex, 25 to 60 percent slopes"||35|36.1|43|||"None"|"None"|"0"|3.79|6.13|8.63|9.57|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.944|"Severe"|"0"|1|"2979661"
"1165G"|"Tropal family, extremely stony-Rock outcrop-Ettienridge family, very stony, complex, 35 to 70 percent slopes"||50|45.8|37|||"None"|"None"|"0"|3.41|5.11|6.65|6.65|"Well drained"|"Well drained"|"D"||100|"7"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2979662"
"1125E"|"Doolittle, bouldery-Doolittle-Scudder, very stony families, complex, 4 to 35 percent slopes, landslides"||20|15.6|71|||"None"|"None"|"0"|5.14|9.21|13.17|14.3|"Well drained"|"Well drained"|"D"||90|"6"|95|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Somewhat limited"|0.368|"Severe"|"5"|0.963|"2979663"
"1142D"|"Duckcreek-Redchief, very stony-Ratiopeak, bouldery families, complex, 4 to 15 percent slopes"||10|9.7|92|||"None"|"None"|"0"|4.64|8.34|14.44|17.99|"Well drained"|"Well drained"|"C"||80|"6"|95|"Somewhat limited"|"Somewhat limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Fair"|"Not limited"|0.267|"Moderate"|"10"|0.789|"2979664"
"1142E"|"Redchief, very stony-Duckcreek-Cheadle, extremely stony families, complex, 8 to 35 percent slopes"||20|15|48|||"None"|"None"|"0"|4.59|8.1|13.67|17.12|"Well drained"|"Well drained"|"C"||80|"6"|85|"Very limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Fair"|"Not limited"|0.4|"Severe"|"10"|0.93|"2979665"
"1169F"|"Sebud, extremely stony-Lake Creek, very stony-Surdal, stony families, complex, 25 to 60 percent slopes"||40|39.2|71|||"None"|"None"|"0"|3.86|6.5|9.38|10.59|"Well drained"|"Well drained"|"C"||100|"7"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"3"|1|"2979666"
"1168F"|"Elve, extremely stony-Lake Creek, very stony-Comad, rubbly families, complex, 35 to 60 percent slopes"||40|39.4|89|||"None"|"None"|"0"|3.56|5.91|8.49|9.36|"Well drained"|"Well drained"|"C"||100|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"2"|1|"2979667"
"1176F"|"Kimpton-Nieman, very stony-Goosepeak, stony families, complex, 25 to 60 percent slopes"||43|41|46|||"None"|"None"|"0"|3.53|5.87|8.53|9.75|"Well drained"|"Well drained"|"C"||97|"7"|85|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"3"|1|"2979668"
"1080E"|"Maiden-Castner, stony-Darret families, complex, 4 to 25 percent slopes"||20|12.9|39|||"None"|"None"|"0"|3.56|6.32|9.66|10.86|"Well drained"|"Well drained"|"C"||100|"4"|40|"Very limited"|"Very limited"|"Somewhat limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Poor"|"Somewhat limited"|0.205|"Slight"|"0"|0.894|"2979669"
"4000E"|"Worock, very stony-Mountedith, extremely stony families-Rubble land complex, 8 to 35 percent slopes"||15|17.2||||"None"|"None"|"0"|3.79|6.19|10.21|13.88|"Well drained"|"Well drained"|"C"||97|"6"|72|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.63|"Moderate"|"3"|1|"2979670"
"1155E"|"Cowcoulee, stony-Tropal, very stony-Elispring families, complex, 15 to 35 percent slopes"||25|22.2|37|||"None"|"None"|"0"|4.29|7.13|10.79|12.12|"Well drained"|"Well drained"|"C"||85|"6"|65|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|0.856|"Severe"|"2"|1|"2979671"
"1181F"|"Hardhart, stony-Knep families, complex, 20 to 60 percent slopes"||40|40|76|||"None"|"None"|"0"|4.16|6.86|9.54|9.54|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2979672"
"1110D"|"Mooseflat-Foxgulch-Redfish families, complex, 2 to 12 percent slopes, occasionally flooded"||4|6.1||15|15|"Occasional"|"Occasional"|"0"|6.01|9.55|13.43|15.05|"Very poorly drained"|"Very poorly drained"|"B/D"|"6"|75|"6"|90|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|0.687|"Moderate"|"50"|1|"2979673"
"1169E"|"Sebud, very stony-Lake Creek, stony-Surdal, stony families, complex, 8 to 35 percent slopes"||15|17.5|71|||"None"|"None"|"0"|3.8|6.42|9.48|11|"Well drained"|"Well drained"|"C"||89|"6"|86|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Somewhat limited"|0.556|"Moderate"|"2"|0.977|"2979674"
"1176D"|"Franconi-Kimpton families, complex, 4 to 15 percent slopes"||6|6.1|67|||"None"|"None"|"0"|4.04|6.8|9.16|9.49|"Well drained"|"Well drained"|"C"|"6"|88|"6"|88|"Somewhat limited"|"Very limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Not limited"|0.078|"Moderate"|"3"|0.964|"2979675"
"1175E"|"Owenspring-Cheadle, extremely stony-Rockisland, stony families, complex, 4 to 25 percent slopes"||15|14.6|48|||"None"|"None"|"0"|4.19|7.47|10.89|12.15|"Well drained"|"Well drained"|"C"||100|"6"|75|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Not limited"|0.269|"Severe"|"0"|0.941|"2979676"
"1264G"|"Dryadine, stony-Helmville families, complex, 35 to 70 percent slopes"||50|52.6|76|||"None"|"None"|"0"|3.7|5.75|8.23|9.75|"Well drained"|"Well drained"|"C"||100|"7"|95|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Poor"|"Not rated"|"Very limited"|1|"Severe"|"0"|1|"2979677"
"1268D"|"Worock-Targhee families, complex, 2 to 15 percent slopes, very stony"||8|8|89|||"None"|"None"|"0"|4.01|6.59|10.42|13.47|"Well drained"|"Well drained"|"C"|"6"|88|"6"|88|"Not limited"|"Not limited"|"Not limited"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Poor"|"Not rated"|"Somewhat limited"|0.532|"Moderate"|"3"|0.642|"2979678"
"2260E"|"Elvick-Como, very stony-Chillybu families, complex, 2 to 25 percent slopes"||12|11.7||15|15|"None"|"None"|"15"|4.66|8.35|14.52|17.58|"Somewhat poorly drained"|"Very poorly drained"|"C"||77|"6"|98|"Somewhat limited"|"Somewhat limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Somewhat limited"|"Fair"|"Not rated"|"Not limited"|0.354|"Moderate"|"23"|0.886|"2979679"
"1268F"|"Tigeron, rubbly-Targhee, very bouldery-Como, very stony families, complex, 35 to 60 percent slopes"||47|43.4|89|||"None"|"None"|"0"|3.63|5.72|8.4|9.89|"Well drained"|"Well drained"|"B"||100|"7"|80|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Not rated"|"Very limited"|"Very limited"|"Very limited"|"Very limited"|"Fair"|"Not rated"|"Very limited"|1|"Severe"|"3"|1|"2979680"
