12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26190590"|"28545084"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, gravelly soil is a minor component."|"26190591"|"28545085"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190592"|"28545086"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190593"|"28545087"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26190594"|"28545088"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon, cobbly component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (Dr) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190595"|"28545089"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26190596"|"28545090"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190597"|"28545091"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon, cobbly component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (Dr) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190598"|"28545092"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190599"|"28545093"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190600"|"28545094"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190601"|"28545095"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190602"|"28545096"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190849"|"28545343"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190850"|"28545344"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190851"|"28545345"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190852"|"28545346"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26190853"|"28545347"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190854"|"28545348"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clasoil, greater slope soil is a minor component."|"26190855"|"28545349"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190856"|"28545350"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190857"|"28545351"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190858"|"28545352"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190859"|"28545353"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190860"|"28545354"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dolus component makes up 55 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190603"|"28545097"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"26190604"|"28545098"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 30 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190605"|"28545099"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190606"|"28545100"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dolus component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190607"|"28545101"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190608"|"28545102"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190609"|"28545103"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"26190610"|"28545104"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Doney component makes up 50 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. "|"26190611"|"28545105"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190612"|"28545106"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dolus component makes up 35 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190613"|"28545107"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"26190614"|"28545108"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 60 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26190615"|"28545109"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26190616"|"28545110"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190617"|"28545111"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190618"|"28545112"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190619"|"28545113"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190620"|"28545114"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 60 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191137"|"28545631"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26191138"|"28545632"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191139"|"28545633"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191140"|"28545634"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26191141"|"28545635"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elliston soil is a minor component."|"26190861"|"28545355"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 60 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190862"|"28545356"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26190863"|"28545357"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 25 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190864"|"28545358"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190865"|"28545359"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"26190866"|"28545360"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191142"|"28545636"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191143"|"28545637"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191144"|"28545638"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dolus component makes up 55 percent of the map unit. Slopes are 4 to 8 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 4s. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191136"|"28545630"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191135"|"28545629"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"26191134"|"28545628"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 30 percent of the map unit. Slopes are 4 to 8 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191133"|"28545627"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26191132"|"28545626"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Clasoil, greater slope soil is a minor component."|"26191131"|"28545625"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26191130"|"28545624"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26191129"|"28545623"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191128"|"28545622"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190848"|"28545342"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190847"|"28545341"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"26190846"|"28545340"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190845"|"28545339"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Baggs component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26191127"|"28545621"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs, fsl soil is a minor component."|"26191126"|"28545620"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs, fsl soil is a minor component."|"26190844"|"28545338"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bohnly soil is a minor component."|"26190843"|"28545337"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Baggs component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26190842"|"28545336"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26190841"|"28545335"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elliston soil is a minor component."|"26190840"|"28545334"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Baggs component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26191125"|"28545619"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs, fsl soil is a minor component."|"26191124"|"28545618"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elliston soil is a minor component."|"26191123"|"28545617"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26190739"|"28545233"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flintcreek soil is a minor component."|"26190738"|"28545232"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190737"|"28545231"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mccabe component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"26190736"|"28545230"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Canarway component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26190735"|"28545229"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wetsand component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during May, June, July, August, September. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"26191122"|"28545616"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten, greater slope soil is a minor component."|"26191121"|"28545615"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26191120"|"28545614"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Carten component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191119"|"28545613"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191118"|"28545612"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26191007"|"28545501"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Canarway component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 7e.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191006"|"28545500"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191005"|"28545499"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mccabe component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 7e.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent.  "|"26191004"|"28545498"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flintcreek soil is a minor component."|"26191003"|"28545497"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bohnly component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 15 inches (depth from the mineral surface is 11 inches) during April, May, June, July, August, September. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 6 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"26190839"|"28545333"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dougcliff soil is a minor component."|"26190838"|"28545332"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26190837"|"28545331"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dumps, Mine is a miscellaneous area."|"26191117"|"28545611"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Pits, Gravel is a miscellaneous area."|"26190836"|"28545330"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"26191116"|"28545610"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191115"|"28545609"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26190734"|"28545228"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190733"|"28545227"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bushong component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 12 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 70 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190732"|"28545226"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190341"|"28544835"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190340"|"28544834"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190339"|"28544833"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190338"|"28544832"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190337"|"28544831"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190336"|"28544830"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190335"|"28544829"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190334"|"28544828"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190333"|"28544827"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190332"|"28544826"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slope soil is a minor component."|"26190331"|"28544825"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190330"|"28544824"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26190329"|"28544823"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190328"|"28544822"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190327"|"28544821"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26190326"|"28544820"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverell component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190325"|"28544819"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn soil is a minor component."|"26190324"|"28544818"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26190323"|"28544817"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverell component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190322"|"28544816"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26190321"|"28544815"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 35 to 50 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190320"|"28544814"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190319"|"28544813"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26190318"|"28544812"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190317"|"28544811"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190316"|"28544810"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, gravelly soil is a minor component."|"26191145"|"28545639"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190867"|"28545361"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190868"|"28545362"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190869"|"28545363"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, gravelly soil is a minor component."|"26190870"|"28545364"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190342"|"28544836"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190343"|"28544837"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190344"|"28544838"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190345"|"28544839"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elkner, bouldery soil is a minor component."|"26190346"|"28544840"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190347"|"28544841"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville, greater slope soil is a minor component."|"26190348"|"28544842"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea soil is a minor component."|"26190349"|"28544843"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190350"|"28544844"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190351"|"28544845"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190352"|"28544846"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville soil is a minor component."|"26190353"|"28544847"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea soil is a minor component."|"26190354"|"28544848"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190355"|"28544849"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190356"|"28544850"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relyea component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190357"|"28544851"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190358"|"28544852"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190871"|"28545365"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190872"|"28545366"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190873"|"28545367"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relyea component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190874"|"28545368"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191146"|"28545640"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mocmont component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191147"|"28545641"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"26191148"|"28545642"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mocmont, greater slope soil is a minor component."|"26191149"|"28545643"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190875"|"28545369"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mocmont component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190876"|"28545370"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The MODERATELY DEEP SOILS soil is a minor component."|"26190877"|"28545371"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190878"|"28545372"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek soil is a minor component."|"26190879"|"28545373"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191150"|"28545644"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191151"|"28545645"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191152"|"28545646"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191153"|"28545647"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190621"|"28545115"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190622"|"28545116"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190623"|"28545117"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190624"|"28545118"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monad soil is a minor component."|"26190625"|"28545119"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190626"|"28545120"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26190627"|"28545121"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190628"|"28545122"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Monad soil is a minor component."|"26190629"|"28545123"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190630"|"28545124"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26190631"|"28545125"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evaro component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190632"|"28545126"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190633"|"28545127"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190634"|"28545128"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro, greater slope soil is a minor component."|"26190635"|"28545129"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190636"|"28545130"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evaro component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190637"|"28545131"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190638"|"28545132"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro, greater slope soil is a minor component."|"26190639"|"28545133"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190640"|"28545134"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190641"|"28545135"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evaro component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190880"|"28545374"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190881"|"28545375"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190882"|"28545376"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26190883"|"28545377"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190884"|"28545378"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191154"|"28545648"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191155"|"28545649"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191156"|"28545650"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps, greater slopes soil is a minor component."|"26191157"|"28545651"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps, bouldery soil is a minor component."|"26191158"|"28545652"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191159"|"28545653"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190885"|"28545379"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190886"|"28545380"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190887"|"28545381"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190888"|"28545382"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191160"|"28545654"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191161"|"28545655"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191162"|"28545656"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190729"|"28545223"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dougcliff component makes up 85 percent of the map unit. Slopes are 0 to 2 percent. This component is on depressions. The parent material consists of organic material. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is very high.  Shrink-swell potential is low. This soil is not flooded. It is frequently ponded. A seasonal zone of water saturation is at 3 inches during April, May, June, July, August, September, October. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria.   "|"26190730"|"28545224"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190731"|"28545225"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26190359"|"28544853"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190360"|"28544854"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190361"|"28544855"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Braziel, greater slope soil is a minor component."|"26190362"|"28544856"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190363"|"28544857"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26190364"|"28544858"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190365"|"28544859"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190366"|"28544860"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 30 percent of the map unit. Slopes are 35 to 50 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190367"|"28544861"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert, greater slope soil is a minor component."|"26190368"|"28544862"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26190369"|"28544863"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, greater slope soil is a minor component."|"26190370"|"28544864"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 2 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190371"|"28544865"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26190372"|"28544866"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, cobbly soil is a minor component."|"26190373"|"28544867"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn soil is a minor component."|"26190374"|"28544868"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26190375"|"28544869"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, greater slope soil is a minor component."|"26190376"|"28544870"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190377"|"28544871"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, cobbly soil is a minor component."|"26190378"|"28544872"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, cobbly soil is a minor component."|"26191163"|"28545657"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26191164"|"28545658"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, greater slope soil is a minor component."|"26191165"|"28545659"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 1 within 30 inches of the soil surface."|"26191166"|"28545660"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26191167"|"28545661"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, cobbly soil is a minor component."|"26190889"|"28545383"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190890"|"28545384"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26190891"|"28545385"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 30 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191168"|"28545662"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, cobbly soil is a minor component."|"26191169"|"28545663"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26191170"|"28545664"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs soil is a minor component."|"26190892"|"28545386"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"26190893"|"28545387"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190894"|"28545388"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs soil is a minor component."|"26190642"|"28545136"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190643"|"28545137"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"26190644"|"28545138"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs soil is a minor component."|"26190645"|"28545139"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"26190646"|"28545140"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190647"|"28545141"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs soil is a minor component."|"26190648"|"28545142"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190649"|"28545143"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190650"|"28545144"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190651"|"28545145"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190652"|"28545146"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 45 percent of the map unit. Slopes are 4 to 8 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190653"|"28545147"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190654"|"28545148"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190895"|"28545389"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190896"|"28545390"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190897"|"28545391"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26191171"|"28545665"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191172"|"28545666"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26191173"|"28545667"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, very gravelly soil is a minor component."|"26191008"|"28545502"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26191009"|"28545503"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191010"|"28545504"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, very gravelly soil is a minor component."|"26190740"|"28545234"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26190741"|"28545235"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190742"|"28545236"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, very gravelly soil is a minor component."|"26190194"|"28544688"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190195"|"28544689"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 0 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190898"|"28545392"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, very stony soil is a minor component."|"26190899"|"28545393"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190900"|"28545394"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191174"|"28545668"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26191175"|"28545669"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26191176"|"28545670"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26190196"|"28544690"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw, greater slope soil is a minor component."|"26190197"|"28544691"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Straw component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 2e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190198"|"28544692"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190379"|"28544873"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 20 percent of the map unit. Slopes are 4 to 8 percent. This component is on plains. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190380"|"28544874"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boxwell, channery soil is a minor component."|"26190381"|"28544875"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 65 percent of the map unit. Slopes are 4 to 8 percent. This component is on plains. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190382"|"28544876"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"26190383"|"28544877"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190384"|"28544878"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190385"|"28544879"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"26190386"|"28544880"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 65 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190387"|"28544881"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Boxwell, channery soil is a minor component."|"26190388"|"28544882"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, calcareous soil is a minor component."|"26190389"|"28544883"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Dolus component makes up 45 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190390"|"28544884"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190391"|"28544885"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Castner component makes up 40 percent of the map unit. Slopes are 15 to 45 percent. This component is on hills. The parent material consists of residuum weathered from sandstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190392"|"28544886"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190393"|"28544887"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26190394"|"28544888"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek, greater slope soil is a minor component."|"26190395"|"28544889"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26190396"|"28544890"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190397"|"28544891"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 75 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190901"|"28545395"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26190902"|"28545396"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek, greater slope soil is a minor component."|"26190903"|"28545397"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26190904"|"28545398"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190905"|"28545399"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 75 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191177"|"28545671"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26191178"|"28545672"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26191179"|"28545673"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rumblecreek, greater slope soil is a minor component."|"26191180"|"28545674"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191181"|"28545675"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190906"|"28545400"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ambrant, greater slope soil is a minor component."|"26190907"|"28545401"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190908"|"28545402"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190909"|"28545403"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26190910"|"28545404"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190911"|"28545405"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191182"|"28545676"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191183"|"28545677"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, greater slope soil is a minor component."|"26191184"|"28545678"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26191185"|"28545679"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191186"|"28545680"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191187"|"28545681"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190655"|"28545149"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190656"|"28545150"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190657"|"28545151"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190658"|"28545152"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26190659"|"28545153"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26190660"|"28545154"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190661"|"28545155"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26190662"|"28545156"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190663"|"28545157"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190664"|"28545158"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190665"|"28545159"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26190666"|"28545160"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190667"|"28545161"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 4 to 25 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191188"|"28545682"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191189"|"28545683"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191190"|"28545684"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191191"|"28545685"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 25 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190912"|"28545406"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190913"|"28545407"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190914"|"28545408"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190915"|"28545409"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderatly deep soils soil is a minor component."|"26190916"|"28545410"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191192"|"28545686"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderatly deep soils soil is a minor component."|"26191193"|"28545687"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191194"|"28545688"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191195"|"28545689"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190917"|"28545411"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190918"|"28545412"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190919"|"28545413"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190920"|"28545414"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slopes soil is a minor component."|"26190921"|"28545415"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190922"|"28545416"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190398"|"28544892"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190399"|"28544893"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190400"|"28544894"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190401"|"28544895"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka, greater slopes soil is a minor component."|"26190402"|"28544896"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190403"|"28544897"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, very gravelly soil is a minor component."|"26190199"|"28544693"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda soil is a minor component."|"26190200"|"28544694"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190201"|"28544695"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, cobbly soil is a minor component."|"26190202"|"28544696"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell, gravelly soil is a minor component."|"26190203"|"28544697"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney, clay loam component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190204"|"28544698"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell, cobbly soil is a minor component."|"26190205"|"28544699"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190743"|"28545237"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"26190744"|"28545238"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190745"|"28545239"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"26190404"|"28544898"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190405"|"28544899"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon, cobbly soil is a minor component."|"26190406"|"28544900"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell, cobbly soil is a minor component."|"26190407"|"28544901"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell, greater slope soil is a minor component."|"26190408"|"28544902"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten soil is a minor component."|"26190409"|"28544903"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beaverell component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA134MT Shallow to Gravel (SwGr) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6s. Irrigated land capability classification is 6e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190410"|"28544904"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Anaconda component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190411"|"28544905"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"26190412"|"28544906"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"26190413"|"28544907"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, cobbly soil is a minor component."|"26190414"|"28544908"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"26190923"|"28545417"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell soil is a minor component."|"26190924"|"28545418"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 60 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. The soil has a very slightly saline horizon within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 2 within 30 inches of the soil surface."|"26190925"|"28545419"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Anaconda component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190926"|"28545420"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26191196"|"28545690"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"26191197"|"28545691"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slopes soil is a minor component."|"26191198"|"28545692"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26191199"|"28545693"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26190927"|"28545421"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26190928"|"28545422"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190929"|"28545423"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slope soil is a minor component."|"26190930"|"28545424"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26191200"|"28545694"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, very cobbly soil is a minor component."|"26191201"|"28545695"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slopes soil is a minor component."|"26191202"|"28545696"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26191203"|"28545697"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191204"|"28545698"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26190931"|"28545425"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190932"|"28545426"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190933"|"28545427"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slope soil is a minor component."|"26190934"|"28545428"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, very cobbly soil is a minor component."|"26190935"|"28545429"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190668"|"28545162"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"26190669"|"28545163"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190670"|"28545164"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190671"|"28545165"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190672"|"28545166"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190673"|"28545167"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190674"|"28545168"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190675"|"28545169"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190676"|"28545170"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190677"|"28545171"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190678"|"28545172"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190679"|"28545173"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cetrack component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"26191011"|"28545505"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack, cobbly soil is a minor component."|"26191012"|"28545506"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack, greater slope soil is a minor component."|"26191013"|"28545507"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26191014"|"28545508"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack, calcareous soil is a minor component."|"26191015"|"28545509"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26191016"|"28545510"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cetrack component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent.  "|"26190746"|"28545240"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190747"|"28545241"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack, cobbly soil is a minor component."|"26190748"|"28545242"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack, greater slope soil is a minor component."|"26190749"|"28545243"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack, calcareous soil is a minor component."|"26190750"|"28545244"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 18 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190680"|"28545174"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, extremely cobbly soil is a minor component."|"26190681"|"28545175"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190682"|"28545176"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans, valleys, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190683"|"28545177"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans, valleys, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190684"|"28545178"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, greater slopes soil is a minor component."|"26190685"|"28545179"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, greater slope soil is a minor component."|"26190936"|"28545430"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190937"|"28545431"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans. The parent material consists of calcareous clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190938"|"28545432"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190939"|"28545433"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, extremely cobbly soil is a minor component."|"26190940"|"28545434"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190941"|"28545435"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, very gravelly soil is a minor component."|"26191205"|"28545699"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale, cobbly component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191206"|"28545700"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26191207"|"28545701"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191208"|"28545702"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, very gravelly soil is a minor component."|"26190942"|"28545436"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190943"|"28545437"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale, cobbly component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190944"|"28545438"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190945"|"28545439"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26190489"|"28544983"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Anaconda, very gravelly soil is a minor component."|"26190490"|"28544984"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Anaconda component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190491"|"28544985"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, clay loam soil is a minor component."|"26190492"|"28544986"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 25 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190493"|"28544987"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 60 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190494"|"28544988"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beaverell, cobbly soil is a minor component."|"26190495"|"28544989"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 60 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190496"|"28544990"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"26190497"|"28544991"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 25 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190498"|"28544992"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cetrack soil is a minor component."|"26190499"|"28544993"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190500"|"28544994"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Varney component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190501"|"28544995"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney, clay loam soil is a minor component."|"26190502"|"28544996"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, cobbly clay loam soil is a minor component."|"26190503"|"28544997"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 30 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26191209"|"28545703"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191210"|"28545704"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26191211"|"28545705"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26191212"|"28545706"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.   "|"26191213"|"28545707"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen, greater slope soil is a minor component."|"26191214"|"28545708"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26190415"|"28544909"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190416"|"28544910"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 30 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190417"|"28544911"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190418"|"28544912"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 55 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190419"|"28544913"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka, greater slope soil is a minor component."|"26190420"|"28544914"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Wildgen component makes up 55 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190421"|"28544915"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka, greater slope soil is a minor component."|"26190422"|"28544916"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26190423"|"28544917"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Courville soil is a minor component."|"26190424"|"28544918"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 30 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190425"|"28544919"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190426"|"28544920"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, gravelly soil is a minor component."|"26190427"|"28544921"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26190428"|"28544922"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190429"|"28544923"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190430"|"28544924"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190431"|"28544925"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26190432"|"28544926"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190433"|"28544927"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190434"|"28544928"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190435"|"28544929"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, gravelly soil is a minor component."|"26190436"|"28544930"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191215"|"28545709"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191216"|"28545710"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ovando soil is a minor component."|"26191217"|"28545711"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"26191218"|"28545712"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190946"|"28545440"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"26190947"|"28545441"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ovando soil is a minor component."|"26190948"|"28545442"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190949"|"28545443"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191219"|"28545713"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The MODERATELY DEEP SOILS (Ellena) soil is a minor component."|"26191220"|"28545714"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191221"|"28545715"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"26191222"|"28545716"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ovando soil is a minor component."|"26191223"|"28545717"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190950"|"28545444"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea soil is a minor component."|"26190951"|"28545445"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190952"|"28545446"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190953"|"28545447"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190954"|"28545448"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190955"|"28545449"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190686"|"28545180"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190687"|"28545181"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190688"|"28545182"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190689"|"28545183"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190690"|"28545184"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danaher component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium and/or colluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190691"|"28545185"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190692"|"28545186"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher, greater slope soil is a minor component."|"26190693"|"28545187"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190694"|"28545188"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190695"|"28545189"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190696"|"28545190"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190697"|"28545191"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190698"|"28545192"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190699"|"28545193"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190700"|"28545194"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190701"|"28545195"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190956"|"28545450"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190957"|"28545451"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190958"|"28545452"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190959"|"28545453"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190960"|"28545454"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26190961"|"28545455"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191224"|"28545718"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191225"|"28545719"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191226"|"28545720"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191227"|"28545721"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191228"|"28545722"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191229"|"28545723"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190962"|"28545456"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190963"|"28545457"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190964"|"28545458"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26190965"|"28545459"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190966"|"28545460"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190967"|"28545461"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191230"|"28545724"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26191231"|"28545725"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26191232"|"28545726"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191233"|"28545727"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26191234"|"28545728"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26191235"|"28545729"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190968"|"28545462"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190969"|"28545463"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190970"|"28545464"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190971"|"28545465"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190972"|"28545466"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190973"|"28545467"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190974"|"28545468"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190437"|"28544931"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190438"|"28544932"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190439"|"28544933"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190440"|"28544934"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26190441"|"28544935"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190442"|"28544936"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190443"|"28544937"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26190444"|"28544938"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190445"|"28544939"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190446"|"28544940"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26190447"|"28544941"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190448"|"28544942"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"26191017"|"28545511"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP804MT Limy Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191018"|"28545512"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191019"|"28545513"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, greater slope soil is a minor component."|"26191020"|"28545514"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26191021"|"28545515"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190751"|"28545245"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, greater slope soil is a minor component."|"26190752"|"28545246"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190753"|"28545247"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"26190754"|"28545248"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP804MT Limy Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190755"|"28545249"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26191022"|"28545516"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP804MT Limy Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191023"|"28545517"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191024"|"28545518"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"26191025"|"28545519"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, greater slope soil is a minor component."|"26191026"|"28545520"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"26190756"|"28545250"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans. The parent material consists of calcareous gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP804MT Limy Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26190757"|"28545251"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190758"|"28545252"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190759"|"28545253"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, greater slope soil is a minor component."|"26190760"|"28545254"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nythar soil is a minor component."|"26190470"|"28544964"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slickens is a miscellaneous area."|"26190471"|"28544965"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190472"|"28544966"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquents component makes up 55 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June.  This component is in the R044BP801MT Bottomland ecological site.   This soil meets hydric criteria.   "|"26190473"|"28544967"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26190474"|"28544968"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26190206"|"28544700"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fergus component makes up 75 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190207"|"28544701"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elliston soil is a minor component."|"26190208"|"28544702"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Fergus, greater slope soil is a minor component."|"26190209"|"28544703"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190210"|"28544704"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190211"|"28544705"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, cobbly soil is a minor component."|"26190212"|"28544706"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190213"|"28544707"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26190214"|"28544708"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190215"|"28544709"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190216"|"28544710"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, stony soil is a minor component."|"26190217"|"28544711"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26190218"|"28544712"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190219"|"28544713"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, cobbly soil is a minor component."|"26190220"|"28544714"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190221"|"28544715"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190222"|"28544716"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190223"|"28544717"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitlash soil is a minor component."|"26190224"|"28544718"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191027"|"28545521"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans. The parent material consists of alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191028"|"28545522"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitlash soil is a minor component."|"26191029"|"28545523"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190761"|"28545255"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"26190762"|"28545256"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"26190763"|"28545257"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Doney soil is a minor component."|"26191030"|"28545524"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191031"|"28545525"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham soil is a minor component."|"26191032"|"28545526"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26190449"|"28544943"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26190450"|"28544944"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Carten component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190451"|"28544945"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten, cobbly soil is a minor component."|"26190452"|"28544946"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26190453"|"28544947"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26190454"|"28544948"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gregson component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26190455"|"28544949"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26190456"|"28544950"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26190975"|"28545469"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nythar soil is a minor component."|"26190976"|"28545470"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonview soil is a minor component."|"26190977"|"28545471"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26190978"|"28545472"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saypo component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 31 inches) during March, April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R043BP801MT Bottomland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"26190979"|"28545473"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191236"|"28545730"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Braziel, greater slope soil is a minor component."|"26191237"|"28545731"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 60 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"26191238"|"28545732"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26191239"|"28545733"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26191240"|"28545734"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26191241"|"28545735"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191242"|"28545736"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190980"|"28545474"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, very stony soil is a minor component."|"26190981"|"28545475"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert, very stony component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190982"|"28545476"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26190983"|"28545477"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, very stony soil is a minor component."|"26190984"|"28545478"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Braziel, greater slopes, very stony soil is a minor component."|"26190985"|"28545479"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 60 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains, mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26190986"|"28545480"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191243"|"28545737"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB136MT Shallow Loamy (SwLo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191244"|"28545738"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, very stony soil is a minor component."|"26191245"|"28545739"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crackerville soil is a minor component."|"26191246"|"28545740"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert, greater slope soil is a minor component."|"26191247"|"28545741"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 60 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191248"|"28545742"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26191249"|"28545743"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26190702"|"28545196"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26190703"|"28545197"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson, very cobbly soil is a minor component."|"26190704"|"28545198"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gregson component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26190705"|"28545199"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo, saline soil is a minor component."|"26190706"|"28545200"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saypo component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 31 inches) during March, April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"26190707"|"28545201"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26190708"|"28545202"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonview soil is a minor component."|"26190709"|"28545203"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26190710"|"28545204"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 50 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190711"|"28545205"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, cobbly soil is a minor component."|"26190712"|"28545206"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 35 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190713"|"28545207"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect soil is a minor component."|"26190714"|"28545208"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 50 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190715"|"28545209"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190716"|"28545210"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26190717"|"28545211"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 35 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190718"|"28545212"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, cobbly soil is a minor component."|"26190719"|"28545213"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191250"|"28545744"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, cobbly soil is a minor component."|"26191251"|"28545745"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191252"|"28545746"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect soil is a minor component."|"26191253"|"28545747"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26191254"|"28545748"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26190987"|"28545481"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26190988"|"28545482"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect soil is a minor component."|"26190989"|"28545483"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"26190990"|"28545484"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slopes soil is a minor component."|"26190991"|"28545485"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26191255"|"28545749"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slope soil is a minor component."|"26191256"|"28545750"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26191257"|"28545751"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"26191258"|"28545752"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191259"|"28545753"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hoyt component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26190992"|"28545486"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt, greater slope soil is a minor component."|"26190993"|"28545487"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190994"|"28545488"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Hoyt component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190457"|"28544951"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt, greater slope soil is a minor component."|"26190458"|"28544952"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190459"|"28544953"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190764"|"28545258"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redchief component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26190765"|"28545259"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190766"|"28545260"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190504"|"28544998"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redchief component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190505"|"28544999"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190506"|"28545000"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley, cobbly component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP819MT Upland Sagebrush Shrubland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190460"|"28544954"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winspect, cobbly soil is a minor component."|"26190461"|"28544955"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190462"|"28544956"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26190507"|"28545001"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190508"|"28545002"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, cobbly soil is a minor component."|"26190509"|"28545003"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, greater slope soil is a minor component."|"26190510"|"28545004"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26190511"|"28545005"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26190512"|"28545006"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26190513"|"28545007"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, greater slope soil is a minor component."|"26190514"|"28545008"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, cobbly soil is a minor component."|"26190515"|"28545009"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190516"|"28545010"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, cobbly soil is a minor component."|"26190517"|"28545011"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy, greater slope soil is a minor component."|"26190518"|"28545012"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190519"|"28545013"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190520"|"28545014"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26190521"|"28545015"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elliston soil is a minor component."|"26190463"|"28544957"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Baggs component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26190464"|"28544958"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs, greater slope soil is a minor component."|"26190465"|"28544959"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26190466"|"28544960"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190467"|"28544961"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190468"|"28544962"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190469"|"28544963"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191260"|"28545754"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191261"|"28545755"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26191262"|"28545756"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relyea component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190995"|"28545489"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190996"|"28545490"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190997"|"28545491"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea, greater slope soil is a minor component."|"26190998"|"28545492"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Relyea component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191263"|"28545757"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191264"|"28545758"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26191265"|"28545759"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville, greater slope soil is a minor component."|"26191266"|"28545760"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190999"|"28545493"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26191000"|"28545494"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191001"|"28545495"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Soils with dark color surface soil is a minor component."|"26191002"|"28545496"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190720"|"28545214"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190721"|"28545215"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190722"|"28545216"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190723"|"28545217"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190724"|"28545218"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190725"|"28545219"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190726"|"28545220"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190727"|"28545221"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26190728"|"28545222"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191711"|"28546205"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191712"|"28546206"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191713"|"28546207"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191267"|"28545761"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 85 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191268"|"28545762"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191269"|"28545763"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollet, greater slope soil is a minor component."|"26190767"|"28545261"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollet component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26190768"|"28545262"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redchief soil is a minor component."|"26190769"|"28545263"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mollet component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of alluvium and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191033"|"28545527"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollet, greater slope soil is a minor component."|"26191034"|"28545528"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redchief soil is a minor component."|"26191035"|"28545529"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191714"|"28546208"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191715"|"28546209"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191716"|"28546210"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191717"|"28546211"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191718"|"28546212"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191270"|"28545764"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191271"|"28545765"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191272"|"28545766"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191273"|"28545767"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191274"|"28545768"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191419"|"28545913"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191420"|"28545914"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191421"|"28545915"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191422"|"28545916"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191423"|"28545917"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26190770"|"28545264"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190771"|"28545265"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, cobbly soil is a minor component."|"26190772"|"28545266"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190773"|"28545267"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190774"|"28545268"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26191036"|"28545530"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191037"|"28545531"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slope soil is a minor component."|"26191038"|"28545532"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26191039"|"28545533"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, cobbly soil is a minor component."|"26191040"|"28545534"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danvers component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190225"|"28544719"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190226"|"28544720"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190227"|"28544721"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, cobbly soil is a minor component."|"26190228"|"28544722"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers, greater slopes soil is a minor component."|"26190229"|"28544723"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nythar soil is a minor component."|"26190475"|"28544969"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190476"|"28544970"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slickens is a miscellaneous area."|"26190477"|"28544971"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Aquents component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June.  This component is in the R044BP801MT Bottomland ecological site.   This soil meets hydric criteria.   "|"26190478"|"28544972"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26190479"|"28544973"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"26190230"|"28544724"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollet soil is a minor component."|"26190231"|"28544725"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26190232"|"28544726"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"26190233"|"28544727"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mollet soil is a minor component."|"26190234"|"28544728"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26190235"|"28544729"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190236"|"28544730"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190237"|"28544731"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"26190238"|"28544732"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190239"|"28544733"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slope soil is a minor component."|"26190775"|"28545269"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, cobbly soil is a minor component."|"26190776"|"28545270"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190777"|"28545271"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190778"|"28545272"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191041"|"28545535"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26191042"|"28545536"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slope soil is a minor component."|"26191043"|"28545537"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26191044"|"28545538"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, cobbly soil is a minor component."|"26191045"|"28545539"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, calcareous soil is a minor component."|"26190779"|"28545273"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slopes soil is a minor component."|"26190780"|"28545274"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190781"|"28545275"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, cobbly soil is a minor component."|"26190782"|"28545276"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190783"|"28545277"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, greater slope soil is a minor component."|"26190522"|"28545016"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190523"|"28545017"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, gravelly soil is a minor component."|"26190524"|"28545018"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190525"|"28545019"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190526"|"28545020"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190527"|"28545021"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, greater slope soil is a minor component."|"26190528"|"28545022"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26190529"|"28545023"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26190530"|"28545024"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190531"|"28545025"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26190532"|"28545026"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, greater slope soil is a minor component."|"26190533"|"28545027"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Carten component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191424"|"28545918"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191425"|"28545919"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191426"|"28545920"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gregson component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26191427"|"28545921"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191428"|"28545922"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo, saline soil is a minor component."|"26191429"|"28545923"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saypo component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 31 inches) during March, April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"26191430"|"28545924"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26191431"|"28545925"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonview soil is a minor component."|"26191432"|"28545926"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slope soil is a minor component."|"26190534"|"28545028"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190535"|"28545029"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190536"|"28545030"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190537"|"28545031"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 45 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190538"|"28545032"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26190539"|"28545033"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Martinsdale component makes up 40 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190540"|"28545034"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut, greater slope soil is a minor component."|"26190541"|"28545035"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191275"|"28545769"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slopes soil is a minor component."|"26191276"|"28545770"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"26191277"|"28545771"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26191278"|"28545772"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Shawmut soil is a minor component."|"26191719"|"28546213"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191720"|"28546214"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 85 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191721"|"28546215"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slope soil is a minor component."|"26191722"|"28546216"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191279"|"28545773"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26191280"|"28545774"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson, cobbly soil is a minor component."|"26191281"|"28545775"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gregson component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26191282"|"28545776"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonview soil is a minor component."|"26191723"|"28546217"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26191724"|"28546218"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Saypo component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of fine-loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 31 inches) during March, April, May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 33 percent. There are no saline horizons within 30 inches of the soil surface. The soil has a maximum sodium adsorption ratio of 3 within 30 inches of the soil surface."|"26191725"|"28546219"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo, saline soil is a minor component."|"26191726"|"28546220"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26191568"|"28546062"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo, saline soil is a minor component."|"26191569"|"28546063"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kleinschmidt component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191570"|"28546064"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191571"|"28546065"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Marcott component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of clayey alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during May, June, July. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. The soil has a slightly saline horizon within 30 inches of the soil surface. "|"26191572"|"28546066"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turrah soil is a minor component."|"26191573"|"28546067"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten soil is a minor component."|"26191574"|"28546068"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26191575"|"28546069"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191046"|"28545540"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26191047"|"28545541"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26191048"|"28545542"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderately deep soils soil is a minor component."|"26191049"|"28545543"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderately deep soils soil is a minor component."|"26190784"|"28545278"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26190785"|"28545279"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190786"|"28545280"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP820MT Upland Shrubland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190787"|"28545281"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley soil is a minor component."|"26191576"|"28546070"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Staad soil is a minor component."|"26191577"|"28546071"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 85 percent of the map unit. Slopes are 8 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 20 percent.  "|"26191578"|"28546072"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191579"|"28546073"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191580"|"28546074"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191581"|"28546075"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crackerville component makes up 35 percent of the map unit. Slopes are 4 to 8 percent. This component is on mountains. The parent material consists of residuum and/or colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic,  inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191582"|"28546076"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert soil is a minor component."|"26191583"|"28546077"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 50 percent of the map unit. Slopes are 4 to 8 percent. This component is on mountains. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26191584"|"28546078"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, stony soil is a minor component."|"26191585"|"28546079"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191586"|"28546080"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria.   "|"26191587"|"28546081"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, stony soil is a minor component."|"26191588"|"28546082"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crackerville component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 38 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191589"|"28546083"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert soil is a minor component."|"26191590"|"28546084"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, stony soil is a minor component."|"26191283"|"28545777"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191284"|"28545778"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191285"|"28545779"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert soil is a minor component."|"26191286"|"28545780"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crackerville component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from granite. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 38 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191287"|"28545781"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kleinschmidt component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191727"|"28546221"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191728"|"28546222"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26191729"|"28546223"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo, saline soil is a minor component."|"26191730"|"28546224"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Carten component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on outwash plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during April, May, June, July. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 3w. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191288"|"28545782"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191289"|"28545783"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191433"|"28545927"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Comad, greater slope soil is a minor component."|"26191434"|"28545928"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 65 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191435"|"28545929"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191436"|"28545930"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191437"|"28545931"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26191438"|"28545932"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 65 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191439"|"28545933"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191440"|"28545934"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"26191441"|"28545935"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coben, cobbly soil is a minor component."|"26191050"|"28545544"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26191051"|"28545545"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coben, greater slope soil is a minor component."|"26191052"|"28545546"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Coben component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191053"|"28545547"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Coben component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190788"|"28545282"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coben, greater slope soil is a minor component."|"26190789"|"28545283"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coben, cobbly soil is a minor component."|"26190790"|"28545284"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190791"|"28545285"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190240"|"28544734"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26190241"|"28544735"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Coben component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190242"|"28544736"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Coben, cobbly soil is a minor component."|"26190243"|"28544737"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191442"|"28545936"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191443"|"28545937"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26191444"|"28545938"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26191445"|"28545939"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26191446"|"28545940"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191447"|"28545941"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191448"|"28545942"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191449"|"28545943"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26191450"|"28545944"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26191451"|"28545945"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26191452"|"28545946"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26191453"|"28545947"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191731"|"28546225"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191732"|"28546226"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191733"|"28546227"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26191734"|"28546228"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26191735"|"28546229"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191736"|"28546230"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Silverchief component makes up 45 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"26191290"|"28545784"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191291"|"28545785"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191292"|"28545786"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191737"|"28546231"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191738"|"28546232"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191739"|"28546233"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Silverchief component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent.  "|"26191740"|"28546234"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190244"|"28544738"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26190245"|"28544739"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, greater slope soil is a minor component."|"26190246"|"28544740"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces, alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190247"|"28544741"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, gravelly soil is a minor component."|"26190248"|"28544742"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, cobbly soil is a minor component."|"26190249"|"28544743"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on alluvial fans, stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190250"|"28544744"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190251"|"28544745"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, greater slope soil is a minor component."|"26190252"|"28544746"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26190253"|"28544747"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on alluvial fans. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BB032MT Loamy (Lo) LRU 01 Subset B ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190254"|"28544748"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, cobbly soil is a minor component."|"26190255"|"28544749"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26190256"|"28544750"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, greater slope soil is a minor component."|"26190257"|"28544751"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Quigley, calcareous soil is a minor component."|"26190258"|"28544752"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26191293"|"28545787"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191294"|"28545788"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bushong component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 17 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191295"|"28545789"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blossberg component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of loamy alluvium over sandy and gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191591"|"28546085"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tetonview soil is a minor component."|"26191592"|"28546086"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flintcreek soil is a minor component."|"26191593"|"28546087"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191594"|"28546088"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tetonview component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP815MT Subirrigated Grassland Group ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191595"|"28546089"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nythar soil is a minor component."|"26191596"|"28546090"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo, saline soil is a minor component."|"26191597"|"28546091"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191598"|"28546092"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191599"|"28546093"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26191600"|"28546094"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191601"|"28546095"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sixbeacon soil is a minor component."|"26191602"|"28546096"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26191603"|"28546097"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flintcreek soil is a minor component."|"26191604"|"28546098"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poronto component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"26191605"|"28546099"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten, calcareous soil is a minor component."|"26191606"|"28546100"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Straw component makes up 20 percent of the map unit. Slopes are 2 to 8 percent. This component is on drainageways. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190792"|"28545286"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley component makes up 55 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190793"|"28545287"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw, silty subsoil soil is a minor component."|"26190794"|"28545288"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26190795"|"28545289"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26191054"|"28545548"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Quigley component makes up 55 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191055"|"28545549"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Straw component makes up 20 percent of the map unit. Slopes are 8 to 25 percent. This component is on drainageways. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191056"|"28545550"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191057"|"28545551"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26191607"|"28546101"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26191608"|"28546102"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191609"|"28546103"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, ex bouldery component makes up 85 percent of the map unit. Slopes are 8 to 50 percent. This component is on moraines. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7s. Irrigated land capability classification is 7s. This soil does not meet hydric criteria.   "|"26191610"|"28546104"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191611"|"28546105"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nythar soil is a minor component."|"26191296"|"28545790"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Turrah component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on stream terraces. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during May, June, July. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria.   "|"26191297"|"28545791"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten, calcareous soil is a minor component."|"26191298"|"28545792"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191299"|"28545793"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191741"|"28546235"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191742"|"28546236"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191743"|"28546237"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 25 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of calcareous till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191744"|"28546238"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26191745"|"28546239"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 50 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191746"|"28546240"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 25 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of calcareous alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191300"|"28545794"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191301"|"28545795"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191302"|"28545796"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 50 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191303"|"28545797"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191304"|"28545798"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26191305"|"28545799"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26191747"|"28546241"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winspect component makes up 25 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of calcareous alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191748"|"28546242"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191749"|"28546243"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Shawmut component makes up 50 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP804MT Limy Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191750"|"28546244"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191751"|"28546245"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191752"|"28546246"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on plains. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191058"|"28545552"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dolus soil is a minor component."|"26191059"|"28545553"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191060"|"28545554"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"26191061"|"28545555"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tanna component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is high. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190542"|"28545036"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cabbart soil is a minor component."|"26190543"|"28545037"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190544"|"28545038"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Comad component makes up 65 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191454"|"28545948"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191455"|"28545949"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elve soil is a minor component."|"26191456"|"28545950"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"26191457"|"28545951"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elkner soil is a minor component."|"26191458"|"28545952"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191459"|"28545953"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ovando soil is a minor component."|"26191460"|"28545954"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26191461"|"28545955"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 90 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191462"|"28545956"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ovando soil is a minor component."|"26191463"|"28545957"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191464"|"28545958"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26191465"|"28545959"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26191466"|"28545960"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191467"|"28545961"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191468"|"28545962"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191469"|"28545963"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191470"|"28545964"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26191471"|"28545965"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26191472"|"28545966"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191473"|"28545967"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191474"|"28545968"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191475"|"28545969"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26191306"|"28545800"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191307"|"28545801"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191308"|"28545802"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191309"|"28545803"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191310"|"28545804"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191311"|"28545805"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191753"|"28546247"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191754"|"28546248"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191755"|"28546249"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191756"|"28546250"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191757"|"28546251"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191312"|"28545806"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191313"|"28545807"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191314"|"28545808"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191315"|"28545809"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191316"|"28545810"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191317"|"28545811"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 85 percent of the map unit. Slopes are 4 to 8 percent. This component is on plains. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 3e. Irrigated land capability classification is 3e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190545"|"28545039"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"26190546"|"28545040"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190547"|"28545041"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tanna soil is a minor component."|"26190548"|"28545042"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190549"|"28545043"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190550"|"28545044"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Boxwell component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190551"|"28545045"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Castner soil is a minor component."|"26190552"|"28545046"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elliston component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of loamy alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches (depth from the mineral surface is 32 inches) during April, May, June, July. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190480"|"28544974"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26190481"|"28544975"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Baggs soil is a minor component."|"26190482"|"28544976"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26190483"|"28544977"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Endoaquolls component makes up 40 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during April, May, June, July.  This component is in the R044BP801MT Bottomland ecological site.   This soil meets hydric criteria.   "|"26190484"|"28544978"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26190485"|"28544979"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquents component makes up 45 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches.   Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 12 inches during April, May, June, July.  This component is in the R044BP801MT Bottomland ecological site.   This soil meets hydric criteria.   "|"26190486"|"28544980"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26190487"|"28544981"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26190488"|"28544982"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 85 percent of the map unit. Slopes are 2 to 8 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191062"|"28545556"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191063"|"28545557"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"26191064"|"28545558"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26191065"|"28545559"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 85 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190796"|"28545290"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26190797"|"28545291"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190798"|"28545292"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winfall component makes up 85 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191066"|"28545560"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191067"|"28545561"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blackcreek soil is a minor component."|"26191068"|"28545562"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191069"|"28545563"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191758"|"28546252"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blossberg component makes up 40 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191759"|"28546253"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tetonview component makes up 45 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 5w.  This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191760"|"28546254"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Nythar soil is a minor component."|"26191761"|"28546255"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26191612"|"28546106"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 50 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191613"|"28546107"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191614"|"28546108"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, very cobbly component makes up 20 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191615"|"28546109"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191616"|"28546110"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191617"|"28546111"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma, very cobbly component makes up 20 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of outwash. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191618"|"28546112"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Straw soil is a minor component."|"26191619"|"28546113"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Braziel component makes up 50 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191620"|"28546114"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Poronto soil is a minor component."|"26191621"|"28546115"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191622"|"28546116"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191623"|"28546117"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tolbert soil is a minor component."|"26191624"|"28546118"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma soil is a minor component."|"26191625"|"28546119"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crackerville component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of residuum and/or colluvium derived from granite. Depth to a root restrictive layer, bedrock, paralithic,  inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191626"|"28546120"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Clasoil component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191627"|"28546121"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, stony soil is a minor component."|"26191628"|"28546122"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191629"|"28546123"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191630"|"28546124"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191631"|"28546125"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191632"|"28546126"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26191633"|"28546127"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191634"|"28546128"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Ovando, greater slope soil is a minor component."|"26191635"|"28546129"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 25 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191762"|"28546256"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191763"|"28546257"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191764"|"28546258"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26191765"|"28546259"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191766"|"28546260"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191318"|"28545812"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191319"|"28545813"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191320"|"28545814"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191321"|"28545815"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191767"|"28546261"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191768"|"28546262"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191769"|"28546263"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191770"|"28546264"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191322"|"28545816"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191323"|"28545817"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191324"|"28545818"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191325"|"28545819"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191476"|"28545970"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191477"|"28545971"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191478"|"28545972"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191479"|"28545973"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 65 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191480"|"28545974"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lap soil is a minor component."|"26191481"|"28545975"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191482"|"28545976"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191483"|"28545977"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191484"|"28545978"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191485"|"28545979"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slope soil is a minor component."|"26191486"|"28545980"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 15 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191487"|"28545981"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191488"|"28545982"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 55 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191489"|"28545983"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191490"|"28545984"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191491"|"28545985"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191492"|"28545986"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191493"|"28545987"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slope soil is a minor component."|"26191494"|"28545988"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 15 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191495"|"28545989"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191496"|"28545990"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester soil is a minor component."|"26190799"|"28545293"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190800"|"28545294"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester, st component makes up 35 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190801"|"28545295"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 50 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6s.  This soil does not meet hydric criteria.   "|"26190802"|"28545296"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190803"|"28545297"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190259"|"28544753"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190260"|"28544754"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, gravelly soil is a minor component."|"26190261"|"28544755"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190262"|"28544756"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190263"|"28544757"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190264"|"28544758"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190265"|"28544759"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ambrant component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190266"|"28544760"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rochester component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190267"|"28544761"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rochester, gravelly soil is a minor component."|"26190268"|"28544762"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elkner, gravelly soil is a minor component."|"26190269"|"28544763"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190270"|"28544764"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190271"|"28544765"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190272"|"28544766"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190273"|"28544767"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elkner, gravelly soil is a minor component."|"26190274"|"28544768"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkner component makes up 45 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190275"|"28544769"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190276"|"28544770"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Ovando component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from granite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26190277"|"28544771"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190278"|"28544772"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, calcareous soil is a minor component."|"26191326"|"28545820"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon, cobbly component makes up 30 percent of the map unit. Slopes are 15 to 35 percent. This component is on alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (Dr) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191327"|"28545821"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"26191328"|"28545822"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, greater slope soil is a minor component."|"26191329"|"28545823"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on stream terraces, alluvial fans. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191330"|"28545824"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sixbeacon, cobbly component makes up 30 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans. The parent material consists of gravelly alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA036MT Droughty (Dr) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191771"|"28546265"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Conn, calcareous soil is a minor component."|"26191772"|"28546266"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Varney soil is a minor component."|"26191773"|"28546267"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Conn component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on alluvial fans, stream terraces. The parent material consists of calcareous alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BA032MT Loamy (Lo) LRU 01 Subset A ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 28 percent.  "|"26191774"|"28546268"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190279"|"28544773"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Helmville soil is a minor component."|"26190280"|"28544774"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190281"|"28544775"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191070"|"28545564"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26191071"|"28545565"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191072"|"28545566"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190804"|"28545298"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190805"|"28545299"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190806"|"28545300"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turrah soil is a minor component."|"26191331"|"28545825"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26191332"|"28545826"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Carten soil is a minor component."|"26191333"|"28545827"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flintcreek soil is a minor component."|"26191334"|"28545828"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bushong component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 17 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191335"|"28545829"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Flintcreek soil is a minor component."|"26191775"|"28546269"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26191776"|"28546270"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Gregson soil is a minor component."|"26191777"|"28546271"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dougcliff soil is a minor component."|"26191778"|"28546272"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turrah soil is a minor component."|"26191779"|"28546273"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Blossberg component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June, July. Organic matter content in the surface horizon is about 5 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 3w. Irrigated land capability classification is 3w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 8 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191780"|"28546274"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Turrah soil is a minor component."|"26191336"|"28545830"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191337"|"28545831"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dougcliff soil is a minor component."|"26191338"|"28545832"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191339"|"28545833"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tetonview component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches during April, May, June. Organic matter content in the surface horizon is about 4 percent. This component is in the R044BP815MT Subirrigated Grassland ecological site. Nonirrigated land capability classification is 4w. Irrigated land capability classification is 4w. This soil meets hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 25 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191340"|"28545834"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26191341"|"28545835"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191636"|"28546130"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26191637"|"28546131"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Blossberg soil is a minor component."|"26191638"|"28546132"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kleinschmidt soil is a minor component."|"26191639"|"28546133"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Poronto component makes up 85 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 15 inches) during April, May, June, July, August. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"26191640"|"28546134"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191641"|"28546135"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191642"|"28546136"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slope soil is a minor component."|"26191643"|"28546137"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191644"|"28546138"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Perma, greater slope soil is a minor component."|"26191645"|"28546139"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitlash component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191646"|"28546140"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Perma component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191647"|"28546141"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191648"|"28546142"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, greater slope soil is a minor component."|"26191649"|"28546143"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191650"|"28546144"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 65 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191651"|"28546145"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191652"|"28546146"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Lap component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from limestone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP811MT Shallow Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191342"|"28545836"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191343"|"28545837"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Windham component makes up 65 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP819MT Upland Sagebrush Shrubland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 50 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191344"|"28545838"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Windham, greater slope soil is a minor component."|"26191345"|"28545839"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 90 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26190807"|"28545301"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow, greater slopes soil is a minor component."|"26190808"|"28545302"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190553"|"28545047"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 90 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190554"|"28545048"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redchief component makes up 65 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191781"|"28546275"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redchief, greater slope soil is a minor component."|"26191782"|"28546276"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copenhaver component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from basalt and/or andesite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191783"|"28546277"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191784"|"28546278"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191346"|"28545840"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Redchief, greater slope soil is a minor component."|"26191347"|"28545841"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copenhaver component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from basalt and/or andesite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191348"|"28545842"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Redchief component makes up 65 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191349"|"28545843"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191497"|"28545991"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danvers soil is a minor component."|"26191498"|"28545992"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 65 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 4e. Irrigated land capability classification is 4e. This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191499"|"28545993"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Martinsdale, cobbly soil is a minor component."|"26191500"|"28545994"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191501"|"28545995"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191502"|"28545996"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 65 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191503"|"28545997"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191504"|"28545998"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191505"|"28545999"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191506"|"28546000"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191507"|"28546001"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Roy component makes up 65 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 9 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191508"|"28546002"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tolbert component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of residuum weathered from igneous rock. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191509"|"28546003"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190555"|"28545049"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190556"|"28545050"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190557"|"28545051"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190558"|"28545052"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190559"|"28545053"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190560"|"28545054"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Helmville component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190561"|"28545055"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190562"|"28545056"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, very cobbly soil is a minor component."|"26191510"|"28546004"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 25 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26191511"|"28546005"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26191512"|"28546006"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copenhaver component makes up 20 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of residuum weathered from basalt and/or andesite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191513"|"28546007"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191514"|"28546008"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191515"|"28546009"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, greater slopes soil is a minor component."|"26191516"|"28546010"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copenhaver component makes up 20 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum weathered from basalt and/or andesite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191785"|"28546279"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26191786"|"28546280"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R044BP818MT Upland Grassland ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191787"|"28546281"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191788"|"28546282"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, greater slopes soil is a minor component."|"26191789"|"28546283"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 25 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 6e. Irrigated land capability classification is 6e. This soil does not meet hydric criteria.   "|"26191790"|"28546284"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, very cobbly soil is a minor component."|"26191791"|"28546285"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Monad component makes up 25 percent of the map unit. Slopes are 35 to 50 percent. This component is on hills. The parent material consists of residuum and/or colluvium derived from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191350"|"28545844"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191351"|"28545845"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Libeg component makes up 40 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the R043BP818MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191352"|"28545846"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver, greater slope soil is a minor component."|"26191353"|"28545847"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg, very cobbly soil is a minor component."|"26191354"|"28545848"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Copenhaver component makes up 20 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of residuum weathered from basalt and/or andesite. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 6 percent. This component is in the R043BP810MT Shallow Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191355"|"28545849"
12/27/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Roy soil is a minor component."|"26191356"|"28545850"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190809"|"28545303"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190810"|"28545304"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190811"|"28545305"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190812"|"28545306"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Loberg component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium and/or residuum weathered from igneous rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191073"|"28545567"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191074"|"28545568"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26191075"|"28545569"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26191076"|"28545570"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26191077"|"28545571"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190813"|"28545307"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190814"|"28545308"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190815"|"28545309"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191078"|"28545572"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191079"|"28545573"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191080"|"28545574"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190282"|"28544776"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190283"|"28544777"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190284"|"28544778"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 85 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190285"|"28544779"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190286"|"28544780"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190287"|"28544781"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danaher component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of alluvium and/or colluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190288"|"28544782"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190289"|"28544783"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190290"|"28544784"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Danaher component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium and/or colluvium derived from volcanic and sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190291"|"28544785"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26190292"|"28544786"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190293"|"28544787"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 40 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191792"|"28546286"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191793"|"28546287"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 45 percent of the map unit. Slopes are 8 to 25 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191794"|"28546288"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191795"|"28546289"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191796"|"28546290"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 40 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191357"|"28545851"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191358"|"28545852"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 45 percent of the map unit. Slopes are 25 to 50 percent. This component is on moraines. The parent material consists of alpine till. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F044BP910MT Upland Cool Woodland ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191359"|"28545853"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191360"|"28545854"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191361"|"28545855"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191653"|"28546147"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191654"|"28546148"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"26191655"|"28546149"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191656"|"28546150"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"26191657"|"28546151"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler, greater slope soil is a minor component."|"26191658"|"28546152"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191659"|"28546153"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191660"|"28546154"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191661"|"28546155"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"26191662"|"28546156"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191663"|"28546157"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler, greater slope soil is a minor component."|"26191664"|"28546158"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Winkler component makes up 50 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191665"|"28546159"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191666"|"28546160"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191667"|"28546161"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"26191668"|"28546162"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"26191669"|"28546163"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191670"|"28546164"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191081"|"28545575"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191082"|"28545576"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow, greater slope soil is a minor component."|"26191083"|"28545577"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190816"|"28545310"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderatly deep soils soil is a minor component."|"26190817"|"28545311"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190818"|"28545312"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 85 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191084"|"28545578"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191085"|"28545579"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Relyea soil is a minor component."|"26191086"|"28545580"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191087"|"28545581"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mocmont component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190819"|"28545313"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190820"|"28545314"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rittel component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of residuum weathered from shale. Depth to a root restrictive layer, bedrock, paralithic, is 20 to 40 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26191088"|"28545582"
12/09/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wilsall soil is a minor component."|"26191089"|"28545583"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slope soil is a minor component."|"26191090"|"28545584"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191091"|"28545585"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190563"|"28545057"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore, greater slope soil is a minor component."|"26190564"|"28545058"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190565"|"28545059"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitore component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190566"|"28545060"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190567"|"28545061"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26190568"|"28545062"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tigeron component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of alluvium and/or colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26190569"|"28545063"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190570"|"28545064"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190571"|"28545065"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tigeron component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of alluvium and/or colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26190572"|"28545066"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190573"|"28545067"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190574"|"28545068"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191092"|"28545586"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191093"|"28545587"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191094"|"28545588"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191095"|"28545589"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191096"|"28545590"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191097"|"28545591"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190821"|"28545315"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26190822"|"28545316"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190823"|"28545317"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190824"|"28545318"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191098"|"28545592"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191099"|"28545593"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26191100"|"28545594"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191101"|"28545595"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winkler soil is a minor component."|"26191102"|"28545596"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191103"|"28545597"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26191384"|"28545878"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Aquic Cumulic Haplustolls soil is a minor component."|"26191385"|"28545879"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26191386"|"28545880"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191387"|"28545881"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26191388"|"28545882"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mccabe soil is a minor component."|"26191389"|"28545883"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquentic Endoaquolls component makes up 75 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 16 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 7s.  This soil meets hydric criteria.   "|"26191390"|"28545884"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slickens is a miscellaneous area."|"26191391"|"28545885"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190294"|"28544788"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190295"|"28544789"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26190296"|"28544790"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190297"|"28544791"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190298"|"28544792"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190299"|"28544793"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190300"|"28544794"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190301"|"28544795"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190302"|"28544796"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190303"|"28544797"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26190304"|"28544798"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190305"|"28544799"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190306"|"28544800"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Copenhaver soil is a minor component."|"26190307"|"28544801"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Danaher soil is a minor component."|"26190308"|"28544802"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26190309"|"28544803"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190310"|"28544804"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190311"|"28544805"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evaro component makes up 85 percent of the map unit. Slopes are 4 to 15 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190312"|"28544806"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro, greater slope soil is a minor component."|"26190313"|"28544807"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190314"|"28544808"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190315"|"28544809"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evaro component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190825"|"28545319"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26190826"|"28545320"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26190827"|"28545321"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190828"|"28545322"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26190829"|"28545323"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro, greater slope soil is a minor component."|"26190830"|"28545324"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Evaro component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191104"|"28545598"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191105"|"28545599"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock soil is a minor component."|"26191106"|"28545600"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Loberg soil is a minor component."|"26191107"|"28545601"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191108"|"28545602"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26191109"|"28545603"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium derived from argillite and/or quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191671"|"28546165"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lonniebee soil is a minor component."|"26191672"|"28546166"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191673"|"28546167"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191674"|"28546168"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tigeron soil is a minor component."|"26191675"|"28546169"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"26191676"|"28546170"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 45 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26191362"|"28545856"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191363"|"28545857"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 40 percent of the map unit. Slopes are 8 to 15 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26191364"|"28545858"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191365"|"28545859"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191366"|"28545860"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow, greater slope soil is a minor component."|"26191367"|"28545861"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 40 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191797"|"28546291"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slope soil is a minor component."|"26191798"|"28546292"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rittel soil is a minor component."|"26191799"|"28546293"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bushong soil is a minor component."|"26191800"|"28546294"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Crow component makes up 45 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191801"|"28546295"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191802"|"28546296"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26191803"|"28546297"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191804"|"28546298"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191368"|"28545862"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The MODERATELY DEEP SOILS soil is a minor component."|"26191369"|"28545863"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"26191370"|"28545864"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191371"|"28545865"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow, greater slopes soil is a minor component."|"26191372"|"28545866"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191373"|"28545867"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Whitecow component makes up 55 percent of the map unit. Slopes are 60 to 80 percent. This component is on mountains. The parent material consists of colluvium derived from limestone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP912MT Limy Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 45 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191805"|"28546299"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26191806"|"28546300"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow, greater slope soil is a minor component."|"26191807"|"28546301"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The MODERATLY DEEP SOILS-Dryadine soil is a minor component."|"26191808"|"28546302"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Wildgen soil is a minor component."|"26191809"|"28546303"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191810"|"28546304"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26190831"|"28545325"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26190832"|"28545326"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26190833"|"28545327"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps, greater slope soil is a minor component."|"26190834"|"28545328"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26190835"|"28545329"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Trapps component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from limestone and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 23 percent. There are no saline horizons within 30 inches of the soil surface. "|"26191110"|"28545604"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps, greater slope soil is a minor component."|"26191111"|"28545605"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell soil is a minor component."|"26191112"|"28545606"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Hoyt soil is a minor component."|"26191113"|"28545607"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191114"|"28545608"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 55 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191517"|"28546011"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191518"|"28546012"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderatly deep soils soil is a minor component."|"26191519"|"28546013"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka, greater slope soil is a minor component."|"26191520"|"28546014"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191521"|"28546015"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Yreka component makes up 55 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191522"|"28546016"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecow soil is a minor component."|"26191523"|"28546017"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191524"|"28546018"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka, greater slope soil is a minor component."|"26191525"|"28546019"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moderatly deep soils soil is a minor component."|"26191526"|"28546020"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191527"|"28546021"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191528"|"28546022"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191529"|"28546023"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26191530"|"28546024"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"26191531"|"28546025"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tigeron soil is a minor component."|"26191532"|"28546026"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on mountains. The parent material consists of colluvium derived from volcanic rock and/or argillite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191533"|"28546027"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitore soil is a minor component."|"26191534"|"28546028"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, greater slope soil is a minor component."|"26191535"|"28546029"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191536"|"28546030"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Evaro soil is a minor component."|"26191537"|"28546031"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tigeron soil is a minor component."|"26191538"|"28546032"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 35 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26191374"|"28545868"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slope soil is a minor component."|"26191375"|"28545869"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26191376"|"28545870"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"26191377"|"28545871"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191378"|"28545872"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 35 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191811"|"28546305"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Bignell, greater slope soil is a minor component."|"26191812"|"28546306"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191813"|"28546307"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191814"|"28546308"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"26191815"|"28546309"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 50 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191379"|"28545873"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26191380"|"28545874"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Trapps soil is a minor component."|"26191381"|"28545875"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Winfall soil is a minor component."|"26191382"|"28545876"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 35 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191383"|"28545877"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 8 to 15 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 4e.  This soil does not meet hydric criteria.   "|"26190575"|"28545069"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190576"|"28545070"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26190577"|"28545071"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190578"|"28545072"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190579"|"28545073"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 15 to 35 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26190580"|"28545074"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190581"|"28545075"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26190582"|"28545076"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190583"|"28545077"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190584"|"28545078"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bignell component makes up 85 percent of the map unit. Slopes are 35 to 60 percent. This component is on hills. The parent material consists of colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26190585"|"28545079"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yreka soil is a minor component."|"26190586"|"28545080"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26190587"|"28545081"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Crow soil is a minor component."|"26190588"|"28545082"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Sharrott soil is a minor component."|"26190589"|"28545083"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Miscellaneous Water is a miscellaneous area."|"26191816"|"28546310"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191677"|"28546171"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquentic Endoaquolls component makes up 35 percent of the map unit. Slopes are 0 to 2 percent. This component is on flood plains. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is occasionally flooded. It is not ponded. A seasonal zone of water saturation is at 18 inches (depth from the mineral surface is 16 inches) during April, May, June, July. Organic matter content in the surface horizon is about 75 percent. This component is in the R044BP801MT Bottomland ecological site. Nonirrigated land capability classification is 7s.  This soil meets hydric criteria.   "|"26191817"|"28546311"
12/22/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Canarway soil is a minor component."|"26191818"|"28546312"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mccabe soil is a minor component."|"26191819"|"28546313"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Saypo soil is a minor component."|"26191820"|"28546314"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Riverwash soil is a minor component."|"26191821"|"28546315"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Aquic Cumulic Haplustolls soil is a minor component."|"26191822"|"28546316"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191823"|"28546317"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Slickens is a miscellaneous area."|"26191824"|"28546318"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Dumps is a miscellaneous area."|"26191392"|"28545886"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet component makes up 30 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of colluvium derived from sandstone and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 4 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 5 percent.  "|"26191393"|"28545887"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Cowood component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of residuum weathered from sandstone and siltstone. Depth to a root restrictive layer, bedrock, lithic, is 10 to 20 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP903MT Shallow Cool Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191394"|"28545888"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191395"|"28545889"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Waldbillig, very bouldery component makes up 20 percent of the map unit. Slopes are 45 to 70 percent. This component is on glacial-valley walls. The parent material consists of volcanic ash over drift derived from sandstone and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 33 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191396"|"28545890"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191397"|"28545891"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Garlet, extremely bouldery component makes up 40 percent of the map unit. Slopes are 10 to 35 percent. This component is on glacial-valley floors. The parent material consists of drift derived from limestone, sandstone, and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191544"|"28546038"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elvick, bouldery component makes up 15 percent of the map unit. Slopes are 0 to 20 percent. This component is on drainageways. The parent material consists of glaciofluvial deposits derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 33 inches during May, June, July. Organic matter content in the surface horizon is about 1 percent. This component is in the F043BP917MT Subirrigated Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191545"|"28546039"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191546"|"28546040"
06/25/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191547"|"28546041"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Worock, stony component makes up 30 percent of the map unit. Slopes are 10 to 35 percent. This component is on glacial-valley floors. The parent material consists of drift derived from sandstone and siltstone. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191548"|"28546042"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Worock, stony soil is a minor component."|"26191678"|"28546172"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 65 percent of the map unit. Slopes are 10 to 35 percent. This component is on stream terraces, mountain slopes. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP909MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191679"|"28546173"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water is a miscellaneous area."|"26191680"|"28546174"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Finn component makes up 15 percent of the map unit. Slopes are 0 to 10 percent. This component is on flood plains. The parent material consists of alluvium derived from sandstone and shale. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during April, May, June. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 7 percent. This component is in the R043BP801MT Bottomland Group ecological site.   This soil meets hydric criteria.   "|"26191681"|"28546175"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cryofluvents soil is a minor component."|"26191682"|"28546176"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191683"|"28546177"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 55 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountain slopes. The parent material consists of colluvium derived from andesite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191684"|"28546178"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Libeg soil is a minor component."|"26191685"|"28546179"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 25 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountain slopes. The parent material consists of colluvium derived from andesite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191686"|"28546180"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land is a miscellaneous area."|"26191539"|"28546033"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Gambler component makes up 25 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountain slopes. The parent material consists of colluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 2 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.  There are no saline horizons within 30 inches of the soil surface. "|"26191540"|"28546034"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elve component makes up 45 percent of the map unit. Slopes are 25 to 50 percent. This component is on mountain slopes. The parent material consists of colluvium derived from basalt. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat excessively drained.  Water movement in the most restrictive layer is high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 1 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191541"|"28546035"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191542"|"28546036"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Cowood, very stony soil is a minor component."|"26191543"|"28546037"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Figaro soil is a minor component."|"26191825"|"28546319"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Illiano soil is a minor component."|"26191826"|"28546320"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Lowder soil is a minor component."|"26191827"|"28546321"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191828"|"28546322"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Goosepeak component makes up 15 percent of the map unit. Slopes are 10 to 35 percent. This component is on ridges, mountain slopes. The parent material consists of colluvium derived from tuff breccia. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191829"|"28546323"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vitroff component makes up 40 percent of the map unit. Slopes are 10 to 35 percent. This component is on mountain slopes. The parent material consists of fine-loamy alluvium and/or colluvium derived from tuff breccia. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191830"|"28546324"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Torpy component makes up 20 percent of the map unit. Slopes are 10 to 35 percent. This component is on mountain slopes. The parent material consists of colluvium derived from tuff breccia. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 50 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043BP910MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191831"|"28546325"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191549"|"28546043"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Elvick soil is a minor component."|"26191550"|"28546044"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kawuneeche component makes up 80 percent of the map unit. Slopes are 0 to 4 percent. This component is on flood plains, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. This component is in the R043AP802MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"26191551"|"28546045"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Moosehead soil is a minor component."|"26191552"|"28546046"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elvick component makes up 60 percent of the map unit. Slopes are 1 to 10 percent. This component is on flood-plain steps, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is rarely flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches (depth from the mineral surface is 29 inches) during April, May, June. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the R043AP802MT Bottomland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"26191553"|"28546047"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191554"|"28546048"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Fluvaquentic Cryaquepts component makes up 25 percent of the map unit. Slopes are 1 to 4 percent. This component is on flood plains, valleys. The parent material consists of alluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is frequently flooded. It is not ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. This component is in the R043AP802MT Bottomland Group ecological site. Nonirrigated land capability classification is 5w. Irrigated land capability classification is 5w. This soil meets hydric criteria.   "|"26191555"|"28546049"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kawuneeche soil is a minor component."|"26191832"|"28546326"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Holloway component makes up 35 percent of the map unit. Slopes are 1 to 25 percent. This component is on alluvial fans, valleys. The parent material consists of volcanic ash over alluvium and/or slope alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191833"|"28546327"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 50 percent of the map unit. Slopes are 1 to 25 percent. This component is on alluvial fans, valleys. The parent material consists of volcanic ash over alluvium and/or slope alluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F044AP903MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191834"|"28546328"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191835"|"28546329"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Kadygulch soil is a minor component."|"26191836"|"28546330"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Rumblecreek component makes up 50 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, mountains. The parent material consists of undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191687"|"28546181"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Larry soil is a minor component."|"26191688"|"28546182"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Sol, very stony component makes up 35 percent of the map unit. Slopes are 5 to 35 percent. This component is on valley-border surfaces, mountains. The parent material consists of undifferentiated slope alluvium and/or colluvium. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191689"|"28546183"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten, very stony soil is a minor component."|"26191690"|"28546184"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Mitten soil is a minor component."|"26191556"|"28546050"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"26191557"|"28546051"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Broadmoor component makes up 90 percent of the map unit. Slopes are 35 to 55 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191558"|"28546052"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"26191837"|"28546331"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCay soil is a minor component."|"26191838"|"28546332"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 60 percent of the map unit. Slopes are 35 to 55 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191839"|"28546333"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis component makes up 30 percent of the map unit. Slopes are 35 to 55 percent. This component is on moderately steep mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191840"|"28546334"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten component makes up 85 percent of the map unit. Slopes are 10 to 35 percent. This component is on broadly convex ridges on mountains, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191691"|"28546185"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191692"|"28546186"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCay soil is a minor component."|"26191693"|"28546187"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Tevis soil is a minor component."|"26191694"|"28546188"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"26191695"|"28546189"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Kintla component makes up 60 percent of the map unit. Slopes are 55 to 85 percent. This component is on cirque headwalls, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP902MT Ashy Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"26191559"|"28546053"
06/25/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Chutes, avalanche soil is a minor component."|"26191560"|"28546054"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, talus soil is a minor component."|"26191561"|"28546055"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191562"|"28546056"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop soil is a minor component."|"26191398"|"28545892"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191399"|"28545893"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Endlich component makes up 25 percent of the map unit. Slopes are 40 to 80 percent. This component is on avalanche chutes, mountains. The parent material consists of colluvium and mass movement deposits over residuum weathered from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is very low. Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"26191400"|"28545894"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bigelow, very bouldery component makes up 50 percent of the map unit. Slopes are 40 to 60 percent. This component is on avalanche chutes, mountains. The parent material consists of colluvium and mass movement deposits. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the R043AP810MT Upland Grassland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191401"|"28545895"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Whitecross, very bouldery soil is a minor component."|"26191402"|"28545896"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191696"|"28546190"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Vaywood, extremely bouldery component makes up 80 percent of the map unit. Slopes are 35 to 45 percent. This component is on moderately steep lateral moraines on glacial-valley floors, mountains. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP902MT Ashy Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 7s.  This soil does not meet hydric criteria.   "|"26191697"|"28546191"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Vaywood, very bouldery, moist soil is a minor component."|"26191698"|"28546192"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metasedimentary soil is a minor component."|"26191699"|"28546193"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mowbray component makes up 20 percent of the map unit. Slopes are 65 to 100 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from argillite and/or limestone. Depth to a root restrictive layer, bedrock, lithic, is 39 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 10 percent.  "|"26191700"|"28546194"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Specie component makes up 45 percent of the map unit. Slopes are 65 to 100 percent. This component is on very steep mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"26191701"|"28546195"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land, talus soil is a minor component."|"26191702"|"28546196"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Beeskove soil is a minor component."|"26191703"|"28546197"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191704"|"28546198"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Beeskove component makes up 40 percent of the map unit. Slopes are 65 to 100 percent. This component is on dissected very steep mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191403"|"28545897"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Argora component makes up 35 percent of the map unit. Slopes are 65 to 100 percent. This component is on dissected very steep mountain slopes, mountains. The parent material consists of colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic, is 59 to 79 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 75 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 15 percent.  "|"26191404"|"28545898"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop is a miscellaneous area."|"26191405"|"28545899"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191406"|"28545900"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Venson soil is a minor component."|"26191407"|"28545901"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metasedimentary soil is a minor component."|"26191408"|"28545902"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Bendahl component makes up 75 percent of the map unit. Slopes are 55 to 75 percent. This component is on steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from metasedimentary rock. Depth to a root restrictive layer, bedrock, lithic,  inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"26191409"|"28545903"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Broadmoor soil is a minor component."|"26191410"|"28545904"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"26191563"|"28546057"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Tevis, very stony component makes up 35 percent of the map unit. Slopes are 55 to 75 percent. This component is on steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"26191564"|"28546058"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rubble land soil is a minor component."|"26191565"|"28546059"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The McCay soil is a minor component."|"26191566"|"28546060"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Mitten, very stony component makes up 45 percent of the map unit. Slopes are 55 to 75 percent. This component is on steep mountain slopes, mountains. The parent material consists of volcanic ash over colluvium derived from quartzite. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 2 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 8.  This soil does not meet hydric criteria.   "|"26191567"|"28546061"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Melrude component makes up 20 percent of the map unit. Slopes are 1 to 5 percent. This component is on potholes, valleys. The parent material consists of alluvium over till derived from metasedimentary rock and/or sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP907MT Subirrigated Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"26191841"|"28546335"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Andic Hapludalfs component makes up 65 percent of the map unit. Slopes are 5 to 35 percent. This component is on moraines, valleys. The parent material consists of volcanic ash over till derived from metasedimentary rock and/or sedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is moderate. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria. The calcium carbonate equivalent within 40 inches, typically, does not exceed 3 percent.  "|"26191842"|"28546336"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191843"|"28546337"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Andic Haplocryalfs soil is a minor component."|"26191844"|"28546338"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Melrude component makes up 15 percent of the map unit. Slopes are 1 to 5 percent. This component is on potholes, valleys. The parent material consists of alluvium over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is high.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 6 inches (depth from the mineral surface is 5 inches) during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP907MT Subirrigated Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"26191411"|"28545905"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191412"|"28545906"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The McCay component makes up 45 percent of the map unit. Slopes are 5 to 35 percent. This component is on moraines, valleys. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP908MT Upland Cold Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191413"|"28545907"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elkridge component makes up 35 percent of the map unit. Slopes are 5 to 35 percent. This component is on moraines, valleys. The parent material consists of volcanic ash over till derived from metasedimentary rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 6e.  This soil does not meet hydric criteria.   "|"26191414"|"28545908"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Elvick component makes up 40 percent of the map unit. Slopes are 1 to 10 percent. This component is on outwash terraces, valleys. The parent material consists of alluvium over outwash derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is somewhat poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. A seasonal zone of water saturation is at 30 inches (depth from the mineral surface is 28 inches) during April, May, June. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP907MT Subirrigated Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil does not meet hydric criteria.   "|"26191415"|"28545909"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Water soil is a minor component."|"26191416"|"28545910"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Holloway soil is a minor component."|"26191417"|"28545911"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Typic Cryaquepts component makes up 45 percent of the map unit. Slopes are 1 to 5 percent. This component is on swales or potholes on outwash terraces, valleys. The parent material consists of alluvium over outwash derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is very poorly drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is occasionally ponded. A seasonal zone of water saturation is at 0 inches during May, June, July. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP907MT Subirrigated Cool Moist Woodland Group ecological site. Nonirrigated land capability classification is 6w. Irrigated land capability classification is 6w. This soil meets hydric criteria.   "|"26191418"|"28545912"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Andic Glossudalfs component makes up 20 percent of the map unit. Slopes are 25 to 55 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high.  Available water to a depth of 60 inches (or restricted depth) is moderate.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 4 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191705"|"28546199"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Yellowbay, very stony soil is a minor component."|"26191706"|"28546200"
07/01/2021 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Zaza, very stony soil is a minor component."|"26191707"|"28546201"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville, moderately deep component makes up 20 percent of the map unit. Slopes are 25 to 55 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till over residuum weathered from metamorphic rock. Depth to a root restrictive layer, bedrock, lithic, is 20 to 39 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is low. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191708"|"28546202"
07/17/2024 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"Generated brief soil descriptions are created for major soil components.  The Rock outcrop, metamorphic soil is a minor component."|"26191709"|"28546203"
08/31/2022 00:00:00|"Nontechnical description"|"GENSOIL"|"generated"|"The Courville component makes up 45 percent of the map unit. Slopes are 25 to 55 percent. This component is on moraines, mountains. The parent material consists of volcanic ash over till derived from metamorphic rock. Depth to a root restrictive layer is greater than 60 inches. The natural drainage class is well drained.  Water movement in the most restrictive layer is moderately high. Available water to a depth of 60 inches (or restricted depth) is low.  Shrink-swell potential is low. This soil is not flooded. It is not ponded. There is no zone of water saturation within a depth of 72 inches. Organic matter content in the surface horizon is about 70 percent. Below this thin organic horizon the organic matter content is about 3 percent. This component is in the F043AP909MT Upland Cool Woodland Group ecological site. Nonirrigated land capability classification is 7e.  This soil does not meet hydric criteria.   "|"26191710"|"28546204"
