Identification_Information
  Citation
    Citation_Information
      Originator:        Montana State Library
      Publication_Date:  19920205
      Title:             Upper Clark Fork Public Land Survey Sections from 1:24,000 scale USGS quadrangles
      Geospatial_Data_Presentation_Form:  map
      Publication_Information
        Publication_Place:  Helena, Montana
        Publisher:          Montana State Library
      Online_Linkage: http://nris.mt.gov/nsdi/nris/e00/ab19.zip
      Online_Linkage: http://nris.mt.gov/nsdi/nris/shape/ab19.zip
  Description
    Abstract:
        Public Land Survey Sections from USGS 1:24,000 scale
        quadrangles, Upper Clark Fork Basin, Montana.  The
        quadrangles have been joined into a single data set, but
        have not been edgematched, except to preserve polygon
        polygon topology.  The USGS major and minor attribute codes
        have been replaced with the codes shown in this metadata
        record.
        See http://nris.mt.gov/nsdi/nris/cf7.dbf for dates of
        the source quadrangles.
    Purpose:
        Base map data, approximate location of features whose
        public land survey location description are known.
  Time_Period_of_Content
    Time_Period_Information
      Range_of_Dates/Times
        Beginning_Date:  19610101
        Ending_Date:     19890101
    Currentness_Reference:  Publication Date
  Status
    Progress:  Complete
    Maintenance_and_Update_Frequency:  Unknown
  Spatial_Domain
    Bounding_Coordinates
      West_Bounding_Coordinate:   -114.036880
      East_Bounding_Coordinate:   -112.298012
      North_Bounding_Coordinate:  47.0592041
      South_Bounding_Coordinate:  45.7051659
    Data_Set_G-Polygon
      Data_Set_G-Polygon_Outer_G-Ring
        G-Ring_Latitude:   47.0075
        G-Ring_Longitude:  -114.1417
        G-Ring_Latitude:   46.7451
        G-Ring_Longitude:  -114.1277
        G-Ring_Latitude:   46.7415
        G-Ring_Longitude:  -113.7623
        G-Ring_Latitude:   46.619
        G-Ring_Longitude:  -113.7613
        G-Ring_Latitude:   46.4954
        G-Ring_Longitude:  -113.6305
        G-Ring_Latitude:   46.3669
        G-Ring_Longitude:  -113.6336
        G-Ring_Latitude:   46.366
        G-Ring_Longitude:  -113.4911
        G-Ring_Latitude:   46.5067
        G-Ring_Longitude:  -113.4842
        G-Ring_Latitude:   46.5077
        G-Ring_Longitude:  -113.6227
        G-Ring_Latitude:   46.6169
        G-Ring_Longitude:  -113.7395
        G-Ring_Latitude:   46.6114
        G-Ring_Longitude:  -113.3923
        G-Ring_Latitude:   46.3637
        G-Ring_Longitude:  -113.3874
        G-Ring_Latitude:   46.3727
        G-Ring_Longitude:  -113.1162
        G-Ring_Latitude:   46.4921
        G-Ring_Longitude:  -113.1156
        G-Ring_Latitude:   46.4893
        G-Ring_Longitude:  -113.0159
        G-Ring_Latitude:   46.3816
        G-Ring_Longitude:  -113.0219
        G-Ring_Latitude:   46.3637
        G-Ring_Longitude:  -113.1156
        G-Ring_Latitude:   46.3591
        G-Ring_Longitude:  -113.2577
        G-Ring_Latitude:   46.1139
        G-Ring_Longitude:  -113.2665
        G-Ring_Latitude:   46.1153
        G-Ring_Longitude:  -113.1335
        G-Ring_Latitude:   45.9926
        G-Ring_Longitude:  -113.1425
        G-Ring_Latitude:   45.9908
        G-Ring_Longitude:  -113.0095
        G-Ring_Latitude:   45.8684
        G-Ring_Longitude:  -113.0102
        G-Ring_Latitude:   45.8661
        G-Ring_Longitude:  -112.8904
        G-Ring_Latitude:   45.7408
        G-Ring_Longitude:  -112.8869
        G-Ring_Latitude:   45.7483
        G-Ring_Longitude:  -112.7338
        G-Ring_Latitude:   45.8648
        G-Ring_Longitude:  -112.7322
        G-Ring_Latitude:   45.8659
        G-Ring_Longitude:  -112.3605
        G-Ring_Latitude:   45.9913
        G-Ring_Longitude:  -112.3628
        G-Ring_Latitude:   45.9885
        G-Ring_Longitude:  -112.2342
        G-Ring_Latitude:   46.1375
        G-Ring_Longitude:  -112.2459
        G-Ring_Latitude:   46.1347
        G-Ring_Longitude:  -112.3574
        G-Ring_Latitude:   46.2569
        G-Ring_Longitude:  -112.3639
        G-Ring_Latitude:   46.2591
        G-Ring_Longitude:  -112.5103
        G-Ring_Latitude:   46.1366
        G-Ring_Longitude:  -112.5121
        G-Ring_Latitude:   46.1368
        G-Ring_Longitude:  -112.6152
        G-Ring_Latitude:   46.4922
        G-Ring_Longitude:  -112.6097
        G-Ring_Latitude:   46.4956
        G-Ring_Longitude:  -112.4846
        G-Ring_Latitude:   46.7582
        G-Ring_Longitude:  -112.4861
        G-Ring_Latitude:   46.7571
        G-Ring_Longitude:  -112.6381
        G-Ring_Latitude:   46.6347
        G-Ring_Longitude:  -112.6396
        G-Ring_Latitude:   46.6343
        G-Ring_Longitude:  -112.8607
        G-Ring_Latitude:   46.7597
        G-Ring_Longitude:  -112.8598
        G-Ring_Latitude:   46.7618
        G-Ring_Longitude:  -112.9903
        G-Ring_Latitude:   46.8845
        G-Ring_Longitude:  -112.9808
        G-Ring_Latitude:   46.8864
        G-Ring_Longitude:  -113.1116
        G-Ring_Latitude:   47.0118
        G-Ring_Longitude:  -113.1114
        G-Ring_Latitude:   47.0097
        G-Ring_Longitude:  -113.2684
        G-Ring_Latitude:   46.8843
        G-Ring_Longitude:  -113.2683
        G-Ring_Latitude:   46.8857
        G-Ring_Longitude:  -113.7389
        G-Ring_Latitude:   47.0113
        G-Ring_Longitude:  -113.7358
        G-Ring_Latitude:   47.0075
        G-Ring_Longitude:  -114.1417
  Keywords
    Theme
      Theme_Keyword_Thesaurus:  None
      Theme_Keyword:  Township
      Theme_Keyword:  Range
      Theme_Keyword:  Section
      Theme_Keyword:  Public Land Survey
    Place
      Place_Keyword_Thesaurus:  None
      Place_Keyword:  Montana
      Place_Keyword:  Butte
      Place_Keyword:  Anaconda
      Place_Keyword:  Missoula
      Place_Keyword:  Clark Fork
  Access_Constraints:
        None
  Use_Constraints:
        Not for use at scales greater than 1:24000.
  Point_of_Contact
    Contact_Information
      Contact_Organization_Primary
        Contact_Organization:  Montana State Library
        Contact_Person:        Gerry Daumiller
      Contact_Position:        Senior GIS Programmer
      Contact_Address
        Address_Type:  mailing address
        Address:            P.O. Box 201800
        City:               Helena
        State_or_Province:  Montana
        Postal_Code:        59620-1800
        Country:            USA
      Contact_Voice_Telephone:          (406) 444-5358
      Contact_Facsimile_Telephone:      (406) 444-0581
      Contact_Electronic_Mail_Address:  gdaumiller@mt.gov
      Hours_of_Service:  Monday-Friday, 8-5, Mountain Time
  Browse_Graphic
    Browse_Graphic_File_Name:  http://nris.mt.gov/nsdi/nris/ab19.gif
    Browse_Graphic_File_Description:
      Simple image of the data set and/or its extent.
    Browse_Graphic_File_Type:  gif
  Native_Data_Set_Environment:
    Arc/Info coverage or ESRI shapefile
 
Data_Quality_Information:
  Attribute_Accuracy
    Attribute_Accuracy_Report:
        Attributes were interpreted from the original DLG files by
        a computer program.  The accuracy of this interpretation
        has not been extensively checked.  Attribute accuracy of the
        original Digital Line Graph data is estimated by the USGS
        at 98.5 percent, and was tested by them as follows:
        - manual comparison of the source with hard copy plots.
        - symbolized display of the digital line graph on an
        interactive compter graphic system.
        - Selected attributes that could not be visually verified on
        plots or on screen, were interactively queried and verified
        on screen.
        In addition, U.S. Geological Survey  (USGS) Production
        System (PROSYS) software tested the attributes against a
        master set of valid attributes for the category; it also
        checked for selected valid attribute combinations, and for
        valid attributes relative to topology and dimensionality.
        All attribute data conform to the attribute codes current
        as of the date of digitizing.
  Logical_Consistency_Report:
        Polygon and arc-node topology exist.
  Completeness_Report:
        For DLG data, Digital Revision Status = Not revised:
        Data completeness reflects the content of the source
        quadrangle.  Features may have been eliminated or
        generalized on the source graphic, due to scale and
        legibility constraints.
        For DLG data, Digital Revision Status = Limited Update:
        This file has undergone limited update digital revision.
        The file contains only (1) those features that are
        photoidentifiable on monoscopic source, supplemented with
        limited ancillary source, and (2) those features, present on
        the original source quadrangle, that can not be reliably
        photoidentified but that are not considered particularly
        prone to change.
        For DLG data, Digital Revision Status = Standard Update:
        This file has undergone standard update digital revision.
        The data completeness of this file meets National Mapping
        Division standards for feature content.
  Positional_Accuracy
    Horizontal_Positional_Accuracy
      Horizontal_Positional_Accuracy_Report:
        Approximate accuracy is 12 meters, assuming the source maps
        meet National Map Accuracy Standards (NMAS).  NMAS
        horizontal accuracy requires that at least 90 percent of
        points tested are within 0.02 inches of the true position.
        The digital data are estimated to contain a horizontal
        positional error of less than or equal to 0.003 inches
        standard error in the two component directions relative to
        the source quadrangle.  Comparison to the graphic source is
        used as control to assess digital positional accuracy.
        Cartographic offsets may be present on the graphic source,
        due to scale and legibility constraints.  Digital map
        elements require edge alignment between data sets.  Data
        along each quadrangle edge are tested against the data set
        for the adjacent quadrangle using PROSYS; tests check for
        positional accuracy between data sets within a 0.02 inches
        tolerance.  Features with like dimensionality, and with or
        without like attribution, that are within the tolerance
        are adjusted by moving the feature equally in both data
        sets.  Features outside the tolerance are not moved.
  Lineage
    Source_Information
      Source_Citation
        Citation_Information
          Originator:
            National Mapping Division
            U.S. Geological Survey
          Publication_Date:  19610101
          Title:  1:24,000-scale Digital Line Graphs
          Geospatial_Data_Presentation_Form:  map
          Publication_Information
            Publication_Place:  Reston, VA
            Publisher:  U.S. Geological Survey
          Other_Citation_Details:
            See http://nris.mt.gov/nsdi/nris/cf7.dbf for publication
            dates of the various quadrangles.
      Source_Scale_Denominator:  24000
      Type_of_Source_Media:  unknown
      Source_Time_Period_of_Content
        Time_Period_Information
          Range_of_Dates/Times
            Beginning_Date:  19610101
            Ending_Date:     19890101
        Source_Currentness_Reference:  Publication Date
      Source_Citation_Abbreviation:  Q7.5
      Source_Contribution:
          The data set is a re-processed copy of this source.
    Process_Step
      Process_Description:
        Interpret USGS attributes, project quadrangles to State Plane
        Coordinates., and join quadrangles into one data set.
      Source_Used_Citation_Abbreviation:  Q7.5
      Process_Date:  19920205
      Source_Produced_Citation_Abbreviation:  fin1
    Process_Step
      Process_Description:
        Import additional quadrangles and append to the data that
        was imported in 1992.
      Source_Used_Citation_Abbreviation:  fin1
      Source_Used_Citation_Abbreviation:  Q7.5
      Process_Date:  19970414
      Source_Produced_Citation_Abbreviation:  fin2
 
Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method:  Vector
  Point_and_Vector_Object_Information
    SDTS_Terms_Description
      SDTS_Point_and_Vector_Object_Type:  Complete Chain
      Point_and_Vector_Object_Count:   8143
      SDTS_Point_and_Vector_Object_Type:  GT-polygon composed of chains
      Point_and_Vector_Object_Count:   2995
      SDTS_Point_and_Vector_Object_Type:  Area Point
      Point_and_Vector_Object_Count:   2994
 
Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition
    Planar
      Grid_Coordinate_System
        Grid_Coordinate_System_Name: State Plane Coordinate System 1983
        State_Plane_Coordinate_System
          SPCS_Zone_Identifier: 2500
          Lambert_Conformal_Conic
            Standard_Parallel:  45
            Standard_Parallel:  49
            Longitude_of_Central_Meridian:  -109.5
            Latitude_of_Projection_Origin:  44.25
            False_Easting:   600000.00000
            False_Northing:  0.00000
      Planar_Coordinate_Information
        Planar_Coordinate_Encoding_Method:  coordinate pair
        Coordinate_Representation
          Abscissa_Resolution:  .1
          Ordinate_Resolution:  .1
        Planar_Distance_Units:  meters
    Geodetic_Model
      Horizontal_Datum_Name:  North American Datum of 1983
      Ellipsoid_Name:   Geodetic Reference System 80
      Semi-major_Axis:  6378137
      Denominator_of_Flattening_Ratio:  298.257
 
Entity_and_Attribute_Information:
  Detailed_Description
    Entity_Type
      Entity_Type_Label:  USPLS.AAT
      Entity_Type_Definition:  Arc Attribute Table
      Entity_Type_Definition_Source:  None
    Attribute
      Attribute_Label:  TLINE
      Attribute_Definition:
        Code for township lines
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  0
          Enumerated_Domain_Value_Definition:  Map Edge
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1
          Enumerated_Domain_Value_Definition:  Section Line
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  2
          Enumerated_Domain_Value_Definition:  Township Line
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  3
          Enumerated_Domain_Value_Definition:  7.5-Minute Quad Boundary
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19920205
      Ending_Date_of_Attribute_Values:  19970414
    Attribute
      Attribute_Label:  CODE
      Attribute_Definition:
        Arc Attribute Code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  0
          Enumerated_Domain_Value_Definition:  Public Land Survey Line
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1
          Enumerated_Domain_Value_Definition:  Approximate
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  3
          Enumerated_Domain_Value_Definition:  Arbitrary Closure
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  6
          Enumerated_Domain_Value_Definition:  Approximate, Arbitrary Closure
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  11
          Enumerated_Domain_Value_Definition:  Approximate, Coincident Boundary
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  101
          Enumerated_Domain_Value_Definition:  Coincident Boundary
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  102
          Enumerated_Domain_Value_Definition:  Coincident Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  103
          Enumerated_Domain_Value_Definition:  Coincident Misc Trans
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  104
          Enumerated_Domain_Value_Definition:  Coincident Man-made Feature
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  110
          Enumerated_Domain_Value_Definition:  Coincident Boundary and Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  111
          Enumerated_Domain_Value_Definition:  Coincident Road and Misc Trans
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  112
          Enumerated_Domain_Value_Definition:  Coincident Hydrography
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19890101
  Detailed_Description
    Entity_Type
      Entity_Type_Label:  USPLS.PAT
      Entity_Type_Definition:  Polygon Attribute Table
      Entity_Type_Definition_Source:  None
    Attribute
      Attribute_Label:  TOWN
      Attribute_Definition:
        Township number
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Range_Domain
          Range_Domain_Minimum:  0
          Range_Domain_Maximum:  14
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19890101
    Attribute
      Attribute_Label:  TPART
      Attribute_Definition:
        Partial Township Identifier
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Unrepresentable_Domain:  Character field
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19890101
    Attribute
      Attribute_Label:  N/S
      Attribute_Definition:
        Township North or South identifier
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  N
          Enumerated_Domain_Value_Definition:  Township is North of the Base Line
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  S
          Enumerated_Domain_Value_Definition:  Township is South of the Base Line
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  RANGE
      Attribute_Definition:
        Range Number
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Range_Domain
          Range_Domain_Minimum:  0
          Range_Domain_Maximum:  20
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  RPART
      Attribute_Definition:
        Partial Range Identifier
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Unrepresentable_Domain:  Character field
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  E/W
      Attribute_Definition:
        Range East or West identifier
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  E
          Enumerated_Domain_Value_Definition:  Range is East of the Principal Meridian
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  W
          Enumerated_Domain_Value_Definition:  Range is West of the Principal Meridian
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  SECTION
      Attribute_Definition:
        Section Number
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Range_Domain
          Range_Domain_Minimum:  0
          Range_Domain_Maximum:  36
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  SPART
      Attribute_Definition:
        Partial Section identifier
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Unrepresentable_Domain:  Character field
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
  Detailed_Description
    Entity_Type
      Entity_Type_Label:  USPLS.NAT
      Entity_Type_Definition:  Node Attribute Table
      Entity_Type_Definition_Source:  None
    Attribute
      Attribute_Label:  CODE
      Attribute_Definition:
        Node type definition code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  100
          Enumerated_Domain_Value_Definition:  Section Corner
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  101
          Enumerated_Domain_Value_Definition:  Section Corner, coinc hyps
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  104
          Enumerated_Domain_Value_Definition:  Section Corner, field location
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  105
          Enumerated_Domain_Value_Definition:  Section Corner, field location, coinc hyps
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  106
          Enumerated_Domain_Value_Definition:  Section Corner, field location, coinc bnd
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  107
          Enumerated_Domain_Value_Definition:  Section Corner, field location, coinc hyps & bnd
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  300
          Enumerated_Domain_Value_Definition:  Closing Corner
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  301
          Enumerated_Domain_Value_Definition:  Closing Corner, coinc hyps
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  304
          Enumerated_Domain_Value_Definition:  Closing Corner, field location
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  305
          Enumerated_Domain_Value_Definition:  Closing Corner, field location, coinc hyps
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  306
          Enumerated_Domain_Value_Definition:  Closing Corner, field location, conic bnd
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  307
          Enumerated_Domain_Value_Definition:  Closing Corner, field location, coinc hyps & bnd
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  400
          Enumerated_Domain_Value_Definition:  Meander Corner
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  700
          Enumerated_Domain_Value_Definition:  Witness Corner
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  704
          Enumerated_Domain_Value_Definition:  Witness Corner, identified in field
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1200
          Enumerated_Domain_Value_Definition:  Quarter-Section Corner
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1204
          Enumerated_Domain_Value_Definition:  Quarter-Section Corner, field location
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1205
          Enumerated_Domain_Value_Definition:  Quarter-Section Corner, field loc, coinc hyps
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1206
          Enumerated_Domain_Value_Definition:  Quarter-Section Corner, field loc, coinc bnd
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1207
          Enumerated_Domain_Value_Definition:  Quarter-Section Corner, field loc, coinc hyps & bn
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1500
          Enumerated_Domain_Value_Definition:  Arbitrary Section Corner
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
 
Distribution_Information:
  Distributor
    Contact_Information
      Contact_Organization_Primary
        Contact_Organization:  Montana State Library
        Contact_Person:        Gerry Daumiller
      Contact_Position:        Senior GIS Programmer
      Contact_Address
        Address_Type:  mailing address
        Address:            P.O. Box 201800
        City:               Helena
        State_or_Province:  Montana
        Postal_Code:        59620-1800
        Country:            USA
      Contact_Voice_Telephone:          (406) 444-5358
      Contact_Facsimile_Telephone:      (406) 444-0581
      Contact_Electronic_Mail_Address:  gdaumiller@mt.gov
      Hours_of_Service:  Monday-Friday, 8-5, Mountain Time
  Distribution_Liability:
    Users must assume responsibility to determine the
    usability of this data for their purposes.
  Standard_Order_Process
    Non-digital_Form:
      Contact the State Library to see if the data is
      available as hardcopy maps.
    Fees:
      For-profit organizations must pay our costs to reproduce the
      data.  Fees can be waived if doing Government work.
  Standard_Order_Process
    Digital_Form
      Digital_Transfer_Information
        Format_Name:            Arc/Info Export
      Digital_Transfer_Option
        Online_Option
          Computer_Contact_Information
            Network_Address
              Network_Resource_Name:   http://nris.mt.gov/nsdi/nris/e00/ab19.zip
      Digital_Transfer_Option
        Offline_Option
          Offline_Media:     CD-ROM
          Recording_Format:  ISO 9660
    Digital_Form
      Digital_Transfer_Information
        Format_Name:     ESRI Shapefile
      Digital_Transfer_Option
        Online_Option
          Computer_Contact_Information
            Network_Address
              Network_Resource_Name:   http://nris.mt.gov/nsdi/nris/shape/ab19.zip
      Digital_Transfer_Option
        Offline_Option
          Offline_Media:     CD-ROM
          Recording_Format:  ISO 9660
    Fees:
      For-profit organizations must pay our costs to reproduce the
      data.  Fees can be waived if doing Government work.
 
Metadata_Reference_Information:
  Metadata_Date:  19970415
  Metadata_Review_Date:  19970822
  Metadata_Contact
    Contact_Information
      Contact_Organization_Primary
        Contact_Organization:  Montana State Library
        Contact_Person:        Gerry Daumiller
      Contact_Address
        Address_Type:  mailing address
        Address:            P.O. Box 201800
        City:               Helena
        State_or_Province:  Montana
        Postal_Code:        59620-1800
        Country:            USA
      Contact_Voice_Telephone:          (406) 444-5358
      Contact_Facsimile_Telephone:      (406) 444-0581
      Contact_Electronic_Mail_Address:  gdaumiller@mt.gov
      Hours_of_Service:  Monday-Friday, 8-5, Mountain Time
  Metadata_Standard_Name:  FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version:  19940608
