Identification_Information
  Citation
    Citation_Information
      Originator:        Montana State Library
      Publication_Date:  19920205
      Title:             Upper Clark Fork Roads from 1:24,000 scale U.S.G.S quadrangles
      Geospatial_Data_Presentation_Form:  map
      Publication_Information
        Publication_Place:  Helena, Montana
        Publisher:          Montana State Library
      Online_Linkage: http://nris.mt.gov/nsdi/nris/e00/rd14.zip
      Online_Linkage: http://nris.mt.gov/nsdi/nris/shape/rd14.zip
  Description
    Abstract:
        Roads from 1:24,000 scale U.S. Geological Survey quad-
        rangles, Upper Clark Fork Basin, Montana  The quadrangles have
        been joined into a single data set, but have not been edgematched.
        The USGS major and minor attribute codes have been replaced with
        the codes shown in this metadata record.
        See http://nris.mt.gov/nsdi/nris/cf7.dbf for dates of
        the source quadrangles.
    Purpose:
        Base map data.
  Time_Period_of_Content
    Time_Period_Information
      Range_of_Dates/Times
        Beginning_Date:  19610101
        Ending_Date:     19890101
    Currentness_Reference:  Publication Date
  Status
    Progress:  Complete
    Maintenance_and_Update_Frequency:  Unknown
  Spatial_Domain
    Bounding_Coordinates
      West_Bounding_Coordinate:   -114.036621
      East_Bounding_Coordinate:   -112.298790
      North_Bounding_Coordinate:  47.0591507
      South_Bounding_Coordinate:  45.7052574
    Data_Set_G-Polygon
      Data_Set_G-Polygon_Outer_G-Ring
        G-Ring_Latitude:   47.0114
        G-Ring_Longitude:  -113.7422
        G-Ring_Latitude:   46.8907
        G-Ring_Longitude:  -113.728
        G-Ring_Latitude:   46.8877
        G-Ring_Longitude:  -113.2671
        G-Ring_Latitude:   47.0059
        G-Ring_Longitude:  -113.2614
        G-Ring_Latitude:   47.0045
        G-Ring_Longitude:  -113.1074
        G-Ring_Latitude:   46.8863
        G-Ring_Longitude:  -113.1134
        G-Ring_Latitude:   46.8838
        G-Ring_Longitude:  -112.9877
        G-Ring_Latitude:   46.7531
        G-Ring_Longitude:  -112.9885
        G-Ring_Latitude:   46.7533
        G-Ring_Longitude:  -112.8771
        G-Ring_Latitude:   46.6325
        G-Ring_Longitude:  -112.8649
        G-Ring_Latitude:   46.6301
        G-Ring_Longitude:  -112.6102
        G-Ring_Latitude:   46.136
        G-Ring_Longitude:  -112.6095
        G-Ring_Latitude:   46.1385
        G-Ring_Longitude:  -112.5179
        G-Ring_Latitude:   46.2568
        G-Ring_Longitude:  -112.5061
        G-Ring_Latitude:   46.2606
        G-Ring_Longitude:  -112.3592
        G-Ring_Latitude:   46.1363
        G-Ring_Longitude:  -112.3572
        G-Ring_Latitude:   46.1329
        G-Ring_Longitude:  -112.2378
        G-Ring_Latitude:   45.996
        G-Ring_Longitude:  -112.231
        G-Ring_Latitude:   45.9925
        G-Ring_Longitude:  -112.368
        G-Ring_Latitude:   45.8684
        G-Ring_Longitude:  -112.3615
        G-Ring_Latitude:   45.8676
        G-Ring_Longitude:  -112.7403
        G-Ring_Latitude:   45.7432
        G-Ring_Longitude:  -112.7421
        G-Ring_Latitude:   45.7452
        G-Ring_Longitude:  -112.8879
        G-Ring_Latitude:   45.8666
        G-Ring_Longitude:  -112.8817
        G-Ring_Latitude:   45.8659
        G-Ring_Longitude:  -113.0095
        G-Ring_Latitude:   45.9965
        G-Ring_Longitude:  -113.0133
        G-Ring_Latitude:   45.9928
        G-Ring_Longitude:  -113.1321
        G-Ring_Latitude:   46.1201
        G-Ring_Longitude:  -113.1406
        G-Ring_Latitude:   46.1225
        G-Ring_Longitude:  -113.26
        G-Ring_Latitude:   46.3683
        G-Ring_Longitude:  -113.254
        G-Ring_Latitude:   46.3646
        G-Ring_Longitude:  -113.6362
        G-Ring_Latitude:   46.5054
        G-Ring_Longitude:  -113.6239
        G-Ring_Latitude:   46.5068
        G-Ring_Longitude:  -113.4946
        G-Ring_Latitude:   46.3764
        G-Ring_Longitude:  -113.485
        G-Ring_Latitude:   46.3799
        G-Ring_Longitude:  -113.3839
        G-Ring_Latitude:   46.5045
        G-Ring_Longitude:  -113.379
        G-Ring_Latitude:   46.5
        G-Ring_Longitude:  -113.1292
        G-Ring_Latitude:   46.379
        G-Ring_Longitude:  -113.1211
        G-Ring_Latitude:   46.3858
        G-Ring_Longitude:  -113.0063
        G-Ring_Latitude:   46.4972
        G-Ring_Longitude:  -113.0135
        G-Ring_Latitude:   46.494
        G-Ring_Longitude:  -113.1149
        G-Ring_Latitude:   46.621
        G-Ring_Longitude:  -113.1327
        G-Ring_Latitude:   46.6217
        G-Ring_Longitude:  -113.7579
        G-Ring_Latitude:   46.7429
        G-Ring_Longitude:  -113.7582
        G-Ring_Latitude:   46.7473
        G-Ring_Longitude:  -114.1346
        G-Ring_Latitude:   47.009
        G-Ring_Longitude:  -114.1339
        G-Ring_Latitude:   47.0114
        G-Ring_Longitude:  -113.7422
  Keywords
    Theme
      Theme_Keyword_Thesaurus:  None
      Theme_Keyword:  Road
      Theme_Keyword:  Highway
      Theme_Keyword:  Trail
      Theme_Keyword:  Street
    Place
      Place_Keyword_Thesaurus:  None
      Place_Keyword:  Montana
  Access_Constraints:
        None
  Use_Constraints:
        Not for use at scales greater than 1:24000.
  Point_of_Contact
    Contact_Information
      Contact_Organization_Primary
        Contact_Organization:  Montana State Library
        Contact_Person:        Gerry Daumiller
      Contact_Position:        Senior GIS Programmer
      Contact_Address
        Address_Type:  mailing address
        Address:            P.O. Box 201800
        City:               Helena
        State_or_Province:  Montana
        Postal_Code:        59620-1800
        Country:            USA
      Contact_Voice_Telephone:          (406) 444-5358
      Contact_Facsimile_Telephone:      (406) 444-0581
      Contact_Electronic_Mail_Address:  gdaumiller@mt.gov
      Hours_of_Service:  Monday-Friday, 8-5, Mountain Time
  Browse_Graphic
    Browse_Graphic_File_Name:  http://nris.mt.gov/nsdi/nris/rd14.gif
    Browse_Graphic_File_Description:
      Simple image of the data set and/or its extent.
    Browse_Graphic_File_Type:  gif
  Native_Data_Set_Environment:
      Arc/Info coverage or ESRI Shapefile

 
Data_Quality_Information:
  Attribute_Accuracy
    Attribute_Accuracy_Report:
        Attributes were interpreted from the original DLG files by
        a computer program.  The accuracy of this interpretation
        has not been extensively checked.  Attribute accuracy of the
        original Digital Line Graph data is estimated by the USGS
        at 98.5 percent, and was tested by them as follows:
        - manual comparison of the source with hard copy plots.
        - symbolized display of the digital line graph on an
        interactive compter graphic system.
        - Selected attributes that could not be visually verified on
        plots or on screen, were interactively queried and verified
        on screen.
        In addition, U.S. Geological Survey  (USGS) Production
        System (PROSYS) software tested the attributes against a
        master set of valid attributes for the category; it also
        checked for selected valid attribute combinations, and for
        valid attributes relative to topology and dimensionality.
        All attribute data conform to the attribute codes current
        as of the date of digitizing.
  Logical_Consistency_Report:
        Arc-node topology exist.
  Completeness_Report:
        For DLG data, Digital Revision Status = Not revised:
        Data completeness reflects the content of the source
        quadrangle.  Features may have been eliminated or
        generalized on the source graphic, due to scale and
        legibility constraints.
        For DLG data, Digital Revision Status = Limited Update:
        This file has undergone limited update digital revision.
        The file contains only (1) those features that are
        photoidentifiable on monoscopic source, supplemented with
        limited ancillary source, and (2) those features, present on
        the original source quadrangle, that can not be reliably
        photoidentified but that are not considered particularly
        prone to change.
        For DLG data, Digital Revision Status = Standard Update:
        This file has undergone standard update digital revision.
        The data completeness of this file meets National Mapping
        Division standards for feature content.
  Positional_Accuracy
    Horizontal_Positional_Accuracy
      Horizontal_Positional_Accuracy_Report:
        Approximate accuracy is 12 meters, assuming the source maps
        meet National Map Accuracy Standards (NMAS).  NMAS
        horizontal accuracy requires that at least 90 percent of
        points tested are within 0.02 inches of the true position.
        The digital data are estimated to contain a horizontal
        positional error of less than or equal to 0.003 inches
        standard error in the two component directions relative to
        the source quadrangle.  Comparison to the graphic source is
        used as control to assess digital positional accuracy.
        Cartographic offsets may be present on the graphic source,
        due to scale and legibility constraints.  Digital map
        elements require edge alignment between data sets.  Data
        along each quadrangle edge are tested against the data set
        for the adjacent quadrangle using PROSYS; tests check for
        positional accuracy between data sets within a 0.02 inches
        tolerance.  Features with like dimensionality, and with or
        without like attribution, that are within the tolerance
        are adjusted by moving the feature equally in both data
        sets.  Features outside the tolerance are not moved.
  Lineage
    Source_Information
      Source_Citation
        Citation_Information
          Originator:
            National Mapping Division
            U.S. Geological Survey
          Publication_Date:  19610101
          Title:  1:24,000-scale Digital Line Graphs
          Geospatial_Data_Presentation_Form:  map
          Publication_Information
            Publication_Place:  Reston, VA
            Publisher:  U.S. Geological Survey
          Other_Citation_Details:
            See /montana/dlg24k/quaddates for the publication dates of
            the various quadrangles.
      Source_Scale_Denominator:  24000
      Type_of_Source_Media:  unknown
      Source_Time_Period_of_Content
        Time_Period_Information
          Range_of_Dates/Times
            Beginning_Date:  19610101
            Ending_Date:     19890101
        Source_Currentness_Reference:  Publication Date
      Source_Citation_Abbreviation:  Q7.5
      Source_Contribution:
          The data set is a re-processed copy of this source.
    Process_Step
      Process_Description:
        Interpret USGS attributes, project quadrangles to State Plane
        Coordinates, and join quadrangles into one data set.
      Source_Used_Citation_Abbreviation:  Q7.5
      Process_Date:  19920205
      Source_Produced_Citation_Abbreviation:  fin1
    Process_Step
      Process_Description:
        Import additional quadrangles and append to the data that
        was imported in 1992.
      Source_Used_Citation_Abbreviation:  fin1
      Source_Used_Citation_Abbreviation:  Q7.5
      Process_Date:  19970414
      Source_Produced_Citation_Abbreviation:  fin2
 
Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method:  Vector
  Point_and_Vector_Object_Information
    SDTS_Terms_Description
      SDTS_Point_and_Vector_Object_Type:  Complete Chain
      Point_and_Vector_Object_Count:   17134
 
Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition
    Planar
      Grid_Coordinate_System
        Grid_Coordinate_System_Name: State Plane Coordinate System 1983
        State_Plane_Coordinate_System
          SPCS_Zone_Identifier: 2500
          Lambert_Conformal_Conic
            Standard_Parallel:  45
            Standard_Parallel:  49
            Longitude_of_Central_Meridian:  -109.5
            Latitude_of_Projection_Origin:  44.25
            False_Easting:   600000.00000
            False_Northing:  0.00000
      Planar_Coordinate_Information
        Planar_Coordinate_Encoding_Method:  coordinate pair
        Coordinate_Representation
          Abscissa_Resolution:  .1
          Ordinate_Resolution:  .1
        Planar_Distance_Units:  meters
    Geodetic_Model
      Horizontal_Datum_Name:  North American Datum of 1983
      Ellipsoid_Name:   Geodetic Reference System 80
      Semi-major_Axis:  6378137
      Denominator_of_Flattening_Ratio:  298.257
 
Entity_and_Attribute_Information:
  Detailed_Description
    Entity_Type
      Entity_Type_Label:  ROAD.AAT
      Entity_Type_Definition:  Arc Attribute Table
      Entity_Type_Definition_Source:  None
    Attribute
      Attribute_Label:  CODE
      Attribute_Definition:
        Road type code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  50
          Enumerated_Domain_Value_Definition:  Interchange
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  51
          Enumerated_Domain_Value_Definition:  Interchange, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  61
          Enumerated_Domain_Value_Definition:  Cul-de-sac
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  100
          Enumerated_Domain_Value_Definition:  Class 1 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  102
          Enumerated_Domain_Value_Definition:  Class 1 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  103
          Enumerated_Domain_Value_Definition:  Class 1 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  110
          Enumerated_Domain_Value_Definition:  Divided Class 1 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  112
          Enumerated_Domain_Value_Definition:  Divided Class 1 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  113
          Enumerated_Domain_Value_Definition:  Divided Class 1 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  120
          Enumerated_Domain_Value_Definition:  Separated Class 1 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  122
          Enumerated_Domain_Value_Definition:  Separated Class 1 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  123
          Enumerated_Domain_Value_Definition:  Separated Class 1 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  130
          Enumerated_Domain_Value_Definition:  One-Way Class 1 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  200
          Enumerated_Domain_Value_Definition:  Class 2 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  202
          Enumerated_Domain_Value_Definition:  Class 2 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  203
          Enumerated_Domain_Value_Definition:  Class 2 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  220
          Enumerated_Domain_Value_Definition:  Separated Class 2 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  300
          Enumerated_Domain_Value_Definition:  Class 3 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  302
          Enumerated_Domain_Value_Definition:  Class 3 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  303
          Enumerated_Domain_Value_Definition:  Class 3 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  304
          Enumerated_Domain_Value_Definition:  Class 3 Road, Arbitrary Closure
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  310
          Enumerated_Domain_Value_Definition:  Divided Class 3 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  312
          Enumerated_Domain_Value_Definition:  Divided Class 3 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  313
          Enumerated_Domain_Value_Definition:  Divided Class 3 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  340
          Enumerated_Domain_Value_Definition:  Traffic Circle, Class 3
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  360
          Enumerated_Domain_Value_Definition:  Rest Area, Class 3
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  400
          Enumerated_Domain_Value_Definition:  Class 4 Road
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  401
          Enumerated_Domain_Value_Definition:  Class 4 Road in Tunnel
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  402
          Enumerated_Domain_Value_Definition:  Class 4 Road, Overpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  403
          Enumerated_Domain_Value_Definition:  Class 4 Road, Underpassing
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  500
          Enumerated_Domain_Value_Definition:  Trail
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  570
          Enumerated_Domain_Value_Definition:  Old Railroad Grade
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  571
          Enumerated_Domain_Value_Definition:  Old Railroad Grade in Tunnel
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  580
          Enumerated_Domain_Value_Definition:  Four-Wheel Drive Trail
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  601
          Enumerated_Domain_Value_Definition:  Footbridge
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  602
          Enumerated_Domain_Value_Definition:  Non-Standard Road
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  ROUTE
      Attribute_Definition:
        List of route names
          This attribute was based on USGS attribute codes and has
          been updated at the State Library.  For example, an arc that
          carries Interstate 90, U.S. 12, and Montana 43 would have
          "I90 US12 MT43" as its ROUTE attribute.
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Unrepresentable_Domain:  Character field
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19970401
    Attribute
      Attribute_Label:  RVIS
      Attribute_Definition:
        Photorevision code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  0
          Enumerated_Domain_Value_Definition:  Not photorevised
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  1
          Enumerated_Domain_Value_Definition:  Photorevised
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  2
          Enumerated_Domain_Value_Definition:  Estimated location or attributes
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  OTHR
      Attribute_Definition:
        Co-incident feature type code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  B
          Enumerated_Domain_Value_Definition:  Boundary
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  H
          Enumerated_Domain_Value_Definition:  Hydrography
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  M
          Enumerated_Domain_Value_Definition:  Man-made feature
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  T
          Enumerated_Domain_Value_Definition:  Miscellaneous Transportation
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  U
          Enumerated_Domain_Value_Definition:  U.S. Public Land Survey line
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  X
          Enumerated_Domain_Value_Definition:  Unknown
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  LANE
      Attribute_Definition:
        Number of Traffic Lanes
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  Any number
          Enumerated_Domain_Value_Definition:  Number of traffic lanes
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  T
          Enumerated_Domain_Value_Definition:  Transition area
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
    Attribute
      Attribute_Label:  WDTH
      Attribute_Definition:
        Roadway Width code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  A
          Enumerated_Domain_Value_Definition:  46-55 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  B
          Enumerated_Domain_Value_Definition:  56-65 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  C
          Enumerated_Domain_Value_Definition:  66-75 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  D
          Enumerated_Domain_Value_Definition:  76-85 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  E
          Enumerated_Domain_Value_Definition:  86-95 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  F
          Enumerated_Domain_Value_Definition:  69-105 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  G
          Enumerated_Domain_Value_Definition:  106-115 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  H
          Enumerated_Domain_Value_Definition:  116-125 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  I
          Enumerated_Domain_Value_Definition:  126-135 feet
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  J
          Enumerated_Domain_Value_Definition:  136-145 feet
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
  Detailed_Description
    Entity_Type
      Entity_Type_Label:  ROAD.NAT
      Entity_Type_Definition:  Node Attribute Table
      Entity_Type_Definition_Source:  None
    Attribute
      Attribute_Label:  CODE
      Attribute_Definition:
        Road node type code
      Attribute_Definition_Source:  None
      Attribute_Domain_Values
        Enumerated_Domain
          Enumerated_Domain_Value:  1
          Enumerated_Domain_Value_Definition:  Bridge Abutment
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  2
          Enumerated_Domain_Value_Definition:  Tunnel Portal
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  5
          Enumerated_Domain_Value_Definition:  Cul-de-sac
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  6
          Enumerated_Domain_Value_Definition:  Dead end
          Enumerated_Domain_Value_Definition_Source:  none
          Enumerated_Domain_Value:  11
          Enumerated_Domain_Value_Definition:  Bridge Abutment-Photorevised
          Enumerated_Domain_Value_Definition_Source:  none
      Beginning_Date_of_Attribute_Values:  19610101
      Ending_Date_of_Attribute_Values:  19900101
 
Distribution_Information:
  Distributor
    Contact_Information
      Contact_Organization_Primary
        Contact_Organization:  Montana State Library
        Contact_Person:        Gerry Daumiller
      Contact_Position:        Senior GIS Programmer
      Contact_Address
        Address_Type:  mailing address
        Address:            P.O. Box 201800
        City:               Helena
        State_or_Province:  Montana
        Postal_Code:        59620-1800
        Country:            USA
      Contact_Voice_Telephone:          (406) 444-5358
      Contact_Facsimile_Telephone:      (406) 444-0581
      Contact_Electronic_Mail_Address:  gdaumiller@mt.gov
      Hours_of_Service:  Monday-Friday, 8-5, Mountain Time
  Distribution_Liability:
    Users must assume responsibility to determine the
    usability of this data for their purposes.
  Standard_Order_Process
    Non-digital_Form:
      Contact the State Library to see if the data is
      available as hardcopy maps.
    Fees:
      For-profit organizations must pay our costs to reproduce the
      data.  Fees can be waived if doing Government work.
  Standard_Order_Process
    Digital_Form
      Digital_Transfer_Information
        Format_Name:            Arc/Info Export
      Digital_Transfer_Option
        Online_Option
          Computer_Contact_Information
            Network_Address
              Network_Resource_Name:   http://nris.mt.gov/nsdi/nris/e00/rd14.zip
      Digital_Transfer_Option
        Offline_Option
          Offline_Media:     CD-ROM
          Recording_Format:  ISO 9660
    Digital_Form
      Digital_Transfer_Information
        Format_Name:     ESRI Shapefile
      Digital_Transfer_Option
        Online_Option
          Computer_Contact_Information
            Network_Address
              Network_Resource_Name:   http://nris.mt.gov/nsdi/nris/shape/rd14.zip
      Digital_Transfer_Option
        Offline_Option
          Offline_Media:     CD-ROM
          Recording_Format:  ISO 9660
    Fees:
      For-profit organizations must pay our costs to reproduce the
      data.  Fees can be waived if doing Government work.
 
Metadata_Reference_Information:
  Metadata_Date:  19970730
  Metadata_Review_Date:  19970731
  Metadata_Contact
    Contact_Information
      Contact_Organization_Primary
        Contact_Organization:  Montana State Library
        Contact_Person:        Gerry Daumiller
      Contact_Address
        Address_Type:  mailing address
        Address:            P.O. Box 201800
        City:               Helena
        State_or_Province:  Montana
        Postal_Code:        59620-1800
        Country:            USA
      Contact_Voice_Telephone:          (406) 444-5358
      Contact_Facsimile_Telephone:      (406) 444-0581
      Contact_Electronic_Mail_Address:  gdaumiller@mt.gov
      Hours_of_Service:  Monday-Friday, 8-5, Mountain Time
  Metadata_Standard_Name:  FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version:  19940608
